(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 50.8 50.8)
    (grid_origin 50.8 50.8)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(COM2-Pin_1-Pad1)")
  (net 2 "unconnected-(COM2-Pin_4-Pad4)")
  (net 3 "unconnected-(COM2-Pin_6-Pad6)")
  (net 4 "unconnected-(COM2-Pin_7-Pad7)")
  (net 5 "unconnected-(COM2-Pin_8-Pad8)")
  (net 6 "unconnected-(COM2-Pin_9-Pad9)")
  (net 7 "unconnected-(COM2-Pin_10-Pad10)")
  (net 8 "unconnected-(COM3-Pin_1-Pad1)")
  (net 9 "unconnected-(COM3-Pin_4-Pad4)")
  (net 10 "unconnected-(COM3-Pin_6-Pad6)")
  (net 11 "unconnected-(COM3-Pin_7-Pad7)")
  (net 12 "unconnected-(COM3-Pin_8-Pad8)")
  (net 13 "unconnected-(COM3-Pin_9-Pad9)")
  (net 14 "unconnected-(COM3-Pin_10-Pad10)")
  (net 15 "/UART1_RX")
  (net 16 "/UART1_TX")
  (net 17 "/UART1_GND")
  (net 18 "/UART2_RX")
  (net 19 "/UART2_TX")
  (net 20 "/UART2_GND")
  (net 21 "/UART3_RX")
  (net 22 "/UART3_TX")
  (net 23 "/UART3_GND")
  (net 24 "unconnected-(CCOM1-Pin_1-Pad1)")
  (net 25 "unconnected-(CCOM1-Pin_2-Pad2)")
  (net 26 "unconnected-(CCOM1-Pin_7-Pad7)")
  (net 27 "unconnected-(CCOM1-Pin_8-Pad8)")
  (net 28 "unconnected-(CCOM1-Pin_11-Pad11)")
  (net 29 "unconnected-(CCOM1-Pin_12-Pad12)")
  (net 30 "unconnected-(CCOM1-Pin_13-Pad13)")
  (net 31 "unconnected-(CCOM1-Pin_14-Pad14)")
  (net 32 "unconnected-(CCOM1-Pin_15-Pad15)")
  (net 33 "unconnected-(CCOM1-Pin_16-Pad16)")
  (net 34 "unconnected-(CCOM1-Pin_17-Pad17)")
  (net 35 "unconnected-(CCOM1-Pin_18-Pad18)")
  (net 36 "unconnected-(CCOM1-Pin_22-Pad22)")
  (net 37 "unconnected-(CPWR1-Pin_14-Pad14)")
  (net 38 "unconnected-(CPWR1-Pin_1-Pad1)")
  (net 39 "/+12V")
  (net 40 "/GND")
  (net 41 "/+5V")
  (net 42 "unconnected-(COM4-Pin_9-Pad9)")
  (net 43 "unconnected-(COM4-Pin_8-Pad8)")
  (net 44 "unconnected-(COM4-Pin_7-Pad7)")
  (net 45 "unconnected-(COM4-Pin_6-Pad6)")
  (net 46 "unconnected-(COM4-Pin_4-Pad4)")
  (net 47 "unconnected-(COM4-Pin_10-Pad10)")
  (net 48 "unconnected-(COM4-Pin_1-Pad1)")
  (footprint "Connector_Molex:Molex_Mini-Fit_Jr_5566-14A_2x07_P4.20mm_Vertical" (layer "F.Cu")
    (at 53.9 79.8975 90)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5566-14A, example for new mpn: 39-28-x14x, 7 Pins per row, Mounting:  (http://www.molex.com/pdm_docs/sd/039281043_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr side entry")
    (property "Sheetfile" "ALLS-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x07, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "CPWR1" (at 27.179 8.382 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x07_Top_Bottom" (at 12.6 9.95 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 12.6 -1.55 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.09259296296)
      (net 38 "unconnected-(CPWR1-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 4.2 0 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 40 "/GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 8.4 0 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 40 "/GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 12.6 0 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 40 "/GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 16.8 0 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 40 "/GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 21 0 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 40 "/GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 25.2 0 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 40 "/GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 5.5 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 39 "/+12V") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 4.2 5.5 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 39 "/+12V") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 8.4 5.5 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 39 "/+12V") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 12.6 5.5 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 41 "/+5V") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 16.8 5.5 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 41 "/+5V") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 21 5.5 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 41 "/+5V") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 25.2 5.5 90) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(CPWR1-Pin_14-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5566-14A_2x07_P4.20mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XAD_B22B-XADSS-1_2x11_P2.50mm_Vertical" (layer "F.Cu")
    (at 75.4125 79.7975 90)
    (descr "JST XA series connector, B11B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XA vertical")
    (property "Sheetfile" "ALLS-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x11, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "CCOM1" (at 26.779 -4.9275 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x11_Odd_Even" (at 12.5 4.4 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 12.5 1.5 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 25 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 24 "unconnected-(CCOM1-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 25 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(CCOM1-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 22.5 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 15 "/UART1_RX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 22.5 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 18 "/UART2_RX") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 20 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 16 "/UART1_TX") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 20 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 19 "/UART2_TX") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 17.5 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(CCOM1-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 17.5 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(CCOM1-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 15 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 17 "/UART1_GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 15 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 20 "/UART2_GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 12.5 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(CCOM1-Pin_11-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 12.5 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(CCOM1-Pin_12-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 10 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(CCOM1-Pin_13-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 10 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(CCOM1-Pin_14-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 7.5 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(CCOM1-Pin_15-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 7.5 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 33 "unconnected-(CCOM1-Pin_16-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 5 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 34 "unconnected-(CCOM1-Pin_17-Pad17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 35 "unconnected-(CCOM1-Pin_18-Pad18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 2.5 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 21 "/UART3_RX") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 22 "/UART3_TX") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 2.5 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 23 "/UART3_GND") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(CCOM1-Pin_22-Pad22)") (pinfunction "Pin_22") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XA_B11B-XASK-1_1x11_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" (layer "B.Cu")
    (at 75.46 145.66875)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
    (property "Sheetfile" "ALLS-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "COM4" (at -4.5 -5 90) (layer "B.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.27 -16.26) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 48 "unconnected-(COM4-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/UART3_RX") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/UART3_TX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(COM4-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "/UART3_GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(COM4-Pin_6-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(COM4-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(COM4-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(COM4-Pin_9-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(COM4-Pin_10-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" (layer "B.Cu")
    (at 75.46 123.2025)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
    (property "Sheetfile" "ALLS-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "COM3" (at -4.5 -5 90) (layer "B.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.27 -16.26) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 8 "unconnected-(COM3-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/UART2_RX") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "/UART2_TX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(COM3-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "/UART2_GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(COM3-Pin_6-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(COM3-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(COM3-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(COM3-Pin_9-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(COM3-Pin_10-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" (layer "B.Cu")
    (at 75.46 100.73625)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
    (property "Sheetfile" "ALLS-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "COM2" (at -4.5 -5 90) (layer "B.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 15.24 -4.572) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 1 "unconnected-(COM2-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "/UART1_RX") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "/UART1_TX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "unconnected-(COM2-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "/UART1_GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "unconnected-(COM2-Pin_6-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "unconnected-(COM2-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "unconnected-(COM2-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "unconnected-(COM2-Pin_9-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "unconnected-(COM2-Pin_10-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_TE-Connectivity:TE_MATE-N-LOK_350211-1_1x04_P5.08mm_Vertical" (layer "B.Cu")
    (at 57.8325 95.170416 -90)
    (descr "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F350211%7FU5%7Fpdf%7FEnglish%7FENG_CD_350211_U5.pdf%7F350211-1")
    (tags "connector TE MATE-N-LOK top entry ATA PATA IDE 5.25 inch floppy drive power")
    (property "Sheetfile" "ALLS-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "PWR1" (at -5.39 4.4925 90) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x04_Pin" (at 7.62 -5.01 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 8 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.78 2.78) (drill 1.78) (layers "*.Cu" "*.Mask")
      (net 39 "/+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 2.78 2.78) (drill 1.78) (layers "*.Cu" "*.Mask")
      (net 40 "/GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 10.16 0 270) (size 2.78 2.78) (drill 1.78) (layers "*.Cu" "*.Mask")
      (net 40 "/GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 15.24 0 270) (size 2.78 2.78) (drill 1.78) (layers "*.Cu" "*.Mask")
      (net 41 "/+5V") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_TE-Connectivity.3dshapes/TE_MATE-N-LOK_350211-1_1x04_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_TE-Connectivity:TE_MATE-N-LOK_350211-1_1x04_P5.08mm_Vertical" (layer "B.Cu")
    (at 57.8325 125.834582 -90)
    (descr "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F350211%7FU5%7Fpdf%7FEnglish%7FENG_CD_350211_U5.pdf%7F350211-1")
    (tags "connector TE MATE-N-LOK top entry ATA PATA IDE 5.25 inch floppy drive power")
    (property "Sheetfile" "ALLS-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "PWR2" (at -5.3475 4.4925 90) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x04_Pin" (at 7.62 -5.01 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 8 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.78 2.78) (drill 1.78) (layers "*.Cu" "*.Mask")
      (net 39 "/+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 2.78 2.78) (drill 1.78) (layers "*.Cu" "*.Mask")
      (net 40 "/GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 10.16 0 270) (size 2.78 2.78) (drill 1.78) (layers "*.Cu" "*.Mask")
      (net 40 "/GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 15.24 0 270) (size 2.78 2.78) (drill 1.78) (layers "*.Cu" "*.Mask")
      (net 41 "/+5V") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_TE-Connectivity.3dshapes/TE_MATE-N-LOK_350211-1_1x04_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line locked (start 50.8 50.8) (end 50.8 152.4)
    (layer "Edge.Cuts"))
  (gr_line locked (start 82.55 50.8) (end 82.55 152.4)
    (layer "Edge.Cuts"))
  (gr_line locked (start 50.8 152.4) (end 82.55 152.4)
    (layer "Edge.Cuts"))
  (gr_line locked (start 50.8 50.8) (end 82.55 50.8)
    (layer "Edge.Cuts"))
  (zone (net 41) (net_name "/+5V") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 0.4064))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 57.15 57.404)
        (xy 57.15 141.986)
        (xy 69.85 141.986)
        (xy 69.85 57.404)
      )
    )
  )
  (zone locked (net 0) (net_name "") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour allowed) (footprints not_allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 63.5 50.8)
        (xy 69.85 50.8)
        (xy 69.85 152.4)
        (xy 63.5 152.4)
      )
    )
  )
  (zone locked (net 40) (net_name "/GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 50.8 50.8)
        (xy 82.55 50.8)
        (xy 82.55 152.4)
        (xy 50.8 152.4)
      )
    )
  )
  (zone (net 39) (net_name "/+12V") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads yes (clearance 0.4064))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 57.15 126.746)
        (xy 57.15 69.85)
        (xy 69.85 69.85)
        (xy 69.85 126.746)
      )
    )
  )
)
