(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 34)
    (no_connects 0)
    (area 146.483722 91.592599 164.401501 111.91038)
    (thickness 1.6)
    (drawings 28)
    (tracks 146)
    (zones 0)
    (modules 20)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.508)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.762)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 3)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 149.2 112.75)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01008_00000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +3V3)
  (net 5 "Net-(C4-Pad1)")
  (net 6 /SDA)
  (net 7 /SCL)
  (net 8 /RESET)
  (net 9 /INT)
  (net 10 "Net-(R5-Pad2)")
  (net 11 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2032)
    (via_dia 0.889)
    (via_drill 0.508)
    (uvia_dia 0.762)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net /INT)
    (add_net /RESET)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad2)")
  )
  (module MyFootprints:castle_pad (layer B.Cu) (tedit 59440CF4)
    (at 161.9 93.065)
    (fp_text reference REF** (at 0 -4.55) (layer B.SilkS))
    (fp_text value castle_pad (at 0 4.55) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 3) (layers B.Cu B.Paste B.Mask))
  )
  (module MyFootprints:castle_pad (layer B.Cu) (tedit 59440CF4)
    (at 159.36 93.065)
    (fp_text reference REF** (at 0 -4.55) (layer B.SilkS))
    (fp_text value castle_pad (at 0 4.55) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 3) (layers B.Cu B.Paste B.Mask))
  )
  (module MyFootprints:castle_pad (layer B.Cu) (tedit 59440CF4)
    (at 156.82 93.065)
    (fp_text reference REF** (at 0 -4.55) (layer B.SilkS))
    (fp_text value castle_pad (at 0 4.55) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 3) (layers B.Cu B.Paste B.Mask))
  )
  (module MyFootprints:castle_pad (layer B.Cu) (tedit 59440CF4)
    (at 154.28 93.065)
    (fp_text reference REF** (at 0 -4.55) (layer B.SilkS))
    (fp_text value castle_pad (at 0 4.55) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 3) (layers B.Cu B.Paste B.Mask))
  )
  (module MyFootprints:castle_pad (layer B.Cu) (tedit 59440CF4)
    (at 151.74 93.065)
    (fp_text reference REF** (at 0 -4.55) (layer B.SilkS))
    (fp_text value castle_pad (at 0 4.55) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 3) (layers B.Cu B.Paste B.Mask))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5651304F)
    (at 149.2 101.32 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.7526 -0.0254 270) (layer F.SilkS))
    (fp_text value 10k (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 56513054)
    (at 149.2 98.78)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.775 0 90) (layer F.SilkS))
    (fp_text value 10k (at 2.54 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 158.175 109.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.0674 -1.4212 180) (layer F.SilkS))
    (fp_text value 22pF (at -3.275 0.025 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Footprints:LGA28 (layer F.Cu) (tedit 5650F004)
    (at 156.5 103.7125 180)
    (fp_text reference U1 (at -0.3 2.5875 180) (layer F.SilkS))
    (fp_text value BNO055 (at -0.32 2.3925 180) (layer F.Fab))
    (pad 20 smd rect (at 2.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDA))
    (pad 21 smd rect (at 1.75 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 0.75 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 0.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at -0.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at -0.75 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 27 smd rect (at -1.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 28 smd rect (at -1.75 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 1 smd rect (at -2.25 -1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 1.75 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 9 /INT))
    (pad 13 smd rect (at 1.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 0.75 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (pad 10 smd rect (at -0.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -0.75 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 8 smd rect (at -1.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -1.75 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.25 1.5625 180) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 2.3125 -0.75 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL))
    (pad 18 smd rect (at 2.3125 -0.25 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 2.3125 0.25 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad1)"))
    (pad 16 smd rect (at 2.3125 0.75 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.3125 -0.75 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.3125 -0.25 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 4 smd rect (at -2.3125 0.25 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (pad 5 smd rect (at -2.3125 0.75 180) (size 0.375 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model "C:/Users/BSI/Google Drive/Kicad/Kicad Projects/BNO055 Breakout - Teensy/Cut.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 154.9 109.475)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.0866 1.4208) (layer F.SilkS))
    (fp_text value 22pF (at -3 0.075) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 565144FA)
    (at 160.35 105.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0.4484 -1.4484 270) (layer F.SilkS))
    (fp_text value 100nF (at 0.55 -1.55 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 565144EF)
    (at 160.375 102.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.114 -1.3726 270) (layer F.SilkS))
    (fp_text value 100nF (at -1.13 -1.525 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565144D7)
    (at 149.2 106.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.675 0 90) (layer F.SilkS))
    (fp_text value 10k (at 2.54 -0.1) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565144D1)
    (at 149.2 103.86)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.7 -0.025 90) (layer F.SilkS))
    (fp_text value 10k (at 2.54 -0.05) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Footprints:ABS07-XTAL (layer F.Cu) (tedit 565217F4)
    (at 156.675 107.2)
    (tags CRYSTAL)
    (fp_text reference Y1 (at 2.875 0.575) (layer F.SilkS))
    (fp_text value Crystal (at 0 0.47) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model "C:/Users/BSI/Google Drive/Kicad/Kicad Projects/BNO055 Breakout - Teensy/Cube.wrl"
      (at (xyz -0.065 -0.03 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 59440602)
    (at 149.2 94.97 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -2.6416 13.1826 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 2.54 7.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SDA))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SCL))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /RESET))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /INT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 163.17 104.38 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.3502 0.1016 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Graphics:small_bsi_logo (layer F.Cu) (tedit 0)
    (at 150.8764 108.9146)
    (fp_text reference G*** (at -24.9428 -2.6416) (layer F.SilkS) hide)
    (fp_text value LOGO (at -24.3078 0.7112) (layer F.SilkS) hide)
  )
  (module MyFootprints:castle_pad (layer B.Cu) (tedit 59440CF4)
    (at 149.2 93.065)
    (fp_text reference REF** (at 0 -4.55) (layer B.SilkS))
    (fp_text value castle_pad (at 0 4.55) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 3) (layers B.Cu B.Paste B.Mask))
  )
  (module MyFootprints:axis_labels (layer F.Cu) (tedit 0)
    (at 153.4926 99.3642 180)
    (fp_text reference G*** (at 21.4884 3.302 180) (layer F.SilkS) hide)
    (fp_text value LOGO (at 20.8534 1.0668 180) (layer F.SilkS) hide)
  )
  (gr_line (start 147.5236 91.6426) (end 163.361623 91.6426) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.361623 91.6426) (end 163.747644 91.716288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.747644 91.716288) (end 164.062209 91.917428) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.062209 91.917428) (end 164.27395 92.216244) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.27395 92.216244) (end 164.3515 92.582964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.3515 92.582964) (end 164.3515 110.920014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.3515 110.920014) (end 164.27395 111.286762) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.27395 111.286762) (end 164.062209 111.585579) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.062209 111.585579) (end 163.747644 111.78669) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.747644 111.78669) (end 163.361623 111.860379) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.361623 111.860379) (end 147.5236 111.860379) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.5236 111.860379) (end 147.137579 111.78669) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.137579 111.78669) (end 146.823015 111.585579) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.823015 111.585579) (end 146.611273 111.286762) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.611273 111.286762) (end 146.533723 110.920014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.533723 110.920014) (end 146.533723 92.582964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.533723 92.582964) (end 146.611273 92.216244) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.611273 92.216244) (end 146.823015 91.917428) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.823015 91.917428) (end 147.137579 91.716288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.137579 91.716288) (end 147.5236 91.6426) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.5236 91.6426) (end 147.5236 91.6426) (layer Edge.Cuts) (width 0.1))
  (gr_text "EME IMU v1.1\nCopyright 2017" (at 155.4992 108.6352) (layer B.SilkS))
  (gr_text INT (at 161.9 93.065) (layer F.SilkS))
  (gr_text RST (at 159.36 93.065) (layer F.SilkS))
  (gr_text SCL (at 156.82 93.065) (layer F.SilkS))
  (gr_text SDA (at 154.28 93.065) (layer F.SilkS))
  (gr_text GND (at 151.74 93.065) (layer F.SilkS))
  (gr_text 3V3 (at 149.2 93.065) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.2696 95.0208) (xy 163.5002 95.0208) (xy 163.5002 110.972) (xy 147.4474 110.972) (xy 147.4474 95.0208)
        (xy 147.4474 95.0208)
      )
    )
  )
)
