(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.10.1)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 19)
    (zones 0)
    (modules 7)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(R1-Pad2)")
  (net 6 "Net-(R2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5D59E083)
    (at 127 61.8)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D1 (at 0 -1.05) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5D59E087)
    (at 121.1 61.8)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D2 (at 0 -1.05) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D2-Pad1)"))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5D59E08E)
    (at 126.9 79 270)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.05 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.05 270) (layer F.Fab))
    (fp_text user %R (at 0 -0.68 270) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5D59E09B)
    (at 119.9 77.2 270)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.05 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.05 270) (layer F.Fab))
    (fp_text user %R (at 0 -0.68 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D2-Pad1)"))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_2Pads_Pitch2.54mm_Drill0.8mm (layer F.Cu) (tedit 5D59E093)
    (at 127 88.6 90)
    (descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference TP1 (at 1.3 -2 90) (layer F.SilkS) hide)
    (fp_text value TestPoint_2Pole (at 1.27 2 90) (layer F.Fab))
    (fp_text user %R (at 1.3 -2 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
  )
  (module TestPoint:TestPoint_2Pads_Pitch2.54mm_Drill0.8mm (layer F.Cu) (tedit 5D59E097)
    (at 119.8 88.7)
    (descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference TP2 (at 1.3 -2) (layer F.SilkS) hide)
    (fp_text value TestPoint_2Pole (at 1.27 2) (layer F.Fab))
    (fp_text user %R (at 1.3 -2) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(R2-Pad2)"))
  )
  (module misc_footprints:makho (layer B.Cu) (tedit 5CEA0DD7)
    (at 121.1 75.4 90)
    (fp_text reference REF** (at -3 -4 90) (layer B.SilkS) hide)
    (fp_text value makho (at 0 3.25 90) (layer B.Fab))
  )
  (gr_text "For use with \nAIO V1 GBC Kit" (at 126.9 72.2 90) (layer B.Cu))
  (gr_line (start 125.1 90) (end 128.7 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.1 60) (end 128.7 60) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.7 90) (end 128.7 60) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.1 90) (end 125.1 60) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.1 60) (end 118 60) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.1 90) (end 124.1 60) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118 90) (end 124.1 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118 60) (end 118 90) (layer Edge.Cuts) (width 0.15))
)
