(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~52~ubuntu17.04.1)
  (general
    (links 8)
    (no_connects 0)
    (area 133.909999 92.040528 149.4016 112.991901)
    (thickness 1.6)
    (drawings 5)
    (tracks 32)
    (zones 0)
    (modules 2)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4064)
    (via_drill 0.254)
    (via_min_size 0.4064)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory svg_v1.1/))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad1)")
  (net 2 "Net-(IC1-Pad2)")
  (net 3 "Net-(IC1-Pad7)")
  (net 4 "Net-(IC1-Pad8)")
  (net 5 "Net-(IC1-Pad3)")
  (net 6 "Net-(IC1-Pad4)")
  (net 7 "Net-(IC1-Pad6)")
  (net 8 "Net-(IC1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.4064)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
  )
  (module "Madbean 40xx-2:DIL08" (layer F.Cu) (tedit 595BDFA5)
    (at 139.192 97.536 270)
    (descr "<b>Dual In Line Package</b>")
    (fp_text reference IC1 (at 0.508 1.27 360) (layer F.SilkS))
    (fp_text value TL072 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -3.81 2.2225 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad8)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad6)"))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad5)"))
  )
  (module headers:8-PIN (layer F.Cu) (tedit 595BDF93)
    (at 145.542 102.616 90)
    (fp_text reference SIL1 (at -6.35 -2.159 90) (layer F.SilkS) hide)
    (fp_text value SIL8 (at 0 2.413 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -8.89 -2.032 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole circle (at 3.81 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole circle (at 6.35 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad8)"))
  )
  (gr_text "DIP-8\nto\nSIL-8" (at 138.176 112.141 90) (layer F.SilkS))
  (gr_line (start 133.985 112.903) (end 146.939 112.903) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.985 92.329) (end 133.985 112.903) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.939 92.329) (end 133.985 92.329) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.939 112.903) (end 146.939 92.329) (angle 90) (layer Edge.Cuts) (width 0.15))
)
