(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 15)
    (zones 0)
    (modules 11)
    (nets 10)
  )
  (page A)
  (title_block
    (title "Audio Attenuator")
    (rev 2)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.1524)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 "Net-(J1-Pad11)")
  (net 3 "Net-(J1-Pad10)")
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J2-Pad3)")
  (net 6 "Net-(J2-Pad11)")
  (net 7 "Net-(J2-Pad10)")
  (net 8 "Net-(J2-Pad2)")
  (net 9 /GND)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
  )
  (module label (layer B.Cu) (tedit 614ADC34)
    (at 140.716 97.917 180)
    (descr "Converted using: scripting")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference kibuzzard-614ADC34 (at 0 0.844) (layer B.SilkS) hide)
    (fp_text value G*** (at 0 -0.844) (layer B.SilkS) hide)
  )
  (module label (layer B.Cu) (tedit 614AD392)
    (at 148.59 103.124 180)
    (descr "Converted using: scripting")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference kibuzzard-614AD392 (at 0 1.025901) (layer B.SilkS) hide)
    (fp_text value G*** (at 0 -1.025901) (layer B.SilkS) hide)
  )
  (module label (layer B.Cu) (tedit 614AD37E)
    (at 132.461 103.124 180)
    (descr "Converted using: scripting")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference kibuzzard-614AD37E (at 0 1.020344) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 -1.020344) (layer F.SilkS) hide)
  )
  (module label (layer F.Cu) (tedit 614AD03C)
    (at 132.207 102.997)
    (descr "Converted using: scripting")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference kibuzzard-614AD03C (at 0 -1.020344) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 1.020344) (layer F.SilkS) hide)
  )
  (module label (layer F.Cu) (tedit 614ACF93)
    (at 148.844 102.997)
    (descr "Converted using: scripting")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference kibuzzard-614ACF93 (at 0 -1.025901) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 1.025901) (layer F.SilkS) hide)
  )
  (module SJ1-3525N:CUI_SJ1-3525N (layer F.Cu) (tedit 61461C01)
    (at 122.174 100.584)
    (fp_text reference J1 (at 8.509 -1.778) (layer F.SilkS))
    (fp_text value INPUT (at -2.54 -8.128) (layer F.Fab) hide)
    (pad None np_thru_hole circle (at 0 5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at -2.5 5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 5 0) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 0 -5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at -2.5 -5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 5 -5) (size 2.616 1.308) (drill oval 1.5 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 11 thru_hole oval (at 5 -2.5) (size 2.616 1.308) (drill oval 1.5 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 5 2.5) (size 2.616 1.308) (drill oval 1.5 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad10)"))
    (pad 2 thru_hole oval (at 5 5) (size 2.616 1.308) (drill oval 1.5 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 1 thru_hole oval (at 0 0) (size 1.308 2.616) (drill oval 0.8 1.5) (layers *.Cu *.Mask)
      (net 9 /GND))
    (model ${KIPRJMOD}/libraries/SJ1-3525N/CUI_DEVICES_SJ1-3525N.step
      (offset (xyz -6.5 0 2.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SJ1-3525N:CUI_SJ1-3525N (layer F.Cu) (tedit 61461C01)
    (at 159.258 100.584 180)
    (fp_text reference J2 (at 8.509 1.778 180) (layer F.SilkS))
    (fp_text value OUTPUT (at 5.207 8.128 180) (layer F.Fab))
    (pad None np_thru_hole circle (at 0 5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at -2.5 5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 5 0 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 0 -5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at -2.5 -5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 5 -5 180) (size 2.616 1.308) (drill oval 1.5 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 11 thru_hole oval (at 5 -2.5 180) (size 2.616 1.308) (drill oval 1.5 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 5 2.5 180) (size 2.616 1.308) (drill oval 1.5 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad10)"))
    (pad 2 thru_hole oval (at 5 5 180) (size 2.616 1.308) (drill oval 1.5 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.308 2.616) (drill oval 0.8 1.5) (layers *.Cu *.Mask)
      (net 9 /GND))
    (model ${KIPRJMOD}/libraries/SJ1-3525N/CUI_DEVICES_SJ1-3525N.step
      (offset (xyz -6.5 0 2.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 149.606 95.504 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 6.35 -2.37) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 141.986 105.664)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 1.27 -2.286) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 139.446 105.664 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 1.27 2.286) (layer F.SilkS))
    (fp_text value 1k (at 3.81 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 139.446 95.504 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 1.27 -2.286) (layer F.SilkS))
    (fp_text value 1k (at 3.81 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "By Todd Eddy" (at 124.333 100.457 90) (layer B.SilkS))
  (gr_text git.io/JzR8k (at 140.589 99.822) (layer B.SilkS))
  (gr_text "v2 2021-09-24" (at 156.972 100.584 90) (layer B.SilkS))
  (gr_line (start 163.83 93.218) (end 163.83 98.552) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.602 93.218) (end 163.83 93.218) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.602 98.552) (end 117.602 93.218) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.872 98.552) (end 117.602 98.552) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.872 102.616) (end 118.872 98.552) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.602 102.616) (end 118.872 102.616) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.602 107.95) (end 117.602 102.616) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.83 107.95) (end 117.602 107.95) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.83 102.616) (end 163.83 107.95) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.56 102.616) (end 163.83 102.616) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.56 98.552) (end 162.56 102.616) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.83 98.552) (end 162.56 98.552) (layer Edge.Cuts) (width 0.1))
  (zone (net 9) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.83 107.95) (xy 117.602 107.95) (xy 117.602 93.218) (xy 163.83 93.218)
      )
    )
  )
)
