(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 263)
    (tracks 92)
    (zones 0)
    (modules 3)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.05)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.1 1.1)
    (pad_drill 0.5)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 L1_7)
  (net 2 L1_8)
  (net 3 L1_5)
  (net 4 L1_6)
  (net 5 L1_3)
  (net 6 L1_4)
  (net 7 L1_1)
  (net 8 L1_2)
  (net 9 L2_7)
  (net 10 L2_8)
  (net 11 L2_5)
  (net 12 L2_6)
  (net 13 L2_3)
  (net 14 L2_4)
  (net 15 L2_1)
  (net 16 L2_2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net L1_1)
    (add_net L1_2)
    (add_net L1_3)
    (add_net L1_4)
    (add_net L1_5)
    (add_net L1_6)
    (add_net L1_7)
    (add_net L1_8)
    (add_net L2_1)
    (add_net L2_2)
    (add_net L2_3)
    (add_net L2_4)
    (add_net L2_5)
    (add_net L2_6)
    (add_net L2_7)
    (add_net L2_8)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 94 89 90)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x08_Odd_Even (at 1.3 21.22 90) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 L1_1))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 L1_2))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 L1_3))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 L1_4))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 L2_1))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 L2_2))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 L2_3))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 L2_4))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 L1_5))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 L1_6))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 L1_7))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 L1_8))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 L2_5))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 L2_6))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 L2_7))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 L2_8))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coil_Footprints:SCoil_L1_9mils_manual (layer F.Cu) (tedit 5BAA34B0)
    (at 152.4346 87.50568 180)
    (fp_text reference L1 (at -0.11 11.76 180) (layer F.SilkS) hide)
    (fp_text value Coil_9mils (at -0.05 -13.64 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.93 -9.1 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 L1_1))
    (pad 2 thru_hole circle (at -2.74 9.11 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 L1_2))
    (pad 3 thru_hole circle (at -4.23 -9.1 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 L1_3))
    (pad 4 thru_hole circle (at -1.05 9.11 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 L1_4))
    (pad 5 thru_hole circle (at 0.91 -9.1 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 L1_5))
    (pad 6 thru_hole circle (at 4.12 9.14 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 L1_6))
    (pad 7 thru_hole circle (at 2.62 -9.11 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 L1_7))
    (pad 8 thru_hole circle (at 5.79 9.11 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 L1_8))
  )
  (module Coil_Footprints:SCoil_L2_9mils_manual (layer F.Cu) (tedit 5BA9F570)
    (at 152.75654 87.486402 180)
    (fp_text reference L2 (at -0.08 -15.79 180) (layer F.SilkS) hide)
    (fp_text value Coil_9mils (at 0.16 -13.26 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.61 -9.12 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 15 L2_1))
    (pad 2 thru_hole circle (at -5.79 9.1 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 16 L2_2))
    (pad 3 thru_hole circle (at -0.92 -9.1 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 13 L2_3))
    (pad 4 thru_hole circle (at -4.11 9.11 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 14 L2_4))
    (pad 5 thru_hole circle (at 4.25 -9.12 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 L2_5))
    (pad 6 thru_hole circle (at 1.06 9.09 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 L2_6))
    (pad 7 thru_hole circle (at 5.94 -9.12 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 L2_7))
    (pad 8 thru_hole circle (at 2.75 9.09 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 L2_8))
  )
  (gr_circle (center 135.41 80.42) (end 136.51 80.42) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 145.4 70.42) (end 146.5 70.42) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 169.59 80.42) (end 170.69 80.42) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 159.58 104.59) (end 160.68 104.59) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 169.59 94.58) (end 170.69 94.58) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 145.41 104.59) (end 146.51 104.59) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 135.41 94.59) (end 136.51 94.59) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 159.58 70.4) (end 160.68 70.4) (layer Edge.Cuts) (width 0.15))
  (gr_text "Purdue MSRAL Serpentine Coil V2" (at 173.33 87.5 90) (layer F.SilkS))
  (gr_circle (center 165.6 100.6) (end 166.7 100.6) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 139.4 100.6) (end 140.5 100.6) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 139.4 74.4) (end 140.5 74.4) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 165.6 74.4) (end 166.7 74.4) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 152.5 106) (end 153.6 106) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 152.5 69) (end 153.6 69) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 134 87.5) (end 135.1 87.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 171 87.5) (end 172.1 87.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175 65) (end 90 65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175 110) (end 175 65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90 110) (end 175 110) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90 65) (end 90 110) (layer Edge.Cuts) (width 0.15))
)
