(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 123)
    (zones 0)
    (modules 51)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 "Net-(C7-Pad1)")
  (net 9 "Net-(C8-Pad1)")
  (net 10 "Net-(C9-Pad1)")
  (net 11 "Net-(C10-Pad1)")
  (net 12 "Net-(J4-Pad13)")
  (net 13 "Net-(J4-Pad7)")
  (net 14 "Net-(J4-Pad6)")
  (net 15 "Net-(J4-Pad5)")
  (net 16 "Net-(J4-Pad4)")
  (net 17 "Net-(J4-Pad3)")
  (net 18 "Net-(J4-Pad2)")
  (net 19 "Net-(J4-Pad1)")
  (net 20 "Net-(J1-Pad2)")
  (net 21 "Net-(J2-Pad2)")
  (net 22 "Net-(J3-Pad2)")
  (net 23 "Net-(P2-Pad1)")
  (net 24 "Net-(P3-Pad1)")
  (net 25 "Net-(P4-Pad1)")
  (net 26 "Net-(P5-Pad1)")
  (net 27 "Net-(P6-Pad1)")
  (net 28 "Net-(P7-Pad1)")
  (net 29 "Net-(P13-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad13)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(P13-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P7-Pad1)")
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 278.765 28.9598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J4-Pad7)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 281.305 28.9598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J4-Pad6)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 283.845 28.9598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J4-Pad5)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 286.385 28.9598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J4-Pad4)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 288.925 28.9598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J4-Pad3)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 268.9606 23.4188 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P7-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 271.5006 23.4188 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P6-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 274.0406 23.4188 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(P5-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 276.5806 23.4188 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 279.1206 23.4188 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 266.065 28.9598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value C (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 268.605 28.9598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value C (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 271.145 28.9598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value C (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 273.685 28.9598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value C (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 276.225 28.9598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value C (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 285.4706 23.4188 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value C (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 288.0106 23.4188 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value C (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 295.6306 23.4188 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value C (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 290.5506 23.4188 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value C (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 293.0906 23.4188 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value C (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7D09AD)
    (at 286.349 32.5374)
    (attr smd)
    (fp_text reference P21 (at 0 -1.27) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.27) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.762 1) (layers F.Cu F.Mask)
      (net 16 "Net-(J4-Pad4)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7D09AD)
    (at 273.7358 32.5628)
    (attr smd)
    (fp_text reference P16 (at 0 -1.27) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.27) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.762 1) (layers F.Cu F.Mask)
      (net 8 "Net-(C7-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7D09AD)
    (at 276.2504 32.512)
    (attr smd)
    (fp_text reference P15 (at 0 -1.27) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.27) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.762 1) (layers F.Cu F.Mask)
      (net 7 "Net-(C6-Pad1)"))
  )
  (module myfootprints:SMA-cinch-142-0701-851 (layer F.Cu) (tedit 5E7D7554)
    (at 290.88715 11.9878 180)
    (descr 142-0701-851)
    (tags Connector)
    (attr smd)
    (fp_text reference J3 (at -2.566 0.809) (layer F.SilkS))
    (fp_text value 142-0701-851 (at -2.566 0.809) (layer F.SilkS) hide)
    (fp_text user %R (at -2.566 0.809) (layer F.Fab))
    (pad 3 smd rect (at 2.19075 4.19 180) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.19075 4.19 180) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad2)"))
    (pad 1 smd rect (at -6.57225 4.19 180) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model /Users/smb2/Documents/PCB/Kicad/Footprints.pretty/3D/SMA-cinch-edge-142-0701-851.stp
      (offset (xyz -2.0574 -6.985000000000001 0.2286))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myfootprints:SMA-cinch-142-0701-851 (layer F.Cu) (tedit 5E7D7554)
    (at 277.26005 11.9878 180)
    (descr 142-0701-851)
    (tags Connector)
    (attr smd)
    (fp_text reference J2 (at -2.566 0.809) (layer F.SilkS))
    (fp_text value 142-0701-851 (at -2.566 0.809) (layer F.SilkS) hide)
    (fp_text user %R (at -2.566 0.809) (layer F.Fab))
    (pad 3 smd rect (at 2.19075 4.19 180) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.19075 4.19 180) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -6.57225 4.19 180) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model /Users/smb2/Documents/PCB/Kicad/Footprints.pretty/3D/SMA-cinch-edge-142-0701-851.stp
      (offset (xyz -2.0574 -6.985000000000001 0.2286))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myfootprints:SMA-cinch-142-0701-851 (layer F.Cu) (tedit 5E7D7554)
    (at 263.35355 11.9624 180)
    (descr 142-0701-851)
    (tags Connector)
    (attr smd)
    (fp_text reference J1 (at -2.566 0.809) (layer F.SilkS))
    (fp_text value 142-0701-851 (at -2.566 0.809) (layer F.SilkS) hide)
    (fp_text user %R (at -2.566 0.809) (layer F.Fab))
    (pad 3 smd rect (at 2.19075 4.19 180) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.19075 4.19 180) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -6.57225 4.19 180) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model /Users/smb2/Documents/PCB/Kicad/Footprints.pretty/3D/SMA-cinch-edge-142-0701-851.stp
      (offset (xyz -2.0574 -6.985000000000001 0.2286))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 287.3502 27.2542)
    (attr smd)
    (fp_text reference P14 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 19 "Net-(J4-Pad1)"))
  )
  (module myfootprints:MicroD-25-M-upsidedown (layer F.Cu) (tedit 5E7D06EB)
    (at 283.1724 37.9984 270)
    (fp_text reference J4 (at -2.54 19.05) (layer F.SilkS))
    (fp_text value MicroD-25-M (at -3.81 3.8354) (layer F.Fab))
    (pad 26 thru_hole circle (at 2.54 -8.445 270) (size 2.79 2.79) (drill 2.79) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at 2.54 16.065 270) (size 2.79 2.79) (drill 2.79) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 1.27 -3.17 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole circle (at 1.27 -1.9 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 16 thru_hole circle (at 1.27 -0.63 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 17 thru_hole circle (at 1.27 0.64 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 18 thru_hole circle (at 1.27 1.91 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 19 thru_hole circle (at 1.27 3.18 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 20 thru_hole circle (at 1.27 4.45 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 21 thru_hole circle (at 1.27 5.72 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 22 thru_hole circle (at 1.27 6.99 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 23 thru_hole circle (at 1.27 8.26 270) (size 0.7112 0.7112) (drill 0.7112) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 24 thru_hole circle (at 1.27 9.53 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 25 thru_hole circle (at 1.27 10.8 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.27 -3.81 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J4-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 -2.54 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J4-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 -1.27 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J4-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 0 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J4-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 1.27 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J4-Pad5)"))
    (pad 6 thru_hole circle (at -1.27 2.54 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J4-Pad6)"))
    (pad 7 thru_hole circle (at -1.27 3.81 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J4-Pad7)"))
    (pad 8 thru_hole circle (at -1.27 5.08 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C6-Pad1)"))
    (pad 9 thru_hole circle (at -1.27 6.35 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C7-Pad1)"))
    (pad 10 thru_hole circle (at -1.27 7.62 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C8-Pad1)"))
    (pad 11 thru_hole circle (at -1.27 8.89 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C9-Pad1)"))
    (pad 12 thru_hole circle (at -1.27 10.16 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C10-Pad1)"))
    (pad 13 thru_hole circle (at -1.27 11.43 270) (size 0.71 0.71) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J4-Pad13)"))
    (model /Users/smb2/Documents/PCB/Kicad/Footprints.pretty/3D/MicroD_381-025-112L565.STEP
      (offset (xyz 7.8486 -3.81 -5.181599999999999))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 90))
    )
  )
  (module myfootprints:SOT65P210X110-3N (layer F.Cu) (tedit 5E7BCFFD)
    (at 294.3606 31.877 90)
    (descr DMN62D0UW-7-1)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q2 (at 0 0 90) (layer F.SilkS))
    (fp_text value DMN62D0UW-7 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at -1 0.65 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.65 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J4-Pad1)"))
    (model DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${DMN}/DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:SOT65P210X110-3N (layer F.Cu) (tedit 5E7BCFFD)
    (at 263.0264 22.718)
    (descr DMN62D0UW-7-1)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q1 (at 0 0) (layer F.SilkS))
    (fp_text value DMN62D0UW-7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P2-Pad1)"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P13-Pad1)"))
    (model DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${DMN}/DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 285.7754 23.241)
    (attr smd)
    (fp_text reference P25 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 18 "Net-(J4-Pad2)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 285.0896 40.132 180)
    (attr smd)
    (fp_text reference P24 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62 180) (size 0.762 1) (layers F.Cu F.Mask)
      (net 13 "Net-(J4-Pad7)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 287.655 40.132 180)
    (attr smd)
    (fp_text reference P23 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62 180) (size 0.762 1) (layers F.Cu F.Mask)
      (net 14 "Net-(J4-Pad6)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 290.195 40.1574 180)
    (attr smd)
    (fp_text reference P22 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62 180) (size 0.762 1) (layers F.Cu F.Mask)
      (net 15 "Net-(J4-Pad5)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 295.275 40.0812 180)
    (attr smd)
    (fp_text reference P20 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62 180) (size 0.762 1) (layers F.Cu F.Mask)
      (net 17 "Net-(J4-Pad3)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 272.4912 40.2082 180)
    (attr smd)
    (fp_text reference P19 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62 180) (size 0.762 1) (layers F.Cu F.Mask)
      (net 11 "Net-(C10-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 274.955 40.1828 180)
    (attr smd)
    (fp_text reference P18 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62 180) (size 0.762 1) (layers F.Cu F.Mask)
      (net 10 "Net-(C9-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 277.495 40.1828 180)
    (attr smd)
    (fp_text reference P17 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62 180) (size 0.762 1) (layers F.Cu F.Mask)
      (net 9 "Net-(C8-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 255.4986 12.7508)
    (attr smd)
    (fp_text reference P13 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 29 "Net-(P13-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 279.1206 12.065)
    (attr smd)
    (fp_text reference P12 (at 5.0292 6.0452) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 6 "Net-(C5-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 281.6606 12.0396)
    (attr smd)
    (fp_text reference P11 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 5 "Net-(C4-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 289.2806 12.065)
    (attr smd)
    (fp_text reference P10 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 284.2006 12.065)
    (attr smd)
    (fp_text reference P9 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 286.7406 12.065)
    (attr smd)
    (fp_text reference P8 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 262.5852 12.0396)
    (attr smd)
    (fp_text reference P7 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 28 "Net-(P7-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 265.1506 12.065)
    (attr smd)
    (fp_text reference P6 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 27 "Net-(P6-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 267.6906 12.065)
    (attr smd)
    (fp_text reference P5 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 26 "Net-(P5-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 270.2306 12.0396)
    (attr smd)
    (fp_text reference P4 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 25 "Net-(P4-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 272.7706 12.065)
    (attr smd)
    (fp_text reference P3 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 24 "Net-(P3-Pad1)"))
  )
  (module myfootprints:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 259.8166 15.24)
    (attr smd)
    (fp_text reference P2 (at 5.1816 6.1468) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 23 "Net-(P2-Pad1)"))
  )
  (module myfootprints:wirebond-3 (layer F.Cu) (tedit 5E7CF830)
    (at 287.2994 22.4282 180)
    (fp_text reference P1 (at 3.81 7.62) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5.08 6.35) (layer F.Fab))
    (pad 3 smd rect (at 8.89 7.62 180) (size 0.762 1) (layers F.Cu F.Mask)
      (net 20 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 7.62 7.62 180) (size 0.762 1) (layers F.Cu F.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at 6.35 7.62 180) (size 0.762 1) (layers F.Cu F.Mask)
      (net 22 "Net-(J3-Pad2)"))
  )
  (gr_line (start 259.0038 5.1816) (end 259.0038 45.8978) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 299.593 5.1816) (end 259.0038 5.1816) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 299.593 45.9232) (end 299.593 5.1816) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 259.0038 45.9232) (end 299.593 45.9232) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 299.7835 36.068) (xy 259.1181 36.068) (xy 258.87045 5.3594) (xy 299.53585 5.3594)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 259.3086 5.4356) (xy 299.1866 5.4356) (xy 299.1866 45.593) (xy 259.3086 45.593) (xy 259.2578 5.3848)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 299.1358 45.4914) (xy 259.4864 45.4914) (xy 259.4864 5.842) (xy 259.5118 5.8166) (xy 299.1358 5.8166)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 301.7012 49.3014) (xy 256.0066 49.3014) (xy 256.0066 3.302) (xy 301.7012 3.302)
      )
    )
  )
)
