(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 82)
    (zones 0)
    (modules 15)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 0.95)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FEFDFF7F)
    (pcbplotparams
      (layerselection 0x010ec_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 GND)
  (net 3 "Net-(J1-Pad1)")
  (net 4 /SERIAL_IN)
  (net 5 /DATA)
  (net 6 "Net-(R1-Pad2)")
  (net 7 "Net-(J4-Pad1)")
  (net 8 "Net-(D1-PadA)")
  (net 9 "Net-(D1-PadK)")
  (net 10 "Net-(D2-PadA)")
  (net 11 "Net-(D3-PadA)")
  (net 12 "Net-(D2-PadK)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DATA)
    (add_net /SERIAL_IN)
    (add_net GND)
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(D1-PadK)")
    (add_net "Net-(D2-PadA)")
    (add_net "Net-(D2-PadK)")
    (add_net "Net-(D3-PadA)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (module board:DC-DC (layer F.Cu) (tedit 5CFC2447)
    (at 147.32 76.2 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference U2 (at -3.81 -3.81 180) (layer F.SilkS))
    (fp_text value "TBA 2-2411" (at 6.2 3.025 180) (layer F.Fab))
    (pad 4 thru_hole circle (at 12.7 -4.9 180) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-PadA)"))
    (pad 3 thru_hole circle (at 7.62 -4.9 180) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 -4.9 180) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-PadK)"))
    (pad 2 thru_hole circle (at 2.54 -4.9 180) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module board:Diode (layer F.Cu) (tedit 5CFC24A7)
    (at 147.955 84.455)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference D1 (at 3.81 -1.86) (layer F.SilkS))
    (fp_text value 1N5817 (at 3.81 1.86) (layer F.Fab))
    (pad K thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-PadK)"))
    (pad A thru_hole circle (at 7.62 0) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-PadA)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module board:Diode (layer F.Cu) (tedit 5CFC24A7)
    (at 119.38 76.2)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference D2 (at 1.27 2.032) (layer F.SilkS))
    (fp_text value 1N5817 (at 3.81 1.86) (layer F.Fab))
    (pad K thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-PadK)"))
    (pad A thru_hole circle (at 7.62 0) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-PadA)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module board:Diode (layer F.Cu) (tedit 5CFC24A7)
    (at 119.38 81.28)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference D3 (at 4.572 -1.86) (layer F.SilkS))
    (fp_text value 1N5817 (at 3.81 1.86) (layer F.Fab))
    (pad K thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-PadK)"))
    (pad A thru_hole circle (at 7.62 0) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-PadA)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module board:Connector_4 (layer F.Cu) (tedit 5CFC33A0)
    (at 127 105.41 270)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference J1 (at 2.54 10.16) (layer F.SilkS))
    (fp_text value Connector_01x04_Male (at 2.27 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 /SERIAL_IN))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-104-X-XX_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module board:Connector_4 (layer F.Cu) (tedit 5CFC33D8)
    (at 139.065 105.41 270)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference J2 (at -3.175 8.255) (layer F.SilkS))
    (fp_text value Connector_01x04_Male (at 2.27 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 /SERIAL_IN))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-104-X-XX_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module board:Connector_3 (layer F.Cu) (tedit 5CFC33EF)
    (at 148.59 105.41 270)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference J3 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value Connector_01x03_Male (at 2.27 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 /DATA))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-PadK)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-103-X-XX_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module board:Terminal-block (layer F.Cu) (tedit 5CFC2350)
    (at 154.305 94.615 90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J4 (at 8.001 -4.699 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_x02 (at 2.54 5.08 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-PadA)"))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module board:Resistor (layer F.Cu) (tedit 5CFC2501)
    (at 155.575 99.695 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 -1.905 180) (layer F.SilkS))
    (fp_text value 1k (at 3.81 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 /SERIAL_IN))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module board:Resistor (layer F.Cu) (tedit 5CFC2501)
    (at 147.955 95.885 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 -1.86 90) (layer F.SilkS))
    (fp_text value 10k (at 3.81 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-PadK)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module board:TEENSY-LC (layer F.Cu) (tedit 5CFC25A9)
    (at 111.125 100.33)
    (fp_text reference U1 (at 0.635 -17.78) (layer F.SilkS))
    (fp_text value Teensy-LC (at -6.35 7.62) (layer F.Fab))
    (fp_text user "before installing!!!" (at 13.8 -5) (layer F.SilkS))
    (fp_text user "Teensy LC" (at 10.395 -11.125) (layer F.SilkS))
    (fp_text user "at bottom of the Teensy LC" (at 17.2 -7.2) (layer F.SilkS))
    (fp_text user "Must cut VIN/VUSB link trace" (at 18.015 -9.22) (layer F.SilkS))
    (pad 19 thru_hole circle (at 33.02 -12.7) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 33.02 -2.54) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 /DATA))
    (pad 34 thru_hole circle (at 2.54 -12.7) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-PadA)"))
    (pad 32 thru_hole circle (at 2.54 -15.24) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 33 thru_hole circle (at 0 -15.24) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-PadK)"))
    (pad 20 thru_hole circle (at 33.02 -15.24) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 33.02 0) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module board:Mounting-hole (layer F.Cu) (tedit 5CFC00C0)
    (at 113.03 105.41)
    (fp_text reference H1 (at 0 0.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module board:Mounting-hole (layer F.Cu) (tedit 5CFC00C0)
    (at 113.03 77.47)
    (fp_text reference H2 (at 0 0.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module board:Mounting-hole (layer F.Cu) (tedit 5CFC00C0)
    (at 154.94 105.41)
    (fp_text reference H3 (at 0 0.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module board:Mounting-hole (layer F.Cu) (tedit 5CFC00C0)
    (at 154.94 77.47)
    (fp_text reference H4 (at 0 0.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "Rev 1.0" (at 142.748 100.838) (layer B.SilkS))
  (gr_text "Status Monitor for Duet3D " (at 142.748 96.774) (layer B.SilkS))
  (gr_text + (at 157.48 85.725 90) (layer F.SilkS))
  (gr_text - (at 157.48 98.425 90) (layer F.SilkS))
  (gr_text "Isolated DC/DC\nInput voltage -> 5VDC" (at 130.81 76.835) (layer F.SilkS))
  (dimension 49.53 (width 0.3) (layer F.SilkS)
    (gr_text "1.9500 in" (at 133.985 116.399999) (layer F.SilkS))
    (feature1 (pts (xy 158.75 106.045) (xy 158.75 114.88642)))
    (feature2 (pts (xy 109.22 106.045) (xy 109.22 114.88642)))
    (crossbar (pts (xy 109.22 114.299999) (xy 158.75 114.299999)))
    (arrow1a (pts (xy 158.75 114.299999) (xy 157.623496 114.88642)))
    (arrow1b (pts (xy 158.75 114.299999) (xy 157.623496 113.713578)))
    (arrow2a (pts (xy 109.22 114.299999) (xy 110.346504 114.88642)))
    (arrow2b (pts (xy 109.22 114.299999) (xy 110.346504 113.713578)))
  )
  (dimension 35.56 (width 0.3) (layer F.SilkS)
    (gr_text "1.4000 in" (at 167.2 91.44 270) (layer F.SilkS))
    (feature1 (pts (xy 154.94 109.22) (xy 165.686421 109.22)))
    (feature2 (pts (xy 154.94 73.66) (xy 165.686421 73.66)))
    (crossbar (pts (xy 165.1 73.66) (xy 165.1 109.22)))
    (arrow1a (pts (xy 165.1 109.22) (xy 164.513579 108.093496)))
    (arrow1b (pts (xy 165.1 109.22) (xy 165.686421 108.093496)))
    (arrow2a (pts (xy 165.1 73.66) (xy 164.513579 74.786504)))
    (arrow2b (pts (xy 165.1 73.66) (xy 165.686421 74.786504)))
  )
  (gr_arc (start 154.94 77.47) (end 158.75 77.47) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 154.94 105.41) (end 154.94 109.22) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 113.03 105.41) (end 109.22 105.41) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 113.03 77.47) (end 113.03 73.66) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 109.22 77.47) (end 109.22 105.41) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 154.94 73.66) (end 113.03 73.66) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 158.75 105.41) (end 158.75 77.47) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 113.03 109.22) (end 154.94 109.22) (layer Edge.Cuts) (width 0.127))
)
