(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~61~ubuntu18.04.1)
  (general
    (links 266)
    (no_connects 25)
    (area 123.139999 100.279999 156.260001 118.160001)
    (thickness 1.6)
    (drawings 10)
    (tracks 1051)
    (zones 0)
    (modules 87)
    (nets 77)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (trace_clearance 0.127)
    (zone_clearance 0.127)
    (zone_45_only yes)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.1 1.2)
    (pad_drill 0.75)
    (pad_to_mask_clearance 0.03)
    (pad_to_paste_clearance -0.0125)
    (aux_axis_origin 0 0)
    (grid_origin 143.764 104.8385)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory V44))
  )
  (net 0 "")
  (net 1 BATT+)
  (net 2 BATT-)
  (net 3 Button1)
  (net 4 Button2)
  (net 5 Button3)
  (net 6 GND)
  (net 7 "Net-(C1-Pad2)")
  (net 8 3.3v)
  (net 9 "Net-(C7-Pad1)")
  (net 10 "Net-(C8-Pad1)")
  (net 11 5v)
  (net 12 vtest)
  (net 13 "Net-(C33-Pad1)")
  (net 14 RESET)
  (net 15 "Net-(C61-Pad1)")
  (net 16 VBUS)
  (net 17 FREE1)
  (net 18 FREE2)
  (net 19 boost_en)
  (net 20 "Net-(IC3-Pad3)")
  (net 21 "Net-(IC3-Pad10)")
  (net 22 id-neopixel_data)
  (net 23 "Net-(LED1-Pad1)")
  (net 24 "Net-(LED2-Pad1)")
  (net 25 "Net-(LED3-Pad1)")
  (net 26 "Net-(LED4-Pad1)")
  (net 27 "Net-(LED5-Pad1)")
  (net 28 "Net-(LED6-Pad1)")
  (net 29 neopixel_data2)
  (net 30 neopixel_data3)
  (net 31 CH1)
  (net 32 CH2)
  (net 33 CH3)
  (net 34 CH4)
  (net 35 CH5)
  (net 36 CH6)
  (net 37 SDA)
  (net 38 SCL)
  (net 39 DP)
  (net 40 "Net-(R41-Pad2)")
  (net 41 DM)
  (net 42 "Net-(R42-Pad2)")
  (net 43 BTN)
  (net 44 sd_en)
  (net 45 amp_en)
  (net 46 RX)
  (net 47 miso)
  (net 48 sclk)
  (net 49 mosi)
  (net 50 "Net-(SP+1-Pad1)")
  (net 51 "Net-(SP-1-Pad1)")
  (net 52 SWDCLK)
  (net 53 SWDIO)
  (net 54 TX)
  (net 55 INT)
  (net 56 I2S_LRCLK)
  (net 57 I2S_BCLK)
  (net 58 I2S_DATA)
  (net 59 "Net-(SD1-Pad8)")
  (net 60 "Net-(SD1-Pad9)")
  (net 61 "Net-(SD1-Pad10)")
  (net 62 "Net-(SD1-PadB)")
  (net 63 "Net-(SD1-Pad11)")
  (net 64 "Net-(SD1-Pad1)")
  (net 65 "Net-(SD1-Pad12)")
  (net 66 "Net-(SD1-PadA)")
  (net 67 "Net-(U0-Pad1)")
  (net 68 "Net-(U1-Pad5)")
  (net 69 "Net-(U1-Pad6)")
  (net 70 "Net-(U1-Pad12)")
  (net 71 "Net-(U1-Pad13)")
  (net 72 "Net-(U2-Pad9)")
  (net 73 "Net-(U2-Pad10)")
  (net 74 "Net-(U2-Pad11)")
  (net 75 "Net-(USB1-Pad4)")
  (net 76 "Net-(C5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BTN)
    (add_net Button1)
    (add_net Button2)
    (add_net Button3)
    (add_net CH1)
    (add_net CH2)
    (add_net CH3)
    (add_net CH4)
    (add_net CH5)
    (add_net CH6)
    (add_net DM)
    (add_net DP)
    (add_net FREE1)
    (add_net FREE2)
    (add_net I2S_BCLK)
    (add_net I2S_DATA)
    (add_net I2S_LRCLK)
    (add_net INT)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C33-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(IC3-Pad10)")
    (add_net "Net-(R41-Pad2)")
    (add_net "Net-(R42-Pad2)")
    (add_net "Net-(SD1-Pad1)")
    (add_net "Net-(SD1-Pad10)")
    (add_net "Net-(SD1-Pad11)")
    (add_net "Net-(SD1-Pad12)")
    (add_net "Net-(SD1-Pad8)")
    (add_net "Net-(SD1-Pad9)")
    (add_net "Net-(SD1-PadA)")
    (add_net "Net-(SD1-PadB)")
    (add_net "Net-(U0-Pad1)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(USB1-Pad4)")
    (add_net RESET)
    (add_net RX)
    (add_net SCL)
    (add_net SDA)
    (add_net SWDCLK)
    (add_net SWDIO)
    (add_net TX)
    (add_net amp_en)
    (add_net boost_en)
    (add_net id-neopixel_data)
    (add_net miso)
    (add_net mosi)
    (add_net neopixel_data2)
    (add_net neopixel_data3)
    (add_net sclk)
    (add_net sd_en)
    (add_net vtest)
  )
  (net_class LED ""
    (clearance 0.2)
    (trace_width 2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
    (add_net "Net-(LED3-Pad1)")
    (add_net "Net-(LED4-Pad1)")
    (add_net "Net-(LED5-Pad1)")
    (add_net "Net-(LED6-Pad1)")
  )
  (net_class Power ""
    (clearance 0.127)
    (trace_width 0.35)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3.3v)
    (add_net 5v)
    (add_net BATT+)
    (add_net BATT-)
    (add_net GND)
    (add_net "Net-(C61-Pad1)")
    (add_net "Net-(IC3-Pad3)")
    (add_net "Net-(SP+1-Pad1)")
    (add_net "Net-(SP-1-Pad1)")
    (add_net VBUS)
  )
  (module lightsaber_footprints:PTS810 (layer F.Cu) (tedit 5A4A7F57)
    (at 148.844 106.172 90)
    (fp_text reference SW1 (at 0 0.05 90) (layer F.SilkS))
    (fp_text value SW_Push (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 43 BTN))
    (pad 2 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 43 BTN))
    (pad 1 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 1 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
  )
  (module modules:DM3D-SF (layer B.Cu) (tedit 5A48E6C0)
    (at 128.143 109.347 90)
    (descr "Micro SD")
    (tags "Micro SD")
    (solder_mask_margin 0.1)
    (solder_paste_margin -0.05)
    (fp_text reference SD1 (at 0 12.75 90) (layer B.SilkS))
    (fp_text value microsd_socket (at 1.5 7 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 -3.25 90) (layer B.Fab))
    (pad 8 smd rect (at -4.5 -0.875 90) (size 0.55 1.75) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(SD1-Pad8)"))
    (pad 9 smd rect (at -5.7 -0.75 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(SD1-Pad9)"))
    (pad 10 smd rect (at -5.95 6.85 90) (size 0.8 1.5) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(SD1-Pad10)"))
    (pad B smd rect (at -5.625 8.35 90) (size 1.45 1) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(SD1-PadB)"))
    (pad 11 smd rect (at 6 7.5 90) (size 0.8 1.4) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(SD1-Pad11)"))
    (pad 7 smd rect (at -3.4 -0.875 90) (size 0.55 1.75) (layers B.Cu B.Paste B.Mask)
      (net 47 miso))
    (pad 6 smd rect (at -2.3 -0.875 90) (size 0.55 1.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 5 smd rect (at -1.2 -0.875 90) (size 0.55 1.75) (layers B.Cu B.Paste B.Mask)
      (net 48 sclk))
    (pad 4 smd rect (at -0.1 -0.875 90) (size 0.55 1.75) (layers B.Cu B.Paste B.Mask)
      (net 8 3.3v))
    (pad 3 smd rect (at 1 -0.875 90) (size 0.55 1.75) (layers B.Cu B.Paste B.Mask)
      (net 49 mosi))
    (pad 2 smd rect (at 2.1 -0.875 90) (size 0.55 1.75) (layers B.Cu B.Paste B.Mask)
      (net 44 sd_en))
    (pad 1 smd rect (at 3.2 -0.875 90) (size 0.55 1.75) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(SD1-Pad1)"))
    (pad 12 smd rect (at 5.65 -0.75 90) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(SD1-Pad12)"))
    (pad A smd rect (at 5.6 9.8 90) (size 1 1.55) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(SD1-PadA)"))
  )
  (module lightsaber_footprints:1pin (layer F.Cu) (tedit 57D8D0F9)
    (at 144.78 101.6)
    (attr virtual)
    (fp_text reference BATT+1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 BATT+))
  )
  (module lightsaber_footprints:1pin (layer F.Cu) (tedit 57D8D0F9)
    (at 154.94 104.14)
    (attr virtual)
    (fp_text reference BATT-1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 BATT-))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A4ABE7C)
    (at 131.572 103.632 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 -0.8 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A48F341)
    (at 132.969 103.632 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 -0.7 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A4A86C6)
    (at 140.462 106.68 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 -0.8 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A48F356)
    (at 138.938 114.3 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0 -0.8 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A4A8567)
    (at 131.318 112.522 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 -0.8 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A4A1939)
    (at 139.7 103.378)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 0 -0.8) (layer F.SilkS))
    (fp_text value 5.6pF (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A4A1922)
    (at 134.874 103.378 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0 -0.8 180) (layer F.SilkS))
    (fp_text value 5.6pF (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5A4A848D)
    (at 148.971 112.903)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 0.8) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5A5A9A66)
    (at 148.717 114.3)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0.635 0.762) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.7) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A4A86DA)
    (at 142.494 114.173)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C21 (at 0 -0.8) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A4A844F)
    (at 145.288 111.633)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at 0 -0.8) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5A4AB87A)
    (at 146.431 102.108 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at 0 0.9 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 BATT+))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5A4C1EA2)
    (at 143.5735 104.775 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C32 (at 0 0.8 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 12 vtest))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5A4A88C8)
    (at 149.225 107.696 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C33 (at 0 0.8 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C33-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5A4A89D0)
    (at 148.971 111.379)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at 0 0.9) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5A4AB84B)
    (at 148.971 109.855)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at 0 0.9) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A4A845F)
    (at 145.796 115.316 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C51 (at 0 -0.8 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 RESET))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A4ABF47)
    (at 145.796 103.378)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C61 (at 0 -0.8) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C61-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A4A8444)
    (at 145.796 106.68 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C62 (at 0 -0.8 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:SOD882D (layer F.Cu) (tedit 5A42C392)
    (at 144.018 103.886 90)
    (fp_text reference D61 (at 0 0 180) (layer F.SilkS))
    (fp_text value PMEG2005ELD (at 0.3 -0.5 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 BATT+) (solder_mask_margin 0.05) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C61-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.05))
  )
  (module lightsaber_footprints:SOD882D (layer F.Cu) (tedit 5A42C392)
    (at 141.986 103.886 90)
    (fp_text reference D62 (at 0 0 180) (layer F.SilkS))
    (fp_text value PMEG2005ELD (at 0.3 -0.5 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 VBUS) (solder_mask_margin 0.05) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C61-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.05))
  )
  (module lightsaber_footprints:SOD882D (layer F.Cu) (tedit 5A42C392)
    (at 143.002 103.886 90)
    (fp_text reference D63 (at 0 0 180) (layer F.SilkS))
    (fp_text value PMEG2005ELD (at 0.3 -0.5 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 5v) (solder_mask_margin 0.05) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C61-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.05))
  )
  (module lightsaber_footprints:QFN-10-PAD (layer B.Cu) (tedit 58AFB0F7)
    (at 146.685 105.664 180)
    (descr 9)
    (fp_text reference IC3 (at 1.5 -1 450) (layer B.SilkS))
    (fp_text value TPS61200 (at 0 0.5 180) (layer B.Fab))
    (pad 15 smd rect (at 1.524 -0.254 180) (size 1.5 0.28) (layers B.Cu B.Paste B.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.25))
    (pad 14 smd rect (at 1.524 0.254 180) (size 1.5 0.28) (layers B.Cu B.Paste B.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.25))
    (pad 13 smd rect (at -1.524 -0.254 180) (size 1.5 0.28) (layers B.Cu B.Paste B.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.25))
    (pad 11 smd rect (at 0 0 180) (size 2.4 1.65) (layers B.Cu B.Paste B.Mask)
      (net 6 GND) (solder_paste_margin -0.14))
    (pad 9 smd oval (at -0.5 1.5 180) (size 0.28 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 5 smd oval (at 1 -1.5 180) (size 0.28 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 BATT+))
    (pad 6 smd oval (at 1 1.5 180) (size 0.28 0.8) (layers B.Cu B.Paste B.Mask)
      (net 19 boost_en))
    (pad 4 smd oval (at 0.5 -1.5 180) (size 0.28 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 3 smd oval (at 0 -1.5 180) (size 0.28 0.8) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(IC3-Pad3)"))
    (pad 1 smd oval (at -1 -1.5 180) (size 0.28 0.8) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C33-Pad1)"))
    (pad 2 smd oval (at -0.5 -1.5 180) (size 0.28 0.8) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 7 smd oval (at 0.5 1.5 180) (size 0.28 0.8) (layers B.Cu B.Paste B.Mask)
      (net 12 vtest))
    (pad 8 smd oval (at 0 1.5 180) (size 0.28 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 BATT+))
    (pad 10 smd oval (at -1 1.5 180) (size 0.28 0.8) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(IC3-Pad10)"))
    (pad 12 smd rect (at -1.524 0.254 180) (size 1.5 0.28) (layers B.Cu B.Paste B.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.25))
  )
  (module lightsaber_footprints:2520 (layer B.Cu) (tedit 57D5112E)
    (at 145.542 108.966 180)
    (fp_text reference L1 (at 0 -0.5 180) (layer B.SilkS))
    (fp_text value "4.7 uH 1.2A" (at 0 0.5 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(IC3-Pad3)"))
    (pad 2 smd rect (at 1 0 180) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 1 BATT+))
  )
  (module Inductors_SMD:L_0402 (layer F.Cu) (tedit 5A4A818B)
    (at 130.048 103.632 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L2 (at 0 -0.8 90) (layer F.SilkS))
    (fp_text value "600 ferrite" (at 0 1.8 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:DMG7430LFG (layer F.Cu) (tedit 58AFB1D7)
    (at 152.4 102.362)
    (fp_text reference Q1 (at 0 0.75) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.975 1.625) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 1.625) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at 0.325 1.625) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 2 smd rect (at 0.975 1.625) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 31 CH1))
    (pad 1 smd rect (at 0.975 -1.3) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at -0.975 -1.3) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at 0 -0.325) (size 2.37 1.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED1-Pad1)") (solder_paste_margin -0.1))
  )
  (module lightsaber_footprints:DMG7430LFG (layer B.Cu) (tedit 58AFB1D7)
    (at 152.4 102.362 180)
    (fp_text reference Q2 (at 0 -0.75 180) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 0.75 180) (layer B.Fab) hide)
    (pad 3 smd rect (at -0.975 -1.625 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 -1.625 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at 0.325 -1.625 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 2 smd rect (at 0.975 -1.625 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 32 CH2))
    (pad 1 smd rect (at 0.975 1.3 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at 0.325 1.3 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at -0.325 1.3 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at -0.975 1.3 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at 0 0.325 180) (size 2.37 1.9) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(LED2-Pad1)") (solder_paste_margin -0.1))
  )
  (module lightsaber_footprints:DMG7430LFG (layer F.Cu) (tedit 58AFB1D7)
    (at 154.178 109.22 270)
    (fp_text reference Q3 (at 0 0.75 270) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75 270) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.975 1.625 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 1.625 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at 0.325 1.625 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 2 smd rect (at 0.975 1.625 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 33 CH3))
    (pad 1 smd rect (at 0.975 -1.3 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at -0.975 -1.3 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at 0 -0.325 270) (size 2.37 1.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED3-Pad1)") (solder_paste_margin -0.1))
  )
  (module lightsaber_footprints:DMG7430LFG (layer B.Cu) (tedit 58AFB1D7)
    (at 154.178 109.22 90)
    (fp_text reference Q4 (at 0 -0.75 90) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 0.75 90) (layer B.Fab) hide)
    (pad 3 smd rect (at -0.975 -1.625 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 -1.625 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at 0.325 -1.625 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 2 smd rect (at 0.975 -1.625 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 34 CH4))
    (pad 1 smd rect (at 0.975 1.3 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(LED4-Pad1)"))
    (pad 1 smd rect (at 0.325 1.3 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(LED4-Pad1)"))
    (pad 1 smd rect (at -0.325 1.3 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(LED4-Pad1)"))
    (pad 1 smd rect (at -0.975 1.3 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(LED4-Pad1)"))
    (pad 1 smd rect (at 0 0.325 90) (size 2.37 1.9) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(LED4-Pad1)") (solder_paste_margin -0.1))
  )
  (module lightsaber_footprints:DMG7430LFG (layer F.Cu) (tedit 58AFB1D7)
    (at 152.4 116.078 180)
    (fp_text reference Q5 (at 0 0.75 180) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75 180) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.975 1.625 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 1.625 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at 0.325 1.625 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 2 smd rect (at 0.975 1.625 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 35 CH5))
    (pad 1 smd rect (at 0.975 -1.3 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(LED5-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(LED5-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(LED5-Pad1)"))
    (pad 1 smd rect (at -0.975 -1.3 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(LED5-Pad1)"))
    (pad 1 smd rect (at 0 -0.325 180) (size 2.37 1.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(LED5-Pad1)") (solder_paste_margin -0.1))
  )
  (module lightsaber_footprints:DMG7430LFG (layer B.Cu) (tedit 58AFB1D7)
    (at 152.4 116.078)
    (fp_text reference Q6 (at 0 -0.75) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 0.75) (layer B.Fab) hide)
    (pad 3 smd rect (at -0.975 -1.625) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 -1.625) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at 0.325 -1.625) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 2 smd rect (at 0.975 -1.625) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 36 CH6))
    (pad 1 smd rect (at 0.975 1.3) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(LED6-Pad1)"))
    (pad 1 smd rect (at 0.325 1.3) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(LED6-Pad1)"))
    (pad 1 smd rect (at -0.325 1.3) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(LED6-Pad1)"))
    (pad 1 smd rect (at -0.975 1.3) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(LED6-Pad1)"))
    (pad 1 smd rect (at 0 0.325) (size 2.37 1.9) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(LED6-Pad1)") (solder_paste_margin -0.1))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5A4A8595)
    (at 141.478 115.824 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R21 (at 0 -0.8 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 SDA))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5A4A85A4)
    (at 143.002 115.824 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R22 (at 0 -0.8 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 SCL))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5A4A88AF)
    (at 144.3355 103.3145)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R31 (at 0 0.8) (layer B.SilkS))
    (fp_text value "2M 1%" (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 BATT+))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 vtest))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5A4AB834)
    (at 149.098 104.013 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R32 (at 0 0.9 90) (layer B.SilkS))
    (fp_text value "2M 1%" (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(IC3-Pad10)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5A4A88EA)
    (at 142.5575 104.775 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R33 (at 0 0.8 270) (layer B.SilkS))
    (fp_text value "220k 1%" (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 vtest))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5A4A88D7)
    (at 148.082 102.108 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R34 (at 0 0.8 90) (layer B.SilkS))
    (fp_text value "220k 1%" (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(IC3-Pad10)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5A4A88E1)
    (at 145.923 110.109 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R35 (at 0 -0.8 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 BTN))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5A4A8504)
    (at 127.254 114.3)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R41 (at 0 -0.8) (layer F.SilkS))
    (fp_text value 22 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 DP))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R41-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5A4A8514)
    (at 127.254 115.57)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R42 (at 0 -0.8) (layer F.SilkS))
    (fp_text value 22 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 DM))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R42-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer B.Cu) (tedit 5A4A2561)
    (at 140.462 103.378 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 1.4 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.5 0.75 270) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 3 smd rect (at -0.5 -0.25 270) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at -0.5 0.25 270) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 4 smd rect (at -0.5 -0.75 270) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 7 smd rect (at 0.5 0.25 270) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 32 CH2))
    (pad 8 smd rect (at 0.5 0.75 270) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 34 CH4))
    (pad 6 smd rect (at 0.5 -0.25 270) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 19 boost_en))
    (pad 5 smd rect (at 0.5 -0.75 270) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 36 CH6))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer F.Cu) (tedit 5A4A2566)
    (at 130.302 105.918 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 -1.4 270) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.5 -0.75 270) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at -0.5 0.25 270) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at -0.5 -0.25 270) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 4 smd rect (at -0.5 0.75 270) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 7 smd rect (at 0.5 -0.25 270) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 33 CH3))
    (pad 8 smd rect (at 0.5 -0.75 270) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 31 CH1))
    (pad 6 smd rect (at 0.5 0.25 270) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 35 CH5))
    (pad 5 smd rect (at 0.5 0.75 270) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 44 sd_en))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:1pin (layer F.Cu) (tedit 57D8D0F9)
    (at 147.32 116.84)
    (attr virtual)
    (fp_text reference SP+1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(SP+1-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer F.Cu) (tedit 57D8D0F9)
    (at 144.78 116.84)
    (attr virtual)
    (fp_text reference SP-1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(SP-1-Pad1)"))
  )
  (module Housings_DFN_QFN:QFN-48-1EP_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 5A48E219)
    (at 135.89 109.728 270)
    (descr "UK Package; 48-Lead Plastic QFN (7mm x 7mm); (see Linear Technology QFN_48_05-08-1704.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U0 (at 0 -4.75 270) (layer F.SilkS))
    (fp_text value STM32L433CCU6 (at 0 4.75 270) (layer F.Fab))
    (pad 1 smd rect (at -3.4 -2.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U0-Pad1)"))
    (pad 2 smd rect (at -3.4 -2.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 INT))
    (pad 3 smd rect (at -3.4 -1.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C7-Pad1)"))
    (pad 4 smd rect (at -3.4 -1.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C8-Pad1)"))
    (pad 5 smd rect (at -3.4 -0.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 boost_en))
    (pad 6 smd rect (at -3.4 -0.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 amp_en))
    (pad 7 smd rect (at -3.4 0.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 RESET))
    (pad 8 smd rect (at -3.4 0.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 9 smd rect (at -3.4 1.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C1-Pad2)"))
    (pad 10 smd rect (at -3.4 1.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 id-neopixel_data))
    (pad 11 smd rect (at -3.4 2.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 CH1))
    (pad 12 smd rect (at -3.4 2.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 TX))
    (pad 13 smd rect (at -2.75 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 FREE1))
    (pad 14 smd rect (at -2.25 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 vtest))
    (pad 15 smd rect (at -1.75 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 sclk))
    (pad 16 smd rect (at -1.25 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 miso))
    (pad 17 smd rect (at -0.75 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 mosi))
    (pad 18 smd rect (at -0.25 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 CH3))
    (pad 19 smd rect (at 0.25 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 CH4))
    (pad 20 smd rect (at 0.75 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 VBUS))
    (pad 21 smd rect (at 1.25 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 neopixel_data2))
    (pad 22 smd rect (at 1.75 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 neopixel_data3))
    (pad 23 smd rect (at 2.25 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 24 smd rect (at 2.75 3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 25 smd rect (at 3.4 2.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 I2S_LRCLK))
    (pad 26 smd rect (at 3.4 2.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 I2S_BCLK))
    (pad 27 smd rect (at 3.4 1.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 sd_en))
    (pad 28 smd rect (at 3.4 1.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 CH5))
    (pad 29 smd rect (at 3.4 0.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 CH2))
    (pad 30 smd rect (at 3.4 0.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 SCL))
    (pad 31 smd rect (at 3.4 -0.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 I2S_DATA))
    (pad 32 smd rect (at 3.4 -0.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 DM))
    (pad 33 smd rect (at 3.4 -1.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 DP))
    (pad 34 smd rect (at 3.4 -1.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 SWDIO))
    (pad 35 smd rect (at 3.4 -2.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 36 smd rect (at 3.4 -2.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 37 smd rect (at 2.75 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 SWDCLK))
    (pad 38 smd rect (at 2.25 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 RX))
    (pad 39 smd rect (at 1.75 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 FREE2))
    (pad 40 smd rect (at 1.25 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 Button3))
    (pad 41 smd rect (at 0.75 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 Button2))
    (pad 42 smd rect (at 0.25 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 Button1))
    (pad 43 smd rect (at -0.25 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C5-Pad1)"))
    (pad 44 smd rect (at -0.75 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 BTN))
    (pad 45 smd rect (at -1.25 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 CH6))
    (pad 46 smd rect (at -1.75 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 SDA))
    (pad 47 smd rect (at -2.25 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 48 smd rect (at -2.75 -3.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 49 smd rect (at 1.93125 1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 -0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 -1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 -0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 -1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 -0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 -1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 -0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 -1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm_ThermalVias (layer B.Cu) (tedit 5A48E71E)
    (at 145.415 113.538 270)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 2.85 270) (layer B.SilkS))
    (fp_text value MAX98357A_TQFN (at 0 -2.85 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd oval (at -1.475 0.75 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 58 I2S_DATA))
    (pad 2 smd oval (at -1.475 0.25 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 3 smd oval (at -1.475 -0.25 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 4 smd oval (at -1.475 -0.75 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 45 amp_en))
    (pad 5 smd oval (at -0.75 -1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(U1-Pad5)"))
    (pad 6 smd oval (at -0.25 -1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(U1-Pad6)"))
    (pad 7 smd oval (at 0.25 -1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 8 smd oval (at 0.75 -1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 9 smd oval (at 1.475 -0.75 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(SP+1-Pad1)"))
    (pad 10 smd oval (at 1.475 -0.25 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(SP-1-Pad1)"))
    (pad 11 smd oval (at 1.475 0.25 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 12 smd oval (at 1.475 0.75 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(U1-Pad12)"))
    (pad 13 smd oval (at 0.75 1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(U1-Pad13)"))
    (pad 14 smd oval (at 0.25 1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 56 I2S_LRCLK))
    (pad 15 smd oval (at -0.25 1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 16 smd oval (at -0.75 1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 57 I2S_BCLK))
    (pad 17 smd rect (at 0.45 -0.45 270) (size 0.9 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 0.45 270) (size 0.9 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45 270) (size 0.9 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45 270) (size 0.9 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 6 GND))
    (pad 17 thru_hole circle (at -0.5 0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 6 GND))
    (pad 17 thru_hole circle (at 0.5 0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 6 GND))
    (pad 17 thru_hole circle (at 0.5 -0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 6 GND))
    (pad 17 thru_hole circle (at -0.5 -0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 6 GND))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:LGA-14L (layer F.Cu) (tedit 59C80A25)
    (at 142.367 112.268)
    (fp_text reference U2 (at 0 0.3) (layer F.SilkS))
    (fp_text value LSM6DS3H (at 0 -0.3) (layer F.Fab))
    (pad 1 smd rect (at -1.175 -0.75) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 2 smd rect (at -1.175 -0.25) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 3 smd rect (at -1.175 0.25) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 4 smd rect (at -1.175 0.75) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 55 INT) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 5 smd rect (at -0.5 0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 6 smd rect (at 0 0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 7 smd rect (at 0.5 0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 8 smd rect (at 1.175 0.75) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 9 smd rect (at 1.175 0.25) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U2-Pad9)") (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 10 smd rect (at 1.175 -0.25) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U2-Pad10)") (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 11 smd rect (at 1.175 -0.75) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U2-Pad11)") (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 12 smd rect (at 0.5 -0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 13 smd rect (at 0 -0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 SCL) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
    (pad 14 smd rect (at -0.5 -0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 SDA) (solder_mask_margin 0.05) (solder_paste_margin -0.0125))
  )
  (module lightsaber_footprints:uQFN6 (layer F.Cu) (tedit 5A4178DE)
    (at 129.032 112.522)
    (fp_text reference U40 (at 0 0) (layer F.SilkS))
    (fp_text value HSP061-2M6 (at -0.025 -0.9) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R42-Pad2)"))
    (pad 1 smd rect (at -0.5 0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R41-Pad2)"))
    (pad 6 smd rect (at -0.5 -0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R41-Pad2)"))
    (pad 4 smd rect (at 0.5 -0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R42-Pad2)"))
    (pad 2 smd rect (at 0 0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 5 smd rect (at 0 -0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 VBUS))
  )
  (module lightsaber_footprints:XDFN4 (layer F.Cu) (tedit 5A43838C)
    (at 145.796 104.902 90)
    (fp_text reference U60 (at 0.7 0 180) (layer F.SilkS))
    (fp_text value NCP177 (at 0 -0.7 90) (layer F.Fab) hide)
    (pad 3 smd trapezoid (at 0.195 -0.36 315) (size 0.12 0.212132) (drill (offset -0.06 -0.106066)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C61-Pad1)"))
    (pad 3 smd rect (at 0.455 -0.6 90) (size 0.11 0.39) (drill (offset -0.055 0.195)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C61-Pad1)"))
    (pad 3 smd rect (at 0.455 -0.6 90) (size 0.26 0.24) (drill (offset -0.13 0.12)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C61-Pad1)"))
    (pad 4 smd trapezoid (at -0.195 -0.36 225) (size 0.12 0.212132) (drill (offset 0.06 -0.106066)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C61-Pad1)"))
    (pad 4 smd rect (at -0.455 -0.6 90) (size 0.11 0.39) (drill (offset 0.055 0.195)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C61-Pad1)"))
    (pad 4 smd rect (at -0.455 -0.6 90) (size 0.26 0.24) (drill (offset 0.13 0.12)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C61-Pad1)"))
    (pad 1 smd trapezoid (at -0.195 0.36 315) (size 0.12 0.212132) (drill (offset 0.06 0.106066)) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 1 smd rect (at -0.455 0.6 90) (size 0.11 0.39) (drill (offset 0.055 -0.195)) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 1 smd rect (at -0.455 0.6 90) (size 0.26 0.24) (drill (offset 0.13 -0.12)) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 5 smd rect (at 0 0 135) (size 0.52 0.52) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 0.455 0.6 90) (size 0.26 0.24) (drill (offset -0.13 -0.12)) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 0.455 0.6 90) (size 0.11 0.39) (drill (offset -0.055 -0.195)) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd trapezoid (at 0.195 0.36 225) (size 0.12 0.212132) (drill (offset -0.06 0.106066)) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
  )
  (module lightsaber_footprints:ST2012SB (layer F.Cu) (tedit 5A438D5A)
    (at 137.287 103.632 180)
    (fp_text reference Y1 (at 0 0 270) (layer F.SilkS))
    (fp_text value "ST2012SB 4pF" (at 0 -0.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C8-Pad1)"))
  )
  (module lightsaber_footprints:5pin (layer F.Cu) (tedit 5A43A57A)
    (at 129.54 101.6)
    (attr virtual)
    (fp_text reference SW3 (at 0 1) (layer F.SilkS))
    (fp_text value Conn_01x05 (at 0 -1) (layer F.Fab))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 RESET))
    (pad 4 thru_hole circle (at 2.54 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 52 SWDCLK))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 53 SWDIO))
    (pad 3 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 8 3.3v))
  )
  (module lightsaber_footprints:1pin-oval (layer F.Cu) (tedit 5A450AAD)
    (at 149.86 101.6 180)
    (attr virtual)
    (fp_text reference LED1 (at 0 1 180) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.4 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(LED1-Pad1)"))
  )
  (module lightsaber_footprints:1pin-oval (layer F.Cu) (tedit 5A450AAD)
    (at 154.94 101.6 180)
    (attr virtual)
    (fp_text reference LED2 (at 0 1 180) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.4 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(LED2-Pad1)"))
  )
  (module lightsaber_footprints:1pin-oval (layer F.Cu) (tedit 5A450AAD)
    (at 154.94 106.68 90)
    (attr virtual)
    (fp_text reference LED3 (at 0 1 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.4 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(LED3-Pad1)"))
  )
  (module lightsaber_footprints:1pin-oval (layer F.Cu) (tedit 5A450AAD)
    (at 154.94 111.76 90)
    (attr virtual)
    (fp_text reference LED4 (at 0 1 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.4 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(LED4-Pad1)"))
  )
  (module lightsaber_footprints:1pin-oval (layer F.Cu) (tedit 5A450AAD)
    (at 154.94 116.84)
    (attr virtual)
    (fp_text reference LED5 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.4 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(LED5-Pad1)"))
  )
  (module lightsaber_footprints:1pin-oval (layer F.Cu) (tedit 5A450AAD)
    (at 149.86 116.84)
    (attr virtual)
    (fp_text reference LED6 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.4 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(LED6-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer F.Cu) (tedit 57D8D0F9)
    (at 154.94 114.3)
    (attr virtual)
    (fp_text reference BATT-2 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 BATT-))
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5A4A875E)
    (at 143.1925 107.823 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 0 -0.8 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.8 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 45 amp_en))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:PTS810 (layer F.Cu) (tedit 5A5708B0)
    (at 148.844 112.268 270)
    (fp_text reference SW2 (at 0 0.05 450) (layer F.SilkS))
    (fp_text value SW_Push (at 0 -0.5 270) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 RESET))
    (pad 2 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 RESET))
    (pad 1 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
  )
  (module lightsaber_footprints:10118192 (layer F.Cu) (tedit 5A4AC18F)
    (at 124.46 109.22 270)
    (fp_text reference USB1 (at 0 -1.4 270) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 -0.5 270) (layer F.Fab) hide)
    (pad 6 smd rect (at 3.1 -2.55 270) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 5 smd rect (at 1.3 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 4 smd rect (at 0.65 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(USB1-Pad4)"))
    (pad 1 smd rect (at -1.3 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 16 VBUS))
    (pad 2 smd rect (at -0.65 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R42-Pad2)"))
    (pad 6 smd rect (at 3.75 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 6 smd rect (at -3.75 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 6 smd rect (at -1.2 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 6 smd rect (at 1.2 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 0 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R41-Pad2)"))
    (pad 6 smd rect (at -3.1 -2.55 270) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
  )
  (module lightsaber_footprints:1pin (layer F.Cu) (tedit 57D8D0F9)
    (at 124.46 116.84)
    (attr virtual)
    (fp_text reference GND2 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C38B2)
    (at 132.08 117.348)
    (fp_text reference FR1 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 17 FREE1))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 137.414 117.348)
    (attr virtual)
    (fp_text reference FR2 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 18 FREE2))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 135.636 117.348)
    (attr virtual)
    (fp_text reference RX1 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 46 RX))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 142.748 117.348)
    (attr virtual)
    (fp_text reference SCL1 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 38 SCL))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 140.97 117.348)
    (attr virtual)
    (fp_text reference SDA1 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 37 SDA))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 133.858 117.348)
    (attr virtual)
    (fp_text reference TX1 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 54 TX))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 140.97 101.092)
    (attr virtual)
    (fp_text reference BT1 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 3 Button1))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 139.192 117.348)
    (attr virtual)
    (fp_text reference BT2 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 4 Button2))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 139.192 101.092)
    (attr virtual)
    (fp_text reference BT3 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 5 Button3))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 126.746 117.348)
    (attr virtual)
    (fp_text reference ID1 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 22 id-neopixel_data))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 128.524 117.348)
    (attr virtual)
    (fp_text reference PX2 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 29 neopixel_data2))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 130.302 117.348)
    (attr virtual)
    (fp_text reference PX3 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 30 neopixel_data3))
  )
  (module lightsaber_footprints:1upin (layer F.Cu) (tedit 5A6C3889)
    (at 142.748 101.092)
    (attr virtual)
    (fp_text reference 5V1 (at 0 0.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.2) (drill 0.75) (layers *.Cu *.Mask F.SilkS)
      (net 11 5v))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5A75411A)
    (at 141.859 109.474)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 -0.8) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:fiduciary-small locked (layer F.Cu) (tedit 5A5A92F3)
    (at 124.46 103.378)
    (attr virtual)
    (fp_text reference Ref** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers F.Cu F.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small locked (layer F.Cu) (tedit 5A5A92F3)
    (at 125.476 115.316)
    (attr virtual)
    (fp_text reference Ref** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers F.Cu F.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small locked (layer F.Cu) (tedit 5A5A92F3)
    (at 148.082 101.346)
    (attr virtual)
    (fp_text reference Ref** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers F.Cu F.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small locked (layer F.Cu) (tedit 5A5A92F3)
    (at 136.652 101.346)
    (attr virtual)
    (fp_text reference Ref** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers F.Cu F.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small locked (layer B.Cu) (tedit 5A5A92F3)
    (at 124.46 103.378)
    (fp_text reference Ref** (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 0.5) (layer B.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers B.Cu B.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small locked (layer B.Cu) (tedit 5A5A92F3)
    (at 124.46 115.062)
    (attr virtual)
    (fp_text reference Ref** (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 0.5) (layer B.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers B.Cu B.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small (layer B.Cu) (tedit 5A5A92F3)
    (at 142.24 112.014)
    (attr virtual)
    (fp_text reference Ref** (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 0.5) (layer B.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers B.Cu B.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (gr_line (start 155.575 118.11) (end 123.825 118.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.825 100.33) (end 155.575 100.33) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.21 100.965) (end 156.21 117.475) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.19 117.475) (end 123.19 100.965) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 155.575 100.965) (end 155.575 100.33) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 123.825 100.965) (end 123.19 100.965) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 123.825 117.475) (end 123.825 118.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 155.575 117.475) (end 156.21 117.475) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "ProffieBoard V1.5\n\n" (at 125.73 109.22 90) (layer B.SilkS))
  (gr_text "ProffieBoard V1.5\n\n\n\n\n" (at 133.4008 120.1801) (layer F.SilkS))
  (zone (net 2) (net_name BATT-) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.956 102.616) (xy 149.9235 102.616) (xy 149.9235 115.697) (xy 155.956 115.824)
      )
    )
  )
  (zone (net 2) (net_name BATT-) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.956 102.616) (xy 150.622 102.616) (xy 150.622 115.824) (xy 155.956 115.824)
      )
    )
  )
  (zone (net 2) (net_name BATT-) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.956 102.616) (xy 150.622 102.616) (xy 150.622 115.824) (xy 155.956 115.824)
      )
    )
  )
  (zone (net 2) (net_name BATT-) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.956 102.616) (xy 150.622 102.616) (xy 150.622 115.824) (xy 155.956 115.824)
      )
    )
  )
  (zone (net 8) (net_name 3.3v) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.19 100.33) (xy 149.86 100.33) (xy 149.86 118.11) (xy 123.19 118.11)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.19 100.33) (xy 150.114 100.33) (xy 150.114 118.11) (xy 123.19 118.11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.1435 106.172) (xy 134.112 106.172) (xy 134.112 114.2365) (xy 132.1435 114.2365)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.3345 108.7755) (xy 138.303 108.7755) (xy 138.303 111.3155) (xy 136.3345 111.3155)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.19 100.33) (xy 149.479 100.3935) (xy 149.479 118.1735) (xy 123.19 118.11)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.19 100.33) (xy 149.479 100.3935) (xy 149.479 118.1735) (xy 123.19 118.11)
      )
    )
  )
)
