<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="46.913915625" x2="1.27" y2="18.922984375" width="0" layer="20"/>
<wire x1="1.27" y1="18.922984375" x2="5.079984375" y2="15.494" width="0" layer="20" curve="90"/>
<wire x1="5.079984375" y1="15.494" x2="40.927725" y2="15.494" width="0" layer="20"/>
<wire x1="40.927725" y1="15.494" x2="44.12" y2="18.559275" width="0" layer="20" curve="90"/>
<wire x1="44.12" y1="18.559275" x2="44.12" y2="47.923171875" width="0" layer="20"/>
<wire x1="44.12" y1="47.923171875" x2="41.253171875" y2="50.79" width="0" layer="20" curve="90"/>
<wire x1="41.253171875" y1="50.79" x2="5.146084375" y2="50.79" width="0" layer="20"/>
<wire x1="5.146084375" y1="50.79" x2="1.27" y2="46.913915625" width="0" layer="20" curve="90"/>
<text>JB (c) 2022</text>
<hole x="5.08" y="47.371" drill="3.81"/>
<hole x="5.08" y="19.304" drill="3.81"/>
<hole x="41.402" y="47.371" drill="3.81"/>
<hole x="41.402" y="19.304" drill="3.81"/>
<text>CAN 2.0A Breakout v1</text>
<text>CAN-L</text>
<text>CAN-H</text>
<text>12v</text>
<text>5v</text>
<text>GND</text>
<text>Err</text>
<text>Wk</text>
<text>Int</text>
<text>Sck</text>
<text>SI</text>
<text>SO</text>
<text>CS</text>
<text>8mhz</text>
<text>CAN-L</text>
<text>CAN-H</text>
<text>Termination</text>
<text>CAN 2.0a</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10">
<description>&lt;h3&gt;Plated Through Hole -10 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="james">
<packages>
<package name="JB-0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Slighly longer to make hand soldering easier&lt;/p&gt;</description>
</package>
<package name="MCP2515_SOIC18W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
SOIC, 0.3 inch width</description>
</package>
<package name="TJA1054">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49U">
<description>&lt;h3&gt;HC49/U 11.6x4.6mm PTH Crystal (13.46mm height)&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.digikey.com/Web%20Export/Supplier%20Content/Citizen_300/PDF/Citizen_HC49US.pdf?redirected=1"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$6" library="james" package="MCP2515_SOIC18W" value="MCP2515">
<attribute name="VALUE"/>
</element>
<element name="C9" library="james" package="JB-0805" value="0.1uf">
<attribute name="VALUE"/>
</element>
<element name="R3" library="james" package="JB-0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R4" library="james" package="JB-0805" value="120r">
<attribute name="VALUE"/>
</element>
<element name="R5" library="james" package="JB-0805" value="120r">
<attribute name="VALUE"/>
</element>
<element name="R6" library="james" package="JB-0805" value="120r">
<attribute name="VALUE"/>
</element>
<element name="R7" library="james" package="JB-0805" value="120r">
<attribute name="VALUE"/>
</element>
<element name="R8" library="james" package="JB-0805" value="120r">
<attribute name="VALUE"/>
</element>
<element name="C12" library="james" package="JB-0805" value="22pf">
<attribute name="VALUE"/>
</element>
<element name="C13" library="james" package="JB-0805" value="22pf">
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-Clocks" package="HC49U" value="">
<attribute name="VALUE"/>
</element>
<element name="U$5" library="james" package="TJA1054" value="TJA1054">
<attribute name="VALUE"/>
</element>
<element name="R12" library="james" package="JB-0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R13" library="james" package="JB-0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="C14" library="james" package="JB-0805" value="0.1uf">
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="CAN2.0a">
<attribute name="PROD_ID" value="CONN-08399"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="james" package="JB-0805" value="~120r">
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="james" package="JB-0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$6" pad="VSS"/>
<contactref element="C9" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U$5" pad="13"/>
<contactref element="C14" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="U$6" pad="VDD"/>
<contactref element="C9" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U$5" pad="10"/>
<contactref element="C14" pad="2"/>
<contactref element="U$5" pad="6"/>
<contactref element="U$5" pad="5"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="VUSB">
</signal>
<signal name="N$33">
<contactref element="U$6" pad="RESET"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="U$6" pad="CS"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="CS">
<contactref element="R7" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="SO">
<contactref element="R6" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$39">
<contactref element="R6" pad="2"/>
<contactref element="U$6" pad="SO"/>
</signal>
<signal name="N$40">
<contactref element="U$6" pad="SI"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="SI">
<contactref element="R5" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$43">
<contactref element="R4" pad="2"/>
<contactref element="U$6" pad="SCK"/>
</signal>
<signal name="N$32">
<contactref element="U$6" pad="INT"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="R4" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$42">
<contactref element="U$6" pad="OSC2"/>
<contactref element="C13" pad="2"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="U$6" pad="OSC1"/>
<contactref element="C12" pad="2"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$5" pad="9"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U$5" pad="8"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="CANL_SLOW">
<contactref element="U$5" pad="12"/>
<contactref element="R12" pad="2"/>
<contactref element="J7" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="CANH_SLOW">
<contactref element="U$5" pad="11"/>
<contactref element="R13" pad="2"/>
<contactref element="J7" pad="1"/>
<contactref element="J8" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$60">
<contactref element="R14" pad="2"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$5" pad="3"/>
<contactref element="U$6" pad="RXCAN"/>
</signal>
<signal name="N$2">
<contactref element="U$5" pad="2"/>
<contactref element="U$6" pad="TXCAN"/>
</signal>
<signal name="ERROR">
<contactref element="U$5" pad="4"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="10"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="WAKE">
<contactref element="J1" pad="8"/>
<contactref element="U$5" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="U$5" pad="14"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="INT">
<contactref element="J1" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
