(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 0.8)
    (drawings 35)
    (tracks 854)
    (zones 0)
    (modules 19)
    (nets 56)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.0254)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x3ffff_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "MBC30-CCEdition-Gerbers"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(R3-Pad2)")
  (net 3 "Net-(B1-Pad1)")
  (net 4 "Net-(C5-Pad2)")
  (net 5 "Net-(U2-Pad5)")
  (net 6 VCC)
  (net 7 XIN)
  (net 8 PWR)
  (net 9 AA14)
  (net 10 A12)
  (net 11 A7)
  (net 12 A6)
  (net 13 A5)
  (net 14 A4)
  (net 15 A3)
  (net 16 A2)
  (net 17 A1)
  (net 18 A0)
  (net 19 D0)
  (net 20 D1)
  (net 21 D2)
  (net 22 D3)
  (net 23 D4)
  (net 24 D5)
  (net 25 D6)
  (net 26 D7)
  (net 27 "#CE")
  (net 28 A10)
  (net 29 \RD)
  (net 30 A11)
  (net 31 A9)
  (net 32 A8)
  (net 33 AA13)
  (net 34 \WR)
  (net 35 XOUT)
  (net 36 CLK)
  (net 37 CS)
  (net 38 A13)
  (net 39 A14)
  (net 40 A15)
  (net 41 RESET)
  (net 42 \RST)
  (net 43 \RAMCS)
  (net 44 RA14)
  (net 45 RA15)
  (net 46 RA16)
  (net 47 RA17)
  (net 48 RA18)
  (net 49 RA19)
  (net 50 RA20)
  (net 51 RA21)
  (net 52 WE_AUDIO)
  (net 53 "Net-(U1-Pad5)")
  (net 54 "Net-(U4-Pad11)")
  (net 55 "Net-(U4-Pad36)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "#CE")
    (add_net A0)
    (add_net A1)
    (add_net A10)
    (add_net A11)
    (add_net A12)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net AA13)
    (add_net AA14)
    (add_net CLK)
    (add_net CS)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net GND)
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U4-Pad36)")
    (add_net PWR)
    (add_net RA14)
    (add_net RA15)
    (add_net RA16)
    (add_net RA17)
    (add_net RA18)
    (add_net RA19)
    (add_net RA20)
    (add_net RA21)
    (add_net RESET)
    (add_net VCC)
    (add_net WE_AUDIO)
    (add_net XIN)
    (add_net XOUT)
    (add_net \RAMCS)
    (add_net \RD)
    (add_net \RST)
    (add_net \WR)
  )
  (module Custom:cc4 (layer B.Cu) (tedit 5DB22860)
    (at 90.412581 99.90646 180)
    (fp_text reference Art1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value "90,412581|99,90646 | Crystal Clear" (at 0.75 0) (layer B.SilkS) hide)
    (fp_text user LOGO (at 0.75 0) (layer B.SilkS) hide)
    (fp_text user G*** (at 0 0) (layer B.SilkS) hide)
  )
  (module Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 79.3904 107.97)
    (descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference RAM (at 0 0.00032 90) (layer F.SilkS))
    (fp_text value FM18W08 (at 0 9.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -4.65 -8.255) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 AA14))
    (pad 2 smd roundrect (at -4.65 -6.985) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 A12))
    (pad 3 smd roundrect (at -4.65 -5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 A7))
    (pad 4 smd roundrect (at -4.65 -4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 A6))
    (pad 5 smd roundrect (at -4.65 -3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 A5))
    (pad 6 smd roundrect (at -4.65 -1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 A4))
    (pad 7 smd roundrect (at -4.65 -0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 A3))
    (pad 8 smd roundrect (at -4.65 0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 A2))
    (pad 9 smd roundrect (at -4.65 1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 A1))
    (pad 10 smd roundrect (at -4.65 3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 A0))
    (pad 11 smd roundrect (at -4.65 4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 D0))
    (pad 12 smd roundrect (at -4.65 5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 D1))
    (pad 13 smd roundrect (at -4.65 6.985) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 D2))
    (pad 14 smd roundrect (at -4.65 8.255) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 15 smd roundrect (at 4.65 8.255) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 D3))
    (pad 16 smd roundrect (at 4.65 6.985) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 D4))
    (pad 17 smd roundrect (at 4.65 5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 D5))
    (pad 18 smd roundrect (at 4.65 4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 D6))
    (pad 19 smd roundrect (at 4.65 3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 D7))
    (pad 20 smd roundrect (at 4.65 1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "#CE"))
    (pad 21 smd roundrect (at 4.65 0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 A10))
    (pad 22 smd roundrect (at 4.65 -0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 \RD))
    (pad 23 smd roundrect (at 4.65 -1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 A11))
    (pad 24 smd roundrect (at 4.65 -3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 A9))
    (pad 25 smd roundrect (at 4.65 -4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 A8))
    (pad 26 smd roundrect (at 4.65 -5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 AA13))
    (pad 27 smd roundrect (at 4.65 -6.985) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 \WR))
    (pad 28 smd roundrect (at 4.65 -8.255) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_GameBoy:GameBoy_GamePak_CGB-002_P1.50mm_Edge (layer F.Cu) (tedit 5F3FFEC0)
    (at 90.4062 120.609)
    (descr "Game Boy Game Pak (CGB) edge connector")
    (tags "game boy game pak cgb gbc color edge connector")
    (fp_text reference U0 (at -22.05 0.35) (layer F.Fab) hide)
    (fp_text value CartBus (at 0 10.9) (layer F.Fab) hide)
    (fp_text user 32 (at 23.5 0.45) (layer F.SilkS))
    (fp_text user 1 (at -23.5 0.45) (layer F.SilkS))
    (pad 32 connect custom (at 23.5 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.75 6.8) (xy -0.75 -0.5) (xy 0.75 -0.5) (xy 0.75 6.3) (xy 0.25 6.8)
) (width 0))
      ))
    (pad 1 connect custom (at -23.5 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 6 VCC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.75 6.4) (xy -0.75 -0.5) (xy 0.75 -0.5) (xy 0.75 6.8) (xy -0.35 6.8)
) (width 0))
      ))
    (pad 31 thru_hole circle (at 21.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 52 WE_AUDIO))
    (pad 30 thru_hole circle (at 20.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 41 RESET))
    (pad 29 thru_hole circle (at 18.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 26 D7))
    (pad 28 thru_hole circle (at 17.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 25 D6))
    (pad 27 thru_hole circle (at 15.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 24 D5))
    (pad 26 thru_hole circle (at 14.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 23 D4))
    (pad 25 thru_hole circle (at 12.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 22 D3))
    (pad 24 thru_hole circle (at 11.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 21 D2))
    (pad 23 thru_hole circle (at 9.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 20 D1))
    (pad 22 thru_hole circle (at 8.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 19 D0))
    (pad 21 thru_hole circle (at 6.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 40 A15))
    (pad 20 thru_hole circle (at 5.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 39 A14))
    (pad 19 thru_hole circle (at 3.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 38 A13))
    (pad 18 thru_hole circle (at 2.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 A12))
    (pad 17 thru_hole circle (at 0.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 30 A11))
    (pad 16 thru_hole circle (at -0.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 28 A10))
    (pad 15 thru_hole circle (at -2.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 31 A9))
    (pad 14 thru_hole circle (at -3.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 A8))
    (pad 13 thru_hole circle (at -5.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 A7))
    (pad 12 thru_hole circle (at -6.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 12 A6))
    (pad 11 thru_hole circle (at -8.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 A5))
    (pad 10 thru_hole circle (at -9.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 A4))
    (pad 9 thru_hole circle (at -11.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 A3))
    (pad 8 thru_hole circle (at -12.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 A2))
    (pad 7 thru_hole circle (at -14.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 A1))
    (pad 6 thru_hole circle (at -15.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 18 A0))
    (pad 5 thru_hole circle (at -17.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 37 CS))
    (pad 4 thru_hole circle (at -18.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 29 \RD))
    (pad 3 thru_hole circle (at -20.25 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 34 \WR))
    (pad 31 connect custom (at 21.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 52 WE_AUDIO)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 30 connect custom (at 20.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 41 RESET)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 29 connect custom (at 18.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 26 D7)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 28 connect custom (at 17.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 25 D6)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 27 connect custom (at 15.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 24 D5)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 26 connect custom (at 14.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 23 D4)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 25 connect custom (at 12.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 22 D3)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 24 connect custom (at 11.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 21 D2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 23 connect custom (at 9.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 20 D1)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 22 connect custom (at 8.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 19 D0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 21 connect custom (at 6.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 40 A15)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 20 connect custom (at 5.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 39 A14)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 19 connect custom (at 3.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 38 A13)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 18 connect custom (at 2.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 10 A12)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 17 connect custom (at 0.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 30 A11)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 16 connect custom (at -0.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 28 A10)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 15 connect custom (at -2.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 31 A9)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 14 connect custom (at -3.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 32 A8)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 13 connect custom (at -5.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 11 A7)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 12 connect custom (at -6.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 12 A6)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 11 connect custom (at -8.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 13 A5)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 10 connect custom (at -9.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 14 A4)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 9 connect custom (at -11.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 15 A3)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 8 connect custom (at -12.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 16 A2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 7 connect custom (at -14.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 17 A1)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 6 connect custom (at -15.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 18 A0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 5 connect custom (at -17.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 37 CS)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 4 connect custom (at -18.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 29 \RD)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 3 connect custom (at -20.25 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 34 \WR)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 2 connect custom (at -21.75 1.9) (size 0.8 0.8) (layers F.Cu)
      (net 36 CLK)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 6.5) (xy -0.5 6.5) (xy -0.5 -0.5) (xy 0.5 -0.5)) (width 0))
      ))
    (pad 32 thru_hole circle (at 23.5 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -23.5 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 2 thru_hole circle (at -21.75 1.9) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 36 CLK))
  )
  (module Custom:AM29F032-MBM29F033C (layer F.Cu) (tedit 5F3FD541)
    (at 101.681 107.97 270)
    (descr AM29F032/MBM29F033C)
    (tags "TSOP I 40")
    (attr smd)
    (fp_text reference ROM (at 0 -0.00028 90) (layer F.SilkS))
    (fp_text value AM29F032/MBM29F033C (at 0 -0.00254 90) (layer F.Fab))
    (pad 40 smd rect (at 9.75 -4.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 RA20))
    (pad 39 smd rect (at 9.75 -4.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 RA21))
    (pad 38 smd rect (at 9.75 -3.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 WE_AUDIO))
    (pad 37 smd rect (at 9.75 -3.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 \RD))
    (pad 36 smd rect (at 9.75 -2.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U4-Pad36)"))
    (pad 35 smd rect (at 9.75 -2.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 D7))
    (pad 34 smd rect (at 9.75 -1.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 D6))
    (pad 33 smd rect (at 9.75 -1.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 D5))
    (pad 32 smd rect (at 9.75 -0.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 D4))
    (pad 31 smd rect (at 9.75 -0.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (pad 30 smd rect (at 9.75 0.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at 9.75 0.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at 9.75 1.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 D3))
    (pad 27 smd rect (at 9.75 1.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 D2))
    (pad 26 smd rect (at 9.75 2.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 D1))
    (pad 25 smd rect (at 9.75 2.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 D0))
    (pad 24 smd rect (at 9.75 3.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 A0))
    (pad 23 smd rect (at 9.75 3.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 A1))
    (pad 22 smd rect (at 9.75 4.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 A2))
    (pad 21 smd rect (at 9.75 4.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 A3))
    (pad 20 smd rect (at -9.75 4.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 A4))
    (pad 19 smd rect (at -9.75 4.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 A5))
    (pad 18 smd rect (at -9.75 3.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 A6))
    (pad 17 smd rect (at -9.75 3.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 A7))
    (pad 16 smd rect (at -9.75 2.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 A8))
    (pad 15 smd rect (at -9.75 2.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 A9))
    (pad 14 smd rect (at -9.75 1.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 A10))
    (pad 13 smd rect (at -9.75 1.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 A11))
    (pad 12 smd rect (at -9.75 0.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 RESET))
    (pad 11 smd rect (at -9.75 0.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U4-Pad11)"))
    (pad 10 smd rect (at -9.75 -0.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (pad 9 smd rect (at -9.75 -0.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 A15))
    (pad 8 smd rect (at -9.75 -1.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 A12))
    (pad 7 smd rect (at -9.75 -1.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 A13))
    (pad 6 smd rect (at -9.75 -2.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 RA14))
    (pad 5 smd rect (at -9.75 -2.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 RA15))
    (pad 4 smd rect (at -9.75 -3.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 RA16))
    (pad 3 smd rect (at -9.75 -3.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 RA17))
    (pad 2 smd rect (at -9.75 -4.25 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 RA18))
    (pad 1 smd rect (at -9.75 -4.75 270) (size 1.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 RA19))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-I-48_18.4x12mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:Resonator_SMD_muRata_CDSCB-2pin_4.5x2.0mm_HandSoldering (layer F.Cu) (tedit 5BCC782B)
    (at 78.6982 76.6688 90)
    (descr "SMD Resomator/Filter Murata CDSCB, http://cdn-reichelt.de/documents/datenblatt/B400/SFECV-107.pdf, hand-soldering, 4.5x2.0mm^2 package")
    (tags "SMD SMT ceramic resonator filter filter hand-soldering")
    (attr smd)
    (fp_text reference X1 (at 2.39 0) (layer F.SilkS))
    (fp_text value Crystal (at -0.01 2.915 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 4.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 1 0 90) (size 1 4.55) (layers F.Cu F.Paste F.Mask)
      (net 7 XIN))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Resonator_SMD_muRata_CDSCB-2pin_4.5x2.0mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 105.834 95.664 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.051 1.524 180) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 VCC))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 93.2764 116.002 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 76.7265 80.5231 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 9.012661 270) (layer F.SilkS))
    (fp_text value "15 pF" (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 XIN))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 78.5122 80.5231 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -9.008281 90) (layer F.SilkS))
    (fp_text value "15 pF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.9094 91.3816 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 VCC))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 86.9594 107.97 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 VCC))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "#CE"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 87.5978 85.471 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(B1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 80.3022 80.5231 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -9.008201 90) (layer F.SilkS))
    (fp_text value 330K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 XOUT))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 84.9053 79.7484 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0 -0.00072 180) (layer F.SilkS))
    (fp_text value BA6129AF (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 VCC))
    (pad 7 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 PWR))
    (pad 5 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(U2-Pad5)"))
    (pad 4 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(R3-Pad2)"))
    (pad 3 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 \RST))
    (pad 2 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 RESET))
    (pad 1 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:BK-6219-TR (layer F.Cu) (tedit 5CDF1AC9)
    (at 102.225 80.6348)
    (fp_text reference B1 (at -0.05058 -7.40406) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0.17272 -12.49934) (layer F.Fab))
    (pad 2 smd circle (at 0 0) (size 12.7 12.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -10.985 0) (size 2.79 5.08) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(B1-Pad1)"))
    (pad 1 smd rect (at 10.985 0) (size 2.79 5.08) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(B1-Pad1)"))
  )
  (module Package_SO:TSOP-6_1.65x3.05mm_P0.95mm (layer F.Cu) (tedit 5A02F25C)
    (at 94.3559 91.2165 90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference U2 (at 0 -2.85 180) (layer F.SilkS))
    (fp_text value 74LVC1G332GW,125 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 43 \RAMCS))
    (pad 2 smd rect (at -1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 36 CLK))
    (pad 4 smd rect (at 1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 27 "#CE"))
    (pad 5 smd rect (at 1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (pad 6 smd rect (at 1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 37 CS))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 66.7131 85.5345 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.30124 0 180) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 PWR))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:LQFP-32_7x7mm_P0.8mm (layer F.Cu) (tedit 5C1823C9)
    (at 74.0131 87.9627 90)
    (descr "LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT358-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (attr smd)
    (fp_text reference MBC30 (at 0 -0.00004 180) (layer F.SilkS))
    (fp_text value MBC30 (at 0 5.88 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -4.175 -2.8 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 CLK))
    (pad 2 smd roundrect (at -4.175 -2 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 AA13))
    (pad 3 smd roundrect (at -4.175 -1.2 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 AA14))
    (pad 4 smd roundrect (at -4.175 -0.4 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 \RAMCS))
    (pad 5 smd roundrect (at -4.175 0.4 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(U1-Pad5)"))
    (pad 6 smd roundrect (at -4.175 1.2 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 RA14))
    (pad 7 smd roundrect (at -4.175 2 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 RA15))
    (pad 8 smd roundrect (at -4.175 2.8 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 RA16))
    (pad 9 smd roundrect (at -2.8 4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 RA17))
    (pad 10 smd roundrect (at -2 4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 RA18))
    (pad 11 smd roundrect (at -1.2 4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RA19))
    (pad 12 smd roundrect (at -0.4 4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 RA20))
    (pad 13 smd roundrect (at 0.4 4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 RA21))
    (pad 14 smd roundrect (at 1.2 4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 \RST))
    (pad 15 smd roundrect (at 2 4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 \WR))
    (pad 16 smd roundrect (at 2.8 4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 XIN))
    (pad 17 smd roundrect (at 4.175 2.8 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 XOUT))
    (pad 18 smd roundrect (at 4.175 2 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 \RD))
    (pad 19 smd roundrect (at 4.175 1.2 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 A15))
    (pad 20 smd roundrect (at 4.175 0.4 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 A14))
    (pad 21 smd roundrect (at 4.175 -0.4 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 A13))
    (pad 22 smd roundrect (at 4.175 -1.2 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 23 smd roundrect (at 4.175 -2 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 24 smd roundrect (at 4.175 -2.8 90) (size 1.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 PWR))
    (pad 25 smd roundrect (at 2.8 -4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 D7))
    (pad 26 smd roundrect (at 2 -4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 D6))
    (pad 27 smd roundrect (at 1.2 -4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 D5))
    (pad 28 smd roundrect (at 0.4 -4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 D4))
    (pad 29 smd roundrect (at -0.4 -4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 D3))
    (pad 30 smd roundrect (at -1.2 -4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 D2))
    (pad 31 smd roundrect (at -2 -4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 D1))
    (pad 32 smd roundrect (at -2.8 -4.175 90) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 D0))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-32_7x7mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 83.312 95.6081)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "github.com/HDR\n" (at 103.681 107.97 90) (layer F.SilkS))
  (gr_arc (start 113.62535 128.427) (end 115.20622 128.362) (angle 86.88278645) (layer Edge.Cuts) (width 0.0254))
  (gr_text "MBC30 REV 1.4.2" (at 101.425 71.33082) (layer F.Mask))
  (gr_line (start 74.12482 75.60204) (end 67.90182 75.60204) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 74.12482 75.60204) (end 74.12482 77.7088) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 67.90182 77.7088) (end 74.12482 77.7088) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 67.90182 75.60204) (end 67.90182 77.7088) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 66.61622 115.35556) (end 66.61622 119.00552) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 66.6115 119.00552) (end 64.90622 119.00556) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 64.90622 119.00556) (end 64.90622 121.402) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 64.90622 111.7056) (end 66.6115 111.70556) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 115.90622 121.402) (end 115.90622 119.00556) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 115.90622 119.00556) (end 114.20094 119.00556) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 114.20094 111.70564) (end 115.90622 111.7056) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 114.20094 115.3556) (end 114.20094 111.70564) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 115.90622 72.502) (end 111.85622 72.502) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 67.13122 128.47668) (end 67.14622 130.002) (angle 91.86616649) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 111.85622 69.802) (end 64.90622 69.802) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 115.20622 128.362) (end 115.20622 121.402) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 115.20622 121.402) (end 115.90622 121.402) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 65.60622 121.402) (end 65.60622 128.442) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 67.14622 130.002) (end 113.77622 130.002) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 64.90622 69.802) (end 64.90622 111.7056) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 111.85622 72.502) (end 111.85622 69.802) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 115.90622 111.7056) (end 115.90622 72.502) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 64.90622 121.402) (end 65.60622 121.402) (layer Edge.Cuts) (width 0.0254))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias allowed) (copperpour allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.377104 109.57814) (xy 76.100264 109.55528) (xy 76.201864 106.20502) (xy 76.824164 105.62082) (xy 77.736024 105.61574)
        (xy 86.303444 105.59034)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.81816 105.6231) (xy 76.1984 106.2073) (xy 76.0968 109.54994) (xy 86.36856 109.57534) (xy 86.2949 105.59516)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias allowed) (copperpour allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.7029 109.03966) (xy 86.7029 109.49686) (xy 92.32646 109.49686) (xy 92.32646 108.85424) (xy 92.97924 108.85424)
        (xy 92.97924 106.3371) (xy 92.34424 106.3371) (xy 92.34424 105.7148) (xy 87.9094 105.73258) (xy 87.9094 108.73486)
        (xy 87.89924 108.73486) (xy 86.71052 108.73232) (xy 86.71306 108.72724) (xy 86.71052 108.72724)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.91034 105.73486) (xy 87.91034 108.73714) (xy 86.714 108.73714) (xy 86.714 109.48136) (xy 92.31216 109.48136)
        (xy 92.31216 108.84382) (xy 92.96748 108.84382) (xy 92.96748 106.34446) (xy 92.33756 106.34446) (xy 92.33756 105.72216)
        (xy 89.8763 105.72216)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias allowed) (copperpour allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.24774 103.34498) (xy 82.18932 100.66528) (xy 103.90886 100.59416) (xy 104.80548 101.30536) (xy 104.95788 103.8606)
        (xy 104.18572 104.59974) (xy 95.29318 104.67848) (xy 94.31528 104.16032) (xy 92.86748 104.89184) (xy 80.53832 105.08488)
        (xy 80.9498 103.79202) (xy 81.09204 103.73868)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.21058 100.67772) (xy 82.26646 103.35488) (xy 80.95328 103.7943) (xy 80.54434 105.077) (xy 92.86588 104.8865)
        (xy 94.31368 104.14736) (xy 95.2992 104.66806) (xy 104.1765 104.58424) (xy 104.94358 103.84764) (xy 104.77848 101.30764)
        (xy 103.90472 100.62438) (xy 93.4958 100.62438)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.90782 122.98934) (xy 65.60566 122.98934) (xy 65.60566 121.40692) (xy 64.90716 121.40692) (xy 64.90716 69.80682)
        (xy 115.90782 69.80682)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.74582 81.27492) (xy 82.1944 81.30286) (xy 82.21599 77.91323) (xy 89.76741 77.88529)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.91194 90.18524) (xy 95.8088 90.297) (xy 95.99676 117.08384) (xy 94.39402 117.5258) (xy 86.42096 106.98988)
        (xy 83.62696 100.28174) (xy 81.68894 95.3643) (xy 81.57718 83.25612) (xy 83.96224 83.21802)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.68742 80.57642) (xy 78.56474 83.7692) (xy 71.49846 82.68335) (xy 75.08494 79.02321)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.74916 88.53932) (xy 68.71208 88.5063) (xy 68.53936 84.58708) (xy 70.72884 83.9978)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.27646 88.56726) (xy 71.0057 88.56726) (xy 71.0057 82.96656) (xy 73.27646 82.96656)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.91544 130.03784) (xy 64.90716 130.03784) (xy 64.90716 69.80682) (xy 115.91544 69.80682)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.86774 84.56168) (xy 87.87638 86.55304) (xy 87.21852 86.55304) (xy 87.21852 83.21294) (xy 89.86774 83.21294)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.62848 76.59751) (xy 85.63864 78.63332) (xy 85.63356 80.947895) (xy 75.09256 81.007335) (xy 75.35164 74.71156)
        (xy 83.07578 74.338815)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.15016 94.70644) (xy 87.5411 94.75724) (xy 87.5411 83.22818) (xy 92.86748 83.22564)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.64012 118.61038) (xy 112.04448 121.49328) (xy 113.157 121.50852) (xy 104.21874 121.8565) (xy 107.64012 118.53926)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.80192 117.33784) (xy 101.631053 117.33784) (xy 101.66096 118.59768) (xy 102.13848 118.70944) (xy 104.33304 121.7422)
        (xy 103.64724 121.98604) (xy 100.39604 119.03964) (xy 98.906239 117.33784) (xy 96.39808 117.33784) (xy 96.39808 97.27692)
        (xy 106.81208 96.98736)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.60052 117.7544) (xy 92.9894 120.36552) (xy 92.2782 119.65432) (xy 92.2782 115.7224)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.4992 94.90456) (xy 83.74888 99.99472) (xy 82.58556 100.81768) (xy 77.60716 95.83928) (xy 77.60716 80.75168)
        (xy 82.4992 80.75168)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.20424 131.0386) (xy 65.6082 131.0386) (xy 65.6082 122.8344) (xy 115.20424 122.8344)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.67084 121.65076) (xy 114.67084 121.1326) (xy 115.6716 121.1326)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.65112 89.18448) (xy 67.24396 89.18448) (xy 67.24396 85.852) (xy 68.65112 84.44484)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.36256 119.04472) (xy 65.04432 119.08536) (xy 65.04432 85.62848) (xy 76.36256 85.58784)
      )
    )
  )
)
