(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 106)
    (zones 0)
    (modules 14)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(R1-Pad1)")
  (net 6 "Net-(BZ1-Pad2)")
  (net 7 PB0)
  (net 8 PB1)
  (net 9 PB5-Reset)
  (net 10 PB2)
  (net 11 "Net-(Q1-Pad1)")
  (net 12 "Net-(R4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(BZ1-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net PB0)
    (add_net PB1)
    (add_net PB2)
    (add_net PB5-Reset)
    (add_net VCC)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 154.35 98.65 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J4 (at 1 7.55 180) (layer F.SilkS))
    (fp_text value CONN-2x3 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 PB5-Reset))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 PB0))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 PB2))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 PB1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buzzer_Beeper:Buzzer_12x9.5RM7.6 (layer B.Cu) (tedit 5A030281)
    (at 144.75 92.9 270)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference BZ1 (at -2.75 4 270) (layer B.SilkS))
    (fp_text value Buzzer (at 3.8 -7.4 270) (layer B.Fab))
    (fp_text user %R (at 3.8 4 270) (layer B.Fab))
    (fp_text user + (at -0.01 2.54 270) (layer B.SilkS))
    (fp_text user + (at -0.01 2.54 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 7.6 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(BZ1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 144.6 87.825 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 11 "Net-(Q1-Pad1)"))
    (pad 1 smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 12 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D28A5E3)
    (at 144.9 96.725 270)
    (attr smd)
    (fp_text reference Q1 (at -0.275 2.8 180) (layer F.SilkS))
    (fp_text value MMBT3904-7-F (at 0.025 3.25 90) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95 270) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q1-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 270) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0 270) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(BZ1-Pad2)") (solder_mask_margin 0.07))
  )
  (module digikey-footprints:PinHeader_1x2_P2.54mm (layer F.Cu) (tedit 5A57D437)
    (at 160.75 100.75 180)
    (fp_text reference J3 (at 1.5 -1.75) (layer F.SilkS))
    (fp_text value CONN-2 (at 1.26 2.84) (layer F.Fab))
    (fp_text user %R (at 1.2 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0.02 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 VCC))
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 149.5 81.75 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 3.35 0.15) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-8 (layer F.Cu) (tedit 5A02FF57)
    (at 151.25 87)
    (descr "module CMS SOT223 8 pins, https://www.diodes.com/assets/Datasheets/ZXSBMR16PT8.pdf")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at -0.05 -2.05) (layer F.SilkS))
    (fp_text value ATtiny13A-PU (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 2 smd rect (at -3.4 -0.76) (size 2.8 0.95) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R4-Pad1)"))
    (pad 4 smd rect (at -3.4 2.3) (size 2.8 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.4 -2.3) (size 2.8 0.95) (layers F.Cu F.Paste F.Mask)
      (net 9 PB5-Reset))
    (pad 3 smd rect (at -3.4 0.76) (size 2.8 0.95) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R1-Pad1)"))
    (pad 6 smd rect (at 3.4 0.76) (size 2.8 0.95) (layers F.Cu F.Paste F.Mask)
      (net 8 PB1))
    (pad 8 smd rect (at 3.4 -2.3) (size 2.8 0.95) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 5 smd rect (at 3.4 2.3) (size 2.8 0.95) (layers F.Cu F.Paste F.Mask)
      (net 7 PB0))
    (pad 7 smd rect (at 3.4 -0.76) (size 2.8 0.95) (layers F.Cu F.Paste F.Mask)
      (net 10 PB2))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:PinHeader_1x2_P2.54mm (layer F.Cu) (tedit 5A57D437)
    (at 158.55 83.35)
    (fp_text reference J2 (at 1.25 -2.45) (layer F.SilkS))
    (fp_text value "Fridge magnetic switches" (at 1.48 4.41) (layer F.Fab))
    (fp_text user %R (at 1.3 -0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0.02) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module digikey-footprints:PinHeader_1x2_P2.54mm (layer F.Cu) (tedit 5A57D437)
    (at 159.75 93.21 270)
    (fp_text reference J1 (at 2.54 2 180) (layer F.SilkS))
    (fp_text value B2B-XH-A_LF__SN_ (at 1.48 4.41 90) (layer F.Fab))
    (fp_text user %R (at 1.3 -0.1 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0.02 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 PB0))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 PB1))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 159.25 87.25 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 3.1 0.05 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 10 PB2))
    (pad 1 smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 161.75 87.25 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -3.1 0.1 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 4 "Net-(J2-Pad2)"))
    (pad 1 smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 10 PB2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 153.75 92.75)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1.25 2) (layer F.SilkS))
    (fp_text value 300 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 5 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 153.8 95.3)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 141.2 83.1 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at -2.75 -0.1 180) (layer F.SilkS))
    (fp_text value 100uF (at 1 3.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 1 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text + (at 154.35 102.85) (layer B.SilkS))
  (gr_text GND (at 149.15 102.75) (layer B.SilkS))
  (gr_text GND (at 157.95 102.25) (layer B.SilkS))
  (gr_text + (at 162.6 100.55) (layer B.SilkS))
  (gr_text GND (at 157.9 102.5) (layer F.SilkS))
  (gr_text + (at 162.55 100.75) (layer F.SilkS))
  (gr_text GND (at 157.65 81.25) (layer F.SilkS))
  (gr_text Pin1 (at 145.45 83.85) (layer F.SilkS))
  (gr_text GND (at 147.85 90.6) (layer F.SilkS))
  (gr_text + (at 155.4 83.55) (layer F.SilkS))
  (gr_text GND (at 149.3 102.9) (layer F.SilkS))
  (gr_text + (at 154.35 102.85) (layer F.SilkS))
  (gr_text Battery (at 159.45 98.8) (layer F.SilkS))
  (gr_text - (at 147.2 101.1) (layer F.SilkS))
  (gr_text RX (at 162.25 95.75) (layer F.SilkS))
  (gr_text TX (at 162.25 93.25) (layer F.SilkS))
  (gr_text "Fridge Alarm V4\nSherman Stebbins\n09/18/2021\nupdated 03/1/2022" (at 149.75 87.55) (layer B.SilkS))
  (dimension 25 (width 0.15) (layer Dwgs.User)
    (gr_text "25.000 mm" (at 150.75 76.95) (layer Dwgs.User))
    (feature1 (pts (xy 163.25 79.25) (xy 163.25 77.663579)))
    (feature2 (pts (xy 138.25 79.25) (xy 138.25 77.663579)))
    (crossbar (pts (xy 138.25 78.25) (xy 163.25 78.25)))
    (arrow1a (pts (xy 163.25 78.25) (xy 162.123496 78.836421)))
    (arrow1b (pts (xy 163.25 78.25) (xy 162.123496 77.663579)))
    (arrow2a (pts (xy 138.25 78.25) (xy 139.376504 78.836421)))
    (arrow2b (pts (xy 138.25 78.25) (xy 139.376504 77.663579)))
  )
  (dimension 24 (width 0.15) (layer Dwgs.User)
    (gr_text "24.000 mm" (at 166.55 91.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 163.25 103.25) (xy 165.836421 103.25)))
    (feature2 (pts (xy 163.25 79.25) (xy 165.836421 79.25)))
    (crossbar (pts (xy 165.25 79.25) (xy 165.25 103.25)))
    (arrow1a (pts (xy 165.25 103.25) (xy 164.663579 102.123496)))
    (arrow1b (pts (xy 165.25 103.25) (xy 165.836421 102.123496)))
    (arrow2a (pts (xy 165.25 79.25) (xy 164.663579 80.376504)))
    (arrow2b (pts (xy 165.25 79.25) (xy 165.836421 80.376504)))
  )
  (gr_text R.S. (at 154.75 82) (layer F.SilkS))
  (gr_text Serial (at 160.75 98) (layer F.SilkS))
  (gr_line (start 138.25 103.25) (end 138.25 79.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 163.25 103.25) (end 138.25 103.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 163.25 79.25) (end 163.25 103.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 138.25 79.25) (end 163.25 79.25) (layer Edge.Cuts) (width 0.05))
)
