(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 51)
    (tracks 311)
    (zones 0)
    (modules 58)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 0.61)
    (user_trace_width 1)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.762 0.381)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 2.9)
    (pad_drill 1.15)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (pad_to_paste_clearance -0.0508)
    (aux_axis_origin 0 0)
    (grid_origin 90.24 150.3)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C2-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C12-Pad1)")
  (net 5 "Net-(C13-Pad1)")
  (net 6 "Net-(U1-Pad5)")
  (net 7 "Net-(U1-Pad1)")
  (net 8 "Net-(U2-Pad1)")
  (net 9 "Net-(U2-Pad5)")
  (net 10 "Net-(C20-Pad1)")
  (net 11 "Net-(C21-Pad1)")
  (net 12 "Net-(C23-Pad2)")
  (net 13 "Net-(C24-Pad2)")
  (net 14 "Net-(C11-Pad2)")
  (net 15 "Net-(C1-Pad2)")
  (net 16 "Net-(J1-Pad8)")
  (net 17 "Net-(J1-Pad6)")
  (net 18 "Net-(J1-Pad4)")
  (net 19 "Net-(J1-Pad2)")
  (net 20 "Net-(C3-Pad2)")
  (net 21 "Net-(C4-Pad1)")
  (net 22 "Net-(C6-Pad1)")
  (net 23 "Net-(C13-Pad2)")
  (net 24 "Net-(C14-Pad1)")
  (net 25 "Net-(C16-Pad1)")
  (net 26 "Net-(C22-Pad1)")
  (net 27 "Net-(C25-Pad2)")
  (net 28 "Net-(C26-Pad2)")
  (net 29 "Net-(C26-Pad1)")
  (net 30 "Net-(R20-Pad2)")
  (net 31 "Net-(R21-Pad1)")
  (net 32 "Net-(R24-Pad2)")
  (net 33 "Net-(J2-Pad7)")
  (net 34 "Net-(J2-Pad5)")
  (net 35 "Net-(J2-Pad3)")
  (net 36 "Net-(J2-Pad1)")
  (net 37 "Net-(C27-Pad1)")
  (net 38 "Net-(C27-Pad2)")
  (net 39 "Net-(C28-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C24-Pad2)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C26-Pad2)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C27-Pad2)")
    (add_net "Net-(C28-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R24-Pad2)")
  )
  (net_class SMD ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class grounds ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
  )
  (net_class signal ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad5)")
  )
  (module AptParts:C_Rect_L7.2mm_W4.5mm_MC (layer F.Cu) (tedit 5E5D3379)
    (at 97.205 146.315 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C2 (at 5.045 1.645) (layer F.SilkS))
    (fp_text value 70p (at 2.5 3.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.65))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:C_Rect_L7.2mm_W4.5mm_MC (layer F.Cu) (tedit 5E5D3379)
    (at 83.205 146.315)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C12 (at 5.035 -1.595) (layer F.SilkS))
    (fp_text value 70p (at 2.5 3.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.65))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:MSOP-16-rect-paste-4 (layer F.Cu) (tedit 5E5ABB76)
    (at 90.24 122.385)
    (descr "MSOP, 16 Pin (http://cds.linear.com/docs/en/datasheet/37551fd.pdf#page=23), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (solder_paste_margin -0.02)
    (zone_connect 2)
    (attr smd)
    (fp_text reference U3 (at -3.44 -1.875) (layer F.SilkS))
    (fp_text value LTC3260 (at 0 2.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 17 smd trapezoid (at 0 1.31 90) (size 0.275 1.5) (rect_delta -0.2 0 ) (layers F.Cu F.Paste)
      (net 3 GND) (zone_connect 2))
    (pad 17 smd trapezoid (at 0 -1.31 90) (size 0.275 1.5) (rect_delta 0.2 0 ) (layers F.Cu F.Paste)
      (net 3 GND) (zone_connect 2))
    (pad 17 smd roundrect (at -0.71 0.575) (size 0.275 1) (layers F.Cu F.Paste) (roundrect_rratio 0.15)
      (net 3 GND) (zone_connect 2))
    (pad 17 smd roundrect (at 0.71 0.575) (size 0.275 1) (layers F.Cu F.Paste) (roundrect_rratio 0.15)
      (net 3 GND) (zone_connect 2))
    (pad 17 smd roundrect (at 0.71 -0.575) (size 0.275 1) (layers F.Cu F.Paste) (roundrect_rratio 0.15)
      (net 3 GND) (zone_connect 2))
    (pad 17 smd roundrect (at -0.71 -0.575) (size 0.275 1) (layers F.Cu F.Paste) (roundrect_rratio 0.15)
      (net 3 GND) (zone_connect 2))
    (pad 1 smd roundrect (at -2.15 -1.75) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C20-Pad1)") (zone_connect 2))
    (pad 2 smd roundrect (at -2.15 -1.25) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(R24-Pad2)") (zone_connect 2))
    (pad 3 smd roundrect (at -2.15 -0.75) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(C25-Pad2)") (zone_connect 2))
    (pad 4 smd roundrect (at -2.15 -0.25) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(R21-Pad1)") (zone_connect 2))
    (pad 5 smd roundrect (at -2.15 0.25) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C23-Pad2)") (zone_connect 2))
    (pad 6 smd roundrect (at -2.15 0.75) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C21-Pad1)") (zone_connect 2))
    (pad 7 smd roundrect (at -2.15 1.25) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(C26-Pad2)") (zone_connect 2))
    (pad 8 smd roundrect (at -2.15 1.75) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(C26-Pad2)") (zone_connect 2))
    (pad 9 smd roundrect (at 2.15 1.75) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(C26-Pad1)") (zone_connect 2))
    (pad 10 smd roundrect (at 2.15 1.25) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(C26-Pad1)") (zone_connect 2))
    (pad 11 smd roundrect (at 2.15 0.75) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C20-Pad1)") (zone_connect 2))
    (pad 12 smd roundrect (at 2.15 0.25) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(C22-Pad1)") (zone_connect 2))
    (pad 13 smd roundrect (at 2.15 -0.25) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C20-Pad1)") (zone_connect 2))
    (pad 14 smd roundrect (at 2.15 -0.75) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (zone_connect 2))
    (pad 15 smd roundrect (at 2.15 -1.25) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R20-Pad2)") (zone_connect 2))
    (pad 16 smd roundrect (at 2.15 -1.75) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C24-Pad2)") (zone_connect 2))
    (pad 17 thru_hole roundrect (at 0 0) (size 1.7 2.9) (drill oval 1.15 2.35) (layers *.Cu *.Mask) (roundrect_rratio 0.15)
      (net 3 GND) (zone_connect 2))
    (model ${KIPRJMOD}/Lib/3D/LTC3260.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:CP_SMD_Tant_AVX-B-25v (layer F.Cu) (tedit 5E59936C)
    (at 64.24 117.045 180)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C15 (at 3.01 0.055 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.725 0 180) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.725 0 180) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 24 "Net-(C14-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/AVX-B-25v.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:CP_SMD_Tant_AVX-B-25v (layer F.Cu) (tedit 5E59936C)
    (at 116.23 126.59 180)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C7 (at -3.1 0 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.725 0 180) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 22 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -1.725 0 180) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 3 GND))
    (model ${KIPRJMOD}/Lib/3D/AVX-B-25v.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:CP_SMD_Tant_AVX-B-25v (layer F.Cu) (tedit 5E59936C)
    (at 64.24 126.595)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C17 (at -3.01 -0.005 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.725 0) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 25 "Net-(C16-Pad1)"))
    (pad 1 smd roundrect (at -1.725 0) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 3 GND))
    (model ${KIPRJMOD}/Lib/3D/AVX-B-25v.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:CP_SMD_Tant_AVX-B-25v (layer F.Cu) (tedit 5E59936C)
    (at 116.23 117.09)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C5 (at 3.1 0 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.725 0) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.725 0) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 21 "Net-(C4-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/AVX-B-25v.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:CP_SMD_Tant_AVX-B-35v (layer F.Cu) (tedit 5E5993C5)
    (at 102.82 121.89 270)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C9 (at -3.09 -0.09 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.725 0 270) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 22 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -1.725 0 270) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 21 "Net-(C4-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/AVX-B-35v.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:CP_SMD_Tant_AVX-B-35v (layer F.Cu) (tedit 5E5993C5)
    (at 77.61 121.87 270)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C19 (at -3.055 0.08 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.725 0 270) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 25 "Net-(C16-Pad1)"))
    (pad 1 smd roundrect (at -1.725 0 270) (size 1.65 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.189)
      (net 24 "Net-(C14-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/AVX-B-35v.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:C_Rect_P10-5_MC_Kemet_Blue_Pinsock (layer F.Cu) (tedit 5E507C6E)
    (at 78.705 146.29 180)
    (descr "C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 10.00mm  length 13mm width 6mm Capacitor")
    (fp_text reference C11 (at -0.195 2.01) (layer F.SilkS))
    (fp_text value 220p (at 5 4.25) (layer F.Fab))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 14 "Net-(C11-Pad2)"))
    (pad 1 thru_hole circle (at 2.5 0 180) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 14 "Net-(C11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/Kem-PFR-box.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (offset (xyz 2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (offset (xyz 7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (offset (xyz 10 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:C_Rect_P10-5_MC_Kemet_Blue_Pinsock (layer F.Cu) (tedit 5E507C6E)
    (at 111.755 146.29 180)
    (descr "C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 10.00mm  length 13mm width 6mm Capacitor")
    (fp_text reference C1 (at 9.975 1.96) (layer F.SilkS))
    (fp_text value 220p (at 5 4.25) (layer F.Fab))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 2.5 0 180) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/Kem-PFR-box.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (offset (xyz 2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (offset (xyz 7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (offset (xyz 10 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55C_3320B_Pinsock (layer F.Cu) (tedit 5E5A902E)
    (at 62.53 130.99 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R16 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 332 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 5 "Net-(C13-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 39 "Net-(C28-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/RN55C_3320B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (offset (xyz 10.16 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55C_3320B_Pinsock (layer F.Cu) (tedit 5E507AB7)
    (at 114.24 131 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 332 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 37 "Net-(C27-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 38 "Net-(C27-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/RN55C_3320B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (offset (xyz 10.16 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55C_7R50B_Pinsock (layer F.Cu) (tedit 5E50786E)
    (at 66.23 130.99 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R15 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 7.5 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 39 "Net-(C28-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/RN55C_7R50B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (offset (xyz 10.16 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55C_7R50B_Pinsock (layer F.Cu) (tedit 5E50786E)
    (at 117.905 130.99 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -0.1 90) (layer F.SilkS))
    (fp_text value 7.5 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.62) (layers *.Cu *.Mask)
      (net 38 "Net-(C27-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/RN55C_7R50B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/Lib/3D/MM-0666.wrl
      (offset (xyz 10.16 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:R_SMD-30k1 (layer F.Cu) (tedit 5B301BBD)
    (at 90.23 117.49 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at -2.55 0 180) (layer F.SilkS))
    (fp_text value 30k1 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 32 "Net-(R24-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (model ${KIPRJMOD}/Lib/3D/R_SMD-30k1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-0.1u (layer F.Cu) (tedit 5E3F7DE4)
    (at 116.13 120.49)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.6 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 "Net-(C4-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C1206C104K3GACTU.step
      (offset (xyz -1.7 0.9 1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-0.1u (layer F.Cu) (tedit 5E3F7DE4)
    (at 116.13 123.19)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.6 -0.1 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 "Net-(C6-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C1206C104K3GACTU.step
      (offset (xyz -1.7 0.9 1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-0.1u (layer F.Cu) (tedit 5E3F7DE4)
    (at 106.03 121.89 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -2.5 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 "Net-(C4-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C1206C104K3GACTU.step
      (offset (xyz -1.7 0.9 1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-0.1u (layer F.Cu) (tedit 5E3F7DE4)
    (at 64.365 120.495 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 2.535 0.005 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 24 "Net-(C14-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C1206C104K3GACTU.step
      (offset (xyz -1.7 0.9 1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-0.1u (layer F.Cu) (tedit 5E3F7DE4)
    (at 64.365 123.195 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 2.535 0.005 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 25 "Net-(C16-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C1206C104K3GACTU.step
      (offset (xyz -1.7 0.9 1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-0.1u (layer F.Cu) (tedit 5E3F7DE4)
    (at 74.43 121.89 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at -2.555 0.06) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 25 "Net-(C16-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 24 "Net-(C14-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C1206C104K3GACTU.step
      (offset (xyz -1.7 0.9 1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-10n (layer F.Cu) (tedit 5E3F7E23)
    (at 93.155 117.49 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at -2.55 0.025 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 "Net-(C24-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (model ${KIPRJMOD}/Lib/3D/C1206C103F3GACTU.step
      (offset (xyz -1.7 0.9 1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-10n (layer F.Cu) (tedit 5E3F7E23)
    (at 87.305 117.49 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at -2.55 -0.025 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 "Net-(C25-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (model ${KIPRJMOD}/Lib/3D/C1206C103F3GACTU.step
      (offset (xyz -1.7 0.9 1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-1uF (layer F.Cu) (tedit 5B301BBE)
    (at 90.21 126.315 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at -0.02 -1.385) (layer F.SilkS))
    (fp_text value 1 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 "Net-(C26-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 29 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.75))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-47p (layer F.Cu) (tedit 5E3EFD97)
    (at 110.18 116.615 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -0.025 1.425) (layer F.SilkS))
    (fp_text value 50p (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 20 "Net-(C3-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 37 "Net-(C27-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C1206C470F4GACTU.step
      (offset (xyz -1.7 0.9 0.85))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module AptParts:C_1206_Kemet-47p (layer F.Cu) (tedit 5E3EFD97)
    (at 70.28 116.59 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -0.05 1.4 180) (layer F.SilkS))
    (fp_text value 50p (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(C13-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(C13-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C1206C470F4GACTU.step
      (offset (xyz -1.7 0.9 0.85))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module AptParts:R_Dale-SMD-95K3 (layer F.Cu) (tedit 5B301BBD)
    (at 95.98 117.49 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -2.55 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 "Net-(R20-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (model ${KIPRJMOD}/Lib/3D/Dale-SMD-95K3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:R_Dale-SMD-95K3 (layer F.Cu) (tedit 5B301BBD)
    (at 84.405 117.49 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at -2.55 -0.025 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 31 "Net-(R21-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (model ${KIPRJMOD}/Lib/3D/Dale-SMD-95K3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:R_Dale-SMD-866k (layer F.Cu) (tedit 5B301BBD)
    (at 98.93 117.49 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 2.55 0 180) (layer F.SilkS))
    (fp_text value 909k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 "Net-(R20-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(C22-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/Dale-SMD-866K.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:R_Dale-SMD-866k (layer F.Cu) (tedit 5B301BBD)
    (at 81.53 117.49 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at -2.55 -0.1 180) (layer F.SilkS))
    (fp_text value 909k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(C23-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 31 "Net-(R21-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/Dale-SMD-866K.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:R_KOA-SMD-10R0 (layer F.Cu) (tedit 5B301BBD)
    (at 104.63 116.59)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0.05 -1.4) (layer F.SilkS))
    (fp_text value 10 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 "Net-(C4-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(C22-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/KOA-SMD-10R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:R_KOA-SMD-10R0 (layer F.Cu) (tedit 5B301BBD)
    (at 104.655 127.14)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.4) (layer F.SilkS))
    (fp_text value 10 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(C23-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/KOA-SMD-10R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:R_KOA-SMD-10R0 (layer F.Cu) (tedit 5B301BBD)
    (at 75.85 116.59 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0.02 1.4 180) (layer F.SilkS))
    (fp_text value 10 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 24 "Net-(C14-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(C22-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/KOA-SMD-10R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:R_KOA-SMD-10R0 (layer F.Cu) (tedit 5B301BBD)
    (at 75.85 127.14 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0.02 1.4 180) (layer F.SilkS))
    (fp_text value 10 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 25 "Net-(C16-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(C23-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/KOA-SMD-10R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:SO_AD797 (layer F.Cu) (tedit 5C97300E)
    (at 70.03 121.89 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at -4.16 -1.94 180) (layer F.SilkS))
    (fp_text value AD797 (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C13-Pad2)"))
    (pad 7 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C14-Pad1)"))
    (pad 6 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C13-Pad1)"))
    (pad 5 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(U1-Pad5)"))
    (pad 4 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C16-Pad1)"))
    (pad 3 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C11-Pad2)"))
    (pad 2 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(C28-Pad2)"))
    (pad 1 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(U1-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/SO_AD797-markup.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:SO_AD797 (layer F.Cu) (tedit 5C97300E)
    (at 110.43 121.89 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at -4.225 -1.94 180) (layer F.SilkS))
    (fp_text value AD797 (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C3-Pad2)"))
    (pad 7 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C4-Pad1)"))
    (pad 6 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C27-Pad1)"))
    (pad 5 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(U2-Pad5)"))
    (pad 4 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C6-Pad1)"))
    (pad 3 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C1-Pad2)"))
    (pad 2 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(C27-Pad2)"))
    (pad 1 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(U2-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/SO_AD797-markup.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:Molex_KK-156_1x10_P3.96mm_Horizontal (layer B.Cu) (tedit 5E5AAAC4)
    (at 108.04 152.12 180)
    (descr "JST VH series connector, B10PS-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST VH top entry")
    (fp_text reference J3 (at 17.653 -2.286 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x10_Female (at 17.7165 -10.8585) (layer B.Fab))
    (fp_text user %R (at 17.78 -6.1595 180) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 GND) (thermal_width 0.762) (thermal_gap 0.508))
    (pad 2 thru_hole circle (at 3.96 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 3 thru_hole circle (at 7.92 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at 11.88 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 4 "Net-(C12-Pad1)"))
    (pad 5 thru_hole circle (at 15.84 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 10 "Net-(C20-Pad1)"))
    (pad 6 thru_hole circle (at 19.8 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at 23.76 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 8 thru_hole circle (at 27.72 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 9 thru_hole circle (at 31.68 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 14 "Net-(C11-Pad2)"))
    (pad 10 thru_hole circle (at 35.64 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 GND) (thermal_width 0.762) (thermal_gap 0.508))
    (model ${KIPRJMOD}/Lib/3D/009483105.stp
      (offset (xyz 17.85619973182678 -9.829799852371217 -4.013199939727783))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 180))
    )
  )
  (module AptParts:TP_THTPad_D2.2mm_Drill1.8mm (layer F.Cu) (tedit 5D6C4E59)
    (at 62.73 151.79)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference H1 (at 0 -2.148) (layer F.Fab))
    (fp_text value MountingHole (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.8) (layers *.Cu *.Mask))
  )
  (module AptParts:TP_THTPad_D2.2mm_Drill1.8mm (layer F.Cu) (tedit 5D6C4E59)
    (at 117.93 151.79)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference H2 (at 0 -2.148) (layer F.Fab))
    (fp_text value MountingHole (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.8) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 84.1 122.22)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0.02 -1.85) (layer F.SilkS))
    (fp_text value 10u (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(C23-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 96.33 122.2)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 10u (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 5E583A5E)
    (at 88.38 139.84 180)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J1 (at 1.25 9.95) (layer F.SilkS) hide)
    (fp_text value Conn_02x04_Counter_Clockwise (at 1.27 9.95) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 5E583A69)
    (at 94.63 139.84 180)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J2 (at 1.255 9.92) (layer F.SilkS) hide)
    (fp_text value Conn_02x04_Counter_Clockwise (at 1.27 9.95) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 96.33 126.29)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 -1.84 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 84.11 126.31 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0.02 1.86 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55D-49R9F (layer F.Cu) (tedit 5E233CE3)
    (at 97.17 141.29)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.04 0) (layer F.SilkS))
    (fp_text value 49.9 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/RN55D-49R9F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55D-1000F (layer F.Cu) (tedit 5E233CE3)
    (at 97.17 137.79)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 0) (layer F.SilkS))
    (fp_text value 100 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad3)"))
    (model ${KIPRJMOD}/Lib/3D/RN55D-1000F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55D-2000F (layer F.Cu) (tedit 5E233CE3)
    (at 97.17 134.29)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.14 0) (layer F.SilkS))
    (fp_text value 200 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad5)"))
    (model ${KIPRJMOD}/Lib/3D/RN55D-2000F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55D-4020F (layer F.Cu) (tedit 5E233CE3)
    (at 97.17 130.79)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.14 0) (layer F.SilkS))
    (fp_text value 402 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad7)"))
    (model ${KIPRJMOD}/Lib/3D/RN55D-4020F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55D_3011F (layer F.Cu) (tedit 5E233CE3)
    (at 110.53 130.99 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 3k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C27-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/RN55D_3011F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55D-49R9F (layer F.Cu) (tedit 5E233CE3)
    (at 83.3 141.29 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 5.08 0) (layer F.SilkS))
    (fp_text value 49.9 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/RN55D-49R9F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55D-1000F (layer F.Cu) (tedit 5E233CE3)
    (at 83.3 137.79 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 5.08 0) (layer F.SilkS))
    (fp_text value 100 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad4)"))
    (model ${KIPRJMOD}/Lib/3D/RN55D-1000F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55D-2000F (layer F.Cu) (tedit 5E233CE3)
    (at 83.3 134.29 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 5.08 0) (layer F.SilkS))
    (fp_text value 200 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad6)"))
    (model ${KIPRJMOD}/Lib/3D/RN55D-2000F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55D-4020F (layer F.Cu) (tedit 5E233CE3)
    (at 83.3 130.79 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at 5.1 0) (layer F.SilkS))
    (fp_text value 402 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad8)"))
    (model ${KIPRJMOD}/Lib/3D/RN55D-4020F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AptParts:RN55D_3011F (layer F.Cu) (tedit 5E233CE3)
    (at 69.93 130.99 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R17 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 3k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C12-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C13-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/RN55D_3011F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 62.54 136.1 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C28 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value C (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 39 "Net-(C28-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 5 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 114.24 136 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C27 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value C (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 37 "Net-(C27-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 38 "Net-(C27-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Apt Holman Preamp\nLOMC plug-in board\nv2.0 ©2020 SCD" (at 110.84 117.7) (layer B.SilkS))
  (gr_text Gain (at 116.04 129.6) (layer F.SilkS))
  (gr_text "Load Capacitance" (at 106.75 149.98) (layer F.SilkS))
  (gr_text "Load Capacitance" (at 73.87 149.99) (layer F.SilkS))
  (gr_text Left (at 93.33 129.99) (layer F.SilkS))
  (gr_text Right (at 87.13 129.99) (layer F.SilkS))
  (gr_text Gain (at 64.43 129.6) (layer F.SilkS))
  (gr_text "Load Resistance" (at 90.33 142.19) (layer F.SilkS))
  (gr_line (start 121.24 114.01) (end 59.23 114.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.24 153.94) (end 121.24 114.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112.76 153.94) (end 121.24 153.94) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 68.04 153.94) (end 68.04 160.02) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 59.23 153.94) (end 68.04 153.94) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112.76 153.94) (end 112.76 160.02) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 59.23 114.01) (end 59.23 153.94) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 68.04 160.02) (end 112.76 160.02) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1))
    (polygon
      (pts
        (xy 98.04 116.5) (xy 101.14 119.2) (xy 106.34 141.6) (xy 108.04 147) (xy 111.24 150.9)
        (xy 111.24 155.09) (xy 105.3 155) (xy 98.24 147.3) (xy 98.24 145) (xy 98.24 130.5)
        (xy 97.44 129.7) (xy 83.04 129.7) (xy 82.24 130.5) (xy 82.24 145) (xy 82.24 146.7)
        (xy 74.6 155.09) (xy 69.24 155.1) (xy 69.24 150.5) (xy 72.34 147.1) (xy 74.14 141.55)
        (xy 79.24 119.2) (xy 82.44 116.5)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1))
    (polygon
      (pts
        (xy 105.39 155.02) (xy 105.39 150.1) (xy 115.54 141.3) (xy 115.54 130.9) (xy 115.54 128.1)
        (xy 115.54 114.4) (xy 120.94 114.4) (xy 120.94 145.2) (xy 110.47 155.02)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 99.95 120.6) (xy 99.94 123.8) (xy 97.04 123.8) (xy 97.05 120.6)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 80.5 120.6) (xy 80.5 127.9) (xy 83.38 127.9) (xy 83.38 120.6)
      )
    )
  )
  (zone (net 1) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.2 152.1) (xy 85.1 155.1) (xy 91.2 155.1)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1))
    (polygon
      (pts
        (xy 74.9 155.1) (xy 74.9 150.09) (xy 65.84 142.424867) (xy 64.94 141.1) (xy 64.94 131)
        (xy 64.94 128.1) (xy 64.94 114.39) (xy 59.44 114.4) (xy 59.44 145.3) (xy 70.04 155.1)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 99.95 124.7) (xy 99.94 127.9) (xy 97.04 127.9) (xy 97.05 124.7)
      )
    )
  )
)
