<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.1">
<drawing>
<board>
<plain>
<wire x1="35.56" y1="0" x2="35.56" y2="17.76" width="0" layer="20"/>
<wire x1="35.56" y1="17.76" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<text>Geppetto Electronics
XMega32E5 breakout
v1.0.2</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>A6</text>
<text>A7</text>
<text>C0</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>GND</text>
<text>PDI
D</text>
<text>PDI
C</text>
<text>C4</text>
<text>C5</text>
<text>C6</text>
<text>C7</text>
<text>D0</text>
<text>D1</text>
<text>D2</text>
<text>D3</text>
<text>D4</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>Vcc</text>
<text>C0</text>
<text>C1</text>
<text>C2</text>
<text>C5</text>
<text>D1</text>
<text>D2</text>
<text>D3</text>
<text>PDI
D</text>
<text>GND</text>
<text>D5</text>
<text>Vcc</text>
<text>A7</text>
<text>A6</text>
<text>A3</text>
<text>D7</text>
<text>D6</text>
<text>A5</text>
<text>A4</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors-new">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X14">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="XTAL3215">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="15pF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="15pF">
<attribute name="NAME"/>
</element>
<element name="IC1" library="avr-7" package="TQFP32-08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors-new" package="1X14" value="M14"/>
<element name="JP2" library="SparkFun-Connectors-new" package="1X14" value="M14"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="U$1" library="avr-7" package="AVR-ISP-6" value="AVR-PDIVERT"/>
<element name="X1" library="adafruit" package="XTAL3215" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="L1" library="SparkFun-Passives" package="0805" value="400Ω">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="JP2" pad="14"/>
<contactref element="IC1" pad="17"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="6"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="14"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="18"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="PDI-D">
<contactref element="JP1" pad="13"/>
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="C3">
<contactref element="IC1" pad="13"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="C2">
<contactref element="IC1" pad="14"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="C1">
<contactref element="IC1" pad="15"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="C0">
<contactref element="IC1" pad="16"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="A7">
<contactref element="IC1" pad="29"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="A6">
<contactref element="IC1" pad="30"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="A5">
<contactref element="IC1" pad="31"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="A4">
<contactref element="IC1" pad="2"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="3"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="4"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="5"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="6"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="PDI-C">
<contactref element="JP2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="C4">
<contactref element="IC1" pad="12"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="C5">
<contactref element="IC1" pad="11"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="C6">
<contactref element="IC1" pad="10"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="C7">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="D0">
<contactref element="IC1" pad="28"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="D1">
<contactref element="IC1" pad="27"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="D2">
<contactref element="IC1" pad="26"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="24"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="23"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="22"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="21"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="D3">
<contactref element="IC1" pad="25"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="N$1">
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="20"/>
<contactref element="X1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="19"/>
<contactref element="X1" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="32"/>
<contactref element="C5" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="L1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
