<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="15.24" y1="25.3899625" x2="15.24" y2="2.54" width="0" layer="20"/>
<wire x1="15.24" y1="2.54" x2="16.51" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="16.51" y1="1.27" x2="69.85" y2="1.27" width="0" layer="20"/>
<wire x1="69.85" y1="1.27" x2="71.12" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="71.12" y1="2.54" x2="71.12" y2="25.4" width="0" layer="20"/>
<wire x1="71.12" y1="25.4" x2="69.8499625" y2="26.66" width="0" layer="20" curve="90"/>
<wire x1="69.8499625" y1="26.66" x2="16.51" y2="26.67" width="0" layer="20"/>
<wire x1="16.51" y1="26.67" x2="15.24" y2="25.3899625" width="0" layer="20" curve="90"/>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>A5</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>GND</text>
<text>ARef</text>
<text>AVcc</text>
<text>D13</text>
<text>D12</text>
<text>D11</text>
<text>D10</text>
<text>D9</text>
<text>D8</text>
<text>D7</text>
<text>D6</text>
<text>D5</text>
<text>X2</text>
<text>X1</text>
<text>GND</text>
<text>VCC</text>
<text>D4</text>
<text>D3</text>
<text>D2</text>
<text>D1</text>
<text>D0</text>
<text>RST</text>
<text>C1</text>
<text>22pF</text>
<text>C2</text>
<text>22pF</text>
<text>Bare Bones Arduino, V2 - Kevin Rye, 2013</text>
<text>SCL</text>
<text>SDA</text>
<text>PWM</text>
<text>PWM</text>
<text>PWM</text>
<text>PWM</text>
<text>PWM</text>
<text>RX</text>
<text>TX</text>
<text>PWM</text>
<text>MISO</text>
<text>SCK</text>
<text>MOSI</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>VCC</text>
<text>GND</text>
</plain>
<libraries>
<library name="atmel">
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="1X02">
</package>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
<package name="OSHW-LOGO-S">
</package>
<package name="1X08">
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="DIL28-3" value="ATMEGA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="AXIAL-0.4" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="SparkFun" package="1X02" value="VCC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun" package="HC49US" value="16MHz">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C025-024X044" value="22pF"/>
<element name="C1" library="adafruit" package="C025-024X044" value="22pF"/>
<element name="LED" library="adafruit" package="LED3MM" value="Pin 13 BLINK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="R1" library="SparkFun" package="AXIAL-0.4" value="For LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="18"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="R2" pad="P$2"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="20"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="22"/>
<contactref element="IC1" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="GND" pad="2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP1" pad="7"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="9"/>
<contactref element="Y1" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="10"/>
<contactref element="Y1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="4"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="5"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="6"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="17"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="M8RXD">
<contactref element="IC1" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="19"/>
<contactref element="JP2" pad="2"/>
<contactref element="LED" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="11"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="12"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="13"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="14"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="15"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="16"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="23"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="24"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="25"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="26"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="IC1" pad="27"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="IC1" pad="28"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="3"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="1"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="P$2"/>
<contactref element="LED" pad="K"/>
</signal>
<signal name="N$23">
<contactref element="JP1" pad="8"/>
<contactref element="IC1" pad="21"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
