(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 33)
    (zones 0)
    (modules 2)
    (nets 14)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VCC)
  (net 2 /GND)
  (net 3 /CS)
  (net 4 /CLK)
  (net 5 /MISO)
  (net 6 /MOSI)
  (net 7 "Net-(J1-Pad7)")
  (net 8 /~HOLD)
  (net 9 "Net-(J2-Pad1)")
  (net 10 "Net-(J2-Pad3)")
  (net 11 "Net-(J2-Pad5)")
  (net 12 "Net-(J2-Pad9)")
  (net 13 "Net-(J2-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CLK)
    (add_net /CS)
    (add_net /GND)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /VCC)
    (add_net /~HOLD)
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad9)")
  )
  (module Connector_PinSocket_1.27mm:PinSocket_2x06_P1.27mm_Vertical_SMD (layer B.Cu) (tedit 5A19A42F)
    (at 201.93 125.73)
    (descr "surface-mounted straight socket strip, 2x06, 1.27mm pitch, double cols (from Kicad 4.0.7!), script generated")
    (tags "Surface mounted socket strip SMD 2x06 1.27mm double row")
    (attr smd)
    (fp_text reference J2 (at 1.27 -5.3975) (layer B.Fab))
    (fp_text value UP (at -1.5875 -5.3975 180) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at 1.8 3.175) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -1.8 3.175) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 3 smd rect (at 1.8 1.905) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at -1.8 1.905) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (pad 5 smd rect (at 1.8 0.635) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at -1.8 0.635) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 /CS))
    (pad 7 smd rect (at 1.8 -0.635) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 /CLK))
    (pad 8 smd rect (at -1.8 -0.635) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 /MISO))
    (pad 9 smd rect (at 1.8 -1.905) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J2-Pad9)"))
    (pad 10 smd rect (at -1.8 -1.905) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J2-Pad10)"))
    (pad 11 smd rect (at 1.8 -3.175) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 /MOSI))
    (pad 12 smd rect (at -1.8 -3.175) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 /~HOLD))
    (model ${KISYS3DMOD}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_2x06_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 59FED5CC)
    (at 193.675 125.095 180)
    (descr "surface-mounted straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x04 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at 3.4925 6.985) (layer F.Fab))
    (fp_text value DediProg (at -1.5875 6.985) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -3.81 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /VCC))
    (pad 2 smd rect (at 2.525 -3.81 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 3 smd rect (at -2.525 -1.27 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /CS))
    (pad 4 smd rect (at 2.525 -1.27 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /CLK))
    (pad 5 smd rect (at -2.525 1.27 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /MISO))
    (pad 6 smd rect (at 2.525 1.27 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI))
    (pad 7 smd rect (at -2.525 3.81 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at 2.525 3.81 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /~HOLD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "UP2/Xtreme\nto DediProg\n(C) 2020\nSerge Kise" (at 202.2475 125.73 270) (layer F.SilkS))
  (gr_line (start 204.978 129.286) (end 204.978 122.174) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 198.628 129.54) (end 204.724 129.54) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 198.628 130.556) (end 198.628 129.54) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 189.357 130.81) (end 198.374 130.81) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 189.103 119.634) (end 189.103 130.556) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 198.374 119.38) (end 189.357 119.38) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 198.628 121.92) (end 198.628 119.634) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 204.724 121.92) (end 198.628 121.92) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 189.357 119.634) (end 189.357 119.38) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 198.374 119.634) (end 198.628 119.634) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 204.724 122.174) (end 204.978 122.174) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 204.724 129.286) (end 204.724 129.54) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 198.374 130.556) (end 198.374 130.81) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 189.357 130.556) (end 189.103 130.556) (angle -90) (layer Edge.Cuts) (width 0.05))
)
