(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 137)
    (no_connects 2)
    (area 64.145 60.219 174.854 90.932)
    (thickness 1.6)
    (drawings 4)
    (tracks 273)
    (zones 0)
    (modules 69)
    (nets 64)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 66.167 90.297)
    (grid_origin 66.167 90.297)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C7-Pad1)")
  (net 5 "Net-(C9-Pad2)")
  (net 6 "Net-(C10-Pad2)")
  (net 7 +3V3)
  (net 8 GNDA)
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 "Net-(D3-Pad2)")
  (net 12 "Net-(D4-Pad2)")
  (net 13 "Net-(D5-Pad1)")
  (net 14 "Net-(IC1-Pad1)")
  (net 15 "Net-(IC1-Pad2)")
  (net 16 "Net-(IC1-Pad9)")
  (net 17 "Net-(IC1-Pad10)")
  (net 18 "Net-(IC1-Pad11)")
  (net 19 "Net-(IC1-Pad12)")
  (net 20 "Net-(IC1-Pad13)")
  (net 21 "Net-(IC1-Pad14)")
  (net 22 "Net-(IC1-Pad15)")
  (net 23 "Net-(IC1-Pad16)")
  (net 24 "Net-(IC1-Pad17)")
  (net 25 "Net-(IC1-Pad19)")
  (net 26 "Net-(IC1-Pad22)")
  (net 27 "Net-(IC1-Pad23)")
  (net 28 "Net-(IC1-Pad24)")
  (net 29 "Net-(IC1-Pad25)")
  (net 30 "Net-(IC1-Pad26)")
  (net 31 "Net-(IC1-Pad27)")
  (net 32 "Net-(IC1-Pad28)")
  (net 33 "Net-(IC1-Pad29)")
  (net 34 "Net-(IC1-Pad30)")
  (net 35 "Net-(IC1-Pad31)")
  (net 36 "Net-(IC1-Pad32)")
  (net 37 "Net-(J1-Pad2)")
  (net 38 "Net-(L1-Pad2)")
  (net 39 "Net-(P1-Pad5)")
  (net 40 "Net-(P1-Pad2)")
  (net 41 "Net-(P1-Pad3)")
  (net 42 "Net-(R1-Pad2)")
  (net 43 "Net-(R2-Pad2)")
  (net 44 "Net-(R6-Pad2)")
  (net 45 "Net-(R7-Pad2)")
  (net 46 "Net-(U1-Pad2)")
  (net 47 "Net-(U1-Pad3)")
  (net 48 "Net-(U1-Pad6)")
  (net 49 "Net-(U1-Pad9)")
  (net 50 "Net-(U1-Pad10)")
  (net 51 "Net-(U1-Pad11)")
  (net 52 "Net-(U1-Pad12)")
  (net 53 "Net-(U1-Pad13)")
  (net 54 "Net-(U1-Pad14)")
  (net 55 "Net-(U1-Pad19)")
  (net 56 "Net-(U1-Pad27)")
  (net 57 "Net-(U1-Pad28)")
  (net 58 "Net-(U5-Pad2)")
  (net 59 "Net-(U5-Pad4)")
  (net 60 "Net-(U5-Pad5)")
  (net 61 "Net-(U5-Pad6)")
  (net 62 "Net-(U5-Pad7)")
  (net 63 "Net-(U6-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad17)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad29)")
    (add_net "Net-(IC1-Pad30)")
    (add_net "Net-(IC1-Pad31)")
    (add_net "Net-(IC1-Pad32)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U6-Pad7)")
    (add_net VCC)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B7247)
    (at 156.718 69.723)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GNDA))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B7247)
    (at 160.528 71.628)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GNDA))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B7247)
    (at 159.385 71.628)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GNDA))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B7247)
    (at 158.369 72.136)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GNDA))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B7247)
    (at 151.638 72.644)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GNDA))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B7247)
    (at 143.129 78.486)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GNDA))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B7247)
    (at 147.955 72.771)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GNDA))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B7247)
    (at 150.495 86.487)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GNDA))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B7247)
    (at 141.097 81.788)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GNDA))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B7247)
    (at 140.97 77.47)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GNDA))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 110.109 81.407)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 127 85.217)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 115.57 67.31)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 127.381 72.644)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 111.76 87.63)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 103.505 80.518)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 93.853 88.011)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 84.963 86.868)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 105.029 76.835)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 111.633 70.739)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 109.728 74.676)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 94.615 73.406)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 79.756 74.168)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 111.633 66.04 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 109.347 79.629 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 85.09 78.74 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 10n (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 102.616 75.946)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 130.81 74.93)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 91.186 87.757)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 85.09 73.66 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 83.82 83.058)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1u (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 107.061 87.63)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 22p (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 116.713 87.63)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 22p (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 91.186 83.185)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1u (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 91.186 85.471)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 4.7u (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 130.81 72.771)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 150.495 70.231)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 140.208 75.565)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 152.527 76.073)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 153.543 72.644 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 100.711 84.582 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value TXLED (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 100.711 82.296 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value RXLED (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 100.711 86.868 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D3 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value PWRLED1 (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 150.622 65.786)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D4 (at 0 -1.75) (layer F.SilkS))
    (fp_text value PWRLED2 (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 57A876D4)
    (at 157.099 74.295 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D5 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D_TVS (at 0.1 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 90) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1.055 0 90) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 110.871 73.025 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -6.05 90) (layer F.SilkS))
    (fp_text value ATMEGA328P-A (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C9-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad15)"))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad16)"))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad17)"))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad29)"))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(IC1-Pad30)"))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(IC1-Pad31)"))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(IC1-Pad32)"))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PTH_sx3wiz:ScrewTerminal_5mm_2Pos (layer F.Cu) (tedit 59FFB48A)
    (at 168.529 76.2 270)
    (fp_text reference J1 (at 3.25 4.25 270) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x02 (at 0.75 -5.25 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 0 270) (size 1.9 1.9) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 GNDA))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.9 1.9) (drill 1.3) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 85.09 76.2 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value Ferrite (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(L1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module USB:USB-B1HSxx (layer F.Cu) (tedit 59FFADF9)
    (at 71.12 74.93 270)
    (fp_text reference P1 (at 5 6 270) (layer F.SilkS))
    (fp_text value USB_B (at -2 -11 270) (layer F.Fab))
    (pad 5 thru_hole circle (at -6.02 0 270) (size 3.33 3.33) (drill 2.33) (layers *.Cu *.Mask)
      (net 39 "Net-(P1-Pad5)"))
    (pad 5 thru_hole circle (at 6.02 0 270) (size 3.33 3.33) (drill 2.33) (layers *.Cu *.Mask)
      (net 39 "Net-(P1-Pad5)"))
    (pad 2 thru_hole circle (at -1.25 -4.71 270) (size 1.42 1.42) (drill 0.92) (layers *.Cu *.Mask)
      (net 40 "Net-(P1-Pad2)"))
    (pad 1 thru_hole circle (at 1.25 -4.71 270) (size 1.42 1.42) (drill 0.92) (layers *.Cu *.Mask)
      (net 38 "Net-(L1-Pad2)"))
    (pad 3 thru_hole circle (at -1.25 -2.71 270) (size 1.42 1.42) (drill 0.92) (layers *.Cu *.Mask)
      (net 41 "Net-(P1-Pad3)"))
    (pad 4 thru_hole circle (at 1.25 -2.71 270) (size 1.42 1.42) (drill 0.92) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 54EA0A4B)
    (at 121.031 66.294)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1) (layer F.SilkS))
    (fp_text value ICSP (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(IC1-Pad16)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad17)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(IC1-Pad15)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(IC1-Pad29)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 96.266 84.582 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 270R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 96.266 82.296 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 270R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 123.063 75.565 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 4.7kR (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(IC1-Pad27)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 125.603 75.565 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 4.7kR (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad28)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 96.266 86.868 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 270R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 144.145 75.311 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 4.7kR (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 146.812 75.311 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 4.7kR (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 150.495 67.945 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 270R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58307BE8)
    (at 160.274 74.295 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value "16K 2%" (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58307BE8)
    (at 162.179 78.74 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value "1M 2%" (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 94.615 73.66 180)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -6.25 180) (layer F.SilkS))
    (fp_text value FT232RL (at 0 6.25 180) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(IC1-Pad30)"))
    (pad 2 smd rect (at -3.6 -3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 5 smd rect (at -3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(IC1-Pad31)"))
    (pad 6 smd rect (at -3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at -3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at -3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at -3.6 3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at -3.6 4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 3.6 4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(P1-Pad3)"))
    (pad 16 smd rect (at 3.6 3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(P1-Pad2)"))
    (pad 17 smd rect (at 3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (pad 18 smd rect (at 3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 21 smd rect (at 3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R2-Pad2)"))
    (pad 23 smd rect (at 3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R1-Pad2)"))
    (pad 24 smd rect (at 3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at 3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 27 smd rect (at 3.6 -3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at 3.6 -4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U1-Pad28)"))
    (model Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-10_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 84.963 86.741)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U2 (at 0 -2.6) (layer F.SilkS))
    (fp_text value AP2112 (at 0 2.6) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at -2.2 -0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.2 0) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at -2.2 0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.2 1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 6 smd rect (at 2.2 1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.2 0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.2 0) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.2 -0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.2 -1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (model Housings_SSOP.3dshapes/MSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 136.144 79.883)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -3.5) (layer F.SilkS))
    (fp_text value SI860x (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(IC1-Pad27)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad28)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R7-Pad2)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R6-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-10_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 150.241 80.645 90)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U5 (at 0 -2.6 90) (layer F.SilkS))
    (fp_text value ADS1015 (at 0 2.6 90) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -1 90) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad 2 smd rect (at -2.2 -0.5 90) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U5-Pad2)"))
    (pad 3 smd rect (at -2.2 0 90) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad 4 smd rect (at -2.2 0.5 90) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U5-Pad4)"))
    (pad 5 smd rect (at -2.2 1 90) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U5-Pad5)"))
    (pad 6 smd rect (at 2.2 1 90) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U5-Pad6)"))
    (pad 7 smd rect (at 2.2 0.5 90) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U5-Pad7)"))
    (pad 8 smd rect (at 2.2 0 90) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 9 smd rect (at 2.2 -0.5 90) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R6-Pad2)"))
    (pad 10 smd rect (at 2.2 -1 90) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R7-Pad2)"))
    (model Housings_SSOP.3dshapes/MSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 157.353 68.072 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 0 -3.5 180) (layer F.SilkS))
    (fp_text value LM358 (at 0 3.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U5-Pad4)"))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U5-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D5-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U6-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-SD_SMD (layer F.Cu) (tedit 0)
    (at 112.903 83.566 180)
    (descr "Crystal Quarz HC49-SD SMD")
    (tags "Crystal Quarz HC49-SD SMD")
    (attr smd)
    (fp_text reference Y1 (at 0 -5.08 180) (layer F.SilkS))
    (fp_text value 16M (at 2.54 5.08 180) (layer F.Fab))
    (pad 1 smd rect (at -4.84886 0 180) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 4.84886 0 180) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C9-Pad2)"))
  )
  (module PTH_sx3wiz:MEF1 (layer F.Cu) (tedit 59FFC290)
    (at 140.081 69.85)
    (descr SIP9)
    (tags SIP9)
    (fp_text reference U4 (at -10 -6.25) (layer F.SilkS))
    (fp_text value MEF1 (at -2 2.75) (layer F.Fab))
    (pad 1 thru_hole rect (at -10.16 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -7.62 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 GNDA))
    (pad 7 thru_hole circle (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model Housings_SIP.3dshapes/SIP9_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 102.743 73.152 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad29)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PTH_sx3wiz:Via-0.6mm (layer F.Cu) (tedit 5A1B6FA2)
    (at 77.343 79.375)
    (fp_text reference REF** (at 0.5 1.25) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm (at 0.25 -1.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (gr_line (start 172.72 90.297) (end 66.167 90.297) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 63.246) (end 172.72 90.297) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.167 63.246) (end 172.72 63.246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.167 90.297) (end 66.167 63.246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 90.297) (xy 66.167 90.297) (xy 66.167 63.246) (xy 134.112 63.373)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 90.17) (xy 66.167 90.17) (xy 66.167 63.246) (xy 134.112 63.246)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.72 90.297) (xy 138.684 90.297) (xy 138.684 63.246) (xy 172.72 63.246)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.72 90.297) (xy 138.684 90.297) (xy 138.684 63.246) (xy 172.72 63.246)
      )
    )
  )
)
