(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 51)
    (tracks 544)
    (zones 0)
    (modules 51)
    (nets 39)
  )
  (page A)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7526 2.6924)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance -0.0508)
    (aux_axis_origin 126.5681 117.6986)
    (grid_origin 126.3141 117.6986)
    (visible_elements 7FFFFF3F)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /A+)
  (net 3 /B-)
  (net 4 "Net-(J4-Pad14)")
  (net 5 "Net-(J4-Pad12)")
  (net 6 "Net-(J4-Pad10)")
  (net 7 "Net-(J4-Pad9)")
  (net 8 "Net-(J4-Pad8)")
  (net 9 "Net-(J4-Pad7)")
  (net 10 /Vbstin)
  (net 11 /Vbat)
  (net 12 /SDA)
  (net 13 /SCL)
  (net 14 "Net-(U3-Pad6)")
  (net 15 /5Vsw)
  (net 16 /3Von)
  (net 17 +3V0)
  (net 18 /RXp)
  (net 19 /TXp)
  (net 20 /TXb)
  (net 21 /RXb)
  (net 22 /D4_AL)
  (net 23 "Net-(J10-Pad2)")
  (net 24 /LEDB)
  (net 25 "Net-(J4-Pad17)")
  (net 26 "Net-(J4-Pad13)")
  (net 27 "Net-(LED1-Pad2)")
  (net 28 "Net-(LED1-Pad4)")
  (net 29 /VbatGnd)
  (net 30 "Net-(R9-Pad2)")
  (net 31 "Net-(TP1-Pad1)")
  (net 32 /unfuse)
  (net 33 +12V)
  (net 34 "Net-(C8-Pad1)")
  (net 35 "Net-(Q1-Pad3)")
  (net 36 /sdiProt)
  (net 37 "Net-(J11-Pad1)")
  (net 38 "Net-(J4-Pad18)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /3Von)
    (add_net /A+)
    (add_net /B-)
    (add_net /D4_AL)
    (add_net /LEDB)
    (add_net /RXb)
    (add_net /RXp)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TXb)
    (add_net /TXp)
    (add_net /VbatGnd)
    (add_net /sdiProt)
    (add_net /unfuse)
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad12)")
    (add_net "Net-(J4-Pad13)")
    (add_net "Net-(J4-Pad14)")
    (add_net "Net-(J4-Pad17)")
    (add_net "Net-(J4-Pad18)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J4-Pad9)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED1-Pad4)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(TP1-Pad1)")
    (add_net "Net-(U3-Pad6)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V0)
    (add_net /5Vsw)
    (add_net /Vbat)
    (add_net /Vbstin)
    (add_net GND)
  )
  (net_class PwrMin ""
    (clearance 0.1524)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 177.8761 112.4154 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value zero (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /sdiProt))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 174.8046 115.4634)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0.2305 1.524) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /sdiProt))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 +3V0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-23-3 (layer Top) (tedit 5D28A5E3)
    (at 174.8281 112.5764 90)
    (attr smd)
    (fp_text reference Q1 (at 0.415 -2.413 180) (layer F.SilkS))
    (fp_text value BSS138 (at 0.025 3.25 90) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95 90) (size 1.3 0.6) (layers Top F.Paste F.Mask)
      (net 17 +3V0) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 90) (size 1.3 0.6) (layers Top F.Paste F.Mask)
      (net 36 /sdiProt) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0 90) (size 1.3 0.6) (layers Top F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad3)") (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOD-123 (layer Top) (tedit 5D28A50F)
    (at 176.9361 107.0814)
    (attr smd)
    (fp_text reference Z1 (at 0.432 2.032) (layer F.SilkS))
    (fp_text value 7.5V (at 0.07 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad A smd rect (at 1.575 0) (size 0.9 0.95) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad K smd rect (at -1.575 0) (size 0.9 0.95) (layers Top F.Paste F.Mask)
      (net 34 "Net-(C8-Pad1)"))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Top) (tedit 5F68FEEE)
    (at 171.9071 104.6029 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 1.2553 -2.413 180) (layer F.SilkS))
    (fp_text value 510R (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 34 "Net-(C8-Pad1)"))
    (pad 1 smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 35 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer Top) (tedit 5F68FEEE)
    (at 175.9581 103.2714)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 2.908 0) (layer F.SilkS))
    (fp_text value 3300pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Top) (tedit 5F68FEEE)
    (at 176.4791 100.1619 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0.0655 2.286 90) (layer F.SilkS))
    (fp_text value 510R (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 37 "Net-(J11-Pad1)"))
    (pad 1 smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 34 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 172.0341 108.7324 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at -0.2032 1.778 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(Q1-Pad3)"))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /5Vsw))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 175.7406 104.9224 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -2.8975 -0.127) (layer F.SilkS))
    (fp_text value 200K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C8-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:PinHeader_1x3_P2.54mm_Drill1.02mm (layer Bottom) (tedit 5A43C851)
    (at 173.4311 96.1594 180)
    (descr http://www.molex.com/pdm_docs/sd/022232031_sd.pdf)
    (fp_text reference J11 (at 3.429 5.461) (layer B.SilkS))
    (fp_text value WireTerm (at 2.82 -4.63) (layer B.SilkS) hide)
    (fp_text user %R (at 2.54 0) (layer B.Fab) hide)
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 33 +12V))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 37 "Net-(J11-Pad1)"))
  )
  (module "RS485_Mayfly:JST_S3B-PH-K-S(LF)(SN)" (layer Top) (tedit 608069C1)
    (at 173.0501 98.9534 180)
    (fp_text reference J12 (at 4.699 -2.413) (layer F.SilkS))
    (fp_text value "S3B-PH-K-S(LF)(SN)" (at 12.07775 7.19784) (layer F.Fab))
    (pad 3 thru_hole circle (at 4 0 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 +12V))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(J11-Pad1)"))
  )
  (module RS485_Mayfly:SOIC65P490X110-8N (layer Top) (tedit 607F1006)
    (at 130.4191 106.8646 90)
    (fp_text reference U5 (at 0.64934 2.37708 90) (layer F.SilkS))
    (fp_text value STC3100 (at 7.625 3.282 90) (layer F.Fab))
    (pad 8 smd rect (at 2.12 -0.975 90) (size 1.62 0.49) (layers Top F.Paste F.Mask)
      (net 11 /Vbat))
    (pad 7 smd rect (at 2.12 -0.325 90) (size 1.62 0.49) (layers Top F.Paste F.Mask)
      (net 11 /Vbat))
    (pad 6 smd rect (at 2.12 0.325 90) (size 1.62 0.49) (layers Top F.Paste F.Mask)
      (net 29 /VbatGnd))
    (pad 5 smd rect (at 2.12 0.975 90) (size 1.62 0.49) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.12 0.975 90) (size 1.62 0.49) (layers Top F.Paste F.Mask)
      (net 13 /SCL))
    (pad 3 smd rect (at -2.12 0.325 90) (size 1.62 0.49) (layers Top F.Paste F.Mask)
      (net 12 /SDA))
    (pad 2 smd rect (at -2.12 -0.325 90) (size 1.62 0.49) (layers Top F.Paste F.Mask)
      (net 30 "Net-(R9-Pad2)"))
    (pad 1 smd rect (at -2.12 -0.975 90) (size 1.62 0.49) (layers Top F.Paste F.Mask)
      (net 31 "Net-(TP1-Pad1)"))
  )
  (module Fiducial:Fiducial_0.75mm_Mask1.5mm (layer Top) (tedit 60429118)
    (at 135.2041 116.9366)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Fiducial_0.75mm_Mask1.5mm (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (module Fiducial:Fiducial_0.75mm_Mask1.5mm (layer Top) (tedit 604290D3)
    (at 177.3681 96.7944)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Fiducial_0.75mm_Mask1.5mm (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (module Fiducial:Fiducial_0.75mm_Mask1.5mm (layer Top) (tedit 60429124)
    (at 178.5111 116.6064)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Fiducial_0.75mm_Mask1.5mm (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (module Fiducial:Fiducial_0.75mm_Mask1.5mm (layer Top) (tedit 604290E6)
    (at 131.1401 93.5686)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -2.032) (layer F.SilkS) hide)
    (fp_text value Fiducial_0.75mm_Mask1.5mm (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (module TestPoint:TestPoint_THTPad_1.0x1.0mm_Drill0.5mm (layer Bottom) (tedit 5A0F774F)
    (at 132.6641 108.0466 90)
    (descr "THT rectangular pad as test Point, square 1.0mm side length, hole diameter 0.5mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 1.448 90) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.45 90) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(TP1-Pad1)"))
  )
  (module RS485_Mayfly:LED_Kingbright_APBD3224SURKCGKC-F01 (layer Top) (tedit 603E917A)
    (at 153.4411 110.3214 180)
    (descr "Kingbright, dual LED, 3.2 x 2.4 mm SMD")
    (tags "dual led smd")
    (attr smd)
    (fp_text reference LED1 (at 0.584 2.3256 180) (layer F.SilkS))
    (fp_text value APBD3224SURKCGKC-F01 (at 0 2.5 180) (layer F.Fab))
    (fp_text user * (at 2.54 0.254 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 4 smd rect (at 1.6 -0.7 180) (size 1.6 0.8) (layers Top F.Paste F.Mask)
      (net 28 "Net-(LED1-Pad4)"))
    (pad 1 smd rect (at -1.6 0.7 180) (size 1.6 0.8) (layers Top F.Paste F.Mask)
      (net 17 +3V0))
    (pad 2 smd rect (at 1.6 0.7 180) (size 1.6 0.8) (layers Top F.Paste F.Mask)
      (net 27 "Net-(LED1-Pad2)"))
    (pad 3 smd rect (at -1.6 -0.7 180) (size 1.6 0.8) (layers Top F.Paste F.Mask)
      (net 17 +3V0))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Kingbright_AAA3528ESGCT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 128.7036 110.8406)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 2.4365 0) (layer F.SilkS))
    (fp_text value 649R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R9-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 127.7619 106.9017 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -2.3133 0.1016) (layer F.SilkS))
    (fp_text value 30mOhm (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /VbatGnd))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 144.7526 110.5104)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -0.5607 -1.2192) (layer F.SilkS))
    (fp_text value "Fuse hold155mA" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /unfuse))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RS485_Mayfly:POLOLU_REG (layer Bottom) (tedit 0)
    (at 145.7451 106.3194 90)
    (fp_text reference U2 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value "12v Boost" (at 0 0 270) (layer B.SilkS) hide)
    (fp_text user "Pololu\nVReg" (at 0 6.35 270) (layer B.SilkS))
    (pad VOUT thru_hole circle (at -2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /unfuse) (solder_mask_margin 0.1016))
    (pad GND thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad VIN thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /Vbstin) (solder_mask_margin 0.1016))
  )
  (module RS485_Mayfly:2.0_1X4 (layer Top) (tedit 0)
    (at 136.6011 98.7756 180)
    (fp_text reference J1 (at -5.3214 -0.7924) (layer F.Mask))
    (fp_text value TWIG-2.0-DIP (at -1.7019 -1.9354 180) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 +12V) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /B-) (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /A+) (solder_mask_margin 0.1016))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 148.0311 109.9789 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at -2.3895 0.127 90) (layer F.SilkS))
    (fp_text value 62R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(LED1-Pad4)"))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /RXb))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 149.5551 110.0259 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -2.4365 0.127 90) (layer F.SilkS))
    (fp_text value 120R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(LED1-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /TXb))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical (layer Top) (tedit 5FC4524B)
    (at 167.1131 106.5734 90)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (fp_text reference J10 (at 2.032 1.619 180) (layer F.SilkS))
    (fp_text value "2mm jumper" (at 0 4.06 90) (layer F.Fab))
    (fp_text user %R (at 0 1) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /B-))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer Top) (tedit 5F68FEEE)
    (at 142.9511 107.1954 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.426 0 90) (layer F.SilkS))
    (fp_text value u1F/0603 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 +3V0))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "RS485_Mayfly:SC-70-6_DCK(R-PDSO-G6)" (layer Top) (tedit 0)
    (at 140.556098 108.874401)
    (attr smd)
    (fp_text reference U4 (at -2.684998 0.238999) (layer F.SilkS))
    (fp_text value SN74LVC2G34DCK3 (at 0 0) (layer F.SilkS) hide)
    (fp_text user Designator9 (at -1.651 -2.3876) (layer F.SilkS) hide)
    (fp_text user .Designator (at -0.0508 -0.6604 270) (layer Dwgs.User) hide)
    (fp_text user .Designator (at -0.0508 -0.6604 270) (layer F.Fab) hide)
    (fp_text user * (at 0 0) (layer F.Fab) hide)
    (fp_text user * (at 0 0) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User) hide)
    (pad 6 smd rect (at 1.125002 -0.650001 90) (size 0.399999 0.850001) (layers Top F.Paste F.Mask)
      (net 20 /TXb))
    (pad 5 smd rect (at 1.125002 0 90) (size 0.399999 0.850001) (layers Top F.Paste F.Mask)
      (net 17 +3V0))
    (pad 4 smd rect (at 1.125002 0.649999 90) (size 0.399999 0.850001) (layers Top F.Paste F.Mask)
      (net 18 /RXp))
    (pad 3 smd rect (at -1.124999 0.649999 90) (size 0.399999 0.850001) (layers Top F.Paste F.Mask)
      (net 21 /RXb))
    (pad 2 smd rect (at -1.124999 0 90) (size 0.399999 0.850001) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.124999 -0.650001 90) (size 0.399999 0.850001) (layers Top F.Paste F.Mask)
      (net 19 /TXp))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer Top) (tedit 5F68FEEE)
    (at 130.2133 102.7126 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.394 1.3462) (layer F.SilkS))
    (fp_text value u1F/0603 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /Vbat))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer Top) (tedit 5F68FEEE)
    (at 165.8111 103.3854 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -0.368 -1.524 90) (layer F.SilkS))
    (fp_text value u1F/0603 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /5Vsw))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer Top) (tedit 5F68FEEE)
    (at 161.2391 110.5104)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0.635 1.524) (layer F.SilkS))
    (fp_text value u1F/0603 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 +3V0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer Top) (tedit 5F68FEEE)
    (at 136.8548 106.47688 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1uF/0603 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /Vbstin))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer Top) (tedit 5F68FEEE)
    (at 134.41924 104.61984 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.38028 0.05842 90) (layer F.SilkS))
    (fp_text value u1F/0603 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /Vbat))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 168.2006 108.8594)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 1.1665 1.3462 180) (layer F.SilkS))
    (fp_text value 120R (at 0 1.43 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(J10-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /A+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 167.3371 113.2078)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0.125 1.9508) (layer F.SilkS))
    (fp_text value 649R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /A+))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /5Vsw))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 165.4536 111.0184)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 2.3895 0.5842) (layer F.SilkS))
    (fp_text value 649R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /B-))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit (layer Top) (tedit 5A1DC085)
    (at 177.1141 94.1274)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
    (tags "solder Pin_ loose fit")
    (fp_text reference J13 (at 0.127 2.6162) (layer B.SilkS))
    (fp_text value "GND Wire" (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RS485_Mayfly:B2B-PH-K-SLFSN (layer Top) (tedit 0)
    (at 131.1401 115.888601 270)
    (fp_text reference J9 (at -5.0165 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at -1 0 90) (layer F.SilkS) hide)
    (fp_text user * (at 0 0 90) (layer F.Fab) hide)
    (fp_text user * (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User) hide)
    (pad 2 thru_hole circle (at -2.000001 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0.000001 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 /Vbat))
  )
  (module RS485_Mayfly:E2,5-6E (layer Bottom) (tedit 0)
    (at 140.24092 105.33896 270)
    (descr "<b>ELECTROLYTIC CAPACITOR</b><p>\ngrid 2.54 mm, diameter 6 mm")
    (fp_text reference C1 (at 2.667 1.524 90) (layer B.SilkS))
    (fp_text value CPOL-EUE2,5-6E (at 2.667 -2.54 90) (layer B.Fab) hide)
    (pad + thru_hole circle (at -1.27 0 270) (size 1.5748 1.5748) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 /Vbstin) (solder_mask_margin 0.1016))
    (pad - thru_hole circle (at 1.27 0 270) (size 1.5748 1.5748) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module RS485_Mayfly:B2B-PH-K-SLFSN (layer Top) (tedit 0)
    (at 128.6001 99.632601 270)
    (fp_text reference J8 (at -4.953 -2.2352) (layer F.SilkS))
    (fp_text value Conn_01x02 (at -1 0 90) (layer F.SilkS) hide)
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0.971799 1.778 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 2 thru_hole circle (at -2.000001 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 /VbatGnd))
    (pad 1 thru_hole circle (at 0.000001 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 /Vbat))
  )
  (module RS485_Mayfly:MAX22025AWA&plus_ (layer Top) (tedit 5FA1A8BF)
    (at 160.3247 105.9384)
    (fp_text reference U1 (at -5.4865 -0.894) (layer F.SilkS))
    (fp_text value MAX22025AWA+ (at 0 0) (layer F.SilkS) hide)
    (fp_text user * (at -2.3241 -2.6543) (layer F.Fab))
    (fp_text user * (at -5.1308 -1.6256) (layer F.SilkS))
    (fp_text user 0.058in/1.473mm (at -3.6576 5.1435) (layer Dwgs.User) hide)
    (fp_text user 0.288in/7.315mm (at 0 -5.1435) (layer Dwgs.User) hide)
    (fp_text user 0.022in/0.559mm (at 6.7056 -1.905) (layer Dwgs.User) hide)
    (fp_text user 0.05in/1.27mm (at -6.7056 -1.27) (layer Dwgs.User) hide)
    (fp_text user * (at -2.3241 -2.6543) (layer F.Fab))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 8 smd rect (at 3.6576 -1.905) (size 1.4732 0.5588) (layers Top F.Paste F.Mask)
      (net 15 /5Vsw))
    (pad 7 smd rect (at 3.6576 -0.635) (size 1.4732 0.5588) (layers Top F.Paste F.Mask)
      (net 3 /B-))
    (pad 6 smd rect (at 3.6576 0.635) (size 1.4732 0.5588) (layers Top F.Paste F.Mask)
      (net 2 /A+))
    (pad 5 smd rect (at 3.6576 1.905) (size 1.4732 0.5588) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -3.6576 1.905) (size 1.4732 0.5588) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.6576 0.635) (size 1.4732 0.5588) (layers Top F.Paste F.Mask)
      (net 17 +3V0))
    (pad 2 smd rect (at -3.6576 -0.635) (size 1.4732 0.5588) (layers Top F.Paste F.Mask)
      (net 20 /TXb))
    (pad 1 smd rect (at -3.6576 -1.905) (size 1.4732 0.5588) (layers Top F.Paste F.Mask)
      (net 21 /RXb))
  )
  (module Package_TO_SOT_SMD:SOT-363_SC-70-6 (layer Top) (tedit 5FA1E9D3)
    (at 136.75608 104.32574 180)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference U3 (at -2.1615 0.40918) (layer F.SilkS))
    (fp_text value "SiP32431DR3 0.1mS TurnOn" (at -0.32 2.286 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 6 smd rect (at 0.95 -0.65 180) (size 0.65 0.4) (layers Top F.Paste F.Mask)
      (net 14 "Net-(U3-Pad6)"))
    (pad 4 smd rect (at 0.95 0.65 180) (size 0.65 0.4) (layers Top F.Paste F.Mask)
      (net 11 /Vbat))
    (pad 2 smd rect (at -0.95 0 180) (size 0.65 0.4) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.95 0 180) (size 0.65 0.4) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.95 0.65 180) (size 0.65 0.4) (layers Top F.Paste F.Mask)
      (net 17 +3V0))
    (pad 1 smd rect (at -0.95 -0.65 180) (size 0.65 0.4) (layers Top F.Paste F.Mask)
      (net 10 /Vbstin))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RS485_Mayfly:2.0_1X4 (layer Top) (tedit 0)
    (at 148.5391 98.7756 180)
    (fp_text reference J2 (at -5.1944 -0.7924) (layer F.Mask))
    (fp_text value TWIG-2.0-DIP (at -5.08 -3.81 180) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 +12V) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /B-) (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /A+) (solder_mask_margin 0.1016))
  )
  (module RS485_Mayfly:2X10 locked (layer Bottom) (tedit 0)
    (at 136.9821 113.1266)
    (descr "<h3>Plated Through Hole - 2x10</h3>\n<p>Specifications:\n<ul><li>Pin count:20</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_10x2</li>\n</ul></p>")
    (solder_paste_margin -0.5)
    (fp_text reference J4 (at -2.413 3.302) (layer B.SilkS))
    (fp_text value CONN_10X2 (at -1.27 -2.413) (layer B.Fab))
    (pad 20 thru_hole circle (at 22.86 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 +3V0) (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 22.86 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /5Vsw) (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at 20.32 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad18)") (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at 20.32 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad17)") (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at 17.78 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /SDA) (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at 17.78 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /SCL) (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at 15.24 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(J4-Pad14)") (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at 15.24 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(J4-Pad13)") (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at 12.7 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(J4-Pad12)") (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 12.7 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /LEDB) (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 10.16 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(J4-Pad10)") (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 10.16 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad9)") (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 7.62 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad8)") (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad7)") (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 5.08 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /RXp) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /sdiProt) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 2.54 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /D4_AL) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /TXp) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /3Von) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module RS485_Mayfly:2.0_1X4 (layer Top) (tedit 0)
    (at 160.4771 98.7756 180)
    (fp_text reference J3 (at -5.5754 -0.2844) (layer F.Mask))
    (fp_text value TWIG-2.0-DIP (at -5.08 -3.81 180) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 +12V) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /B-) (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /A+) (solder_mask_margin 0.1016))
  )
  (module RS485_Mayfly:1X04_NOSILK (layer Top) (tedit 0)
    (at 136.6011 95.8546 180)
    (descr "<h3>Plated Through Hole - 4 Pin</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (fp_text reference J5 (at -1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value CONN_42.54_NOSILK (at -1.27 2.032 180) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 +12V) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /B-) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A+) (solder_mask_margin 0.1016))
  )
  (module RS485_Mayfly:1X04_NOSILK (layer Top) (tedit 0)
    (at 148.5391 95.8546 180)
    (descr "<h3>Plated Through Hole - 4 Pin</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (fp_text reference J6 (at -1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value CONN_42.54_NOSILK (at -1.27 2.032 180) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 +12V) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /B-) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A+) (solder_mask_margin 0.1016))
  )
  (module RS485_Mayfly:1X04_NOSILK (layer Top) (tedit 0)
    (at 160.4771 95.8546 180)
    (descr "<h3>Plated Through Hole - 4 Pin</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (fp_text reference J7 (at -1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value CONN_42.54_NOSILK (at -1.27 2.032 180) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 +12V) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /B-) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A+) (solder_mask_margin 0.1016))
  )
  (module RS485_Mayfly:SMT-JUMPER_2_NO_SILK (layer Bottom) (tedit 0)
    (at 148.0311 106.7258 90)
    (fp_text reference JP1 (at -2.159 0 180) (layer B.SilkS))
    (fp_text value JUMPER-SMT_2_NO_SILK (at 0 -1.143 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 0.4064 0 90) (size 0.635 1.27) (layers Bottom B.Mask)
      (net 15 /5Vsw) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.4064 0 90) (size 0.635 1.27) (layers Bottom B.Mask)
      (net 32 /unfuse) (solder_mask_margin 0.1016))
  )
  (module RS485_Mayfly:OSHW-LOGO-MINI (layer Top) (tedit 0)
    (at 134.4421 109.2404)
    (descr "<h3>Open-Source Hardware (OSHW) Logo - Mini - Silkscreen</h3>\n<p>Silkscreen logo for open-source hardware designs.</p>\n<p>Devices using:\n<ul><li>OSHW_LOGO</li></ul></p>")
    (fp_text reference LOGO1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-LOGOMINI (at 0 0) (layer F.SilkS) hide)
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer Top) (tedit 5F68FEEE)
    (at 148.2851 104.7954 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.27) (layer F.SilkS))
    (fp_text value zero (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /5Vsw))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /Vbstin))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "V G D " (at 171.2849 101.7424) (layer F.SilkS))
  (gr_text "V G D " (at 171.2849 94.1224) (layer F.SilkS))
  (gr_text "V G D " (at 171.2849 101.5238 180) (layer B.SilkS))
  (gr_text "V G D " (at 171.1579 93.9038 180) (layer B.SilkS))
  (dimension 25.4 (width 0.15) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 183.6211 104.9986 270) (layer Dwgs.User))
    (feature1 (pts (xy 180.1621 117.6986) (xy 182.907521 117.6986)))
    (feature2 (pts (xy 180.1621 92.2986) (xy 182.907521 92.2986)))
    (crossbar (pts (xy 182.3211 92.2986) (xy 182.3211 117.6986)))
    (arrow1a (pts (xy 182.3211 117.6986) (xy 181.734679 116.572096)))
    (arrow1b (pts (xy 182.3211 117.6986) (xy 182.907521 116.572096)))
    (arrow2a (pts (xy 182.3211 92.2986) (xy 181.734679 93.425104)))
    (arrow2b (pts (xy 182.3211 92.2986) (xy 182.907521 93.425104)))
  )
  (dimension 53.721 (width 0.15) (layer Dwgs.User)
    (gr_text "2.1150 in" (at 153.1746 122.9356) (layer Dwgs.User))
    (feature1 (pts (xy 180.0351 117.6986) (xy 180.0351 122.222021)))
    (feature2 (pts (xy 126.3141 117.6986) (xy 126.3141 122.222021)))
    (crossbar (pts (xy 126.3141 121.6356) (xy 180.0351 121.6356)))
    (arrow1a (pts (xy 180.0351 121.6356) (xy 178.908596 122.222021)))
    (arrow1b (pts (xy 180.0351 121.6356) (xy 178.908596 121.049179)))
    (arrow2a (pts (xy 126.3141 121.6356) (xy 127.440604 122.222021)))
    (arrow2b (pts (xy 126.3141 121.6356) (xy 127.440604 121.049179)))
  )
  (gr_text KNH002r7 (at 162.7631 106.9544 90) (layer B.SilkS))
  (gr_text * (at 128.78298 108.199) (layer F.SilkS))
  (gr_text May (at 128.0921 115.6666 -90) (layer F.SilkS))
  (gr_text + (at 132.2577 116.7334 270) (layer B.SilkS))
  (gr_text + (at 134.9501 115.1586 270) (layer F.SilkS))
  (gr_text + (at 127.2285 101.2902 270) (layer B.SilkS))
  (gr_text + (at 129.06238 103.57874 270) (layer F.SilkS))
  (gr_text * (at 151.2061 109.2404) (layer F.SilkS))
  (gr_text Battery (at 131.1401 97.3786 270) (layer B.SilkS))
  (gr_text Bat (at 127.5079 103.5254 270) (layer F.SilkS))
  (gr_text Mayfly (at 128.6001 113.3806 270) (layer B.SilkS))
  (gr_text * (at 140.335 107.696) (layer F.SilkS))
  (gr_text "Mayfly RS485" (at 165.8111 106.7766 90) (layer B.SilkS))
  (gr_text "G V B A" (at 136.4741 101.1886 180) (layer B.SilkS))
  (gr_text "G V B A" (at 160.1978 101.092 180) (layer B.SilkS))
  (gr_text "G V B A" (at 160.4899 93.6498 180) (layer B.SilkS))
  (gr_text "G V B A" (at 136.3853 93.5228 180) (layer B.SilkS))
  (gr_text "G V B A" (at 148.3487 93.3958 180) (layer B.SilkS))
  (gr_text "G V B A" (at 148.4122 100.9904 180) (layer B.SilkS))
  (gr_text * (at 139.2681 105.8876) (layer F.SilkS))
  (gr_text KNH002r7 (at 139.5221 110.6374) (layer F.SilkS))
  (gr_text "G V B A" (at 148.9075 102.108) (layer F.SilkS))
  (gr_text * (at 154.8891 103.3984) (layer F.SilkS))
  (gr_text "G V B A" (at 160.6041 102.362) (layer F.SilkS))
  (gr_text "G V B A" (at 160.4645 93.7895) (layer F.SilkS))
  (gr_text "G V B A" (at 148.2725 93.472) (layer F.SilkS))
  (gr_text "G V B A" (at 135.89 102.1715) (layer F.SilkS))
  (gr_text "G V B A" (at 136.017 93.5355) (layer F.SilkS))
  (gr_line (start 126.3141 117.6986) (end 180.0352 117.7394) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 180.0352 117.7394) (end 180.0351 92.3086) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 180.0351 92.3086) (end 131.3941 92.2986) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.3941 92.2986) (end 126.3141 97.3086) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.3141 97.3086) (end 126.3141 117.6986) (layer Edge.Cuts) (width 0.05))
  (gr_text Mayfly (at 170.0021 100.6806 90) (layer F.Fab))
  (gr_text "SMC\nRS-485" (at 145.8721 109.8246) (layer F.Fab))
  (gr_text " gnd +V  B  A  gnd +V  B  A   gnd +V  B  A" (at 147.32 93.98) (layer F.Fab))
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.7811 93.1114) (xy 179.5271 117.2414) (xy 127.0761 117.2414) (xy 127.0761 109.2404) (xy 129.4891 107.5894)
        (xy 129.7431 95.9054) (xy 131.6481 94.2544) (xy 133.1721 92.9844)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.4001 117.1144) (xy 135.0136 116.8604) (xy 134.8866 100.0964) (xy 133.2991 100.0964) (xy 131.9021 96.7944)
        (xy 131.9021 92.9844) (xy 179.0191 92.9844)
      )
    )
  )
  (zone (net 11) (net_name /Vbat) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.7911 100.6044) (xy 134.1246 100.6044) (xy 134.2516 115.5904) (xy 131.2671 115.5904) (xy 131.2671 111.6534)
        (xy 129.2351 98.8264) (xy 131.7751 98.8264)
      )
    )
  )
)
