<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="56" x2="0" y2="0" width="0" layer="20"/>
<wire x1="48" y1="56" x2="0" y2="56" width="0" layer="20"/>
<wire x1="47.76" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="8.61" y1="10.01" x2="14" y2="10.01" width="0" layer="20"/>
<wire x1="14" y1="10.01" x2="14" y2="1.81" width="0" layer="20"/>
<wire x1="14" y1="1.81" x2="8.61" y2="1.81" width="0" layer="20"/>
<wire x1="8.61" y1="10.01" x2="8.61" y2="1.81" width="0" layer="20"/>
<wire x1="23.98" y1="10.02" x2="29.37" y2="10.02" width="0" layer="20"/>
<wire x1="29.37" y1="10.02" x2="29.37" y2="1.82" width="0" layer="20"/>
<wire x1="29.37" y1="1.82" x2="23.98" y2="1.82" width="0" layer="20"/>
<wire x1="23.98" y1="10.02" x2="23.98" y2="1.82" width="0" layer="20"/>
<wire x1="47.76" y1="11.88" x2="47.76" y2="0" width="0" layer="20"/>
<wire x1="47.76" y1="11.88" x2="48" y2="56" width="0" layer="20"/>
<wire x1="39.74" y1="10.02" x2="45.13" y2="10.02" width="0" layer="20"/>
<wire x1="45.13" y1="10.02" x2="45.13" y2="1.82" width="0" layer="20"/>
<wire x1="45.13" y1="1.82" x2="39.74" y2="1.82" width="0" layer="20"/>
<wire x1="39.74" y1="10.02" x2="39.74" y2="1.82" width="0" layer="20"/>
<hole x="1.23" y="10.6" drill="0.35"/>
<wire x1="23.98" y1="20" x2="29.37" y2="20" width="0" layer="20"/>
<wire x1="29.37" y1="20" x2="29.37" y2="11.8" width="0" layer="20"/>
<wire x1="29.37" y1="11.8" x2="23.98" y2="11.8" width="0" layer="20"/>
<wire x1="23.98" y1="20" x2="23.98" y2="11.8" width="0" layer="20"/>
<wire x1="39.74" y1="20" x2="45.13" y2="20" width="0" layer="20"/>
<wire x1="45.13" y1="20" x2="45.13" y2="11.8" width="0" layer="20"/>
<wire x1="45.13" y1="11.8" x2="39.74" y2="11.8" width="0" layer="20"/>
<wire x1="39.74" y1="20" x2="39.74" y2="11.8" width="0" layer="20"/>
<wire x1="8.62" y1="20" x2="14.01" y2="20" width="0" layer="20"/>
<wire x1="14.01" y1="20" x2="14.01" y2="11.8" width="0" layer="20"/>
<wire x1="14.01" y1="11.8" x2="8.62" y2="11.8" width="0" layer="20"/>
<wire x1="8.62" y1="20" x2="8.62" y2="11.8" width="0" layer="20"/>
<wire x1="23.98" y1="30.2" x2="29.37" y2="30.2" width="0" layer="20"/>
<wire x1="29.37" y1="30.2" x2="29.37" y2="22" width="0" layer="20"/>
<wire x1="29.37" y1="22" x2="23.98" y2="22" width="0" layer="20"/>
<wire x1="23.98" y1="30.2" x2="23.98" y2="22" width="0" layer="20"/>
<wire x1="39.74" y1="30.2" x2="45.13" y2="30.2" width="0" layer="20"/>
<wire x1="45.13" y1="30.2" x2="45.13" y2="22" width="0" layer="20"/>
<wire x1="45.13" y1="22" x2="39.74" y2="22" width="0" layer="20"/>
<wire x1="39.74" y1="30.2" x2="39.74" y2="22" width="0" layer="20"/>
<wire x1="8.62" y1="30.2" x2="14.01" y2="30.2" width="0" layer="20"/>
<wire x1="14.01" y1="30.2" x2="14.01" y2="22" width="0" layer="20"/>
<wire x1="14.01" y1="22" x2="8.62" y2="22" width="0" layer="20"/>
<wire x1="8.62" y1="30.2" x2="8.62" y2="22" width="0" layer="20"/>
<wire x1="23.96" y1="40.39" x2="29.35" y2="40.39" width="0" layer="20"/>
<wire x1="29.35" y1="40.39" x2="29.35" y2="32.19" width="0" layer="20"/>
<wire x1="29.35" y1="32.19" x2="23.96" y2="32.19" width="0" layer="20"/>
<wire x1="23.96" y1="40.39" x2="23.96" y2="32.19" width="0" layer="20"/>
<wire x1="39.72" y1="40.39" x2="45.11" y2="40.39" width="0" layer="20"/>
<wire x1="45.11" y1="40.39" x2="45.11" y2="32.19" width="0" layer="20"/>
<wire x1="45.11" y1="32.19" x2="39.72" y2="32.19" width="0" layer="20"/>
<wire x1="39.72" y1="40.39" x2="39.72" y2="32.19" width="0" layer="20"/>
<wire x1="8.6" y1="40.39" x2="13.99" y2="40.39" width="0" layer="20"/>
<wire x1="13.99" y1="40.39" x2="13.99" y2="32.19" width="0" layer="20"/>
<wire x1="13.99" y1="32.19" x2="8.6" y2="32.19" width="0" layer="20"/>
<wire x1="8.6" y1="40.39" x2="8.6" y2="32.19" width="0" layer="20"/>
<wire x1="23.96" y1="50.59" x2="29.35" y2="50.59" width="0" layer="20"/>
<wire x1="29.35" y1="50.59" x2="29.35" y2="42.39" width="0" layer="20"/>
<wire x1="29.35" y1="42.39" x2="23.96" y2="42.39" width="0" layer="20"/>
<wire x1="23.96" y1="50.59" x2="23.96" y2="42.39" width="0" layer="20"/>
<wire x1="39.72" y1="50.59" x2="45.11" y2="50.59" width="0" layer="20"/>
<wire x1="45.11" y1="50.59" x2="45.11" y2="42.39" width="0" layer="20"/>
<wire x1="45.11" y1="42.39" x2="39.72" y2="42.39" width="0" layer="20"/>
<wire x1="39.72" y1="50.59" x2="39.72" y2="42.39" width="0" layer="20"/>
<wire x1="8.6" y1="50.59" x2="13.99" y2="50.59" width="0" layer="20"/>
<wire x1="13.99" y1="50.59" x2="13.99" y2="42.39" width="0" layer="20"/>
<wire x1="13.99" y1="42.39" x2="8.6" y2="42.39" width="0" layer="20"/>
<wire x1="8.6" y1="50.59" x2="8.6" y2="42.39" width="0" layer="20"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>A</text>
<text>B</text>
<text>C</text>
</plain>
<libraries>
<library name="transistor-fetSOT223">
<description>&lt;b&gt;Field Effect Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
Symbols changed according to IEC617&lt;p&gt; 
All types, packages and assignment to symbols and pins checked&lt;p&gt;
Package outlines partly checked&lt;p&gt;
&lt;p&gt;
JFET = junction FET&lt;p&gt;
IGBT-x = insulated gate bipolar transistor&lt;p&gt;
x=N: NPN; x=P: PNP&lt;p&gt;
IGFET-mc-nnn; (IGFET=insulated gate field effect transistor)&lt;P&gt;
m=D: depletion mode (Verdr&amp;auml;ngungstyp)&lt;p&gt;
m=E: enhancement mode (Anreicherungstyp)&lt;p&gt;
c: N=N-channel; P=P-Channel&lt;p&gt;
GDSB: gate, drain, source, bulk&lt;p&gt;
&lt;p&gt;
by R. Vogg  15.March.2002</description>
<packages>
<package name="SOT230P700X180-4N">
<description>4-SOT223, 2.30 mm pitch, 7.00 mm span, 6.50 X 3.50 X 1.80 mm body
&lt;p&gt;4-pin SOT223 package with 2.30 mm pitch, 7.00 mm span with body size 6.50 X 3.50 X 1.80 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ORIGINALFOOTPRINT" library="transistor-fetSOT223" package="SOT230P700X180-4N" value="BSP170P">
<attribute name="POPULARITY" value="0"/>
</element>
</elements>
<signals>
<signal name="POUR">
</signal>
<signal name="POUR1">
</signal>
</signals>
</board>
</drawing>
</eagle>
