(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~52~ubuntu17.04.1)
  (general
    (links 16)
    (no_connects 0)
    (area 160.960999 63.26632 181.939001 78.815001)
    (thickness 1.6)
    (drawings 4)
    (tracks 101)
    (zones 0)
    (modules 3)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4064)
    (via_drill 0.127)
    (via_min_size 0.4064)
    (via_min_drill 0.127)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad1)")
  (net 2 "Net-(IC1-Pad2)")
  (net 3 "Net-(IC1-Pad7)")
  (net 4 "Net-(IC1-Pad8)")
  (net 5 "Net-(IC1-Pad3)")
  (net 6 "Net-(IC1-Pad4)")
  (net 7 "Net-(IC1-Pad6)")
  (net 8 "Net-(IC1-Pad5)")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.4064)
    (via_drill 0.127)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
  )
  (module headers:8-PIN (layer F.Cu) (tedit 595BD9DC)
    (at 171.45 66.04)
    (fp_text reference SIL1 (at 0 0) (layer F.SilkS))
    (fp_text value SIL8 (at 0 0) (layer F.SilkS) hide)
    (fp_text user 1 (at -8.89 1.778 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 0) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 0) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 0) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 0) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole circle (at 3.81 0) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole circle (at 6.35 0) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 0) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad8)"))
  )
  (module "Madbean 40xx-2:DIL08" (layer F.Cu) (tedit 595BD9B7)
    (at 176.53 73.025 270)
    (descr "<b>Dual In Line Package</b>")
    (fp_text reference IC2 (at 0.635 1.778 360) (layer F.SilkS))
    (fp_text value TL072 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -3.81 2.159 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad8)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad6)"))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad5)"))
  )
  (module "Madbean 40xx-2:DIL08" (layer F.Cu) (tedit 595BD9A2)
    (at 166.37 73.025 270)
    (descr "<b>Dual In Line Package</b>")
    (fp_text reference IC1 (at 0.635 1.27 360) (layer F.SilkS))
    (fp_text value TL072 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -3.81 2.0955 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad8)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad6)"))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad5)"))
  )
  (gr_line (start 161.036 78.74) (end 161.036 64.516) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.864 78.74) (end 161.036 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.864 64.516) (end 181.864 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.036 64.516) (end 181.864 64.516) (angle 90) (layer Edge.Cuts) (width 0.15))
)
