(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 61)
    (zones 0)
    (modules 3)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4572)
    (via_min_drill 0.2032)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad26)")
  (net 2 "Net-(J1-Pad25)")
  (net 3 "Net-(J1-Pad24)")
  (net 4 "Net-(J1-Pad23)")
  (net 5 "Net-(J1-Pad22)")
  (net 6 "Net-(J1-Pad21)")
  (net 7 "Net-(J1-Pad20)")
  (net 8 "Net-(J1-Pad19)")
  (net 9 "Net-(J1-Pad18)")
  (net 10 "Net-(J1-Pad17)")
  (net 11 "Net-(J1-Pad16)")
  (net 12 "Net-(J1-Pad15)")
  (net 13 "Net-(J1-Pad14)")
  (net 14 "Net-(J1-Pad13)")
  (net 15 /MAI_TTL_RX)
  (net 16 /MAI_TTL_TX)
  (net 17 GND)
  (net 18 +5V)
  (net 19 /MAI_3V3)
  (net 20 "Net-(J1-Pad2)")
  (net 21 "Net-(J1-Pad1)")
  (net 22 "Net-(J2-Pad26)")
  (net 23 "Net-(J2-Pad25)")
  (net 24 /MAI_MOSI)
  (net 25 /MAI_MISO)
  (net 26 /MAG_DRDY)
  (net 27 /MAI_SCK)
  (net 28 /MAG_SS)
  (net 29 /MAG_CLEAR)
  (net 30 "Net-(J2-Pad18)")
  (net 31 "Net-(J2-Pad17)")
  (net 32 "Net-(J2-Pad16)")
  (net 33 "Net-(J2-Pad15)")
  (net 34 "Net-(J2-Pad14)")
  (net 35 "Net-(J2-Pad13)")
  (net 36 "Net-(J2-Pad12)")
  (net 37 "Net-(J2-Pad11)")
  (net 38 "Net-(J2-Pad10)")
  (net 39 "Net-(J2-Pad9)")
  (net 40 "Net-(J2-Pad8)")
  (net 41 "Net-(J2-Pad7)")
  (net 42 "Net-(J2-Pad6)")
  (net 43 "Net-(J2-Pad5)")
  (net 44 "Net-(J2-Pad4)")
  (net 45 "Net-(J2-Pad3)")
  (net 46 "Net-(J2-Pad2)")
  (net 47 "Net-(J2-Pad1)")
  (net 48 "Net-(J1-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /MAG_CLEAR)
    (add_net /MAG_DRDY)
    (add_net /MAG_SS)
    (add_net /MAI_3V3)
    (add_net /MAI_MISO)
    (add_net /MAI_MOSI)
    (add_net /MAI_SCK)
    (add_net /MAI_TTL_RX)
    (add_net /MAI_TTL_TX)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad25)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x13_P2.00mm_Vertical_SMD (layer B.Cu) (tedit 59FED667)
    (at 40 50 90)
    (descr "surface-mounted straight pin header, 2x13, 2.00mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x13 2.00mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 14.06 270) (layer B.SilkS))
    (fp_text value MAI400_J2_flip (at 0 -14.06 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 26 smd rect (at 2.085 -12 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J2-Pad26)"))
    (pad 25 smd rect (at -2.085 -12 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J2-Pad25)"))
    (pad 24 smd rect (at 2.085 -10 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 25 /MAI_MISO))
    (pad 23 smd rect (at -2.085 -10 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 24 /MAI_MOSI))
    (pad 22 smd rect (at 2.085 -8 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 27 /MAI_SCK))
    (pad 21 smd rect (at -2.085 -8 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 26 /MAG_DRDY))
    (pad 20 smd rect (at 2.085 -6 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 29 /MAG_CLEAR))
    (pad 19 smd rect (at -2.085 -6 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 28 /MAG_SS))
    (pad 18 smd rect (at 2.085 -4 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J2-Pad18)"))
    (pad 17 smd rect (at -2.085 -4 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(J2-Pad17)"))
    (pad 16 smd rect (at 2.085 -2 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J2-Pad16)"))
    (pad 15 smd rect (at -2.085 -2 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J2-Pad15)"))
    (pad 14 smd rect (at 2.085 0 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J2-Pad14)"))
    (pad 13 smd rect (at -2.085 0 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(J2-Pad13)"))
    (pad 12 smd rect (at 2.085 2 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J2-Pad12)"))
    (pad 11 smd rect (at -2.085 2 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J2-Pad11)"))
    (pad 10 smd rect (at 2.085 4 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J2-Pad10)"))
    (pad 9 smd rect (at -2.085 4 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J2-Pad9)"))
    (pad 8 smd rect (at 2.085 6 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J2-Pad8)"))
    (pad 7 smd rect (at -2.085 6 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(J2-Pad7)"))
    (pad 6 smd rect (at 2.085 8 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(J2-Pad6)"))
    (pad 5 smd rect (at -2.085 8 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(J2-Pad5)"))
    (pad 4 smd rect (at 2.085 10 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(J2-Pad4)"))
    (pad 3 smd rect (at -2.085 10 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 2.085 12 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -2.085 12 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x13_P2.00mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x13_P2.00mm_Vertical_SMD (layer B.Cu) (tedit 59FED667)
    (at 39 38.9 90)
    (descr "surface-mounted straight pin header, 2x13, 2.00mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x13 2.00mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 14.06 270) (layer B.SilkS))
    (fp_text value MAI400_J1_flip (at 0 -14.06 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 26 smd rect (at 2.085 -12 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad26)"))
    (pad 25 smd rect (at -2.085 -12 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad25)"))
    (pad 24 smd rect (at 2.085 -10 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad24)"))
    (pad 23 smd rect (at -2.085 -10 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad23)"))
    (pad 22 smd rect (at 2.085 -8 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad22)"))
    (pad 21 smd rect (at -2.085 -8 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad21)"))
    (pad 20 smd rect (at 2.085 -6 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad20)"))
    (pad 19 smd rect (at -2.085 -6 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad19)"))
    (pad 18 smd rect (at 2.085 -4 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad18)"))
    (pad 17 smd rect (at -2.085 -4 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J1-Pad17)"))
    (pad 16 smd rect (at 2.085 -2 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J1-Pad16)"))
    (pad 15 smd rect (at -2.085 -2 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J1-Pad15)"))
    (pad 14 smd rect (at 2.085 0 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J1-Pad14)"))
    (pad 13 smd rect (at -2.085 0 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J1-Pad13)"))
    (pad 12 smd rect (at 2.085 2 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 16 /MAI_TTL_TX))
    (pad 11 smd rect (at -2.085 2 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 15 /MAI_TTL_RX))
    (pad 10 smd rect (at 2.085 4 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(J1-Pad10)"))
    (pad 9 smd rect (at -2.085 4 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 8 smd rect (at 2.085 6 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (pad 7 smd rect (at -2.085 6 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 6 smd rect (at 2.085 8 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (pad 5 smd rect (at -2.085 8 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 4 smd rect (at 2.085 10 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 19 /MAI_3V3))
    (pad 3 smd rect (at -2.085 10 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 2 smd rect (at 2.085 12 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -2.085 12 90) (size 2.58 1) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x13_P2.00mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 5EAC9A07)
    (at 48.4 56.3 270)
    (descr "Through hole IDC box header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x08 2.54mm double row")
    (fp_text reference J3 (at 1.27 -6.1 90) (layer F.SilkS))
    (fp_text value Conn_02x08_Odd_Even (at 1.27 23.88 90) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 19 /MAI_3V3))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 5 thru_hole circle (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 7 thru_hole circle (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 9 thru_hole circle (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /MAI_TTL_TX))
    (pad 11 thru_hole circle (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /MAG_CLEAR))
    (pad 13 thru_hole circle (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /MAI_SCK))
    (pad 15 thru_hole circle (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /MAI_MISO))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 4 thru_hole circle (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 6 thru_hole circle (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 8 thru_hole circle (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 10 thru_hole circle (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /MAI_TTL_RX))
    (pad 12 thru_hole circle (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /MAG_SS))
    (pad 14 thru_hole circle (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /MAG_DRDY))
    (pad 16 thru_hole circle (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /MAI_MOSI))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MAS 2.0 MAI-400 Adapter Board Rev01\n\nDesigned by Thomas Bennett" (at 40 44.4) (layer F.SilkS))
  (gr_arc (start 25.1 30) (end 25.1 28) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 25.1 60) (end 23.1 60) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 55.1 30) (end 57.1 30) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 55.1 60) (end 55.1 62) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 23.1 60) (end 23.1 30) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 55.1 62) (end 25.1 62) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 57.1 30) (end 57.1 60) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 25.1 28) (end 55.1 28) (layer Edge.Cuts) (width 0.05))
  (gr_text 2 (at 52 54.6 270) (layer B.SilkS))
  (gr_text 1 (at 52 45.2 270) (layer B.SilkS))
  (gr_text 2 (at 51 43.6 270) (layer B.SilkS))
  (gr_text 1 (at 51 34.2 270) (layer B.SilkS))
  (zone (net 17) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58 63) (xy 22 63) (xy 22 27) (xy 58 27)
      )
    )
  )
  (zone (net 17) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58 63) (xy 22 63) (xy 22 27) (xy 58 27)
      )
    )
  )
  (zone (net 18) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48 39) (xy 44 39) (xy 44 33) (xy 48 33)
      )
    )
  )
)
