(kicad_pcb (version 20171130) (host pcbnew 5.1.6+dfsg1-1~bpo10+1)
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 266)
    (zones 0)
    (modules 15)
    (nets 9)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.200001 3.200001)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 133.2611 115.7986)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VDD)
  (net 3 /CLK0)
  (net 4 /CLK1)
  (net 5 /CLK2)
  (net 6 /SDA_3V)
  (net 7 /SCL_3V)
  (net 8 /CLKI)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CLK0)
    (add_net /CLK1)
    (add_net /CLK2)
    (add_net /CLKI)
    (add_net /SCL_3V)
    (add_net /SDA_3V)
    (add_net GND)
    (add_net VDD)
  )
  (module Package_SO:MSOP-10_3x3mm_P0.5mm (layer Top) (tedit 5A02F25C)
    (at 148.7551 103.6066 90)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U1 (at -2.667 -2.794 180) (layer F.SilkS))
    (fp_text value Si5351A-B-GT (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 10 smd rect (at 2.2 -1 90) (size 1.4 0.3) (layers Top F.Paste F.Mask)
      (net 3 /CLK0))
    (pad 9 smd rect (at 2.2 -0.5 90) (size 1.4 0.3) (layers Top F.Paste F.Mask)
      (net 4 /CLK1))
    (pad 8 smd rect (at 2.2 0 90) (size 1.4 0.3) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.2 0.5 90) (size 1.4 0.3) (layers Top F.Paste F.Mask)
      (net 2 VDD))
    (pad 6 smd rect (at 2.2 1 90) (size 1.4 0.3) (layers Top F.Paste F.Mask)
      (net 5 /CLK2))
    (pad 5 smd rect (at -2.2 1 90) (size 1.4 0.3) (layers Top F.Paste F.Mask)
      (net 6 /SDA_3V))
    (pad 4 smd rect (at -2.2 0.5 90) (size 1.4 0.3) (layers Top F.Paste F.Mask)
      (net 7 /SCL_3V))
    (pad 3 smd rect (at -2.2 0 90) (size 1.4 0.3) (layers Top F.Paste F.Mask))
    (pad 2 smd rect (at -2.2 -0.5 90) (size 1.4 0.3) (layers Top F.Paste F.Mask)
      (net 8 /CLKI))
    (pad 1 smd rect (at -2.2 -1 90) (size 1.4 0.3) (layers Top F.Paste F.Mask)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer Top) (tedit 56D1B4CB)
    (at 122.5931 125.4506 180)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference "" (at 0.254 3.556) (layer F.SilkS))
    (fp_text value MOUNTINGHOLE2.5 (at 0 3.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer Top) (tedit 56D1B4CB)
    (at 160.6931 125.4506 180)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 3.556) (layer F.SilkS))
    (fp_text value MOUNTINGHOLE2.5 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 123.3551 117.0686 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 1.524) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 VDD))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 /SDA_3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 123.3551 111.9886 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 VDD))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 /SCL_3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 152.8191 103.3526)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10µF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 152.8191 105.8926)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.778) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 145.7071 103.8606 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Trinket M0:TrinketM0" (layer Top) (tedit 5F217C17)
    (at 133.2611 114.5286 90)
    (fp_text reference U2 (at -7.18 0) (layer F.SilkS))
    (fp_text value TrinketM0 (at 0 0 90) (layer F.Fab))
    (pad 5 thru_hole oval (at 5.08 6.35 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 5.08 -6.35 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VDD))
    (pad 4 thru_hole oval (at 2.54 6.35 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 2.54 -6.35 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /SCL_3V))
    (pad 3 thru_hole oval (at 0 6.35 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -6.35 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -2.54 6.35 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at -2.54 -6.35 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /SDA_3V))
    (pad 1 thru_hole oval (at -5.08 6.35 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -5.08 -6.35 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module "Adafruit Si5351A:SMA_EDGELAUNCH" (layer Top) (tedit 0)
    (at 126.9111 94.7166 270)
    (fp_text reference X4 (at 4.826 -4.064) (layer F.SilkS))
    (fp_text value SMACONNECTOR_EDGE (at -2.032 -4.064 270) (layer F.Fab))
    (pad GND@4 smd rect (at 2.032 2.54) (size 1.524 4.064) (layers Bottom B.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad GND@3 smd rect (at 2.032 -2.54) (size 1.524 4.064) (layers Bottom B.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad P smd rect (at 2.032 0) (size 1.27 4.064) (layers Top F.Mask)
      (net 8 /CLKI) (solder_mask_margin 0.0508) (zone_connect 2))
    (pad GND@1 smd rect (at 2.032 2.54) (size 1.524 4.064) (layers Top F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad GND@2 smd rect (at 2.032 -2.54) (size 1.524 4.064) (layers Top F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
  )
  (module "Adafruit Si5351A:SMA_EDGELAUNCH" (layer Top) (tedit 0)
    (at 138.3411 94.7166 270)
    (fp_text reference X1 (at 4.572 -4.318) (layer F.SilkS))
    (fp_text value SMACONNECTOR_EDGE (at -2.032 -4.064 90) (layer F.Fab))
    (pad GND@4 smd rect (at 2.032 2.54) (size 1.524 4.064) (layers Bottom B.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad GND@3 smd rect (at 2.032 -2.54) (size 1.524 4.064) (layers Bottom B.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad P smd rect (at 2.032 0) (size 1.27 4.064) (layers Top F.Mask)
      (net 3 /CLK0) (solder_mask_margin 0.0508) (zone_connect 2))
    (pad GND@1 smd rect (at 2.032 2.54) (size 1.524 4.064) (layers Top F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad GND@2 smd rect (at 2.032 -2.54) (size 1.524 4.064) (layers Top F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
  )
  (module "Adafruit Si5351A:SMA_EDGELAUNCH" (layer Top) (tedit 0)
    (at 148.5011 94.7166 270)
    (fp_text reference X2 (at 4.572 -4.064) (layer F.SilkS))
    (fp_text value SMACONNECTOR_EDGE (at -2.032 -4.064 90) (layer F.Fab))
    (pad GND@4 smd rect (at 2.032 2.54) (size 1.524 4.064) (layers Bottom B.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad GND@3 smd rect (at 2.032 -2.54) (size 1.524 4.064) (layers Bottom B.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad P smd rect (at 2.032 0) (size 1.27 4.064) (layers Top F.Mask)
      (net 4 /CLK1) (solder_mask_margin 0.0508) (zone_connect 2))
    (pad GND@1 smd rect (at 2.032 2.54) (size 1.524 4.064) (layers Top F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad GND@2 smd rect (at 2.032 -2.54) (size 1.524 4.064) (layers Top F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
  )
  (module "Adafruit Si5351A:SMA_EDGELAUNCH" (layer Top) (tedit 0)
    (at 158.6611 94.7166 270)
    (fp_text reference X3 (at 4.826 -4.064) (layer F.SilkS))
    (fp_text value SMACONNECTOR_EDGE (at -2.032 -4.064 90) (layer F.Fab))
    (pad GND@4 smd rect (at 2.032 2.54) (size 1.524 4.064) (layers Bottom B.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad GND@3 smd rect (at 2.032 -2.54) (size 1.524 4.064) (layers Bottom B.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad P smd rect (at 2.032 0) (size 1.27 4.064) (layers Top F.Mask)
      (net 5 /CLK2) (solder_mask_margin 0.0508) (zone_connect 2))
    (pad GND@1 smd rect (at 2.032 2.54) (size 1.524 4.064) (layers Top F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad GND@2 smd rect (at 2.032 -2.54) (size 1.524 4.064) (layers Top F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
  )
  (module "Adafruit Si5351A:FIDUCIAL_1MM" (layer Top) (tedit 0)
    (at 124.1171 121.3866)
    (fp_text reference FID2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value FIDUCIAL"" (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd roundrect (at 0 0) (size 1 1) (layers Top F.Mask) (roundrect_rratio 0.5)
      (solder_mask_margin 0.0508))
  )
  (module "Adafruit Si5351A:FIDUCIAL_1MM" (layer Top) (tedit 0)
    (at 160.5661 102.8446 180)
    (fp_text reference FID1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value FIDUCIAL"" (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd roundrect (at 0 0 180) (size 1 1) (layers Top F.Mask) (roundrect_rratio 0.5)
      (solder_mask_margin 0.0508))
  )
  (gr_text "Si5351 8 kHz - 160 MHz\nClock Generator" (at 126.1491 122.4026) (layer B.SilkS))
  (dimension 6.35 (width 0.15) (layer Dwgs.User)
    (gr_text "6.350 mm" (at 130.0861 83.5106) (layer Dwgs.User))
    (feature1 (pts (xy 133.2611 96.7486) (xy 133.2611 84.224179)))
    (feature2 (pts (xy 126.9111 96.7486) (xy 126.9111 84.224179)))
    (crossbar (pts (xy 126.9111 84.8106) (xy 133.2611 84.8106)))
    (arrow1a (pts (xy 133.2611 84.8106) (xy 132.134596 85.397021)))
    (arrow1b (pts (xy 133.2611 84.8106) (xy 132.134596 84.224179)))
    (arrow2a (pts (xy 126.9111 84.8106) (xy 128.037604 85.397021)))
    (arrow2b (pts (xy 126.9111 84.8106) (xy 128.037604 84.224179)))
  )
  (dimension 38.1 (width 0.15) (layer Dwgs.User)
    (gr_text "1.5000 in" (at 141.6431 136.6566) (layer Dwgs.User))
    (feature1 (pts (xy 122.5931 125.4506) (xy 122.5931 135.943021)))
    (feature2 (pts (xy 160.6931 125.4506) (xy 160.6931 135.943021)))
    (crossbar (pts (xy 160.6931 135.3566) (xy 122.5931 135.3566)))
    (arrow1a (pts (xy 122.5931 135.3566) (xy 123.719604 134.770179)))
    (arrow1b (pts (xy 122.5931 135.3566) (xy 123.719604 135.943021)))
    (arrow2a (pts (xy 160.6931 135.3566) (xy 159.566596 134.770179)))
    (arrow2b (pts (xy 160.6931 135.3566) (xy 159.566596 135.943021)))
  )
  (gr_text "Trinket M0\n" (at 133.2611 114.7826 90) (layer F.SilkS))
  (dimension 44.196 (width 0.15) (layer Dwgs.User)
    (gr_text "1.7400 in" (at 141.6431 138.9426) (layer Dwgs.User))
    (feature1 (pts (xy 119.5451 125.9586) (xy 119.5451 138.229021)))
    (feature2 (pts (xy 163.7411 125.9586) (xy 163.7411 138.229021)))
    (crossbar (pts (xy 163.7411 137.6426) (xy 119.5451 137.6426)))
    (arrow1a (pts (xy 119.5451 137.6426) (xy 120.671604 137.056179)))
    (arrow1b (pts (xy 119.5451 137.6426) (xy 120.671604 138.229021)))
    (arrow2a (pts (xy 163.7411 137.6426) (xy 162.614596 137.056179)))
    (arrow2b (pts (xy 163.7411 137.6426) (xy 162.614596 138.229021)))
  )
  (gr_text "CLKIN\n" (at 128.6891 99.7966) (layer F.SilkS))
  (gr_text "based on adafru.it/2045\nwith external clock input\nby @jepler" (at 159.6771 112.4966 90) (layer B.SilkS))
  (gr_line (start 135.5471 128.4986) (end 122.0851 128.4986) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.0851 94.2086) (end 135.5471 94.2086) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.5451 125.9586) (end 119.5451 96.7486) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 122.0851 96.7486) (end 119.5451 96.7486) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.5471 94.2086) (end 161.2011 94.2086) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 161.2011 96.7486) (end 161.2011 94.2086) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 163.7411 96.7486) (end 163.7411 125.9586) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 161.2011 125.9586) (end 163.7411 125.9586) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 161.2011 128.4986) (end 135.5471 128.4986) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 122.0851 125.9586) (end 122.0851 128.4986) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_text CLK0 (at 138.0871 99.7966) (layer F.SilkS))
  (gr_text CLK1 (at 148.5011 99.7966) (layer F.SilkS))
  (gr_text CLK2 (at 158.9151 99.7966) (layer F.SilkS))
  (gr_text "SI5351\nClock Gen" (at 155.4861 119.3546) (layer F.SilkS))
  (gr_text "\"24-26MHz\" in\n8kHz-160 MHz out" (at 156.8831 123.1646) (layer F.SilkS))
  (dimension 5.08 (width 0.1) (layer Dwgs.User)
    (gr_text "5.080 mm" (at 135.8011 89.4026) (layer Dwgs.User))
    (feature1 (pts (xy 138.3411 96.7486) (xy 138.3411 90.066179)))
    (feature2 (pts (xy 133.2611 96.7486) (xy 133.2611 90.066179)))
    (crossbar (pts (xy 133.2611 90.6526) (xy 138.3411 90.6526)))
    (arrow1a (pts (xy 138.3411 90.6526) (xy 137.214596 91.239021)))
    (arrow1b (pts (xy 138.3411 90.6526) (xy 137.214596 90.066179)))
    (arrow2a (pts (xy 133.2611 90.6526) (xy 134.387604 91.239021)))
    (arrow2b (pts (xy 133.2611 90.6526) (xy 134.387604 90.066179)))
  )
  (dimension 15.24 (width 0.1) (layer Dwgs.User)
    (gr_text "15.240 mm" (at 140.8811 83.5606) (layer Dwgs.User))
    (feature1 (pts (xy 148.5011 96.4946) (xy 148.5011 84.224179)))
    (feature2 (pts (xy 133.2611 96.4946) (xy 133.2611 84.224179)))
    (crossbar (pts (xy 133.2611 84.8106) (xy 148.5011 84.8106)))
    (arrow1a (pts (xy 148.5011 84.8106) (xy 147.374596 85.397021)))
    (arrow1b (pts (xy 148.5011 84.8106) (xy 147.374596 84.224179)))
    (arrow2a (pts (xy 133.2611 84.8106) (xy 134.387604 85.397021)))
    (arrow2b (pts (xy 133.2611 84.8106) (xy 134.387604 84.224179)))
  )
  (dimension 25.4 (width 0.1) (layer Dwgs.User)
    (gr_text "25.400 mm" (at 145.9611 78.2266) (layer Dwgs.User))
    (feature1 (pts (xy 158.6611 96.6216) (xy 158.6611 78.890179)))
    (feature2 (pts (xy 133.2611 96.6216) (xy 133.2611 78.890179)))
    (crossbar (pts (xy 133.2611 79.4766) (xy 158.6611 79.4766)))
    (arrow1a (pts (xy 158.6611 79.4766) (xy 157.534596 80.063021)))
    (arrow1b (pts (xy 158.6611 79.4766) (xy 157.534596 78.890179)))
    (arrow2a (pts (xy 133.2611 79.4766) (xy 134.387604 80.063021)))
    (arrow2b (pts (xy 133.2611 79.4766) (xy 134.387604 78.890179)))
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 163.8427 128.5367) (xy 119.1895 128.4605) (xy 119.3673 94.1578) (xy 163.8681 94.0816)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 163.7411 128.4986) (xy 119.9261 128.4986) (xy 119.9261 94.2086) (xy 163.8681 94.0816)
      )
    )
  )
)
