(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 8)
    (no_connects 0)
    (area 123.83844 82.728999 150.0761 125.801124)
    (thickness 1.6)
    (drawings 5)
    (tracks 56)
    (zones 0)
    (modules 5)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.778 1.778)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad4)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J2-Pad3)")
  (net 6 "Net-(J2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Custom_Connectors:USB_A_Plug (layer F.Cu) (tedit 599B27D2)
    (at 148.5011 105.0036 90)
    (fp_text reference J1 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value USB_A (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 11 -12 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 13.5 -12 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 15.5 -12 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 18 -12 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad "" np_thru_hole circle (at 12.2 -9.85 90) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 16.8 -9.85 90) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 8.65 -9.85 90) (size 2.4 2.4) (drill 2.1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 20.35 -9.85 90) (size 2.4 2.4) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module Custom_Connectors:USB_A_Plug (layer F.Cu) (tedit 599B27D2)
    (at 148.49856 123.2916 90)
    (fp_text reference J2 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value USB_A (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 11 -12 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 13.5 -12 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 2 thru_hole circle (at 15.5 -12 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 18 -12 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad "" np_thru_hole circle (at 12.2 -9.85 90) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 16.8 -9.85 90) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 8.65 -9.85 90) (size 2.4 2.4) (drill 2.1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 20.35 -9.85 90) (size 2.4 2.4) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module Custom_Connectors:USB_Extender_2_Port (layer F.Cu) (tedit 599B28DB)
    (at 125.31344 88.27008 270)
    (fp_text reference J3 (at 0 0.5 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -0.5 270) (layer F.Fab) hide)
    (fp_text user 2- (at 17.78 -9.398 270) (layer F.SilkS))
    (fp_text user 2+ (at 15.24 -9.398 270) (layer F.SilkS))
    (fp_text user G (at 12.7 -9.398 270) (layer F.SilkS))
    (fp_text user 5V (at 10.16 -9.3345 270) (layer F.SilkS))
    (fp_text user 1- (at 7.747 -9.4615 270) (layer F.SilkS))
    (fp_text user 1+ (at 5.207 -9.4615 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 5.08 -7.62 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 7.62 -7.62 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 -7.62 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 4 thru_hole circle (at 12.7 -7.62 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 15.24 -7.62 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 6 thru_hole circle (at 17.78 -7.62 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)"))
  )
  (module Custom_Connectors:OSH (layer F.Cu) (tedit 0)
    (at 133.35 113.538 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module Custom_Connectors:Logo (layer F.Cu) (tedit 0)
    (at 133.35 86.106 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (gr_line (start 140.462 82.804) (end 140.208 82.804) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.064 116.332) (end 140.462 116.332) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.064 82.804) (end 131.064 116.332) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.208 82.804) (end 131.064 82.804) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.462 116.332) (end 140.462 82.804) (angle 90) (layer Edge.Cuts) (width 0.15))
)
