<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="80.95" y2="0" width="0" layer="20"/>
<wire x1="80.95" y1="0" x2="80.95" y2="45.71" width="0" layer="20"/>
<wire x1="80.95" y1="45.71" x2="1.27" y2="45.71" width="0" layer="20"/>
<wire x1="1.27" y1="45.71" x2="1.27" y2="0" width="0" layer="20"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>Active Channel</text>
<text>Channel1</text>
<text>Channel2</text>
<text>Channel3</text>
<text>GND INPUT 9V</text>
<text>GND INPUT 9V</text>
<text>GND INPUT 9V</text>
<text>ON-OFF Switch</text>
<text>Alarm Output</text>
<text>RV-Project.Com
Water Alarm 
Monitor Board
Rev D        7/2/2018</text>
<text>GND</text>
<text>5V</text>
<text>CH1A</text>
<text>CH1B</text>
<text>CH2A</text>
<text>CH2B</text>
<text>CH3A</text>
<text>CH3B</text>
<text>Alarm</text>
<text>9V</text>
<text>Reset</text>
<text>Warning:
 Do NOT power via USB
before removing jumper.</text>
<text>12V</text>
<text>GND</text>
<text>Remove Jumper
for USB Power</text>
<text>12V</text>
<text>GND</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="RADIAL_ELECTROLYTIC_100MIL(5MM)">
<description>Generic Electrolytic Capacitor 0.100 spacing 0.200 diameter.</description>
</package>
<package name="1206-CAP">
</package>
<package name="DO214AC_JBEND">
</package>
<package name="SOD-123(LARGE)">
<description>100V/150mA 1N4148 - Super Cheap</description>
</package>
<package name="3544-2">
</package>
<package name="KF7.62CONNECTOR2">
</package>
<package name="TO-92-AMMO">
</package>
<package name="G5V">
</package>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="TO-220-HEATSINK-(3SQIN)">
</package>
<package name="KEYSTONE_RIGHT_ANGLE_TAB1">
</package>
<package name="WAFER2PINVERTICAL">
</package>
<package name="1206-RES">
</package>
<package name="ARDUINO_NANO">
</package>
<package name="WAFER3PIN">
</package>
<package name="1X01_HEADER">
</package>
<package name="MO1-18AWG">
</package>
<package name="DIP14">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="CREATIVECOMMONS_SMALL">
</package>
<package name="ART_CHEROKEE_MEDIUM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="a-lib" package="RADIAL_ELECTROLYTIC_100MIL(5MM)" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="C2" library="a-lib" package="1206-CAP" value="0.33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="a-lib" package="SOD-123(LARGE)" value="TVS-SEASY_SOD-123">
<attribute name="NAME"/>
</element>
<element name="D2" library="a-lib" package="DO214AC_JBEND" value="1N400x">
<attribute name="NAME"/>
<attribute name="VALUE" value="1N400x"/>
</element>
<element name="F1" library="a-lib" package="3544-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="a-lib" package="KF7.62CONNECTOR2" value="KF762-2CONNECTOR">
<attribute name="NAME"/>
</element>
<element name="R2" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RY1" library="a-lib" package="G5V" value="G5V9V">
<attribute name="INPUT" value="9v"/>
</element>
<element name="S2" library="a-lib" package="DIL06" value="DIPSWITCH-3"/>
<element name="U1" library="a-lib" package="TO-220-HEATSINK-(3SQIN)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TAB1" library="a-lib" package="KEYSTONE_RIGHT_ANGLE_TAB1" value="">
<attribute name="ORIENTATION" value="BOTTOM"/>
<attribute name="PARTNUM" value="614"/>
<attribute name="THREAD" value="6-32"/>
</element>
<element name="TAB2" library="a-lib" package="KEYSTONE_RIGHT_ANGLE_TAB1" value="">
<attribute name="ORIENTATION" value="BOTTOM"/>
<attribute name="PARTNUM" value="614"/>
<attribute name="THREAD" value="6-32"/>
</element>
<element name="J6" library="a-lib" package="WAFER2PINVERTICAL" value="WAFER2PVERTICAL"/>
<element name="R11" library="a-lib" package="1206-RES" value="22K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="a-lib" package="1206-RES" value="22K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="a-lib" package="1206-RES" value="22K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="a-lib" package="ARDUINO_NANO" value="ARDUINO_NANO">
<attribute name="NAME"/>
</element>
<element name="R13" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="a-lib" package="TO-92-AMMO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="a-lib" package="WAFER3PIN" value="WAFER3PHORIZONTAL"/>
<element name="J3" library="a-lib" package="WAFER3PIN" value="WAFER3PHORIZONTAL"/>
<element name="J5" library="a-lib" package="WAFER3PIN" value="WAFER3PHORIZONTAL"/>
<element name="JP9" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP11" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP12" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="U3" library="a-lib" package="DIP14" value="QUAD_OP_AMPLM324">
<attribute name="NAME"/>
</element>
<element name="JP13" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="a-lib" package="SOD-123(LARGE)" value="TVS-SEASY_SOD-123">
<attribute name="NAME"/>
</element>
<element name="D4" library="a-lib" package="SOD-123(LARGE)" value="TVS-SEASY_SOD-123">
<attribute name="NAME"/>
</element>
<element name="D5" library="a-lib" package="SOD-123(LARGE)" value="TVS-SEASY_SOD-123">
<attribute name="NAME"/>
</element>
<element name="U$1" library="a-lib" package="CREATIVECOMMONS_SMALL" value=""/>
<element name="U$2" library="a-lib" package="ART_CHEROKEE_MEDIUM" value=""/>
<element name="JP14" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP15" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="GND"/>
<contactref element="C3" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="R12" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="U2" pad="GND1"/>
<contactref element="C4" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="J5" pad="P$3"/>
<contactref element="J3" pad="P$3"/>
<contactref element="J4" pad="P$3"/>
<contactref element="U3" pad="11"/>
<contactref element="D3" pad="A"/>
<contactref element="D5" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="TAB1" pad="P$1"/>
<contactref element="TAB2" pad="P$1"/>
<contactref element="U2" pad="GND"/>
<contactref element="R1" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="J1" pad="2A"/>
</signal>
<signal name="9V">
<contactref element="U1" pad="OUT"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="RY1" pad="2"/>
<contactref element="J3" pad="P$1"/>
<contactref element="J4" pad="P$1"/>
<contactref element="U3" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="J5" pad="P$1"/>
<contactref element="JP14" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="S2" pad="4"/>
<contactref element="R4" pad="1"/>
<contactref element="U2" pad="D12"/>
</signal>
<signal name="N$18">
<contactref element="S2" pad="5"/>
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="D11"/>
</signal>
<signal name="N$19">
<contactref element="S2" pad="6"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="D10"/>
</signal>
<signal name="N$27">
<contactref element="U2" pad="D9"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="RY1" pad="9"/>
<contactref element="D2" pad="A"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="RY1" pad="COM1"/>
<contactref element="RY1" pad="COM2"/>
<contactref element="J6" pad="P$2"/>
</signal>
<signal name="N$36">
<contactref element="RY1" pad="NO"/>
<contactref element="J6" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="U2" pad="A2"/>
</signal>
<signal name="N$5">
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="U2" pad="A1"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="U2" pad="A3"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="D8"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U2" pad="D2"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U2" pad="D3"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="U2" pad="D4"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="U2" pad="D5"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U2" pad="D6"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U2" pad="D7"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="U2" pad="A4"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="Q1" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="F1" pad="P$2-1"/>
<contactref element="F1" pad="P$2-2"/>
<contactref element="D1" pad="C"/>
<contactref element="JP11" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="R7" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="IN"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="JP12" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="J5" pad="P$2"/>
<contactref element="U3" pad="3"/>
<contactref element="D4" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="J4" pad="P$2"/>
<contactref element="U3" pad="10"/>
<contactref element="D3" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R9" pad="2"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U3" pad="5"/>
<contactref element="J3" pad="P$2"/>
<contactref element="D5" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R11" pad="2"/>
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="5V">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="JP13" pad="1"/>
<contactref element="U2" pad="5V"/>
</signal>
<signal name="N$12">
<contactref element="U2" pad="VIN"/>
<contactref element="JP15" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="F1" pad="P$1-1"/>
<contactref element="F1" pad="P$1-2"/>
<contactref element="J1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
