(kicad_pcb (version 20171130) (host pcbnew "(5.1.7-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 39)
    (tracks 390)
    (zones 0)
    (modules 97)
    (nets 95)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.29972)
    (user_trace_width 0.381)
    (user_trace_width 0.44958)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (user_via 1.016 0.635)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9 0.95)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 30.48 53.34)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x00008_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "meta/"))
  )
  (net 0 "")
  (net 1 "Net-(R1-Pad1)")
  (net 2 "Net-(R3-Pad1)")
  (net 3 "Net-(R2-Pad1)")
  (net 4 "Net-(R6-Pad2)")
  (net 5 GND)
  (net 6 /PDI_DATA)
  (net 7 /PDI_CLK)
  (net 8 +3.3V)
  (net 9 +12V)
  (net 10 /IGN)
  (net 11 /REV)
  (net 12 /HB)
  (net 13 /SW1)
  (net 14 /SW2)
  (net 15 /V1_EN)
  (net 16 /V2_EN)
  (net 17 /REV_IN)
  (net 18 /SW2_IN)
  (net 19 /HB_IN)
  (net 20 /SW1_IN)
  (net 21 /IGN_IN)
  (net 22 "Net-(C21-Pad2)")
  (net 23 "Net-(C23-Pad1)")
  (net 24 "Net-(C24-Pad1)")
  (net 25 "Net-(C28-Pad1)")
  (net 26 /SWL1)
  (net 27 /SWL2)
  (net 28 "Net-(R26-Pad1)")
  (net 29 "Net-(R33-Pad2)")
  (net 30 "Net-(U1-Pad7)")
  (net 31 "Net-(U1-Pad6)")
  (net 32 "Net-(U1-Pad3)")
  (net 33 "Net-(U2-Pad11)")
  (net 34 "Net-(U2-Pad7)")
  (net 35 "Net-(U2-Pad4)")
  (net 36 GNDPWR)
  (net 37 /HSWLB)
  (net 38 /HSWLG)
  (net 39 /HSWLR)
  (net 40 /HSW)
  (net 41 "Net-(C16-Pad1)")
  (net 42 /H+)
  (net 43 /V2+)
  (net 44 /V1+)
  (net 45 /HSW_IN)
  (net 46 /SWL2_EN)
  (net 47 /SWL1_EN)
  (net 48 /HSWLG_EN)
  (net 49 /HSWLB_EN)
  (net 50 /HSWLR_EN)
  (net 51 /H_EN)
  (net 52 "Net-(C4-Pad2)")
  (net 53 "Net-(C7-Pad2)")
  (net 54 "Net-(C11-Pad1)")
  (net 55 "Net-(C14-Pad2)")
  (net 56 "Net-(C17-Pad1)")
  (net 57 "Net-(C18-Pad1)")
  (net 58 "Net-(C19-Pad1)")
  (net 59 "Net-(C20-Pad1)")
  (net 60 "Net-(C25-Pad1)")
  (net 61 "Net-(C26-Pad1)")
  (net 62 "Net-(J11-Pad4)")
  (net 63 "Net-(J11-Pad3)")
  (net 64 "Net-(R4-Pad1)")
  (net 65 "Net-(R8-Pad2)")
  (net 66 "Net-(R11-Pad1)")
  (net 67 "Net-(R13-Pad1)")
  (net 68 "Net-(R18-Pad2)")
  (net 69 "Net-(R23-Pad1)")
  (net 70 "Net-(R28-Pad1)")
  (net 71 "Net-(R34-Pad2)")
  (net 72 "Net-(U2-Pad6)")
  (net 73 "Net-(U2-Pad5)")
  (net 74 "Net-(U3-Pad11)")
  (net 75 "Net-(U3-Pad7)")
  (net 76 "Net-(U3-Pad4)")
  (net 77 "Net-(U5-Pad11)")
  (net 78 "Net-(U5-Pad7)")
  (net 79 "Net-(U5-Pad4)")
  (net 80 "Net-(U6-Pad31)")
  (net 81 "Net-(U6-Pad30)")
  (net 82 "Net-(U6-Pad29)")
  (net 83 "Net-(U6-Pad28)")
  (net 84 "Net-(U6-Pad27)")
  (net 85 "Net-(U6-Pad26)")
  (net 86 "Net-(U6-Pad21)")
  (net 87 "Net-(U6-Pad20)")
  (net 88 "Net-(U6-Pad19)")
  (net 89 "Net-(U6-Pad16)")
  (net 90 "Net-(U8-Pad13)")
  (net 91 "Net-(U8-Pad12)")
  (net 92 "Net-(U8-Pad3)")
  (net 93 "Net-(U6-Pad9)")
  (net 94 "Net-(U6-Pad22)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net +12V)
    (add_net +3.3V)
    (add_net /H+)
    (add_net /HB)
    (add_net /HB_IN)
    (add_net /HSW)
    (add_net /HSWLB)
    (add_net /HSWLB_EN)
    (add_net /HSWLG)
    (add_net /HSWLG_EN)
    (add_net /HSWLR)
    (add_net /HSWLR_EN)
    (add_net /HSW_IN)
    (add_net /H_EN)
    (add_net /IGN)
    (add_net /IGN_IN)
    (add_net /PDI_CLK)
    (add_net /PDI_DATA)
    (add_net /REV)
    (add_net /REV_IN)
    (add_net /SW1)
    (add_net /SW1_IN)
    (add_net /SW2)
    (add_net /SW2_IN)
    (add_net /SWL1)
    (add_net /SWL1_EN)
    (add_net /SWL2)
    (add_net /SWL2_EN)
    (add_net /V1+)
    (add_net /V1_EN)
    (add_net /V2+)
    (add_net /V2_EN)
    (add_net GND)
    (add_net GNDPWR)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(J11-Pad3)")
    (add_net "Net-(J11-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R26-Pad1)")
    (add_net "Net-(R28-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R33-Pad2)")
    (add_net "Net-(R34-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U6-Pad16)")
    (add_net "Net-(U6-Pad19)")
    (add_net "Net-(U6-Pad20)")
    (add_net "Net-(U6-Pad21)")
    (add_net "Net-(U6-Pad22)")
    (add_net "Net-(U6-Pad26)")
    (add_net "Net-(U6-Pad27)")
    (add_net "Net-(U6-Pad28)")
    (add_net "Net-(U6-Pad29)")
    (add_net "Net-(U6-Pad30)")
    (add_net "Net-(U6-Pad31)")
    (add_net "Net-(U6-Pad9)")
    (add_net "Net-(U8-Pad12)")
    (add_net "Net-(U8-Pad13)")
    (add_net "Net-(U8-Pad3)")
  )
  (net_class +3V3 ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (module Symbol:KiCad-Logo2_5mm_SilkScreen locked (layer B.Cu) (tedit 0)
    (at 52.07 39.6875 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference "#LOGO2" (at 0 5.08) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_5mm_SilkScreen (at 0 -5.08) (layer B.Fab) hide)
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen locked (layer B.Cu) (tedit 0)
    (at 63.5 38.4175 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference "#LOGO1" (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Package_SO:VSSOP-8_2.3x2mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 45.085 41.021)
    (descr "VSSOP-8 2.3x2mm Pitch 0.5mm")
    (tags "VSSOP-8 2.3x2mm Pitch 0.5mm")
    (attr smd)
    (fp_text reference U7 (at 0 -2) (layer F.SilkS))
    (fp_text value 74LVC3G17 (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 1.55 -0.75 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 7 smd rect (at 1.55 -0.25 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 /HSW_IN))
    (pad 6 smd rect (at 1.55 0.25 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C26-Pad1)"))
    (pad 5 smd rect (at 1.55 0.75 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 /SW1_IN))
    (pad 4 smd rect (at -1.55 0.75 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 3 smd rect (at -1.55 0.25 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at -1.55 -0.25 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 /SW2_IN))
    (pad 1 smd rect (at -1.55 -0.75 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C28-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/VSSOP-8_2.3x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 44.8945 37.846)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at -2.667 0) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3V))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO-ML:Infineon_PG-TSDSO-14-22 (layer F.Cu) (tedit 5CC66CA7)
    (at 64.135 41.275 180)
    (descr Infineon_PG-TSDSO-14-22)
    (tags "DSO DSO-14 TSDSO TSDSO-14 SOIC SOIC-14")
    (attr smd)
    (fp_text reference U8 (at -4.6355 1.651) (layer F.SilkS))
    (fp_text value BTS7200-4EPA (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 14 smd rect (at 2.85 -1.95 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C23-Pad1)"))
    (pad 13 smd rect (at 2.85 -1.3 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U8-Pad13)"))
    (pad 12 smd rect (at 2.85 -0.65 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U8-Pad12)"))
    (pad 11 smd rect (at 2.85 0 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C21-Pad2)"))
    (pad 10 smd rect (at 2.85 0.65 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R33-Pad2)"))
    (pad 9 smd rect (at 2.85 1.3 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R33-Pad2)"))
    (pad 15 smd rect (at 0 -1 180) (size 2.65 2) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V) (solder_paste_margin_ratio -0.2))
    (pad 15 smd rect (at 0 1 180) (size 2.65 2) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V) (solder_paste_margin_ratio -0.2))
    (pad 8 smd rect (at 2.85 1.95 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R28-Pad1)"))
    (pad 7 smd rect (at -2.85 1.95 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R23-Pad1)"))
    (pad 6 smd rect (at -2.85 1.3 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R26-Pad1)"))
    (pad 5 smd rect (at -2.85 0.65 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R34-Pad2)"))
    (pad 4 smd rect (at -2.85 0 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R34-Pad2)"))
    (pad 3 smd rect (at -2.85 -0.65 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U8-Pad3)"))
    (pad 2 smd rect (at -2.85 -1.3 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C24-Pad1)"))
    (pad 1 smd rect (at -2.85 -1.95 180) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14-1EP_4.4x5mm_P0.65mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO-ML:Infineon_PG-TSDSO-14-22 (layer F.Cu) (tedit 5CC66CA7)
    (at 53.34 41.5925 270)
    (descr Infineon_PG-TSDSO-14-22)
    (tags "DSO DSO-14 TSDSO TSDSO-14 SOIC SOIC-14")
    (attr smd)
    (fp_text reference U5 (at -1.4605 3.3655 270) (layer F.SilkS))
    (fp_text value BTS7200-2EPA (at 0 4 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 14 smd rect (at 2.85 -1.95 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C17-Pad1)"))
    (pad 13 smd rect (at 2.85 -1.3 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C17-Pad1)"))
    (pad 12 smd rect (at 2.85 -0.65 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C17-Pad1)"))
    (pad 11 smd rect (at 2.85 0 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U5-Pad11)"))
    (pad 10 smd rect (at 2.85 0.65 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C16-Pad1)"))
    (pad 9 smd rect (at 2.85 1.3 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C16-Pad1)"))
    (pad 15 smd rect (at 0 -1 270) (size 2.65 2) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V) (solder_paste_margin_ratio -0.2))
    (pad 15 smd rect (at 0 1 270) (size 2.65 2) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V) (solder_paste_margin_ratio -0.2))
    (pad 8 smd rect (at 2.85 1.95 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C16-Pad1)"))
    (pad 7 smd rect (at -2.85 1.95 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U5-Pad7)"))
    (pad 6 smd rect (at -2.85 1.3 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R13-Pad1)"))
    (pad 5 smd rect (at -2.85 0.65 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R18-Pad2)"))
    (pad 4 smd rect (at -2.85 0 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U5-Pad4)"))
    (pad 3 smd rect (at -2.85 -0.65 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R18-Pad2)"))
    (pad 2 smd rect (at -2.85 -1.3 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R11-Pad1)"))
    (pad 1 smd rect (at -2.85 -1.95 270) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C14-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14-1EP_4.4x5mm_P0.65mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO-ML:Infineon_PG-TSDSO-14-22 (layer F.Cu) (tedit 5F934275)
    (at 66.04 24.765)
    (descr Infineon_PG-TSDSO-14-22)
    (tags "DSO DSO-14 TSDSO TSDSO-14 SOIC SOIC-14")
    (attr smd)
    (fp_text reference U2 (at 2.8575 -3.302) (layer F.SilkS))
    (fp_text value BTS7002-1EPP (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 14 smd rect (at 2.85 -1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 /H+))
    (pad 13 smd rect (at 2.85 -1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 /H+))
    (pad 12 smd rect (at 2.85 -0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 /H+))
    (pad 11 smd rect (at 2.85 0) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad11)"))
    (pad 10 smd rect (at 2.85 0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 /H+))
    (pad 9 smd rect (at 2.85 1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 /H+))
    (pad 15 smd rect (at 0 -1) (size 2.65 2) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 15 smd rect (at 0 1) (size 2.65 2) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 8 smd rect (at 2.85 1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 /H+))
    (pad 7 smd rect (at -2.85 1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad7)"))
    (pad 6 smd rect (at -2.85 1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at -2.85 0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U2-Pad5)"))
    (pad 4 smd rect (at -2.85 0) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -2.85 -0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at -2.85 -1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(R1-Pad1)"))
    (pad 1 smd rect (at -2.85 -1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14-1EP_4.4x5mm_P0.65mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO-ML:Infineon_PG-TSDSO-14-22 (layer F.Cu) (tedit 5F934261)
    (at 66.04 32.7025)
    (descr Infineon_PG-TSDSO-14-22)
    (tags "DSO DSO-14 TSDSO TSDSO-14 SOIC SOIC-14")
    (attr smd)
    (fp_text reference U3 (at 2.8575 -3.3655) (layer F.SilkS))
    (fp_text value BTS7008-2EPA (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 14 smd rect (at 2.85 -1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 /V1+))
    (pad 13 smd rect (at 2.85 -1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 /V1+))
    (pad 12 smd rect (at 2.85 -0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 /V1+))
    (pad 11 smd rect (at 2.85 0) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U3-Pad11)"))
    (pad 10 smd rect (at 2.85 0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 /V2+))
    (pad 9 smd rect (at 2.85 1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 /V2+))
    (pad 15 smd rect (at 0 -1) (size 2.65 2) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 15 smd rect (at 0 1) (size 2.65 2) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 8 smd rect (at 2.85 1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 /V2+))
    (pad 7 smd rect (at -2.85 1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U3-Pad7)"))
    (pad 6 smd rect (at -2.85 1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R4-Pad1)"))
    (pad 5 smd rect (at -2.85 0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R8-Pad2)"))
    (pad 4 smd rect (at -2.85 0) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U3-Pad4)"))
    (pad 3 smd rect (at -2.85 -0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R8-Pad2)"))
    (pad 2 smd rect (at -2.85 -1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R2-Pad1)"))
    (pad 1 smd rect (at -2.85 -1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14-1EP_4.4x5mm_P0.65mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.6425 25.7025)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -1.42875 0.015) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(R6-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 59.055 39.975)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R33 (at 0 2.57) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R33-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 53.34 36.5125 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -1.3335 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(R18-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.6425 32.7025)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -1.27 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(R8-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D2mm_OD3.81mm (layer F.Cu) (tedit 5F711BAD)
    (at 76.2 25.4)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J7 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 3.81 3.81) (drill 2) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 36 GNDPWR))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 45.085 44.196 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0.0585 -1.27 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3V))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 41.91 44.196 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R32 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3V))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C28-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm (layer F.Cu) (tedit 5F711A5A)
    (at 67.31 51.435)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J18 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 37 /HSWLB))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm (layer F.Cu) (tedit 5F711A5A)
    (at 64.135 51.435)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J16 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 38 /HSWLG))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm (layer F.Cu) (tedit 5F711A5A)
    (at 60.96 51.435)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J19 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 39 /HSWLR))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:VSSOP-8_2.3x2mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 43.18 35.56)
    (descr "VSSOP-8 2.3x2mm Pitch 0.5mm")
    (tags "VSSOP-8 2.3x2mm Pitch 0.5mm")
    (attr smd)
    (fp_text reference U4 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 74LVC3G17 (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 1.55 -0.75 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 7 smd rect (at 1.55 -0.25 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 /IGN_IN))
    (pad 6 smd rect (at 1.55 0.25 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C19-Pad1)"))
    (pad 5 smd rect (at 1.55 0.75 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 /REV_IN))
    (pad 4 smd rect (at -1.55 0.75 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 3 smd rect (at -1.55 0.25 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at -1.55 -0.25 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 /HB_IN))
    (pad 1 smd rect (at -1.55 -0.75 270) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/VSSOP-8_2.3x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 67.945 47.625 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 0 1.651 90) (layer F.SilkS) hide)
    (fp_text value 560R (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 24 "Net-(C24-Pad1)"))
    (pad 1 smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 37 /HSWLB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 64.135 47.625 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0 1.651 90) (layer F.SilkS) hide)
    (fp_text value 560R (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 60 "Net-(C25-Pad1)"))
    (pad 1 smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 38 /HSWLG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.325 47.625 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at -0.635 1.651 90) (layer F.SilkS) hide)
    (fp_text value 560R (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 23 "Net-(C23-Pad1)"))
    (pad 1 smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 39 /HSWLR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D2mm_OD3.81mm (layer F.Cu) (tedit 5F9305B3)
    (at 76.2 20.32)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J2 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 3.81 3.81) (drill 2) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 42 /H+) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm (layer F.Cu) (tedit 5F711A5A)
    (at 41.91 51.435)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J21 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 40 /HSW))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 41.91 48.26 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R36 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /HSW))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C28-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 42.685 46.228)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C28-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged2Bar_Pad1.0x1.5mm (layer F.Cu) (tedit 5C756A82)
    (at 33.02 47.3075 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 2 copper strips")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value Jumper (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 36 GNDPWR))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 59.055 41.275)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R35 (at 0 2.54) (layer F.SilkS))
    (fp_text value 47R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C21-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 69.5475 42.1 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R34 (at -0.0005 1.4455 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(R34-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.46 37.7825 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 0 1.27) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /HSWLR_EN))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(R28-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 64.135 36.3855 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at -2.8575 0) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /HSWLB_EN))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 64.135 37.7825 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at -2.8575 0) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /HSWLG_EN))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(R23-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 56.8325 37.9175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -2.675 0 90) (layer F.SilkS))
    (fp_text value 47R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(C14-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 51.7525 36.5125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 1.3335 0 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /SWL1_EN))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 54.9275 36.5125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 1.3335 0 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /SWL2_EN))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.6425 23.1325)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 47R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.6425 24.4475 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1.42875 0) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /H_EN))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 66.04 46.9375 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 69.85 46.9375 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C24-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 62.23 46.9375 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 66.04 44.7675 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at -2.8575 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 63.36 44.7675 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 2.7175 -0.254) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C21-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 57.15 46.9375 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 53.34 46.9375 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 49.8475 42.3675 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0.9655 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 56.8325 40.8175 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -2.68 0 90) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(C14-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F93208A)
    (at 63.965 29.36875 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.3925 0.03175) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V) (zone_connect 2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F936672)
    (at 73.3425 22.86 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 GNDPWR))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 42 /H+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F932596)
    (at 63.965 28.09875)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.3925 -0.03175) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V) (zone_connect 2))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 GNDPWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F93434A)
    (at 58.1025 22.5425 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V) (zone_connect 2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.6425 35.306)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -2.286 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 GNDPWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 48.26 48.26 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R31 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /SW2))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 45.085 48.26 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /SW1))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 35.306 41.275 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /HB))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 35.306 36.195 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /REV))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 35.306 31.115 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /IGN))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 49.035 46.228)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 1.537 -0.381 90) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 45.86 46.228)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at -2.68 0) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 37.465 40.513 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0.762 -2.032 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 37.465 35.42 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0.749 -2.032 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 37.465 30.34 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0.749 -2.032 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Tag_Connect-ML:TC2030-IDC-NP (layer F.Cu) (tedit 5F8063BB)
    (at 48.5775 34.925 270)
    (fp_text reference J11 (at -5.461 0 270) (layer F.SilkS) hide)
    (fp_text value DNF (at 0 -3.556 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.54 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 6 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad 5 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 7 /PDI_CLK))
    (pad 4 smd circle (at 0 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 62 "Net-(J11-Pad4)"))
    (pad 3 smd circle (at 0 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 63 "Net-(J11-Pad3)"))
    (pad 2 smd circle (at -1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 8 +3.3V))
    (pad 1 smd circle (at -1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 6 /PDI_DATA))
  )
  (module Diode_SMD:D_SMC_Handsoldering (layer B.Cu) (tedit 58642B03)
    (at 42.2275 35.2425 270)
    (descr "Diode SMC (DO-214AB) Handsoldering")
    (tags "Diode SMC (DO-214AB) Handsoldering")
    (attr smd)
    (fp_text reference D1 (at -8.001 0.127 180) (layer B.SilkS))
    (fp_text value SM15T33CA (at 0 -4.2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 2 smd rect (at 4.4 0 180) (size 3.3 4.5) (layers B.Cu B.Paste B.Mask)
      (net 36 GNDPWR))
    (pad 1 smd rect (at -4.4 0 180) (size 3.3 4.5) (layers B.Cu B.Paste B.Mask)
      (net 9 +12V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A (layer F.Cu) (tedit 5EBA9318)
    (at 41.2115 28.8455 270)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C3 (at -0.0165 -1.778 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.35 0 270) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 5 GND))
    (pad 1 smd roundrect (at -1.35 0 270) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 8 +3.3V))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm (layer F.Cu) (tedit 5F711A5A)
    (at 32.385 41.275)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J15 (at -3.81 0 180) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 12 /HB))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm locked (layer F.Cu) (tedit 5F711A5A)
    (at 32.385 36.195)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J13 (at -3.175 0 180) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 11 /REV))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm locked (layer F.Cu) (tedit 5F711A5A)
    (at 32.385 31.115)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J9 (at -3.175 0 180) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 10 /IGN))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-32-1EP_4x4mm_P0.4mm_EP2.65x2.65mm (layer F.Cu) (tedit 5DC5F6A4)
    (at 51.8795 26.9905)
    (descr "QFN, 32 Pin (https://www.renesas.com/eu/en/package-image/pdf/outdrawing/l32.4x4a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U6 (at 0 -3.3) (layer F.SilkS))
    (fp_text value ATXMEGA8E5-M4U (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd roundrect (at 0.66 0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at 0.66 -0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at -0.66 0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at -0.66 -0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad 33 smd rect (at 0 0) (size 2.65 2.65) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad 32 smd custom (at -1.4 -1.95) (size 0.129289 0.129289) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.35) (xy 0.05 -0.35) (xy 0.05 0.35) (xy 0.020711 0.35) (xy -0.05 0.279289)
) (width 0.1))
      ))
    (pad 31 smd roundrect (at -1 -1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(U6-Pad31)"))
    (pad 30 smd roundrect (at -0.6 -1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(U6-Pad30)"))
    (pad 29 smd roundrect (at -0.2 -1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(U6-Pad29)"))
    (pad 28 smd roundrect (at 0.2 -1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(U6-Pad28)"))
    (pad 27 smd roundrect (at 0.6 -1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(U6-Pad27)"))
    (pad 26 smd roundrect (at 1 -1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(U6-Pad26)"))
    (pad 25 smd custom (at 1.4 -1.95) (size 0.129289 0.129289) (layers F.Cu F.Paste F.Mask)
      (net 51 /H_EN)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.35) (xy 0.05 -0.35) (xy 0.05 0.279289) (xy -0.020711 0.35) (xy -0.05 0.35)
) (width 0.1))
      ))
    (pad 24 smd custom (at 1.95 -1.4) (size 0.129289 0.129289) (layers F.Cu F.Paste F.Mask)
      (net 15 /V1_EN)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 0.020711) (xy -0.279289 -0.05) (xy 0.35 -0.05) (xy 0.35 0.05) (xy -0.35 0.05)
) (width 0.1))
      ))
    (pad 23 smd roundrect (at 1.95 -1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /V2_EN))
    (pad 22 smd roundrect (at 1.95 -0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 "Net-(U6-Pad22)"))
    (pad 21 smd roundrect (at 1.95 -0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(U6-Pad21)"))
    (pad 20 smd roundrect (at 1.95 0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(U6-Pad20)"))
    (pad 19 smd roundrect (at 1.95 0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(U6-Pad19)"))
    (pad 18 smd roundrect (at 1.95 1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 17 smd custom (at 1.95 1.4) (size 0.129289 0.129289) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 -0.05) (xy 0.35 -0.05) (xy 0.35 0.05) (xy -0.279289 0.05) (xy -0.35 -0.020711)
) (width 0.1))
      ))
    (pad 16 smd custom (at 1.4 1.95) (size 0.129289 0.129289) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U6-Pad16)")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.35) (xy -0.020711 -0.35) (xy 0.05 -0.279289) (xy 0.05 0.35) (xy -0.05 0.35)
) (width 0.1))
      ))
    (pad 15 smd roundrect (at 1 1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /HSWLB_EN))
    (pad 14 smd roundrect (at 0.6 1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /HSWLG_EN))
    (pad 13 smd roundrect (at 0.2 1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /HSWLR_EN))
    (pad 12 smd roundrect (at -0.2 1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /SWL2_EN))
    (pad 11 smd roundrect (at -0.6 1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /SWL1_EN))
    (pad 10 smd roundrect (at -1 1.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /SW1_IN))
    (pad 9 smd custom (at -1.4 1.95) (size 0.129289 0.129289) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U6-Pad9)")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.279289) (xy 0.020711 -0.35) (xy 0.05 -0.35) (xy 0.05 0.35) (xy -0.05 0.35)
) (width 0.1))
      ))
    (pad 8 smd custom (at -1.95 1.4) (size 0.129289 0.129289) (layers F.Cu F.Paste F.Mask)
      (net 7 /PDI_CLK)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 -0.05) (xy 0.35 -0.05) (xy 0.35 -0.020711) (xy 0.279289 0.05) (xy -0.35 0.05)
) (width 0.1))
      ))
    (pad 7 smd roundrect (at -1.95 1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /PDI_DATA))
    (pad 6 smd roundrect (at -1.95 0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /HSW_IN))
    (pad 5 smd roundrect (at -1.95 0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /SW2_IN))
    (pad 4 smd roundrect (at -1.95 -0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /REV_IN))
    (pad 3 smd roundrect (at -1.95 -0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /IGN_IN))
    (pad 2 smd roundrect (at -1.95 -1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /HB_IN))
    (pad 1 smd custom (at -1.95 -1.4) (size 0.129289 0.129289) (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 -0.05) (xy 0.279289 -0.05) (xy 0.35 0.020711) (xy 0.35 0.05) (xy -0.35 0.05)
) (width 0.1))
      ))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-32-1EP_4x4mm_P0.4mm_EP2.65x2.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 48.26 44.196 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at -0.005 -1.27 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3V))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 55.245 47.625 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 1.651 90) (layer F.SilkS) hide)
    (fp_text value 560R (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 56 "Net-(C17-Pad1)"))
    (pad 1 smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 27 /SWL2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 38.862 40.463 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(C19-Pad1)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 51.435 47.625 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 1.651 90) (layer F.SilkS) hide)
    (fp_text value 560R (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 41 "Net-(C16-Pad1)"))
    (pad 1 smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 26 /SWL1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 38.862 35.37 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0.0255 -1.27 90) (layer F.SilkS))
    (fp_text value 1.27M (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(C18-Pad1)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm (layer F.Cu) (tedit 5F711A5A)
    (at 48.26 51.435)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J20 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 14 /SW2))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm (layer F.Cu) (tedit 5F931303)
    (at 57.785 51.435)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J14 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 5 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm (layer F.Cu) (tedit 5F711A5A)
    (at 45.085 51.435)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J17 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 13 /SW1))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm (layer F.Cu) (tedit 5F711A5A)
    (at 54.61 51.435)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J10 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 27 /SWL2))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D1mm_OD2.54mm (layer F.Cu) (tedit 5F711A5A)
    (at 51.435 51.435)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J12 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.54 2.54) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 26 /SWL1))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D2mm_OD3.81mm locked (layer F.Cu) (tedit 5F711BAD)
    (at 76.2 50.8)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J8 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 3.81 3.81) (drill 2) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 36 GNDPWR))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D2mm_OD3.81mm locked (layer F.Cu) (tedit 5F711BAD)
    (at 33.02 50.8)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J6 (at -3.81 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 3.81 3.81) (drill 2) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 36 GNDPWR))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D2mm_OD3.81mm locked (layer F.Cu) (tedit 5F711BAD)
    (at 76.2 38.1)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J5 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 3.81 3.81) (drill 2) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 36 GNDPWR))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D2mm_OD3.81mm locked (layer F.Cu) (tedit 5F711BAD)
    (at 76.2 45.72)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J4 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 3.81 3.81) (drill 2) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 43 /V2+))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D2mm_OD3.81mm locked (layer F.Cu) (tedit 5F711BAD)
    (at 76.2 33.02)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (attr virtual)
    (fp_text reference J3 (at 0 -2.2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 3.81 3.81) (drill 2) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 44 /V1+))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire-ML:SolderWire-1x01_D2mm_OD3.81mm locked (layer F.Cu) (tedit 5F711BAD)
    (at 33.02 20.32)
    (descr "Soldered wire connection, for a single 0.25 mm² wire, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.25sqmm")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference J1 (at -3.81 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 3.81 3.81) (drill 2) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 9 +12V) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x01_D0.65mm_OD2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 33.02 26.0325 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm (layer F.Cu) (tedit 5EA4BDD8)
    (at 36.703 25.0825 180)
    (descr "DD Package; 8-Lead Plastic DFN (3mm x 3mm) (see Linear Technology DFN_8_05-08-1698.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 2.4765) (layer F.SilkS))
    (fp_text value LT3014IDD (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at -0.415 -0.595 180) (size 0.64 1) (layers F.Paste))
    (pad "" smd rect (at 0.415 -0.595 180) (size 0.64 1) (layers F.Paste))
    (pad "" smd rect (at -0.415 0.595 180) (size 0.64 1) (layers F.Paste))
    (pad 9 smd rect (at 0 0 180) (size 1.66 2.38) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad "" smd rect (at 0.415 0.595 180) (size 0.64 1) (layers F.Paste))
    (pad 8 smd rect (at 1.4 -0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 7 smd rect (at 1.4 -0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at 1.4 0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad6)"))
    (pad 5 smd rect (at 1.4 0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 4 smd rect (at -1.4 0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 3 smd rect (at -1.4 0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at -1.4 -0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(R3-Pad1)"))
    (pad 1 smd rect (at -1.4 -0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 38.862 30.29 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 2.222 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(C11-Pad1)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.6425 30.099)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -1.27 0) (layer F.SilkS))
    (fp_text value 47R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 40.386 24.3205)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 2.159 0) (layer F.SilkS))
    (fp_text value 1.27M (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(R3-Pad1)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 40.386 25.8325 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.159 -0.012) (layer F.SilkS))
    (fp_text value 2.15M (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3V))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.6425 34.0025 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 1.27 0) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /V2_EN))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.6425 31.4025 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 1.27 0) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /V1_EN))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 54.9275 28.7655 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -2.8575 0 270) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3V))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 48.4505 24.8285 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 1.143) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 73.3425 35.56 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 1.42875 270) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 GNDPWR))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 /V1+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 73.3425 48.26 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 1.42875 90) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 GNDPWR))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 /V2+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 38.811 27.4955 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.4255 -0.0635) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text H- (at 73.66 25.4) (layer B.SilkS))
  (gr_text H+ (at 73.66 20.32) (layer B.SilkS))
  (gr_text HSWLB (at 67.31 49.4665 270) (layer B.SilkS))
  (gr_text HSWLG (at 64.135 49.4665 270) (layer B.SilkS))
  (gr_text HSWLR (at 60.96 49.4665 270) (layer B.SilkS))
  (gr_text HSW (at 41.91 49.53 270) (layer B.SilkS))
  (gr_text "ATV Control" (at 38.4175 20.32) (layer F.SilkS))
  (gr_text V2- (at 73.66 50.8) (layer B.SilkS))
  (gr_text V2+ (at 73.66 45.72) (layer B.SilkS))
  (gr_text V1- (at 73.66 38.1) (layer B.SilkS))
  (gr_text "Mike Lawrence" (at 62.611 27.305) (layer B.SilkS))
  (gr_text "Rev 1.0" (at 62.738 32.385) (layer B.SilkS))
  (gr_text "Oct 2020" (at 62.611 29.845) (layer B.SilkS))
  (gr_text "ATV Control" (at 62.611 24.765) (layer B.SilkS))
  (gr_text SW1 (at 45.085 49.53 270) (layer B.SilkS))
  (gr_text HB (at 33.9725 41.275) (layer B.SilkS))
  (gr_text SW2 (at 48.26 49.53 270) (layer B.SilkS))
  (gr_text SWL1 (at 51.435 49.53 270) (layer B.SilkS))
  (gr_text SWL2 (at 54.61 49.53 270) (layer B.SilkS))
  (gr_text GND (at 57.785 49.53 270) (layer B.SilkS))
  (gr_text REV (at 33.9725 36.195) (layer B.SilkS))
  (gr_text IGN (at 33.9725 31.115) (layer B.SilkS))
  (gr_text GND (at 31.115 47.625) (layer B.SilkS))
  (gr_text +12V (at 31.0515 23.749) (layer B.SilkS))
  (gr_text GND (at 29.21 44.45) (layer F.Fab))
  (gr_text ACC2 (at 29.21 39.878) (layer F.Fab))
  (gr_text "ACC1\n" (at 29.464 34.798) (layer F.Fab))
  (gr_text +12V (at 29.21 30.48) (layer F.Fab))
  (gr_text V1+ (at 73.66 33.02) (layer B.SilkS))
  (dimension 25.4 (width 0.3) (layer F.Fab)
    (gr_text "1.0000 in" (at 18.22 40.64 90) (layer F.Fab))
    (feature1 (pts (xy 29.21 27.94) (xy 19.733579 27.94)))
    (feature2 (pts (xy 29.21 53.34) (xy 19.733579 53.34)))
    (crossbar (pts (xy 20.32 53.34) (xy 20.32 27.94)))
    (arrow1a (pts (xy 20.32 27.94) (xy 20.906421 29.066504)))
    (arrow1b (pts (xy 20.32 27.94) (xy 19.733579 29.066504)))
    (arrow2a (pts (xy 20.32 53.34) (xy 20.906421 52.213496)))
    (arrow2b (pts (xy 20.32 53.34) (xy 19.733579 52.213496)))
  )
  (gr_line (start 30.48 19.05) (end 30.48 52.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 77.47 53.34) (end 31.75 53.34) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 78.74 19.05) (end 78.74 52.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 31.75 17.78) (end 77.47 17.78) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 48.26 (width 0.3) (layer F.Fab)
    (gr_text "1.9000 in" (at 54.61 20.76) (layer F.Fab))
    (feature1 (pts (xy 78.74 26.67) (xy 78.74 22.273579)))
    (feature2 (pts (xy 30.48 26.67) (xy 30.48 22.273579)))
    (crossbar (pts (xy 30.48 22.86) (xy 78.74 22.86)))
    (arrow1a (pts (xy 78.74 22.86) (xy 77.613496 23.446421)))
    (arrow1b (pts (xy 78.74 22.86) (xy 77.613496 22.273579)))
    (arrow2a (pts (xy 30.48 22.86) (xy 31.606504 23.446421)))
    (arrow2b (pts (xy 30.48 22.86) (xy 31.606504 22.273579)))
  )
  (gr_arc (start 31.75 19.05) (end 30.48 19.05) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 31.75 52.07) (end 31.75 53.34) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 77.47 52.07) (end 78.74 52.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 77.47 19.05) (end 77.47 17.78) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 44) (net_name /V1+) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 68.2625 28.2575) (xy 68.2625 32.385) (xy 74.295 35.56) (xy 78.74 35.56) (xy 78.74 28.2575)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 78.74 17.78) (xy 78.74 53.34) (xy 30.48 53.34) (xy 30.48 17.78)
      )
    )
  )
  (zone (net 36) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 30.48 35.56) (xy 68.58 35.56) (xy 68.58 22.86) (xy 78.74 22.86) (xy 78.74 53.34)
        (xy 30.48 53.34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 69.215 53.2765) (xy 40.005 53.34) (xy 40.005 49.657) (xy 69.215 49.5935)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 34.29 43.18) (xy 30.48 43.18) (xy 30.48 29.21) (xy 34.29 29.21)
      )
    )
  )
  (zone (net 9) (net_name +12V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 30.48 17.78) (xy 67.945 17.78) (xy 67.945 34.925) (xy 30.48 34.925)
      )
    )
  )
  (zone (net 43) (net_name /V2+) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 68.2625 32.131) (xy 74.295 35.56) (xy 78.74 35.56) (xy 78.74 47.9425) (xy 71.755 47.9425)
        (xy 71.755 42.545) (xy 68.2625 38.1)
      )
    )
  )
  (zone (net 9) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.945 34.925) (xy 64.135 34.925) (xy 64.135 22.479) (xy 30.48 22.5425) (xy 30.48 17.78)
        (xy 67.945 17.78)
      )
    )
  )
  (zone (net 42) (net_name /H+) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 78.74 27.94) (xy 68.2625 27.94) (xy 68.2625 17.78) (xy 78.74 17.78)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 47.9425 33.655) (xy 49.2125 33.655) (xy 49.2125 36.195) (xy 47.9425 36.195)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 67.945 34.925) (xy 64.135 34.925) (xy 64.135 17.78) (xy 67.945 17.78)
      )
    )
  )
  (zone (net 36) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.5475 22.5425) (xy 62.5475 36.5125) (xy 57.785 36.5125) (xy 57.785 22.5425)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 67.945 22.5425) (xy 30.48 22.5425) (xy 30.48 17.78) (xy 67.945 17.78)
      )
    )
  )
)
