(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 41)
    (tracks 562)
    (zones 0)
    (modules 57)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (trace_clearance 0.15)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 3)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers"))
  )
  (net 0 "")
  (net 1 GNDA)
  (net 2 "Net-(J7-Pad1)")
  (net 3 GNDD)
  (net 4 /meter_module/CLKIN)
  (net 5 +3V3)
  (net 6 /meter_module/~IRQ0)
  (net 7 /meter_module/~IRQ1)
  (net 8 /meter_module/~CS)
  (net 9 /meter_module/MISO)
  (net 10 /meter_module/MOSI)
  (net 11 /meter_module/SCLK)
  (net 12 /meter_module/HSCLK)
  (net 13 /meter_module/~RESET)
  (net 14 "Net-(C22-Pad1)")
  (net 15 IAP)
  (net 16 IBP)
  (net 17 ICP)
  (net 18 IDP)
  (net 19 IEP)
  (net 20 IFP)
  (net 21 VP)
  (net 22 IAN)
  (net 23 IBN)
  (net 24 ICN)
  (net 25 IN)
  (net 26 VN)
  (net 27 /meter_module/AVDD)
  (net 28 /meter_module/DVDD)
  (net 29 /meter_module/CLKOUT)
  (net 30 "Net-(J1-Pad3)")
  (net 31 "Net-(J2-Pad3)")
  (net 32 "Net-(J3-Pad3)")
  (net 33 "Net-(J4-Pad3)")
  (net 34 "Net-(J5-Pad3)")
  (net 35 "Net-(J6-Pad3)")
  (net 36 "Net-(J7-Pad3)")
  (net 37 "Net-(U1-Pad40)")
  (net 38 "Net-(U1-Pad34)")
  (net 39 "Net-(U1-Pad33)")
  (net 40 "Net-(U1-Pad31)")
  (net 41 "Net-(U1-Pad30)")
  (net 42 "Net-(U1-Pad21)")
  (net 43 "Net-(U1-Pad20)")
  (net 44 "Net-(U1-Pad11)")
  (net 45 "Net-(U1-Pad10)")
  (net 46 "Net-(U1-Pad1)")
  (net 47 /analog_inputs/IA)
  (net 48 /analog_inputs/IB)
  (net 49 /analog_inputs/IC)
  (net 50 /analog_inputs/ID)
  (net 51 /analog_inputs/IE)
  (net 52 /analog_inputs/IF)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /analog_inputs/IA)
    (add_net /analog_inputs/IB)
    (add_net /analog_inputs/IC)
    (add_net /analog_inputs/ID)
    (add_net /analog_inputs/IE)
    (add_net /analog_inputs/IF)
    (add_net /meter_module/AVDD)
    (add_net /meter_module/CLKIN)
    (add_net /meter_module/CLKOUT)
    (add_net /meter_module/DVDD)
    (add_net /meter_module/HSCLK)
    (add_net /meter_module/MISO)
    (add_net /meter_module/MOSI)
    (add_net /meter_module/SCLK)
    (add_net /meter_module/~CS)
    (add_net /meter_module/~IRQ0)
    (add_net /meter_module/~IRQ1)
    (add_net /meter_module/~RESET)
    (add_net GNDA)
    (add_net GNDD)
    (add_net IAN)
    (add_net IAP)
    (add_net IBN)
    (add_net IBP)
    (add_net ICN)
    (add_net ICP)
    (add_net IDP)
    (add_net IEP)
    (add_net IFP)
    (add_net IN)
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad40)")
    (add_net VN)
    (add_net VP)
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 140.335 51.435)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference LOGO1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value Logo_Open_Hardware_Small (at 0.75 0) (layer F.Fab) hide)
  )
  (module Housings_DFN_QFN:QFN-40-1EP_6x6mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 132.525 67.475 270)
    (descr "40-Lead Plastic Quad Flat, No Lead Package (ML) - 6x6x0.9mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at -2.775 -4.625 180) (layer F.SilkS))
    (fp_text value ADE7816ACPZ (at 0 4.25 90) (layer F.Fab))
    (pad 41 smd rect (at -1.725 -1.725 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at -1.725 -0.575 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at -1.725 0.575 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at -1.725 1.725 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at -0.575 -1.725 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at -0.575 -0.575 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at -0.575 0.575 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at -0.575 1.725 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at 0.575 -1.725 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at 0.575 -0.575 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at 0.575 0.575 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at 0.575 1.725 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at 1.725 -1.725 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at 1.725 -0.575 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at 1.725 0.575 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 41 smd rect (at 1.725 1.725 270) (size 1.15 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 40 smd rect (at -2.25 -3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad40)"))
    (pad 39 smd rect (at -1.75 -3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /meter_module/~CS))
    (pad 38 smd rect (at -1.25 -3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /meter_module/MOSI))
    (pad 37 smd rect (at -0.75 -3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /meter_module/MISO))
    (pad 36 smd rect (at -0.25 -3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /meter_module/SCLK))
    (pad 35 smd rect (at 0.25 -3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /meter_module/HSCLK))
    (pad 34 smd rect (at 0.75 -3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad34)"))
    (pad 33 smd rect (at 1.25 -3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad33)"))
    (pad 32 smd rect (at 1.75 -3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /meter_module/~IRQ1))
    (pad 31 smd rect (at 2.25 -3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad31)"))
    (pad 30 smd rect (at 3 -2.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad30)"))
    (pad 29 smd rect (at 3 -1.75 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /meter_module/~IRQ0))
    (pad 28 smd rect (at 3 -1.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /meter_module/CLKOUT))
    (pad 27 smd rect (at 3 -0.75 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /meter_module/CLKIN))
    (pad 26 smd rect (at 3 -0.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 25 smd rect (at 3 0.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 24 smd rect (at 3 0.75 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /meter_module/AVDD))
    (pad 23 smd rect (at 3 1.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 IDP))
    (pad 22 smd rect (at 3 1.75 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 IEP))
    (pad 21 smd rect (at 3 2.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad21)"))
    (pad 20 smd rect (at 2.25 3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad20)"))
    (pad 19 smd rect (at 1.75 3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 IFP))
    (pad 18 smd rect (at 1.25 3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 IN))
    (pad 17 smd rect (at 0.75 3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C22-Pad1)"))
    (pad 16 smd rect (at 0.25 3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 VN))
    (pad 15 smd rect (at -0.25 3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 VP))
    (pad 14 smd rect (at -0.75 3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 ICN))
    (pad 13 smd rect (at -1.25 3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 ICP))
    (pad 12 smd rect (at -1.75 3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 IBN))
    (pad 11 smd rect (at -2.25 3) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad11)"))
    (pad 10 smd rect (at -3 2.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at -3 1.75 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 IBP))
    (pad 8 smd rect (at -3 1.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 IAN))
    (pad 7 smd rect (at -3 0.75 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 IAP))
    (pad 6 smd rect (at -3 0.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD))
    (pad 5 smd rect (at -3 -0.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /meter_module/DVDD))
    (pad 4 smd rect (at -3 -0.75 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /meter_module/~RESET))
    (pad 3 smd rect (at -3 -1.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD))
    (pad 2 smd rect (at -3 -1.75 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -3 -2.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-40-1EP_6x6mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-40-1EP_6x6mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.75 67.91 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -2.11 0.5 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J7-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 VP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A (layer F.Cu) (tedit 5B301BBE)
    (at 129.97 74.85)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C19 (at -3.77 -0.05) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.35 0) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -1.35 0) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 27 /meter_module/AVDD))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 56D1B4CB)
    (at 127 34.29)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 56D1B4CB)
    (at 156.21 102.87)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference H4 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 56D1B4CB)
    (at 156.21 34.29)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 56D1B4CB)
    (at 127 102.87)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 134.274 62.16 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 2.41 0.626 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /meter_module/~RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.7 69.8 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at -3.9 0.6 180) (layer F.SilkS))
    (fp_text value 220n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A (layer F.Cu) (tedit 5B301BBE)
    (at 125.6 70.6 270)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C22 (at -3.05 0.2 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.35 0 270) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -1.35 0 270) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 14 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136.14 62.16 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 2.41 1.81 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /meter_module/~RESET))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A (layer F.Cu) (tedit 5B301BBE)
    (at 130.86 59.96 180)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C20 (at 3.81 0) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.35 0 180) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 28 /meter_module/DVDD))
    (pad 2 smd roundrect (at 1.35 0 180) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 3 GNDD))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 131.44 62.17 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 2.99 0) (layer F.SilkS))
    (fp_text value 220n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /meter_module/DVDD))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GNDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.77 72.66)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at -2.77 0.04) (layer F.SilkS))
    (fp_text value 220n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /meter_module/AVDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 132.27 77.19)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at -2.78 -0.01) (layer F.SilkS))
    (fp_text value Ferrite (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GNDD))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.3642 74.77668 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0.0642 -1.52332) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 VN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.3642 73.10168 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -0.0358 1.40168) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 VN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2520-4Pin_2.5x2.0mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 135.133 72.822 180)
    (descr "SMD Crystal SERIES SMD2520/4 http://www.newxtal.com/UploadFiles/Images/2012-11-12-09-29-09-776.pdf, 2.5x2.0mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at -1.927 2.202) (layer F.SilkS))
    (fp_text value 16.384MHz (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -0.875 -0.7 180) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD))
    (pad 3 smd rect (at 0.875 -0.7 180) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /meter_module/CLKIN))
    (pad 2 smd rect (at 0.875 0.7 180) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GNDD))
    (pad 1 smd rect (at -0.875 0.7 180) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /meter_module/CLKOUT))
    (model ${KIPRJMOD}/3dmodels/SW3dPS-CRY_2520.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 135.133 75.362 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at -2.957 -0.078) (layer F.SilkS))
    (fp_text value 20p (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /meter_module/CLKIN))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GNDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.927 72.822 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -0.878 2.373 180) (layer F.SilkS))
    (fp_text value 20p (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /meter_module/CLKOUT))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GNDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 124.762 80.765)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -0.062 1.435) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 IN))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116.07724 68.78148)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 1.46852) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 ICN))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.362 63.07)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0.038 1.43) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 IBN))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.362 57.105)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0.038 1.495) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 IAN))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.762 78.99 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -0.038 1.39) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 IN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.07724 67.00648 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 1.45648) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 ICN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.362 61.295 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0.062 1.395) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 IBN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.362 55.33 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.062 1.43) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 IAN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.28 68.85)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -0.03 1.5) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 VP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.734 74.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0.034 -1.5) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /analog_inputs/IF))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 IFP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.134 80.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -0.066 -1.5) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /analog_inputs/IE))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 IEP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131 81.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.6) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /analog_inputs/ID))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 IDP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.8 63.1 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /analog_inputs/IC))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 ICP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.7 57.1 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /analog_inputs/IB))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 IBP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 128.134 57.11 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -0.066 -1.59) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /analog_inputs/IA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 IAP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116 73.9 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.2 0 180) (layer F.SilkS))
    (fp_text value 4.7R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /analog_inputs/IF))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.4 79.9 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.2 -0.05 180) (layer F.SilkS))
    (fp_text value 4.7R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /analog_inputs/IE))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 128.3 81 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.2 0.05 180) (layer F.SilkS))
    (fp_text value 4.7R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /analog_inputs/ID))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116.2 62.2 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.15 0.1 180) (layer F.SilkS))
    (fp_text value 4.7R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /analog_inputs/IC))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116 56.2 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.25 0.05 180) (layer F.SilkS))
    (fp_text value 4.7R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /analog_inputs/IB))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.4 56.1875 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.2375 0.05 180) (layer F.SilkS))
    (fp_text value 4.7R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /analog_inputs/IA))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 157.988 56.896)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 0 25.19) (layer F.Fab))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GNDD))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /meter_module/~IRQ0))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /meter_module/~IRQ1))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /meter_module/HSCLK))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /meter_module/SCLK))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /meter_module/MISO))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /meter_module/MOSI))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /meter_module/~CS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /meter_module/~RESET))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.28 67.05)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -0.03 -1.35) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 VP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.734 72.995 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.034 1.395) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 IFP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.134 78.99 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.034 1.39) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 IEP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 131.034 80.12 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -0.066 1.42) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 IDP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.835 61.295 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0.035 1.395) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 ICP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.735 55.33 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0.035 1.53) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 IBP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.134 55.335 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.034 1.435) (layer F.SilkS))
    (fp_text value 22n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 IAP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal (layer F.Cu) (tedit 5E689D85)
    (at 100.621 39.37 90)
    (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
    (tags "3.5mm audio cui horizontal jack stereo")
    (attr smd)
    (fp_text reference J1 (at 4.02 7.779 180) (layer F.SilkS))
    (fp_text value AudioJack3 (at 0 10.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 4.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -2.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad 2 smd rect (at -3.7 5.8 90) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 47 /analog_inputs/IA))
    (pad 1 smd rect (at -3.7 -3.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 3 smd rect (at 3.7 -1.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J1-Pad3)"))
    (model ${KIPRJMOD}/3dmodels/CUI_SJ-3523.step
      (offset (xyz 0 2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module modules:Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal (layer F.Cu) (tedit 5E689D85)
    (at 100.621 50.8 90)
    (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
    (tags "3.5mm audio cui horizontal jack stereo")
    (attr smd)
    (fp_text reference J2 (at 3.95 7.929 180) (layer F.SilkS))
    (fp_text value AudioJack3 (at 0 10.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 3.7 -1.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J2-Pad3)"))
    (pad 1 smd rect (at -3.7 -3.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 2 smd rect (at -3.7 5.8 90) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 48 /analog_inputs/IB))
    (pad "" np_thru_hole circle (at 0 -2.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 4.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/3dmodels/CUI_SJ-3523.step
      (offset (xyz 0 2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module modules:Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal (layer F.Cu) (tedit 5E689D85)
    (at 100.621 62.23 90)
    (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
    (tags "3.5mm audio cui horizontal jack stereo")
    (attr smd)
    (fp_text reference J3 (at 4.03 7.879 180) (layer F.SilkS))
    (fp_text value AudioJack3 (at 0 10.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 3.7 -1.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J3-Pad3)"))
    (pad 1 smd rect (at -3.7 -3.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 2 smd rect (at -3.7 5.8 90) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 49 /analog_inputs/IC))
    (pad "" np_thru_hole circle (at 0 -2.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 4.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/3dmodels/CUI_SJ-3523.step
      (offset (xyz 0 2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module modules:Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal (layer F.Cu) (tedit 5E689D85)
    (at 100.621 97.79 90)
    (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
    (tags "3.5mm audio cui horizontal jack stereo")
    (attr smd)
    (fp_text reference J4 (at 3.94 7.829 180) (layer F.SilkS))
    (fp_text value AudioJack3 (at 0 10.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 4.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -2.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad 2 smd rect (at -3.7 5.8 90) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 50 /analog_inputs/ID))
    (pad 1 smd rect (at -3.7 -3.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 3 smd rect (at 3.7 -1.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J4-Pad3)"))
    (model ${KIPRJMOD}/3dmodels/CUI_SJ-3523.step
      (offset (xyz 0 2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module modules:Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal (layer F.Cu) (tedit 5E689D85)
    (at 100.621 86.36 90)
    (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
    (tags "3.5mm audio cui horizontal jack stereo")
    (attr smd)
    (fp_text reference J5 (at 3.96 7.629 180) (layer F.SilkS))
    (fp_text value AudioJack3 (at 0 10.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 4.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -2.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad 2 smd rect (at -3.7 5.8 90) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 51 /analog_inputs/IE))
    (pad 1 smd rect (at -3.7 -3.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 3 smd rect (at 3.7 -1.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J5-Pad3)"))
    (model ${KIPRJMOD}/3dmodels/CUI_SJ-3523.step
      (offset (xyz 0 2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module modules:Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal (layer F.Cu) (tedit 5E689D85)
    (at 100.621 74.93 90)
    (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
    (tags "3.5mm audio cui horizontal jack stereo")
    (attr smd)
    (fp_text reference J6 (at 3.98 7.879 180) (layer F.SilkS))
    (fp_text value AudioJack3 (at 0 10.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 3.7 -1.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J6-Pad3)"))
    (pad 1 smd rect (at -3.7 -3.6 90) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDA))
    (pad 2 smd rect (at -3.7 5.8 90) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 52 /analog_inputs/IF))
    (pad "" np_thru_hole circle (at 0 -2.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 4.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/3dmodels/CUI_SJ-3523.step
      (offset (xyz 0 2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module modules:Barrel_Jack_CUI_PJ-002A (layer F.Cu) (tedit 5E6AB4AF)
    (at 140.97 93.345)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J7 (at -3.77 -1.945 180) (layer F.SilkS))
    (fp_text value Barrel_Jack_Switch (at -5.5 6.2 90) (layer F.Fab))
    (fp_text user %R (at 0 6.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 4.5 2) (drill oval 3.5 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J7-Pad1)"))
    (pad 2 thru_hole oval (at 0 6) (size 4 2) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 3 thru_hole oval (at 4.7 3) (size 2 4) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 36 "Net-(J7-Pad3)"))
    (model ${KIPRJMOD}/3dmodels/AB2_PB_2MM_JACK_PTH.wrl
      (offset (xyz 0 -14 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 29.21 (width 0.15) (layer Dwgs.User)
    (gr_text "29.210 mm" (at 141.605 116.235) (layer Dwgs.User))
    (feature1 (pts (xy 156.21 102.87) (xy 156.21 115.521421)))
    (feature2 (pts (xy 127 102.87) (xy 127 115.521421)))
    (crossbar (pts (xy 127 114.935) (xy 156.21 114.935)))
    (arrow1a (pts (xy 156.21 114.935) (xy 155.083496 115.521421)))
    (arrow1b (pts (xy 156.21 114.935) (xy 155.083496 114.348579)))
    (arrow2a (pts (xy 127 114.935) (xy 128.126504 115.521421)))
    (arrow2b (pts (xy 127 114.935) (xy 128.126504 114.348579)))
  )
  (gr_text "AC IN\n9 V - 12 V" (at 140.97 87.63) (layer F.SilkS))
  (gr_text ID (at 111.76 97.79) (layer F.SilkS))
  (gr_text IE (at 111.712381 86.36) (layer F.SilkS))
  (gr_text IF (at 111.688571 74.93) (layer F.SilkS))
  (gr_text IC (at 111.76 62.23) (layer F.SilkS))
  (gr_text IB (at 111.76 50.8) (layer F.SilkS))
  (gr_text IA (at 111.688571 39.37) (layer F.SilkS))
  (gr_text GNDD (at 153.67 80.01) (layer B.SilkS))
  (gr_text 3V3 (at 154.305 77.47) (layer B.SilkS))
  (gr_text ~IRQ0 (at 153.955715 74.93) (layer B.SilkS))
  (gr_text ~IRQ1 (at 153.955715 72.39) (layer B.SilkS))
  (gr_text HSCLK (at 153.289048 69.85) (layer B.SilkS))
  (gr_text SCLK (at 153.812857 67.31) (layer B.SilkS))
  (gr_text MISO (at 153.884286 64.77) (layer B.SilkS))
  (gr_text MOSI (at 153.884286 62.23) (layer B.SilkS))
  (gr_text ~CS (at 154.717619 59.69) (layer B.SilkS))
  (gr_text ~RESET (at 153.431905 57.15) (layer B.SilkS))
  (gr_text "OSHW TAPR" (at 140.97 56.515) (layer F.SilkS))
  (gr_text "ADE7816 Breakout\nv0.1 2020-03-15\nby Tisham (whatnick) Dhar\nhttp://whatnick.com" (at 140.97 42.545) (layer F.SilkS))
  (gr_text GNDD (at 153.67 80.01) (layer F.SilkS))
  (gr_text 3V3 (at 154.312857 77.47) (layer F.SilkS))
  (gr_text ~IRQ0 (at 153.955715 74.93) (layer F.SilkS))
  (gr_text ~IRQ1 (at 153.955715 72.39) (layer F.SilkS))
  (gr_text HSCLK (at 153.289048 69.85) (layer F.SilkS))
  (gr_text SCLK (at 153.812857 67.31) (layer F.SilkS))
  (gr_text MISO (at 153.884286 64.77) (layer F.SilkS))
  (gr_text MOSI (at 153.884286 62.23) (layer F.SilkS))
  (gr_text ~CS (at 154.717619 59.69) (layer F.SilkS))
  (gr_text ~RESET (at 153.431905 57.15) (layer F.SilkS))
  (gr_arc (start 97.79 34.29) (end 97.79 30.48) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 97.79 102.87) (end 93.98 102.87) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156.21 102.87) (end 156.21 106.68) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156.21 34.29) (end 160.02 34.29) (angle -90) (layer Edge.Cuts) (width 0.05))
  (dimension 66.04 (width 0.15) (layer Dwgs.User)
    (gr_text "66.040 mm" (at 127 17.75) (layer Dwgs.User))
    (feature1 (pts (xy 93.98 30.48) (xy 93.98 18.463579)))
    (feature2 (pts (xy 160.02 30.48) (xy 160.02 18.463579)))
    (crossbar (pts (xy 160.02 19.05) (xy 93.98 19.05)))
    (arrow1a (pts (xy 93.98 19.05) (xy 95.106504 18.463579)))
    (arrow1b (pts (xy 93.98 19.05) (xy 95.106504 19.636421)))
    (arrow2a (pts (xy 160.02 19.05) (xy 158.893496 18.463579)))
    (arrow2b (pts (xy 160.02 19.05) (xy 158.893496 19.636421)))
  )
  (dimension 76.2 (width 0.15) (layer Dwgs.User)
    (gr_text "76.200 mm" (at 172.75 68.58 270) (layer Dwgs.User))
    (feature1 (pts (xy 160.02 106.68) (xy 172.036421 106.68)))
    (feature2 (pts (xy 160.02 30.48) (xy 172.036421 30.48)))
    (crossbar (pts (xy 171.45 30.48) (xy 171.45 106.68)))
    (arrow1a (pts (xy 171.45 106.68) (xy 170.863579 105.553496)))
    (arrow1b (pts (xy 171.45 106.68) (xy 172.036421 105.553496)))
    (arrow2a (pts (xy 171.45 30.48) (xy 170.863579 31.606504)))
    (arrow2b (pts (xy 171.45 30.48) (xy 172.036421 31.606504)))
  )
  (gr_line (start 156.21 30.48) (end 97.79 30.48) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 160.02 102.87) (end 160.02 34.29) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.79 106.68) (end 156.21 106.68) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.98 34.29) (end 93.98 102.87) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 160 82) (xy 132.9 82) (xy 132.9 69.9) (xy 130.1 69.9) (xy 130.1 64.75)
        (xy 130.1 55) (xy 130.5 55) (xy 160 55)
      )
    )
  )
  (zone (net 1) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 160 106.5) (xy 94 106.5) (xy 94 30.5) (xy 160 30.5)
      )
    )
  )
  (zone (net 1) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 160 106.5) (xy 94 106.5) (xy 94 30.55) (xy 160 30.5)
      )
    )
  )
  (zone (net 3) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 160 55) (xy 160 82) (xy 132.9 82) (xy 132.9 69.9) (xy 130.1 69.9)
        (xy 130.1 55)
      )
    )
  )
)
