<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="33" y2="0" width="0" layer="20"/>
<wire x1="33" y1="0" x2="33" y2="65.71" width="0" layer="20"/>
<wire x1="33" y1="65.71" x2="0" y2="65.71" width="0" layer="20"/>
<wire x1="0" y1="65.71" x2="0" y2="0" width="0" layer="20"/>
<text>ANT</text>
<text>G</text>
<text>D</text>
<text>V</text>
<text>A</text>
<text>REED</text>
<text>DHT</text>
<text>V</text>
<text>D</text>
<text>G</text>
<text>&lt;--USB</text>
<text>nodeSensor</text>
<text>friedcircuits.us</text>
<text>07/04/2016</text>
<text>v0.1</text>
<text>v0.1</text>
<text>nodeSensor</text>
<text>friedcircuits.us</text>
<text>G</text>
<text>5V</text>
<text>3v</text>
<text>TX</text>
<text>RX</text>
<text>D8</text>
<text>D5</text>
<text>D4</text>
<text>D3</text>
<text>D1</text>
<text>D0</text>
<text>*Optional</text>
<text>G</text>
<text>5V</text>
<text>3v</text>
<text>TX</text>
<text>RX</text>
<text>D8</text>
<text>D5</text>
<text>D4</text>
<text>D3</text>
<text>D1</text>
<text>D0</text>
<text>V</text>
<text>D</text>
<text>G</text>
<text>REED</text>
<text>DHT</text>
<text>V</text>
<text>V</text>
<text>G</text>
<text>G</text>
<text>ANT</text>
<text>10K-LDR</text>
</plain>
<libraries>
<library name="FriedCircuits">
<description>FriedCircuits - friedcircuits.us</description>
<packages>
<package name="FC_CREDIT">
</package>
</packages>
</library>
<library name="ESP12E_DEVKIT">
<packages>
<package name="ESP12E_DEVKIT">
<description>ESP12E_DEVKIT</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK">
</package>
<package name="1X02_LOCK">
</package>
<package name="1X01_LONGPAD">
</package>
<package name="1X11_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
<package name="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="AXIAL-0.3-KIT">
<description>&lt;h3&gt;AXIAL-0.3-KIT&lt;/h3&gt;

Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of the AXIAL-0.3 package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RF-LINK_RX">
<description>RF-LINK receivers WRL-8947, 8948, 8949, 8950</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="PHOTOCELL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="FriedCircuits" package="FC_CREDIT" value="FRAME_DINA4_L">
<attribute name="URL1" value="friedcircuits.us"/>
<attribute name="AUTHOR" value="W. Garrido"/>
<attribute name="LICENSE" value=""/>
<attribute name="FF1" value="by"/>
<attribute name="PROJECT" value="Projectname"/>
<attribute name="FF2" value="FriedCircuits"/>
</element>
<element name="U$2" library="ESP12E_DEVKIT" package="ESP12E_DEVKIT" value="ESP12E_DEVKIT">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-1000UF-25V" value="100uf">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U$3" library="SparkFun-RF" package="RF-LINK_RX" value="RF-LINK_RX">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X01_LONGPAD" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK" value="S_-RF-PWR">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3-KIT" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="PHOTOCELL" value="10K-LDR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X11_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3-KIT" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RF_DATA">
<contactref element="U$2" pad="D6"/>
<contactref element="U$3" pad="DATA@1"/>
</signal>
<signal name="REED">
<contactref element="J3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$2" pad="D2"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="GND@2"/>
<contactref element="U$2" pad="GND@3"/>
<contactref element="U$2" pad="GND@1"/>
<contactref element="U$2" pad="GND@0"/>
<contactref element="U$3" pad="GND@1"/>
<contactref element="J1" pad="3"/>
<contactref element="R1" pad="P$1"/>
<contactref element="J3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="N$4">
<contactref element="U$3" pad="ANT"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$3" pad="+5V@1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="JP1" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="9"/>
<contactref element="U$2" pad="3V3@1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="DHT_DATA">
<contactref element="J1" pad="2"/>
<contactref element="U$2" pad="D7"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="LDR">
<contactref element="U$2" pad="AD0"/>
<contactref element="R3" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="D0">
<contactref element="U$2" pad="D0"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="D1">
<contactref element="U$2" pad="D1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="D3">
<contactref element="U$2" pad="D3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="D4">
<contactref element="U$2" pad="D4"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="D8">
<contactref element="U$2" pad="D8"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="RX">
<contactref element="U$2" pad="RX"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="TX">
<contactref element="U$2" pad="TX"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="+5V">
<contactref element="U$2" pad="VIN"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="D5">
<contactref element="U$2" pad="D5"/>
<contactref element="J2" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
