<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="10.095" y2="0" width="0" layer="20"/>
<wire x1="10.095" y1="0" x2="10.095" y2="18.73" width="0" layer="20"/>
<wire x1="10.095" y1="18.73" x2="0" y2="18.73" width="0" layer="20"/>
<wire x1="0" y1="18.73" x2="0" y2="0" width="0" layer="20"/>
<text>TDI</text>
<text>TMS</text>
<text>TDO</text>
<text>TCK</text>
<text>GND</text>
<text>VREF</text>
<text>GND</text>
<text>FPGA</text>
<text>Lazy Pano G2 JTAG Adapter V1</text>
<text>This side faces down</text>
</plain>
<libraries>
<library name="archi_laptop">
<packages>
<package name="1X6_127MM">
</package>
<package name="2X5_PIN_SOCKET">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="archi_laptop" package="1X6_127MM" value="1X6_127MM"/>
<element name="JTAG" library="archi_laptop" package="2X5_PIN_SOCKET" value="2X5_PIN_SOCKET">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VREF">
<contactref element="JTAG" pad="P$7"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="TDI">
<contactref element="JTAG" pad="P$1"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="TMS">
<contactref element="U$1" pad="P$3"/>
<contactref element="JTAG" pad="P$3"/>
</signal>
<signal name="TDO">
<contactref element="U$1" pad="P$4"/>
<contactref element="JTAG" pad="P$4"/>
</signal>
<signal name="TCK">
<contactref element="U$1" pad="P$5"/>
<contactref element="JTAG" pad="P$5"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$6"/>
<contactref element="JTAG" pad="P$6"/>
<contactref element="JTAG" pad="P$10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
