(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 366)
    (zones 0)
    (modules 27)
    (nets 61)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.000152)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.000508)
    (via_min_drill 0.000254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.000051)
    (solder_mask_min_width 0.000102)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D3-Pad2)")
  (net 5 "Net-(D4-Pad2)")
  (net 6 "Net-(D5-Pad2)")
  (net 7 "Net-(D6-Pad2)")
  (net 8 "Net-(D7-Pad2)")
  (net 9 "Net-(D8-Pad2)")
  (net 10 "Net-(D9-Pad2)")
  (net 11 "Net-(D10-Pad2)")
  (net 12 "Net-(D11-Pad2)")
  (net 13 "Net-(RN1-Pad8)")
  (net 14 "Net-(RN1-Pad7)")
  (net 15 "Net-(RN1-Pad6)")
  (net 16 "Net-(RN1-Pad5)")
  (net 17 "Net-(RN1-Pad4)")
  (net 18 "Net-(RN1-Pad3)")
  (net 19 "Net-(RN1-Pad2)")
  (net 20 "Net-(RN1-Pad1)")
  (net 21 "Net-(RN2-Pad8)")
  (net 22 "Net-(RN2-Pad7)")
  (net 23 "Net-(RN2-Pad6)")
  (net 24 "Net-(RN2-Pad5)")
  (net 25 "Net-(RN2-Pad12)")
  (net 26 "Net-(RN2-Pad4)")
  (net 27 "Net-(RN2-Pad11)")
  (net 28 "Net-(RN2-Pad3)")
  (net 29 "Net-(RN2-Pad10)")
  (net 30 "Net-(RN2-Pad2)")
  (net 31 "Net-(RN2-Pad9)")
  (net 32 "Net-(RN2-Pad1)")
  (net 33 "Net-(SW1-Pad1)")
  (net 34 "Net-(SW2-Pad1)")
  (net 35 "Net-(SW3-Pad1)")
  (net 36 "Net-(SW4-Pad1)")
  (net 37 "Net-(SW5-Pad1)")
  (net 38 "Net-(SW6-Pad1)")
  (net 39 "Net-(SW7-Pad1)")
  (net 40 "Net-(SW8-Pad1)")
  (net 41 "Net-(SW9-Pad1)")
  (net 42 "Net-(SW10-Pad1)")
  (net 43 "Net-(SW11-Pad1)")
  (net 44 "Net-(SW12-Pad1)")
  (net 45 "Net-(U$1-Pad23)")
  (net 46 "Net-(U$1-Pad28)")
  (net 47 "Net-(U$1-Pad30)")
  (net 48 "Net-(U$1-Pad33)")
  (net 49 "Net-(U$1-Pad35)")
  (net 50 "Net-(U$1-Pad36)")
  (net 51 "Net-(U$1-Pad37)")
  (net 52 "Net-(U$1-Pad38)")
  (net 53 "Net-(U$1-Pad39)")
  (net 54 "Net-(U$1-Pad40)")
  (net 55 "Net-(U$1-Pad20)")
  (net 56 "Net-(U$1-Pad16)")
  (net 57 "Net-(U$1-Pad13)")
  (net 58 "Net-(U$1-Pad8)")
  (net 59 "Net-(U$1-Pad3)")
  (net 60 "Net-(D12-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(RN1-Pad1)")
    (add_net "Net-(RN1-Pad2)")
    (add_net "Net-(RN1-Pad3)")
    (add_net "Net-(RN1-Pad4)")
    (add_net "Net-(RN1-Pad5)")
    (add_net "Net-(RN1-Pad6)")
    (add_net "Net-(RN1-Pad7)")
    (add_net "Net-(RN1-Pad8)")
    (add_net "Net-(RN2-Pad1)")
    (add_net "Net-(RN2-Pad10)")
    (add_net "Net-(RN2-Pad11)")
    (add_net "Net-(RN2-Pad12)")
    (add_net "Net-(RN2-Pad2)")
    (add_net "Net-(RN2-Pad3)")
    (add_net "Net-(RN2-Pad4)")
    (add_net "Net-(RN2-Pad5)")
    (add_net "Net-(RN2-Pad6)")
    (add_net "Net-(RN2-Pad7)")
    (add_net "Net-(RN2-Pad8)")
    (add_net "Net-(RN2-Pad9)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(SW10-Pad1)")
    (add_net "Net-(SW11-Pad1)")
    (add_net "Net-(SW12-Pad1)")
    (add_net "Net-(SW2-Pad1)")
    (add_net "Net-(SW3-Pad1)")
    (add_net "Net-(SW4-Pad1)")
    (add_net "Net-(SW5-Pad1)")
    (add_net "Net-(SW6-Pad1)")
    (add_net "Net-(SW7-Pad1)")
    (add_net "Net-(SW8-Pad1)")
    (add_net "Net-(SW9-Pad1)")
    (add_net "Net-(U$1-Pad13)")
    (add_net "Net-(U$1-Pad16)")
    (add_net "Net-(U$1-Pad20)")
    (add_net "Net-(U$1-Pad23)")
    (add_net "Net-(U$1-Pad28)")
    (add_net "Net-(U$1-Pad3)")
    (add_net "Net-(U$1-Pad30)")
    (add_net "Net-(U$1-Pad33)")
    (add_net "Net-(U$1-Pad35)")
    (add_net "Net-(U$1-Pad36)")
    (add_net "Net-(U$1-Pad37)")
    (add_net "Net-(U$1-Pad38)")
    (add_net "Net-(U$1-Pad39)")
    (add_net "Net-(U$1-Pad40)")
    (add_net "Net-(U$1-Pad8)")
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 30.48 25.4)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at -3.81 0) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 52.07 25.4)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at -3.81 0) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 73.66 25.4)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at -3.81 0) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 95.25 25.4)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D4 (at -2.54 0) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 30.48 45.72)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 52.07 45.72)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 73.66 45.72)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D7 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 95.25 45.72)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D8 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D8-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 30.48 66.04)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D9 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 52.07 66.04)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D10 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 73.66 66.04)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D11 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 95.25 66.04)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D12 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED5MM (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 60 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer B.Cu) (tedit 5A02E8C5)
    (at 45.72 30.48 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference RN1 (at 3.81 2.33) (layer B.SilkS))
    (fp_text value R_Pack08 (at 3.81 -20.11) (layer B.Fab))
    (fp_text user %R (at 3.81 -8.89) (layer B.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(RN1-Pad8)"))
    (pad 15 thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(RN1-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(RN1-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(RN1-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(RN1-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(RN1-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D7-Pad2)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(RN1-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D8-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(RN1-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer B.Cu) (tedit 5A02E8C5)
    (at 45.72 59.69 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference RN2 (at 3.81 2.33) (layer B.SilkS))
    (fp_text value R_Pack08 (at 3.81 -20.11) (layer B.Fab))
    (fp_text user %R (at 3.81 -8.89) (layer B.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D9-Pad2)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(RN2-Pad8)"))
    (pad 15 thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(D10-Pad2)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(RN2-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D11-Pad2)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(RN2-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(D12-Pad2)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(RN2-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(RN2-Pad12)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(RN2-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(RN2-Pad11)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(RN2-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(RN2-Pad10)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(RN2-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(RN2-Pad9)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(RN2-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 34.29 30.48)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW1 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 33 "Net-(SW1-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 55.88 30.48)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW2 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 34 "Net-(SW2-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 77.47 30.48)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW3 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(SW3-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 99.06 30.48)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW4 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 36 "Net-(SW4-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 34.29 50.8)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW5 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 37 "Net-(SW5-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 55.88 50.8)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW6 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 38 "Net-(SW6-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 77.47 50.8)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW7 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 39 "Net-(SW7-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 99.06 50.8)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW8 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 40 "Net-(SW8-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 34.29 71.12)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW9 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 41 "Net-(SW9-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 55.88 71.12)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW10 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 42 "Net-(SW10-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 77.47 71.12)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW11 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 43 "Net-(SW11-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_Keyboard:SW_Cherry_MX_1.00u_Plate (layer F.Cu) (tedit 5A02FE24)
    (at 99.06 71.12)
    (descr "Cherry MX keyswitch, 1.00u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u plate")
    (fp_text reference SW12 (at -2.54 -2.794) (layer F.SilkS))
    (fp_text value MX (at -2.54 12.954) (layer F.Fab))
    (fp_text user %R (at -2.54 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 44 "Net-(SW12-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_Plate.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model :CherryMX:SW_Cherry_MX_Plate.wrl
      (offset (xyz -2.5 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Raspberry Pi:RPi_Pico_SMD_TH" (layer B.Cu) (tedit 6032544B)
    (at 74.93 54.61 180)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference U$1 (at 0 0 180) (layer B.SilkS))
    (fp_text value RPI_PICO-SMD (at 0 -2.159 180) (layer B.Fab))
    (fp_text user SWDIO (at 5.6 -26.2 180) (layer B.SilkS))
    (fp_text user SWCLK (at -5.7 -26.2 180) (layer B.SilkS))
    (fp_text user AGND (at 13.054 6.35 135) (layer B.SilkS))
    (fp_text user GND (at 12.8 19.05 135) (layer B.SilkS))
    (fp_text user GND (at 12.8 -6.35 135) (layer B.SilkS))
    (fp_text user GND (at 12.8 -19.05 135) (layer B.SilkS))
    (fp_text user GND (at -12.8 -19.05 135) (layer B.SilkS))
    (fp_text user GND (at -12.8 -6.35 135) (layer B.SilkS))
    (fp_text user GND (at -12.8 6.35 135) (layer B.SilkS))
    (fp_text user GND (at -12.8 19.05 135) (layer B.SilkS))
    (fp_text user VBUS (at 13.3 24.2 135) (layer B.SilkS))
    (fp_text user VSYS (at 13.2 21.59 135) (layer B.SilkS))
    (fp_text user 3V3_EN (at 13.7 17.2 135) (layer B.SilkS))
    (fp_text user 3V3 (at 12.9 13.9 135) (layer B.SilkS))
    (fp_text user ADC_VREF (at 14 12.5 135) (layer B.SilkS))
    (fp_text user GP28 (at 13.054 9.144 135) (layer B.SilkS))
    (fp_text user GP27 (at 13.054 3.8 135) (layer B.SilkS))
    (fp_text user GP26 (at 13.054 1.27 135) (layer B.SilkS))
    (fp_text user RUN (at 13 -1.27 135) (layer B.SilkS))
    (fp_text user GP22 (at 13.054 -3.81 135) (layer B.SilkS))
    (fp_text user GP21 (at 13.054 -8.9 135) (layer B.SilkS))
    (fp_text user GP20 (at 13.054 -11.43 135) (layer B.SilkS))
    (fp_text user GP19 (at 13.054 -13.97 135) (layer B.SilkS))
    (fp_text user GP18 (at 13.054 -16.51 135) (layer B.SilkS))
    (fp_text user GP17 (at 13.054 -21.59 135) (layer B.SilkS))
    (fp_text user GP16 (at 13.054 -24.13 135) (layer B.SilkS))
    (fp_text user GP15 (at -13.054 -24.13 135) (layer B.SilkS))
    (fp_text user GP14 (at -13.1 -21.59 135) (layer B.SilkS))
    (fp_text user GP13 (at -13.054 -16.51 135) (layer B.SilkS))
    (fp_text user GP12 (at -13.2 -13.97 135) (layer B.SilkS))
    (fp_text user GP11 (at -13.2 -11.43 135) (layer B.SilkS))
    (fp_text user GP10 (at -13.054 -8.89 135) (layer B.SilkS))
    (fp_text user GP9 (at -12.8 -3.81 135) (layer B.SilkS))
    (fp_text user GP8 (at -12.8 -1.27 135) (layer B.SilkS))
    (fp_text user GP7 (at -12.7 1.3 135) (layer B.SilkS))
    (fp_text user GP6 (at -12.8 3.81 135) (layer B.SilkS))
    (fp_text user GP5 (at -12.8 8.89 135) (layer B.SilkS))
    (fp_text user GP4 (at -12.8 11.43 135) (layer B.SilkS))
    (fp_text user GP3 (at -12.8 13.97 135) (layer B.SilkS))
    (fp_text user GP0 (at -12.8 24.13 135) (layer B.SilkS))
    (fp_text user GP2 (at -12.9 16.51 135) (layer B.SilkS))
    (fp_text user GP1 (at -12.9 21.6 135) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 40 thru_hole oval (at 8.89 24.13 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 54 "Net-(U$1-Pad40)"))
    (pad 39 thru_hole oval (at 8.89 21.59 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 53 "Net-(U$1-Pad39)"))
    (pad 38 thru_hole rect (at 8.89 19.05 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 52 "Net-(U$1-Pad38)"))
    (pad 37 thru_hole oval (at 8.89 16.51 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 51 "Net-(U$1-Pad37)"))
    (pad 36 thru_hole oval (at 8.89 13.97 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 50 "Net-(U$1-Pad36)"))
    (pad 35 thru_hole oval (at 8.89 11.43 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 49 "Net-(U$1-Pad35)"))
    (pad 34 thru_hole oval (at 8.89 8.89 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 26 "Net-(RN2-Pad4)"))
    (pad 33 thru_hole rect (at 8.89 6.35 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 48 "Net-(U$1-Pad33)"))
    (pad 32 thru_hole oval (at 8.89 3.81 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 28 "Net-(RN2-Pad3)"))
    (pad 31 thru_hole oval (at 8.89 1.27 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 "Net-(RN2-Pad2)"))
    (pad 30 thru_hole oval (at 8.89 -1.27 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 47 "Net-(U$1-Pad30)"))
    (pad 29 thru_hole oval (at 8.89 -3.81 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 32 "Net-(RN2-Pad1)"))
    (pad 28 thru_hole rect (at 8.89 -6.35 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 46 "Net-(U$1-Pad28)"))
    (pad 27 thru_hole oval (at 8.89 -8.89 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(RN1-Pad8)"))
    (pad 26 thru_hole oval (at 8.89 -11.43 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 "Net-(RN1-Pad7)"))
    (pad 25 thru_hole oval (at 8.89 -13.97 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 "Net-(RN1-Pad6)"))
    (pad 24 thru_hole oval (at 8.89 -16.51 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 "Net-(RN1-Pad5)"))
    (pad 23 thru_hole rect (at 8.89 -19.05 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 45 "Net-(U$1-Pad23)"))
    (pad 22 thru_hole oval (at 8.89 -21.59 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 "Net-(RN1-Pad4)"))
    (pad 21 thru_hole oval (at 8.89 -24.13 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 "Net-(RN1-Pad3)"))
    (pad 20 thru_hole oval (at -8.89 -24.13 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 55 "Net-(U$1-Pad20)"))
    (pad 19 thru_hole oval (at -8.89 -21.59 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 "Net-(RN1-Pad2)"))
    (pad 18 thru_hole rect (at -8.89 -19.05 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 17 thru_hole oval (at -8.89 -16.51 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 "Net-(RN1-Pad1)"))
    (pad 16 thru_hole oval (at -8.89 -13.97 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 56 "Net-(U$1-Pad16)"))
    (pad 15 thru_hole oval (at -8.89 -11.43 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 44 "Net-(SW12-Pad1)"))
    (pad 14 thru_hole oval (at -8.89 -8.89 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 43 "Net-(SW11-Pad1)"))
    (pad 13 thru_hole rect (at -8.89 -6.35 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 57 "Net-(U$1-Pad13)"))
    (pad 12 thru_hole oval (at -8.89 -3.81 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 42 "Net-(SW10-Pad1)"))
    (pad 11 thru_hole oval (at -8.89 -1.27 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 41 "Net-(SW9-Pad1)"))
    (pad 10 thru_hole oval (at -8.89 1.27 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 40 "Net-(SW8-Pad1)"))
    (pad 9 thru_hole oval (at -8.89 3.81 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 39 "Net-(SW7-Pad1)"))
    (pad 8 thru_hole rect (at -8.89 6.35 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 58 "Net-(U$1-Pad8)"))
    (pad 7 thru_hole oval (at -8.89 8.89 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 38 "Net-(SW6-Pad1)"))
    (pad 6 thru_hole oval (at -8.89 11.43 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 37 "Net-(SW5-Pad1)"))
    (pad 5 thru_hole oval (at -8.89 13.97 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 36 "Net-(SW4-Pad1)"))
    (pad 4 thru_hole oval (at -8.89 16.51 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 35 "Net-(SW3-Pad1)"))
    (pad 3 thru_hole rect (at -8.89 19.05 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 59 "Net-(U$1-Pad3)"))
    (pad 2 thru_hole oval (at -8.89 21.59 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 34 "Net-(SW2-Pad1)"))
    (pad 1 thru_hole oval (at -8.89 24.13 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 33 "Net-(SW1-Pad1)"))
  )
  (gr_text @pete_codes (at 99.06 82.55) (layer B.SilkS))
  (gr_line (start 104.14 22.86) (end 104.14 83.82) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.13 22.86) (end 104.14 22.86) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 24.13 83.82) (end 24.13 22.86) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.14 83.82) (end 24.13 83.82) (layer Edge.Cuts) (width 0.1))
  (gr_text "Pico Producer V1.0 - © Pete Gallagher 2021" (at 43.18 82.55) (layer B.SilkS))
)
