(kicad_pcb (version 20171130) (host pcbnew 5.0.0-rc2-dev-unknown-9f5316e~63~ubuntu17.10.1)
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 22)
    (zones 0)
    (modules 2)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
  )
  (module part:HRS_DM3AT-SF-PEJM5 (layer F.Cu) (tedit 0)
    (at 122.4788 68.834)
    (descr "Micro SD card holder with push-to-eject feature.")
    (attr smd)
    (fp_text reference J2 (at -7.90154 2.46515 90) (layer F.SilkS))
    (fp_text value Micro_SD_Card_Det_Hirose_DM3AT (at 8.88715 2.3308 90) (layer F.SilkS))
    (pad 1 smd rect (at 3.2 0) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 2 smd rect (at 2.1 0) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 3 smd rect (at 1 0) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 4 smd rect (at -0.1 0) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 5 smd rect (at -1.2 0) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 6 smd rect (at -2.3 0) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 7 smd rect (at -3.4 0) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 8 smd rect (at -4.5 0) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad SWB smd rect (at -5.45 0) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask))
    (pad P4 smd rect (at 4.75 0) (size 1 1.2) (layers F.Cu F.Paste F.Mask))
    (pad P1 smd rect (at -6.4 4.3) (size 1 1.2) (layers F.Cu F.Paste F.Mask))
    (pad SWA smd rect (at -6.4 10.5) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad P2 smd rect (at -6.4 14.65) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
    (pad P3 smd rect (at 7.1 15.1) (size 1.3 1.9) (layers F.Cu F.Paste F.Mask))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 114.3 65.405 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J1 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 20.55 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 114.935 85.09) (end 114.3 85.09) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 131.445 85.09) (end 131.445 85.725) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3 68.58) (end 114.3 85.09) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.08 68.58) (end 132.08 85.09) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.985 67.945) (end 132.08 68.58) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.395 67.945) (end 114.3 68.58) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 133.35 63.5) (end 133.985 63.5) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 113.03 63.5) (end 113.03 62.865) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.395 67.945) (end 112.395 63.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.445 85.725) (end 114.935 85.725) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.985 63.5) (end 133.985 67.945) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.03 62.865) (end 133.35 62.865) (layer Edge.Cuts) (width 0.1))
  (gr_text DAT2 (at 132.5372 63.3476) (layer F.SilkS))
  (gr_text DAT3/CD (at 129.208303 63.3476) (layer F.SilkS))
  (gr_text CMD (at 125.98655 63.3476) (layer F.SilkS))
  (gr_text VDD (at 123.705274 63.3476) (layer F.SilkS))
  (gr_text CLK (at 121.507332 63.3476) (layer F.SilkS))
  (gr_text VSS (at 119.333199 63.3476) (layer F.SilkS))
  (gr_text "DAT0\n" (at 116.96859 63.3476) (layer F.SilkS))
  (gr_text "DAT1\n" (at 114.4016 63.3476) (layer F.SilkS))
)
