(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 0)
    (area 83.924999 72.924999 149.075001 103.075001)
    (thickness 1.6)
    (drawings 256)
    (tracks 532)
    (zones 0)
    (modules 51)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.7)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.7 0.7)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x10030_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory I:/Electronics/Projects/Hardware/kicad_projects/BenchPi_ZeroFlasher/PCB_PDFs/))
  )
  (net 0 "")
  (net 1 /V33)
  (net 2 GND)
  (net 3 /V50)
  (net 4 /V18)
  (net 5 "Net-(F1-Pad2)")
  (net 6 "Net-(F2-Pad1)")
  (net 7 /I2C_SDA)
  (net 8 /I2C_SCL)
  (net 9 /SPI0_MOSI)
  (net 10 /SPI0_MISO)
  (net 11 /SPI0_SCK)
  (net 12 /SPI0_CE0)
  (net 13 /SPI0_CE0_EXT)
  (net 14 /SPI0_SCK_EXT)
  (net 15 /SPI0_MISO_EXT)
  (net 16 /SPI0_MOSI_EXT)
  (net 17 /SCL_EXT)
  (net 18 /SDA_EXT)
  (net 19 /VEXT_I2C)
  (net 20 /VEXT_SPI)
  (net 21 /VCC_SPI)
  (net 22 /VCC_I2C)
  (net 23 "Net-(IC2-Pad2)")
  (net 24 "Net-(IC3-Pad4)")
  (net 25 "Net-(IC4-Pad4)")
  (net 26 "Net-(IC5-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.7)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /I2C_SCL)
    (add_net /I2C_SDA)
    (add_net /SCL_EXT)
    (add_net /SDA_EXT)
    (add_net /SPI0_CE0)
    (add_net /SPI0_CE0_EXT)
    (add_net /SPI0_MISO)
    (add_net /SPI0_MISO_EXT)
    (add_net /SPI0_MOSI)
    (add_net /SPI0_MOSI_EXT)
    (add_net /SPI0_SCK)
    (add_net /SPI0_SCK_EXT)
    (add_net /V18)
    (add_net /V33)
    (add_net /V50)
    (add_net /VCC_I2C)
    (add_net /VCC_SPI)
    (add_net /VEXT_I2C)
    (add_net /VEXT_SPI)
    (add_net GND)
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(F2-Pad1)")
    (add_net "Net-(IC2-Pad2)")
    (add_net "Net-(IC3-Pad4)")
    (add_net "Net-(IC4-Pad4)")
    (add_net "Net-(IC5-Pad4)")
  )
  (module H_logos:KiCad-Logo_Copper_11mmx5mm (layer B.Cu) (tedit 5974FBC2)
    (at 115.83 93.49 180)
    (fp_text reference G*** (at -0.8 1.6 180) (layer Cmts.User))
    (fp_text value "KiCad Logo" (at 2.8 1 180) (layer B.SilkS) hide)
    (pad 1 smd circle (at -2.17 1.49 180) (size 0.9 0.9) (layers B.Cu B.Mask)
      (solder_mask_margin -0.01))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 124.275 91.825)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 119.4 89.05)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 113.25 81.55)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 116 87.125)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 116 84.45)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 126.1 84.8)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 122.125 81.825)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 118.6 81.8)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 93.925 99.85)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 143.25 85.55)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 131.4 81.55)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 129.375 88.625)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module conn-100mil:CONN-100MIL-F-1x6 (layer F.Cu) (tedit 58C3248F)
    (at 145.775 88.025 90)
    (fp_text reference P1 (at -7.175 -2.775 90) (layer F.Fab))
    (fp_text value CONN_01X06 (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -6.35 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 20 /VEXT_SPI))
    (pad 2 thru_hole oval (at -3.81 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at -1.27 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SPI0_SCK_EXT))
    (pad 4 thru_hole oval (at 1.27 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 /SPI0_MISO_EXT))
    (pad 5 thru_hole oval (at 3.81 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SPI0_MOSI_EXT))
    (pad 6 thru_hole oval (at 6.35 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SPI0_CE0_EXT))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_dev_kits:z_RPiZero_Hat_NPTH locked (layer F.Cu) (tedit 58C321F4)
    (at 116.5 88)
    (fp_text reference IC1 (at 0 -14) (layer Cmts.User))
    (fp_text value RPi_A+_B+_2B_Hat (at 0 -14.5) (layer F.Fab))
    (pad "" smd circle (at 29 -11.5) (size 6 6) (layers *.Mask)
      (clearance 2))
    (pad "" smd circle (at 29 11.5) (size 6 6) (layers *.Mask)
      (clearance 2))
    (pad "" smd circle (at -29 -11.5) (size 6 6) (layers *.Mask))
    (pad "" np_thru_hole circle (at -29 11.5) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_paste_margin 0.001) (clearance 2))
    (pad "" np_thru_hole circle (at 29 -11.5) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_paste_margin 0.001) (clearance 2))
    (pad "" np_thru_hole circle (at -29 -11.5) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_paste_margin 0.001) (clearance 2))
    (pad "" np_thru_hole circle (at 29 11.5) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_paste_margin 0.001) (clearance 2))
    (pad 1 thru_hole rect (at -24.13 -10.23 180) (size 1.6 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at -24.13 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(F2-Pad1)"))
    (pad 3 thru_hole oval (at -21.59 -10.23 180) (size 1.6 2) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /I2C_SDA))
    (pad 4 thru_hole circle (at -21.59 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at -19.05 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /I2C_SCL))
    (pad 6 thru_hole circle (at -19.05 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole circle (at -16.51 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at -16.51 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at -13.97 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole circle (at -13.97 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole circle (at -11.43 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at -11.43 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at -8.89 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at -8.89 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole circle (at -6.35 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at -6.35 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at -3.81 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at -3.81 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole circle (at -1.27 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SPI0_MOSI))
    (pad 20 thru_hole circle (at -1.27 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 21 thru_hole circle (at 1.27 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SPI0_MISO))
    (pad 22 thru_hole circle (at 1.27 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole circle (at 3.81 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SPI0_SCK))
    (pad 24 thru_hole circle (at 3.81 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /SPI0_CE0))
    (pad 25 thru_hole circle (at 6.35 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 26 thru_hole circle (at 6.35 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 27 thru_hole circle (at 8.89 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 28 thru_hole circle (at 8.89 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 29 thru_hole circle (at 11.43 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 30 thru_hole circle (at 11.43 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 31 thru_hole circle (at 13.97 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 32 thru_hole circle (at 13.97 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 33 thru_hole circle (at 16.51 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 34 thru_hole circle (at 16.51 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 35 thru_hole circle (at 19.05 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 36 thru_hole circle (at 19.05 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 37 thru_hole circle (at 21.59 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 38 thru_hole circle (at 21.59 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 39 thru_hole circle (at 24.13 -10.23 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 40 thru_hole circle (at 24.13 -12.77 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad "" smd circle (at -29 11.5) (size 6 6) (layers *.Mask))
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 94.2 85.6 90)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C9 (at -2.4 0 90) (layer B.SilkS))
    (fp_text value 1u (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0 90) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 3 /V50))
    (pad 2 smd rect (at 0.79756 0 90) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 95.8 85.6 90)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C11 (at -2.2 0 90) (layer B.SilkS))
    (fp_text value 100n (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0 90) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 3 /V50))
    (pad 2 smd rect (at 0.79756 0 90) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 101.4 86 270)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C13 (at -2.4 -1.8 360) (layer B.SilkS))
    (fp_text value 100n (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0 270) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 4 /V18))
    (pad 2 smd rect (at 0.79756 0 270) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 103 86 270)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C14 (at -0.8 -1.6 270) (layer B.SilkS))
    (fp_text value 1u (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0 270) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 4 /V18))
    (pad 2 smd rect (at 0.79756 0 270) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 108.1 82.1 270)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C1 (at 2.375 -0.05 270) (layer B.SilkS))
    (fp_text value 1u (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0 270) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 1 /V33))
    (pad 2 smd rect (at 0.79756 0 270) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 114.4 82.3 90)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C2 (at -2.15 -1.15 180) (layer B.SilkS))
    (fp_text value 100n (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0 90) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 21 /VCC_SPI))
    (pad 2 smd rect (at 0.79756 0 90) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 101.2 95 180)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C6 (at -2.4 0 180) (layer B.SilkS))
    (fp_text value 1u (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0 180) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 1 /V33))
    (pad 2 smd rect (at 0.79756 0 180) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 101.2 93.4 180)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C7 (at -2.4 0.2 180) (layer B.SilkS))
    (fp_text value 100n (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0 180) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 1 /V33))
    (pad 2 smd rect (at 0.79756 0 180) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 115.2 85.7)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C8 (at 0 1.475) (layer B.SilkS))
    (fp_text value 1u (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 21 /VCC_SPI))
    (pad 2 smd rect (at 0.79756 0) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 98 93.4)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C10 (at -3.2 -2.6 90) (layer B.SilkS))
    (fp_text value 100n (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 22 /VCC_I2C))
    (pad 2 smd rect (at 0.79756 0) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 98 95)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C12 (at 0 1.5) (layer B.SilkS))
    (fp_text value 1u (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 22 /VCC_I2C))
    (pad 2 smd rect (at 0.79756 0) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_diodes:DO-214-AC_SMA (layer B.Cu) (tedit 58D26461)
    (at 98.5 81.5 180)
    (descr "DO-214AC (SMA)  PACKAGE.")
    (tags DO-214AC_SMA)
    (attr smd)
    (fp_text reference D1 (at -3.7 -0.7 180) (layer B.SilkS))
    (fp_text value SS14 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.89992 0 180) (size 1.6002 2.19964) (layers B.Cu B.Paste B.Mask)
      (net 4 /V18))
    (pad 2 smd rect (at 1.89992 0 180) (size 1.6002 2.19964) (layers B.Cu B.Paste B.Mask)
      (net 3 /V50))
    (model SMD_Packages.3dshapes/DO-214-AC_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.95 0.95 0.95))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_Fuses:Fuse_SMD1206_Reflow (layer B.Cu) (tedit 58D26457)
    (at 91 81.7 90)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann, Reflow,")
    (tags "Fuse, Sicherung, SMD1206,  Littlefuse-Wickmann, Reflow,")
    (attr smd)
    (fp_text reference F1 (at -1.4 -2 90) (layer B.SilkS))
    (fp_text value 50mA (at -0.25 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.20396 0) (size 2.02946 1.14046) (layers B.Cu B.Paste B.Mask)
      (net 1 /V33))
    (pad 2 smd rect (at 1.20396 0) (size 2.02946 1.14046) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(F1-Pad2)"))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/fuses/Polyfuse_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_Fuses:Fuse_SMD1206_Reflow (layer B.Cu) (tedit 58D2644D)
    (at 93.8 81.7 270)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann, Reflow,")
    (tags "Fuse, Sicherung, SMD1206,  Littlefuse-Wickmann, Reflow,")
    (attr smd)
    (fp_text reference F2 (at 2.9 1.4 270) (layer B.SilkS))
    (fp_text value 100mA (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.20396 0 180) (size 2.02946 1.14046) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(F2-Pad1)"))
    (pad 2 smd rect (at 1.20396 0 180) (size 2.02946 1.14046) (layers B.Cu B.Paste B.Mask)
      (net 3 /V50))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/fuses/Polyfuse_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_SOT:SOT-23 (layer B.Cu) (tedit 55F66754)
    (at 98.5 86 270)
    (fp_text reference IC8 (at 1.8 1.3 450) (layer B.SilkS))
    (fp_text value MCP1700T-1802E/TT (at -2.5 -3 360) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 270) (size 1.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.1 -0.95 270) (size 1.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 /V18))
    (pad 3 smd rect (at 1.1 0 270) (size 1.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 /V50))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/smd_transistor/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module IPC7351-Nominal:SOP65P490X110-8AN (layer B.Cu) (tedit 58C322E3)
    (at 100 90.6)
    (descr "SOP,0.65mm pitch;8 pin,3.00mm W X 3.10mm L X 1.10mm H Body")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference IC6 (at 1 -2.3) (layer B.SilkS))
    (fp_text value PCA9617A (at -0.8 0) (layer B.Fab))
    (pad 1 smd rect (at -2.14884 0.97282) (size 1.39954 0.44958) (layers B.Cu B.Paste B.Mask)
      (net 22 /VCC_I2C))
    (pad 2 smd rect (at -2.14884 0.32258) (size 1.39954 0.44958) (layers B.Cu B.Paste B.Mask)
      (net 17 /SCL_EXT))
    (pad 3 smd rect (at -2.14884 -0.32258) (size 1.39954 0.44958) (layers B.Cu B.Paste B.Mask)
      (net 18 /SDA_EXT))
    (pad 4 smd rect (at -2.14884 -0.97282) (size 1.39954 0.44958) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.14884 -0.97282) (size 1.39954 0.44958) (layers B.Cu B.Paste B.Mask)
      (net 1 /V33))
    (pad 6 smd rect (at 2.14884 -0.32258) (size 1.39954 0.44958) (layers B.Cu B.Paste B.Mask)
      (net 7 /I2C_SDA))
    (pad 7 smd rect (at 2.14884 0.32258) (size 1.39954 0.44958) (layers B.Cu B.Paste B.Mask)
      (net 8 /I2C_SCL))
    (pad 8 smd rect (at 2.14884 0.97282) (size 1.39954 0.44958) (layers B.Cu B.Paste B.Mask)
      (net 1 /V33))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/smd_ics/msoic-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module H_PDIP:DIP-8 (layer F.Cu) (tedit 54CEED28)
    (at 131.5 88 90)
    (fp_text reference IC7 (at 0.2 -4.1 90) (layer F.SilkS))
    (fp_text value 25LC_EEPROM (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.81 -3.81 90) (size 1.778 1.3) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SPI0_CE0_EXT))
    (pad 2 thru_hole oval (at -3.81 -1.27 90) (size 1.778 1.3) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 15 /SPI0_MISO_EXT))
    (pad 3 thru_hole oval (at -3.81 1.27 90) (size 1.778 1.3) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 /VCC_SPI))
    (pad 4 thru_hole oval (at -3.81 3.81 90) (size 1.778 1.3) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 3.81 3.81 90) (size 1.778 1.3) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SPI0_MOSI_EXT))
    (pad 6 thru_hole oval (at 3.81 1.27 90) (size 1.778 1.3) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SPI0_SCK_EXT))
    (pad 7 thru_hole oval (at 3.81 -1.27 90) (size 1.778 1.3) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 /VCC_SPI))
    (pad 8 thru_hole oval (at 3.81 -3.81 90) (size 1.778 1.3) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 /VCC_SPI))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/pth_circuits/dil_8-300_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module H_switches:SLB1470_1P4T_slideSW (layer F.Cu) (tedit 58C30BA8)
    (at 128 99.5 180)
    (fp_text reference SW1 (at -8.6 1.5 180) (layer F.SilkS))
    (fp_text value 1P4T_generic_switch (at 0 -3.5 180) (layer F.Fab))
    (fp_text user C (at -5.75 -1.75 180) (layer F.SilkS))
    (fp_text user C (at 5.75 -1.75 180) (layer F.SilkS))
    (fp_text user 1 (at -3.5 -1.75 180) (layer F.SilkS))
    (fp_text user 2 (at -1.15 -1.75 180) (layer F.SilkS))
    (fp_text user 3 (at 1.15 -1.75 180) (layer F.SilkS))
    (fp_text user 4 (at 3.45 -1.75 180) (layer F.SilkS))
    (pad 4 thru_hole oval (at 1.15 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /V50))
    (pad 3 thru_hole oval (at -1.15 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 /V33))
    (pad 5 thru_hole oval (at 3.45 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 /VEXT_SPI))
    (pad 1 thru_hole oval (at 5.75 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 /VCC_SPI))
    (pad 1 thru_hole oval (at -5.75 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 /VCC_SPI))
    (pad 2 thru_hole oval (at -3.45 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /V18))
  )
  (module H_switches:SLB1470_1P4T_slideSW (layer F.Cu) (tedit 58C30BA8)
    (at 105.5 99.5 180)
    (fp_text reference SW2 (at -8.5 1.5 180) (layer F.SilkS))
    (fp_text value 1P4T_generic_switch (at 0 -3.5 180) (layer F.Fab))
    (fp_text user C (at -5.75 -1.75 180) (layer F.SilkS))
    (fp_text user C (at 5.75 -1.75 180) (layer F.SilkS))
    (fp_text user 1 (at -3.5 -1.75 180) (layer F.SilkS))
    (fp_text user 2 (at -1.15 -1.75 180) (layer F.SilkS))
    (fp_text user 3 (at 1.15 -1.75 180) (layer F.SilkS))
    (fp_text user 4 (at 3.45 -1.75 180) (layer F.SilkS))
    (pad 4 thru_hole oval (at 1.15 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /V50))
    (pad 3 thru_hole oval (at -1.15 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 /V33))
    (pad 5 thru_hole oval (at 3.45 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 /VEXT_I2C))
    (pad 1 thru_hole oval (at 5.75 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 /VCC_I2C))
    (pad 1 thru_hole oval (at -5.75 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 /VCC_I2C))
    (pad 2 thru_hole oval (at -3.45 0 180) (size 1.524 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /V18))
  )
  (module H_smd_passives:RESC_0603_1508X63N (layer B.Cu) (tedit 55F3D9B5)
    (at 105.1 92.35 270)
    (descr "Resistor,Chip;1.52mm L X 0.85mm W X 0.63mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference R1 (at -0.1 -1.45 270) (layer B.SilkS))
    (fp_text value 1k5 (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.6477 0 270) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 1 /V33))
    (pad 2 smd rect (at 0.6477 0 270) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 8 /I2C_SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:RESC_0603_1508X63N (layer B.Cu) (tedit 55F3D9B5)
    (at 105.1 89.75 90)
    (descr "Resistor,Chip;1.52mm L X 0.85mm W X 0.63mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference R2 (at 0 1.35 90) (layer B.SilkS))
    (fp_text value 1k5 (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.6477 0 90) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 1 /V33))
    (pad 2 smd rect (at 0.6477 0 90) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 7 /I2C_SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:RESC_0603_1508X63N (layer B.Cu) (tedit 55F3D9B5)
    (at 94.8 94 270)
    (descr "Resistor,Chip;1.52mm L X 0.85mm W X 0.63mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference R7 (at 2.2 0 270) (layer B.SilkS))
    (fp_text value 1k5 (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.6477 0 270) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 18 /SDA_EXT))
    (pad 2 smd rect (at 0.6477 0 270) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 22 /VCC_I2C))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:RESC_0603_1508X63N (layer B.Cu) (tedit 55F3D9B5)
    (at 92.8 94 270)
    (descr "Resistor,Chip;1.52mm L X 0.85mm W X 0.63mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference R8 (at 2.2 0 270) (layer B.SilkS))
    (fp_text value 1k5 (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.6477 0 270) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 17 /SCL_EXT))
    (pad 2 smd rect (at 0.6477 0 270) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 22 /VCC_I2C))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module conn-100mil:CONN-100MIL-F-1x6 (layer F.Cu) (tedit 58D55DB5)
    (at 86.575 88.275 90)
    (fp_text reference P2 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -6.35 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 /VEXT_I2C))
    (pad 2 thru_hole oval (at -3.81 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at -1.27 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 22 /VCC_I2C))
    (pad 4 thru_hole oval (at 1.27 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 3.81 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 /SCL_EXT))
    (pad 6 thru_hole oval (at 6.35 0 90) (size 1.524 2.286) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 18 /SDA_EXT))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 120.1 84.8)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C3 (at 0 1.27) (layer B.SilkS))
    (fp_text value 100n (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 21 /VCC_SPI))
    (pad 2 smd rect (at 0.79756 0) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 107.3 79.8 180)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C4 (at 0.9 -1.4 180) (layer B.SilkS))
    (fp_text value 100n (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0 180) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 1 /V33))
    (pad 2 smd rect (at 0.79756 0 180) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:CAPC_0603_1608X86N (layer B.Cu) (tedit 56B9939B)
    (at 124 84.8)
    (descr "Capacitor,non-polarized,Chip;1.60mm L X 0.81mm W X 0.86mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference C5 (at 0 1.27) (layer B.SilkS))
    (fp_text value 100n (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.79756 0) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 21 /VCC_SPI))
    (pad 2 smd rect (at 0.79756 0) (size 0.94996 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_SOT:SOT23-5 (layer B.Cu) (tedit 58DC1B55)
    (at 111.4 81.8)
    (fp_text reference IC2 (at -2.05 -1.225 90) (layer B.SilkS))
    (fp_text value SN74LV1T125_SOT23_5 (at 0 -2.8) (layer B.Fab))
    (pad 2 smd rect (at 0 1.2) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(IC2-Pad2)"))
    (pad 1 smd rect (at 0.95 1.2) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.95 1.2) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.95 -1.2) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 /SPI0_MISO))
    (pad 5 smd rect (at 0.95 -1.2) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 /V33))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/sot23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module H_SOT:SOT23-5 (layer B.Cu) (tedit 58DA2510)
    (at 116.8 81.8 180)
    (fp_text reference IC3 (at 2.475 1.7 180) (layer B.SilkS))
    (fp_text value SN74LV1T125_SOT23_5 (at 0 -2.8 180) (layer B.Fab))
    (pad 2 smd rect (at 0 1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 /SPI0_MOSI))
    (pad 1 smd rect (at 0.95 1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.95 1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.95 -1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(IC3-Pad4)"))
    (pad 5 smd rect (at 0.95 -1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /VCC_SPI))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/sot23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module H_SOT:SOT23-5 (layer B.Cu) (tedit 58DA2510)
    (at 123.8 81.8 180)
    (fp_text reference IC5 (at -2.45 1.775 180) (layer B.SilkS))
    (fp_text value SN74LV1T125_SOT23_5 (at 0 -2.8 180) (layer B.Fab))
    (pad 2 smd rect (at 0 1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 /SPI0_CE0))
    (pad 1 smd rect (at 0.95 1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.95 1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.95 -1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(IC5-Pad4)"))
    (pad 5 smd rect (at 0.95 -1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /VCC_SPI))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/sot23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module H_SOT:SOT23-5 (layer B.Cu) (tedit 58DA2510)
    (at 120.4 81.8 180)
    (fp_text reference IC4 (at -1.175 2.575 180) (layer B.SilkS))
    (fp_text value SN74LV1T125_SOT23_5 (at 0 -2.8 180) (layer B.Fab))
    (pad 2 smd rect (at 0 1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 /SPI0_SCK))
    (pad 1 smd rect (at 0.95 1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.95 1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.95 -1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(IC4-Pad4)"))
    (pad 5 smd rect (at 0.95 -1.2 180) (size 0.65 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /VCC_SPI))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/sot23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module H_smd_passives:RESC_0603_1508X63N (layer B.Cu) (tedit 55F3D9B5)
    (at 117.7 85.4 90)
    (descr "Resistor,Chip;1.52mm L X 0.85mm W X 0.63mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference R3 (at -2.05 0.1 90) (layer B.SilkS))
    (fp_text value 33R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.6477 0 90) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 16 /SPI0_MOSI_EXT))
    (pad 2 smd rect (at 0.6477 0 90) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(IC3-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:RESC_0603_1508X63N (layer B.Cu) (tedit 55F3D9B5)
    (at 111.4 85.4 90)
    (descr "Resistor,Chip;1.52mm L X 0.85mm W X 0.63mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference R4 (at 0.025 -1.2 90) (layer B.SilkS))
    (fp_text value 33R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.6477 0 90) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 15 /SPI0_MISO_EXT))
    (pad 2 smd rect (at 0.6477 0 90) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(IC2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:RESC_0603_1508X63N (layer B.Cu) (tedit 55F3D9B5)
    (at 121.9 86.9 90)
    (descr "Resistor,Chip;1.52mm L X 0.85mm W X 0.63mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference R5 (at -2.1 0.075 90) (layer B.SilkS))
    (fp_text value 33R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.6477 0 90) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 14 /SPI0_SCK_EXT))
    (pad 2 smd rect (at 0.6477 0 90) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(IC4-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_smd_passives:RESC_0603_1508X63N (layer B.Cu) (tedit 55F3D9B5)
    (at 126.8 81.5 180)
    (descr "Resistor,Chip;1.52mm L X 0.85mm W X 0.63mm H")
    (tags "CMS XXX")
    (attr smd)
    (fp_text reference R6 (at -2.225 -0.05 180) (layer B.SilkS))
    (fp_text value 33R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.6477 0 180) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 13 /SPI0_CE0_EXT))
    (pad 2 smd rect (at 0.6477 0 180) (size 0.79756 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(IC5-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_vias:Via0703_GND (layer F.Cu) (tedit 58DC1AEA)
    (at 127.325 87.2)
    (fp_text reference Via0703_GND (at 0.00508 -0.42164) (layer F.Fab) hide)
    (fp_text value VAL** (at 0.03556 0.44196) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (gr_text "REV. 2.0" (at 140.975 94.925) (layer B.SilkS))
  (gr_text GND (at 140.31 79.15 90) (layer F.SilkS))
  (gr_text GP21 (at 141.56 79.1 90) (layer F.SilkS))
  (gr_text GP26 (at 137.77 79.15 90) (layer F.SilkS))
  (gr_text GP20 (at 139.02 79.1 90) (layer F.SilkS))
  (gr_text GP19 (at 135.23 79.15 90) (layer F.SilkS))
  (gr_text GP16 (at 136.48 79.1 90) (layer F.SilkS))
  (gr_text GP13 (at 132.69 79.15 90) (layer F.SilkS))
  (gr_text GND (at 133.94 79.1 90) (layer F.SilkS))
  (gr_text GP6 (at 130.15 79.15 90) (layer F.SilkS))
  (gr_text GP12 (at 131.4 79.1 90) (layer F.SilkS))
  (gr_text GP5 (at 127.61 79.15 90) (layer F.SilkS))
  (gr_text GND (at 128.86 79.1 90) (layer F.SilkS))
  (gr_text EED (at 125.07 79.15 90) (layer F.SilkS))
  (gr_text EEC (at 126.32 79.1 90) (layer F.SilkS))
  (gr_text GND (at 122.53 79.15 90) (layer F.SilkS))
  (gr_text CE1 (at 123.78 79.1 90) (layer F.SilkS))
  (gr_text SCLK (at 119.99 79.15 90) (layer F.SilkS))
  (gr_text CE0 (at 121.24 79.1 90) (layer F.SilkS))
  (gr_text MISO (at 117.45 79.15 90) (layer F.SilkS))
  (gr_text GP25 (at 118.7 79.1 90) (layer F.SilkS))
  (gr_text MOSI (at 114.91 79.15 90) (layer F.SilkS))
  (gr_text GND (at 116.16 79.1 90) (layer F.SilkS))
  (gr_text 3V3 (at 112.37 79.15 90) (layer F.SilkS))
  (gr_text GP24 (at 113.62 79.1 90) (layer F.SilkS))
  (gr_text GP22 (at 109.83 79.15 90) (layer F.SilkS))
  (gr_text GP23 (at 111.08 79.1 90) (layer F.SilkS))
  (gr_text GP27 (at 107.29 79.15 90) (layer F.SilkS))
  (gr_text GND (at 108.54 79.1 90) (layer F.SilkS))
  (gr_text GP17 (at 104.75 79.15 90) (layer F.SilkS))
  (gr_text GP18 (at 106 79.1 90) (layer F.SilkS))
  (gr_text GND (at 102.21 79.15 90) (layer F.SilkS))
  (gr_text RX0 (at 103.46 79.1 90) (layer F.SilkS))
  (gr_text GP4 (at 99.67 79.15 90) (layer F.SilkS))
  (gr_text TX0 (at 100.92 79.1 90) (layer F.SilkS))
  (gr_text SCL1 (at 97.13 79.15 90) (layer F.SilkS))
  (gr_text GND (at 98.38 79.1 90) (layer F.SilkS))
  (gr_text SDA1 (at 94.59 79.15 90) (layer F.SilkS))
  (gr_text 5V0 (at 95.84 79.1 90) (layer F.SilkS))
  (gr_text 5V0 (at 93.3 79.1 90) (layer F.SilkS))
  (gr_text 3V3 (at 92.05 79.15 90) (layer F.SilkS))
  (gr_text "(NC)" (at 90.17 92.075) (layer F.SilkS))
  (gr_text VDD (at 90.17 89.535) (layer F.SilkS))
  (gr_text 5.5V (at 93.481 100.05) (layer F.SilkS))
  (gr_text ... (at 93.081 98.55 90) (layer F.SilkS))
  (gr_text 0.8V (at 93.431 97.25) (layer F.SilkS))
  (gr_text ... (at 140 98.3 90) (layer F.SilkS))
  (gr_text 5.5V (at 140.4 99.8) (layer F.SilkS))
  (gr_text 1.65V (at 140.35 97) (layer F.SilkS))
  (gr_text "design by:\nPiotr Zapart (c) 2017\n" (at 141 87.8) (layer B.SilkS))
  (gr_text "RasberryPi Zero\nSPI&I2C programmer" (at 123.75 88.75) (layer F.SilkS))
  (gr_text FLASH-Pi (at 113.2 84.05) (layer F.SilkS))
  (gr_text "25XX \nSPI FLASH/EEPROM" (at 139 88 90) (layer F.SilkS))
  (gr_text I2C (at 113 93.5) (layer F.SilkS))
  (gr_text SPI0 (at 121.5 93.5) (layer F.SilkS))
  (gr_text VDD (at 127.7 82.4) (layer F.SilkS))
  (gr_text ~HLD (at 130.25 82.45) (layer F.SilkS))
  (gr_text SCK (at 132.8 82.4) (layer F.SilkS))
  (gr_text MOSI (at 135.5 82.4) (layer F.SilkS))
  (gr_text ~CS (at 127.75 94) (layer F.SilkS))
  (gr_text MISO (at 130.25 93.95) (layer F.SilkS))
  (gr_text ~WP (at 132.85 94) (layer F.SilkS))
  (gr_text 1V8 (at 109 96.2) (layer F.SilkS))
  (gr_text 3V3 (at 106.6 96.2) (layer F.SilkS))
  (gr_text 5V (at 104.4 96.2) (layer F.SilkS))
  (gr_text EXT (at 102 96.2) (layer F.SilkS))
  (gr_text 1V8 (at 131.5 96.2) (layer F.SilkS))
  (gr_text 3V3 (at 129.1 96.2) (layer F.SilkS))
  (gr_text 5V (at 126.9 96.2) (layer F.SilkS))
  (gr_text EXT (at 124.5 96.2) (layer F.SilkS))
  (gr_text GND (at 135.3 93.95) (layer F.SilkS))
  (gr_text "VDD\nEXT" (at 142 94.4) (layer F.SilkS))
  (gr_text GND (at 142 91.8) (layer F.SilkS))
  (gr_text SCK (at 142 89.2) (layer F.SilkS))
  (gr_text MISO (at 142 86.8) (layer F.SilkS))
  (gr_text MOSI (at 142 84.2) (layer F.SilkS))
  (gr_text CE0 (at 142.4 82) (layer F.SilkS))
  (gr_text "VDD\nEXT" (at 90.424 95.123) (layer F.SilkS))
  (gr_text GND (at 90.2 87.122) (layer F.SilkS))
  (gr_text SCL (at 90.2 84.455) (layer F.SilkS))
  (gr_text SDA (at 90.17 81.915) (layer F.SilkS))
  (gr_arc (start 146 76) (end 146 73) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146 100) (end 149 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 87 100) (end 87 103) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 87 76) (end 84 76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84 100) (end 84 76) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146 103) (end 87 103) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149 76) (end 149 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87 73) (end 146 73) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.35) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 149 73) (xy 84 73) (xy 84 103) (xy 149 103)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.35) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 149 73) (xy 84 73) (xy 84 103) (xy 149 103)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.8 81.25) (xy 89.8 82.1) (xy 95 82.1) (xy 95 81.25)
      )
    )
  )
)
