<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="45.72" y2="0" width="0" layer="20"/>
<wire x1="45.72" y1="0" x2="45.72" y2="35.56" width="0" layer="20"/>
<wire x1="45.72" y1="35.56" x2="0" y2="35.56" width="0" layer="20"/>
<wire x1="0" y1="35.56" x2="0" y2="0" width="0" layer="20"/>
<hole x="40.64" y="17.78" drill="3.2"/>
<hole x="5.08" y="17.78" drill="3.2"/>
<text>- PWR +</text>
<text>GPI</text>
<text>START</text>
<text>STOP</text>
</plain>
<libraries>
<library name="discrete">
<packages>
<package name="CPR02">
</package>
<package name="CPR01">
</package>
<package name="R02">
</package>
</packages>
</library>
<library name="myconn">
<packages>
<package name="TBLK02">
</package>
</packages>
</library>
<library name="diodes">
<packages>
<package name="LED">
</package>
</packages>
</library>
<library name="mypic">
<packages>
<package name="08DIP300">
</package>
</packages>
</library>
<library name="mylinear">
<packages>
<package name="TO92">
</package>
</packages>
</library>
<library name="npn">
<packages>
<package name="TO-92B">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="discrete" package="CPR02" value="470μF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="discrete" package="CPR01" value="10μF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="CON1" library="myconn" package="TBLK02" value="TBLK02">
<attribute name="NAME"/>
</element>
<element name="CON2" library="myconn" package="TBLK02" value="TBLK02">
<attribute name="NAME"/>
</element>
<element name="CON3" library="myconn" package="TBLK02" value="TBLK02">
<attribute name="NAME"/>
</element>
<element name="CON4" library="myconn" package="TBLK02" value="TBLK02">
<attribute name="NAME"/>
</element>
<element name="D1" library="diodes" package="LED" value="">
<attribute name="NAME"/>
</element>
<element name="D2" library="diodes" package="LED" value="">
<attribute name="NAME"/>
</element>
<element name="IC1" library="mypic" package="08DIP300" value="PIC12F1572">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="mylinear" package="TO92" value="79L05">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="npn" package="TO-92B" value="2N3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="npn" package="TO-92B" value="2N3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="discrete" package="R02" value="100Ω">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="discrete" package="R02" value="33K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="discrete" package="R02" value="4.7K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="discrete" package="R02" value="4.7K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="discrete" package="R02" value="330Ω">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="discrete" package="R02" value="4.7K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R7" library="discrete" package="R02" value="4.7K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="discrete" package="R02" value="330Ω">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R9" library="discrete" package="R02" value="33K"/>
</elements>
<signals>
<signal name="GND">
<contactref element="CON4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="Q2" pad="3"/>
<contactref element="CON3" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="CON2" pad="2"/>
<contactref element="CON1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="CON4" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="IC2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="1"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="Q2" pad="1"/>
<contactref element="CON3" pad="1"/>
<contactref element="D2" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="1"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="1"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R4" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="D1" pad="2"/>
<contactref element="CON2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R5" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="CON1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
