(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "Beetje 32U4 Blok")
    (date "2018-08-10")
    (rev "0.0")
    (company "www.MakersBox.us")
    (comment 1 "648.ken@gmail.com")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "/10")
  (net 2 "/01")
  (net 3 "/02")
  (net 4 "/04")
  (net 5 "/05")
  (net 6 "/06")
  (net 7 "/07")
  (net 8 "/08")
  (net 9 "/09")
  (net 10 "/11")
  (net 11 "/12")
  (net 12 "/13")
  (net 13 "/14")
  (net 14 "/15")
  (net 15 "/16")
  (net 16 "/17")
  (net 17 "/18")
  (net 18 "/19")
  (net 19 "/20")
  (net 20 "/03")
  (net 21 "/D2_SDA")
  (net 22 "GND")
  (net 23 "/D3_SCL")
  (net 24 "+5V")
  (net 25 "/A")
  (net 26 "Net-(R1-Pad1)")
  (net 27 "Net-(U1-Pad7)")
  (net 28 "/RESET")
  (footprint "footprints:MEC8-113-CARD_2" locked (layer "F.Cu")
    (tedit 637EA67F)
    (at 0 -0.1 90)
    (attr through_hole)
    (fp_text reference "X0" (at 4.375 -1.25 90) (layer "F.Fab"))
    (fp_text value "Card Edge" (at 10.9 -1 90) (layer "F.Fab"))
    (fp_line (start 17.5 0.5) (end 17.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 18.5 6.5) (end 19 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 8.4 0.5) (end 8.4 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 1 6.5) (end 1.5 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 0 51.5) (end 1 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 10.8 5.5) (end 10.8 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 21 7.5) (end 21 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start -1 47.5) (end -1 7.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start -1 50.5) (end -1 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 2.5 0.5) (end 2.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 19 51.5) (end 20 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 0 6.5) (end 1 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 11.5 51.5) (end 19 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 3 0) (end 7.9 0) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 8.5 51.5) (end 1 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 17 0) (end 11.3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 9.4 6.5) (end 9.8 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 19 6.5) (end 20 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 21 50.5) (end 21 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 18.5 6.5) (mid 17.792893 6.207107) (end 17.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 2.5 5.5) (mid 2.207107 6.207107) (end 1.5 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 7.9 0) (mid 8.253553 0.146447) (end 8.4 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start -1 7.5) (mid -0.707107 6.792893) (end 0 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 17 0) (mid 17.353553 0.146447) (end 17.5 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 20 6.5) (mid 20.707107 6.792893) (end 21 7.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 0 51.5) (mid -0.707107 51.207107) (end -1 50.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 10.8 5.5) (mid 10.507107 6.207107) (end 9.8 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 8.5 51.5) (mid 10 50) (end 11.5 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 9.4 6.5) (mid 8.692893 6.207107) (end 8.4 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 2.5 0.5) (mid 2.646447 0.146447) (end 3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 21 50.5) (mid 20.707107 51.207107) (end 20 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 10.8 0.5) (mid 10.946447 0.146447) (end 11.3 0) (layer "Edge.Cuts") (width 0.12))
    (pad "1" smd rect locked (at 3.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "/01"))
    (pad "2" smd rect locked (at 4.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/02"))
    (pad "3" smd rect locked (at 5.2 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/03"))
    (pad "4" smd rect locked (at 6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "/04"))
    (pad "5" smd rect locked (at 6.8 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "/05"))
    (pad "6" smd rect locked (at 7.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "/06"))
    (pad "7" smd rect locked (at 11.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/07"))
    (pad "8" smd rect locked (at 12.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/08"))
    (pad "9" smd rect locked (at 13.2 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "/09"))
    (pad "10" smd rect locked (at 14 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "/10"))
    (pad "11" smd rect locked (at 14.8 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/RESET"))
    (pad "12" smd rect locked (at 15.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/A"))
    (pad "13" smd rect locked (at 16.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "+5V"))
    (pad "14" smd rect locked (at 3.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/11"))
    (pad "15" smd rect locked (at 4.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/12"))
    (pad "16" smd rect locked (at 5.2 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/13"))
    (pad "17" smd rect locked (at 6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/14"))
    (pad "18" smd rect locked (at 6.8 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/15"))
    (pad "19" smd rect locked (at 7.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/16"))
    (pad "20" smd rect locked (at 11.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/17"))
    (pad "21" smd rect locked (at 12.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/18"))
    (pad "22" smd rect locked (at 13.2 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/19"))
    (pad "23" smd rect locked (at 14 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/20"))
    (pad "24" smd rect locked (at 14.8 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/D3_SCL"))
    (pad "25" smd rect locked (at 15.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/D2_SDA"))
    (pad "26" smd rect locked (at 16.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GND"))
  )
  (footprint "footprints:DFN-8-1EP_3x2mm" (layer "F.Cu")
    (tedit 638826C0)
    (at 45 -18.5 180)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.55 180) (layer "F.SilkS") hide)
    (fp_text value "24LC32" (at 0.075 1.725 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "" smd rect locked (at -0.325 0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at -0.325 -0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at 0.325 -0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at 0.325 0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "1" smd rect locked (at -1.45 -0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(R1-Pad1)"))
    (pad "2" smd rect locked (at -1.45 -0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GND"))
    (pad "3" smd rect locked (at -1.45 0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GND"))
    (pad "4" smd rect locked (at -1.45 0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GND"))
    (pad "5" smd rect locked (at 1.45 0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/D2_SDA"))
    (pad "6" smd rect locked (at 1.45 0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/D3_SCL"))
    (pad "7" smd rect locked (at 1.45 -0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(U1-Pad7)"))
    (pad "8" smd rect locked (at 1.45 -0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "+5V"))
    (pad "9" smd rect locked (at 0 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Mask"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 48 -18.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "R1" (at 1.905 0 270) (layer "Dwgs.User"))
    (fp_text value "10K" (at 1.75 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(R1-Pad1)"))
    (pad "2" smd rect locked (at 0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/A"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoints_1x10_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 6381A7A4)
    (at 13.95 -5.9)
    (descr "Molex PicoBlade Connector System, 53047-1010, 10 Pins per row (http://www.molex.com/pdm_docs/sd/530470610_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade side entry")
    (attr through_hole)
    (fp_text reference "J3" (at 5.62 -1.5) (layer "F.SilkS") hide)
    (fp_text value "TestPoints" (at 5.62 1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.62 -1.35) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 "/10"))
    (pad "2" thru_hole circle locked (at 1.25 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 9 "/09"))
    (pad "3" thru_hole circle locked (at 2.5 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 8 "/08"))
    (pad "4" thru_hole circle locked (at 3.75 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 7 "/07"))
    (pad "5" thru_hole circle locked (at 5 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 6 "/06"))
    (pad "6" thru_hole circle locked (at 6.25 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 5 "/05"))
    (pad "7" thru_hole circle locked (at 7.5 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 "/04"))
    (pad "8" thru_hole circle locked (at 8.75 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 20 "/03"))
    (pad "9" thru_hole circle locked (at 10 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 "/02"))
    (pad "10" thru_hole circle locked (at 11.25 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 "/01"))
    (model "${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53047-1010_1x10_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoints_1x10_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 6381A7A4)
    (at 13.95 -13.6)
    (descr "Molex PicoBlade Connector System, 53047-1010, 10 Pins per row (http://www.molex.com/pdm_docs/sd/530470610_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade side entry")
    (attr through_hole)
    (fp_text reference "J2" (at 5.62 -1.5) (layer "F.SilkS") hide)
    (fp_text value "TestPoints" (at 5.62 1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.62 -1.35) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 10 "/11"))
    (pad "2" thru_hole circle locked (at 1.25 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 11 "/12"))
    (pad "3" thru_hole circle locked (at 2.5 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 12 "/13"))
    (pad "4" thru_hole circle locked (at 3.75 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 13 "/14"))
    (pad "5" thru_hole circle locked (at 5 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 "/15"))
    (pad "6" thru_hole circle locked (at 6.25 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 15 "/16"))
    (pad "7" thru_hole circle locked (at 7.5 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 16 "/17"))
    (pad "8" thru_hole circle locked (at 8.75 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 17 "/18"))
    (pad "9" thru_hole circle locked (at 10 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 18 "/19"))
    (pad "10" thru_hole circle locked (at 11.25 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 19 "/20"))
    (model "${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53047-1010_1x10_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SAMTEC_TFM-108-02-L-D-WT" (layer "F.Cu")
    (tedit 64591D31)
    (at 39.25 -9.75)
    (attr smd)
    (fp_text reference "J4" (at -7.05 -1.95) (layer "F.SilkS"))
    (fp_text value "16P" (at 6.05 6.35) (layer "F.SilkS"))
    (pad "01" smd rect locked (at -4.445 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/10"))
    (pad "02" smd rect locked (at -4.445 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/11"))
    (pad "03" smd rect locked (at -3.175 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/09"))
    (pad "04" smd rect locked (at -3.175 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/12"))
    (pad "05" smd rect locked (at -1.905 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/08"))
    (pad "06" smd rect locked (at -1.905 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/13"))
    (pad "07" smd rect locked (at -0.635 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/07"))
    (pad "08" smd rect locked (at -0.635 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/14"))
    (pad "09" smd rect locked (at 0.635 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/06"))
    (pad "10" smd rect locked (at 0.635 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/15"))
    (pad "11" smd rect locked (at 1.905 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/05"))
    (pad "12" smd rect locked (at 1.905 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/16"))
    (pad "13" smd rect locked (at 3.175 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/04"))
    (pad "14" smd rect locked (at 3.175 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/17"))
    (pad "15" smd rect locked (at 4.445 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/03"))
    (pad "16" smd rect locked (at 4.445 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/18"))
    (pad "S1" thru_hole circle locked (at 7.035 0) (size 1.19 1.19) (drill 0.84) (layers *.Cu *.Mask))
    (pad "S2" thru_hole circle locked (at -7.035 0) (size 1.19 1.19) (drill 0.84) (layers *.Cu *.Mask))
  )
  (footprint "SAMTEC_TFM-110-02-L-D-WT" (layer "F.Cu")
    (tedit 64591BE8)
    (at 19.5 -9.75)
    (attr smd)
    (fp_text reference "J1" (at -8.25 -1.950001) (layer "F.SilkS"))
    (fp_text value "20P" (at 7.4 6.55) (layer "F.SilkS"))
    (pad "01" smd rect locked (at -5.715 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/10"))
    (pad "02" smd rect locked (at -5.715 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/11"))
    (pad "03" smd rect locked (at -4.445 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/09"))
    (pad "04" smd rect locked (at -4.445 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/12"))
    (pad "05" smd rect locked (at -3.175 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/08"))
    (pad "06" smd rect locked (at -3.175 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/13"))
    (pad "07" smd rect locked (at -1.905 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/07"))
    (pad "08" smd rect locked (at -1.905 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/14"))
    (pad "09" smd rect locked (at -0.635 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/06"))
    (pad "10" smd rect locked (at -0.635 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/15"))
    (pad "11" smd rect locked (at 0.635 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/05"))
    (pad "12" smd rect locked (at 0.635 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/16"))
    (pad "13" smd rect locked (at 1.905 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/04"))
    (pad "14" smd rect locked (at 1.905 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/17"))
    (pad "15" smd rect locked (at 3.175 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/03"))
    (pad "16" smd rect locked (at 3.175 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/18"))
    (pad "17" smd rect locked (at 4.445 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/02"))
    (pad "18" smd rect locked (at 4.445 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/19"))
    (pad "19" smd rect locked (at 5.715 1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/01"))
    (pad "20" smd rect locked (at 5.715 -1.715) (size 0.74 2.92) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/20"))
    (pad "S1" thru_hole circle locked (at 8.305 0) (size 1.19 1.19) (drill 0.84) (layers *.Cu *.Mask))
    (pad "S2" thru_hole circle locked (at -8.305 0) (size 1.19 1.19) (drill 0.84) (layers *.Cu *.Mask))
  )
  (footprint "footprints:test_pads_125mm_x08" (layer "F.Cu")
    (tedit 6384298A)
    (at 34.95 -5.8)
    (descr "Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X")
    (tags "connector harwin gecko")
    (attr through_hole)
    (fp_text reference "J5" (at 1 1.5) (layer "F.SilkS") hide)
    (fp_text value "TestPoints" (at 5.5 -1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 "/10"))
    (pad "2" thru_hole circle locked (at 1.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 9 "/09"))
    (pad "3" thru_hole circle locked (at 2.5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 8 "/08"))
    (pad "4" thru_hole circle locked (at 3.75 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 7 "/07"))
    (pad "5" thru_hole circle locked (at 5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 6 "/06"))
    (pad "6" thru_hole circle locked (at 6.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 5 "/05"))
    (pad "7" thru_hole circle locked (at 7.5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 "/04"))
    (pad "8" thru_hole circle locked (at 8.75 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 20 "/03"))
    (model "${KISYS3DMOD}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:test_pads_125mm_x08" (layer "F.Cu")
    (tedit 6384298A)
    (at 34.95 -13.7)
    (descr "Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X")
    (tags "connector harwin gecko")
    (attr through_hole)
    (fp_text reference "J6" (at 1 1.5) (layer "F.SilkS") hide)
    (fp_text value "TestPoints" (at 5.5 -1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 10 "/11"))
    (pad "2" thru_hole circle locked (at 1.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 11 "/12"))
    (pad "3" thru_hole circle locked (at 2.5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 12 "/13"))
    (pad "4" thru_hole circle locked (at 3.75 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 13 "/14"))
    (pad "5" thru_hole circle locked (at 5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 "/15"))
    (pad "6" thru_hole circle locked (at 6.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 15 "/16"))
    (pad "7" thru_hole circle locked (at 7.5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 16 "/17"))
    (pad "8" thru_hole circle locked (at 8.75 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 17 "/18"))
    (model "${KISYS3DMOD}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Rev 0.0\nMay 2024" (at 49.75 -1.25) (layer "B.SilkS"))
  (gr_text "TFM-108-02-L-D-WT" (at 39.3 -7.9) (layer "B.SilkS"))
  (gr_text "ken.olsen@agilityrobotics.com" (at 29 -1) (layer "B.SilkS"))
  (gr_text "Rapid Prototyping Card" (at 29 -3) (layer "B.SilkS"))
  (gr_text "TFM-110-02-L-D-WT" (at 19.2 -8) (layer "B.SilkS"))
  (gr_text "2 4 6 8 10 12 14 16" (at 39.3 -14.9) (layer "F.SilkS"))
  (gr_text "1 3 5 7 9 11 13 15" (at 39.5 -4.7) (layer "F.SilkS"))
  (gr_text "Samtec TigerEYE" (at 29.3 -1.1) (layer "F.SilkS"))
  (gr_text "1 3 5 7 9 11 13 15 17 19" (at 19.6 -4.9) (layer "F.SilkS"))
  (gr_text "2 4 6 8 10 12 14 16 18 20" (at 19.6 -14.7) (layer "F.SilkS"))
  (dimension (type aligned) (layer "F.SilkS")
    (pts (xy 51.5 -0.1) (xy 6.5 -0.1))
    (height -3.1)
    (gr_text "45.0000 mm" (at 29 1.85) (layer "F.SilkS"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.SilkS")
    (pts (xy 50.5 -21.1) (xy 50.5 0.9))
    (height -2.5)
    (gr_text "22.0000 mm" (at 51.85 -10.1 90) (layer "F.SilkS"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 45 -18) (xy 51.5 -18))
    (height -4.5)
    (gr_text "6.5000 mm" (at 48.25 -23.65) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 45.5 -18.7) (xy 45.5 -21.2))
    (height 10)
    (gr_text "2.5000 mm" (at 54.35 -19.95 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 29 0) (xy 6.5 -0.1))
    (height -6.99993)
    (gr_text "22.5002 mm" (at 17.724001 5.799872 -0.2546462323) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
)
