(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 36)
    (no_connects 0)
    (area 141.148999 63.424999 172.795001 102.183001)
    (thickness 1.6)
    (drawings 16)
    (tracks 120)
    (zones 0)
    (modules 20)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/yi/kicad/gerbers/))
  )
  (net 0 "")
  (net 1 /VDD)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(D3-Pad1)")
  (net 7 /MCLR)
  (net 8 /ICSPDAT)
  (net 9 /ICSPCLK)
  (net 10 "Net-(P1-Pad6)")
  (net 11 "Net-(P2-Pad1)")
  (net 12 "Net-(P2-Pad2)")
  (net 13 +48V)
  (net 14 "Net-(U1-Pad7)")
  (net 15 "Net-(U1-Pad11)")
  (net 16 PHNGRN)
  (net 17 "Net-(D4-Pad3)")
  (net 18 "Net-(P2-Pad3)")
  (net 19 "Net-(D4-Pad2)")
  (net 20 "Net-(U1-Pad9)")
  (net 21 "Net-(D3-Pad2)")
  (net 22 "Net-(D1-Pad1)")
  (net 23 "Net-(R3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +48V)
    (add_net /ICSPCLK)
    (add_net /ICSPDAT)
    (add_net /MCLR)
    (add_net /VDD)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D4-Pad3)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net PHNGRN)
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 585F537C)
    (at 144.78 99.06 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -2.54 7.366 450) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 2.54 6.096 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /MCLR))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /VDD))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /ICSPDAT))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /ICSPCLK))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 147.32 80.645 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value C (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /VDD))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 150.495 92.71 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value C (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 155.575 92.71 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value C (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5848DB1A)
    (at 159.385 71.755 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0.127 1.651 90) (layer F.SilkS))
    (fp_text value C (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 PHNGRN))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 585F62FA)
    (at 163.83 87.376 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference TL431 (at 2.794 0 360) (layer F.SilkS))
    (fp_text value TL431 (at 0.254 2.54 450) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D3-Pad2)"))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5848BFB4)
    (at 163.576 71.628 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 2N7002 (at 2.54 0.635 360) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 16 PHNGRN))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5848C094)
    (at 147.32 66.04 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2.032 450) (layer F.SilkS))
    (fp_text value R (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /VDD))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D4-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 585F62D0)
    (at 159.766 82.042 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.54 0 540) (layer F.SilkS))
    (fp_text value R (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /VDD))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5848C00F)
    (at 163.576 75.692 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P2-Pad3)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5848DB10)
    (at 154.94 71.755 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0.127 1.778 90) (layer F.SilkS))
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 PHNGRN))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 5848DB3A)
    (at 153.035 87.63)
    (descr "Crystal Quarz HC49/U vertical stehend")
    (tags "Crystal Quarz HC49/U vertical stehend")
    (fp_text reference Y1 (at -0.127 0.762) (layer F.SilkS))
    (fp_text value Crystal (at 0 -1.27 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.44094 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.44094 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Big (layer F.Cu) (tedit 5848C078)
    (at 158.115 66.04)
    (descr "Mesurement Point, Square, Trough Hole,  3mm x 3mm, Drill 1.5mm,")
    (tags "Mesurement Point Square Trough Hole 3x3mm Drill 1.5mm")
    (attr virtual)
    (fp_text reference P48V (at -2.54 0 90) (layer F.SilkS))
    (fp_text value PHN48V (at 0 3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 13 +48V))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Big (layer F.Cu) (tedit 5848C085)
    (at 163.83 66.04)
    (descr "Mesurement Point, Square, Trough Hole,  3mm x 3mm, Drill 1.5mm,")
    (tags "Mesurement Point Square Trough Hole 3x3mm Drill 1.5mm")
    (attr virtual)
    (fp_text reference PSW (at -2.54 0 90) (layer F.SilkS))
    (fp_text value PHNGRN (at 0 3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 16 PHNGRN))
  )
  (module footprints:SOIC-14_39mm_127p (layer F.Cu) (tedit 585F62C7)
    (at 149.225 83.185)
    (fp_text reference U1 (at 6.223 -2.667 90) (layer F.SilkS))
    (fp_text value PIC16F1704 (at 3.81 -2.7) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VDD))
    (pad 2 smd rect (at 1.27 0) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at 2.54 0) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 4 smd rect (at 3.81 0) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /MCLR))
    (pad 5 smd rect (at 5.08 0) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P2-Pad1)"))
    (pad 6 smd rect (at 6.35 0) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P2-Pad2)"))
    (pad 7 smd rect (at 7.62 0) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 7.62 -5.4) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 9 smd rect (at 6.35 -5.4) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 5.08 -5.4) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 11 smd rect (at 3.81 -5.4) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 2.54 -5.4) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /ICSPCLK))
    (pad 13 smd rect (at 1.27 -5.4) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /ICSPDAT))
    (pad 14 smd rect (at 0 -5.4) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D1-Pad1)"))
  )
  (module footprints:TO-269 (layer F.Cu) (tedit 585F5E06)
    (at 151.384 72.644 90)
    (fp_text reference D4 (at -1.524 -3.048 180) (layer F.SilkS))
    (fp_text value Diode_Bridge (at 3.048 -8.382 270) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 +48V))
    (pad 2 smd rect (at 2.5 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D4-Pad2)"))
    (pad 3 smd rect (at 2.5 -6.1 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D4-Pad3)"))
    (pad 4 smd rect (at 0 -6.1 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Big (layer F.Cu) (tedit 5848C046)
    (at 152.4 66.04)
    (descr "Mesurement Point, Square, Trough Hole,  3mm x 3mm, Drill 1.5mm,")
    (tags "Mesurement Point Square Trough Hole 3x3mm Drill 1.5mm")
    (attr virtual)
    (fp_text reference PGND (at -2.54 0 90) (layer F.SilkS))
    (fp_text value PHNGND (at -0.635 3.175) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 19 "Net-(D4-Pad2)"))
  )
  (module footprints:CTerminalBlock (layer F.Cu) (tedit 585F0218)
    (at 168.91 97.79 90)
    (fp_text reference P2 (at 15 0 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 15 5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad1)"))
    (pad 2 thru_hole rect (at 10 0 90) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad2)"))
    (pad 3 thru_hole rect (at 20 0 90) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 18 "Net-(P2-Pad3)"))
    (pad 4 thru_hole rect (at 30 0 90) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 18 "Net-(P2-Pad3)"))
  )
  (module Diodes_SMD:DO-214BA (layer F.Cu) (tedit 585F5049)
    (at 164.084 80.772 90)
    (descr "Microsemi LSM115J")
    (tags "DO-214BA diode")
    (attr smd)
    (fp_text reference D3 (at -3.81 -0.254 180) (layer F.SilkS))
    (fp_text value D (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 1.7 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.7 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad1)"))
  )
  (module footprints:SuperCap (layer F.Cu) (tedit 585F62B4)
    (at 159.258 98.552)
    (fp_text reference C1 (at 2.286 -3.048 90) (layer F.SilkS))
    (fp_text value C (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25) (layers *.Cu *.Mask)
      (net 1 /VDD))
    (pad 2 thru_hole rect (at 5 0) (size 2 2) (drill 1.25) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (gr_text Master_D (at 152.4 96.266) (layer F.SilkS))
  (gr_line (start 172.72 98.552) (end 172.72 67.056) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 102.108) (end 169.164 102.108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.224 67.056) (end 141.224 98.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.164 63.5) (end 144.78 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.78 67.056) (end 141.224 67.056) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.78 98.552) (end 144.78 102.108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 169.164 98.552) (end 172.72 98.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 169.164 67.056) (end 169.164 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name /VDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 98.552) (xy 142.24 67.056) (xy 144.78 64.516) (xy 169.164 64.516) (xy 171.704 67.056)
        (xy 171.704 98.552) (xy 169.164 101.092) (xy 144.78 101.092)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.704 67.056) (xy 171.704 98.552) (xy 169.164 101.092) (xy 144.78 101.092) (xy 142.24 98.552)
        (xy 142.24 67.056) (xy 144.78 64.516) (xy 169.164 64.516)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.368 68.072) (xy 150.368 73.66) (xy 145.796 73.66) (xy 145.796 69.596) (xy 148.844 66.548)
      )
    )
  )
)
