(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 128)
    (no_connects 0)
    (area 113.417999 80.045619 149.130001 98.895)
    (thickness 1.6)
    (drawings 9)
    (tracks 499)
    (zones 0)
    (modules 42)
    (nets 67)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (trace_clearance 0.127)
    (zone_clearance 0.127)
    (zone_45_only yes)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.355)
    (via_drill 0.254)
    (via_min_size 0.355)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 0.3 0.3)
    (mod_edge_width 0.15)
    (mod_text_size 0.4 0.4)
    (mod_text_width 0.075)
    (pad_size 1.5 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010ff_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../gerbers-jan-9-2017/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C5-Pad1)")
  (net 3 "Net-(C5-Pad2)")
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(L1-Pad2)")
  (net 8 "Net-(R2-Pad1)")
  (net 9 "Net-(U3-Pad4)")
  (net 10 "Net-(U3-Pad1)")
  (net 11 "Net-(U4-Pad1)")
  (net 12 "Net-(U4-Pad10)")
  (net 13 "Net-(U4-Pad11)")
  (net 14 "Net-(U4-Pad12)")
  (net 15 "Net-(U4-Pad14)")
  (net 16 "Net-(U5-Pad2)")
  (net 17 "Net-(U5-Pad3)")
  (net 18 "Net-(U5-Pad26)")
  (net 19 "Net-(U5-Pad27)")
  (net 20 "Net-(U5-Pad28)")
  (net 21 "Net-(U5-Pad40)")
  (net 22 "Net-(U5-Pad41)")
  (net 23 "Net-(U5-Pad42)")
  (net 24 "Net-(U5-Pad43)")
  (net 25 "Net-(U5-Pad44)")
  (net 26 "Net-(U5-Pad45)")
  (net 27 "Net-(U4-Pad22)")
  (net 28 "Net-(U4-Pad23)")
  (net 29 "Net-(ANT1-Pad1)")
  (net 30 /TX)
  (net 31 /RX)
  (net 32 "Net-(U5-Pad11)")
  (net 33 /Reset)
  (net 34 "Net-(U5-Pad46)")
  (net 35 /EXTVCC)
  (net 36 /Regulator_In)
  (net 37 /VBAT)
  (net 38 "Net-(J1-Pad4)")
  (net 39 "Net-(U6-Pad6)")
  (net 40 /Backlight)
  (net 41 /ClockINT)
  (net 42 /Accel_INT)
  (net 43 /XC2)
  (net 44 "Net-(C4-Pad1)")
  (net 45 /VCC)
  (net 46 "Net-(C9-Pad1)")
  (net 47 /XC1)
  (net 48 /BatterySense)
  (net 49 /Display_MOSI)
  (net 50 /Display_SCK)
  (net 51 /Display_SS)
  (net 52 /EX15)
  (net 53 /EX14)
  (net 54 /EX13)
  (net 55 /EX12)
  (net 56 /EX11)
  (net 57 /EX10)
  (net 58 /EX9)
  (net 59 /EX8)
  (net 60 /SCL)
  (net 61 /SDA)
  (net 62 /Bal1)
  (net 63 /Bal2)
  (net 64 "Net-(C11-Pad1)")
  (net 65 "Net-(U5-Pad30)")
  (net 66 /SWDCLK)
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.355)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Accel_INT)
    (add_net /Backlight)
    (add_net /Bal1)
    (add_net /Bal2)
    (add_net /BatterySense)
    (add_net /ClockINT)
    (add_net /Display_MOSI)
    (add_net /Display_SCK)
    (add_net /Display_SS)
    (add_net /EX10)
    (add_net /EX11)
    (add_net /EX12)
    (add_net /EX13)
    (add_net /EX14)
    (add_net /EX15)
    (add_net /EX8)
    (add_net /EX9)
    (add_net /RX)
    (add_net /Reset)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SWDCLK)
    (add_net /TX)
    (add_net /VCC)
    (add_net /XC1)
    (add_net /XC2)
    (add_net GND)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad10)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad14)")
    (add_net "Net-(U4-Pad22)")
    (add_net "Net-(U4-Pad23)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad26)")
    (add_net "Net-(U5-Pad27)")
    (add_net "Net-(U5-Pad28)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U5-Pad30)")
    (add_net "Net-(U5-Pad40)")
    (add_net "Net-(U5-Pad41)")
    (add_net "Net-(U5-Pad42)")
    (add_net "Net-(U5-Pad43)")
    (add_net "Net-(U5-Pad44)")
    (add_net "Net-(U5-Pad45)")
    (add_net "Net-(U5-Pad46)")
    (add_net "Net-(U6-Pad6)")
  )
  (net_class 50ohm ""
    (clearance 0.127)
    (trace_width 0.33)
    (via_dia 0.355)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(ANT1-Pad1)")
  )
  (net_class power ""
    (clearance 0.127)
    (trace_width 0.2)
    (via_dia 0.355)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /EXTVCC)
    (add_net /Regulator_In)
    (add_net /VBAT)
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer B.Cu) (tedit 588650DC)
    (at 139.975 93.225)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 -0.7) (layer B.SilkS) hide)
    (fp_text value F2 (at 0 1.8) (layer B.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Pin_Header_Straight_1x10_Pitch2.00mm (layer F.Cu) (tedit 5885B763)
    (at 138.9 96.6)
    (descr "Through hole pin header, 1x10, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference P1 (at 0 -5) (layer F.SilkS))
    (fp_text value "Expansion Header" (at 0 -3) (layer F.Fab) hide)
    (fp_text user 15 (at 8.9916 -1.0668) (layer F.SilkS))
    (fp_text user 14 (at 6.9596 -1.0922) (layer F.SilkS))
    (fp_text user 13 (at 4.953 -1.0922) (layer F.SilkS))
    (fp_text user 12 (at 2.9972 -1.1176) (layer F.SilkS))
    (fp_text user 11 (at 0.9906 -1.1176) (layer F.SilkS))
    (fp_text user 10 (at -0.9906 -1.1684) (layer F.SilkS))
    (fp_text user 9 (at -3.048 -1.1938) (layer F.SilkS))
    (fp_text user 8 (at -5.1816 -1.2446) (layer F.SilkS))
    (fp_text user VCC (at -6.985 -1.1938) (layer F.SilkS))
    (fp_text user GND (at -9.017 -1.143) (layer F.SilkS))
    (pad 1 thru_hole rect (at -9.017 -0.0635 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -7.017 -0.0635 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /VCC))
    (pad 3 thru_hole circle (at -5.017 -0.0635 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /EX8))
    (pad 4 thru_hole circle (at -3.017 -0.0635 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /EX9))
    (pad 5 thru_hole circle (at -1.017 -0.0635 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /EX10))
    (pad 6 thru_hole circle (at 0.983 -0.0635 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /EX11))
    (pad 7 thru_hole circle (at 2.983 -0.0635 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /EX12))
    (pad 8 thru_hole circle (at 4.983 -0.0635 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /EX13))
    (pad 9 thru_hole circle (at 6.983 -0.0635 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /EX14))
    (pad 10 thru_hole circle (at 8.983 -0.0635 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /EX15))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58071761)
    (at 135.175 94.025)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 6.26 -6.51) (layer B.SilkS) hide)
    (fp_text value 10uf (at 0 0.1 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module watch-v4:omron_XF2M-1015-1A-2 (layer F.Cu) (tedit 57020490)
    (at 131.35 91.9 180)
    (fp_text reference J1 (at 0 3.5 180) (layer F.SilkS) hide)
    (fp_text value CONN_10 (at 0 -3.5 180) (layer F.Fab) hide)
    (pad "" smd rect (at -3.7 2.4 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.75 -1 180) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 49 /Display_MOSI))
    (pad 3 smd rect (at -1.25 -1 180) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 50 /Display_SCK))
    (pad 4 smd rect (at -0.75 -1 180) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -0.25 -1 180) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 45 /VCC))
    (pad 6 smd rect (at 0.25 -1 180) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 45 /VCC))
    (pad 7 smd rect (at 0.75 -1 180) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 45 /VCC))
    (pad 8 smd rect (at 1.25 -1 180) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 45 /VCC))
    (pad 9 smd rect (at 1.75 -1 180) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.25 -1 180) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.25 -1 180) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 51 /Display_SS))
    (pad "" smd rect (at 3.7 2.4 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
  )
  (module Housings_DFN_QFN:UQFN-48-1EP_6x6mm_Pitch0.4mm (layer F.Cu) (tedit 5885A293)
    (at 140.62 91.21)
    (descr "48-Lead Plastic Ultra Thin Quad Flat, No Lead Package (MV) - 6x6x0.5 mm Body [UQFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.4")
    (attr smd)
    (fp_text reference U5 (at 0.23 -4.11) (layer F.SilkS))
    (fp_text value NRF51822 (at -22.195 -8.91) (layer F.Fab) hide)
    (pad 1 smd rect (at -3 -2.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /VCC))
    (pad 2 smd rect (at -3 -1.8) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U5-Pad2)"))
    (pad 3 smd rect (at -3 -1.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U5-Pad3)"))
    (pad 4 smd rect (at -3 -1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 30 /TX))
    (pad 5 smd rect (at -3 -0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /RX))
    (pad 6 smd rect (at -3 -0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 60 /SCL))
    (pad 7 smd rect (at -3 0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 61 /SDA))
    (pad 8 smd rect (at -3 0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 51 /Display_SS))
    (pad 9 smd rect (at -3 1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 49 /Display_MOSI))
    (pad 10 smd rect (at -3 1.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 50 /Display_SCK))
    (pad 11 smd rect (at -3 1.8) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U5-Pad11)"))
    (pad 12 smd rect (at -3 2.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /VCC))
    (pad 13 smd rect (at -2.2 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -1.8 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 59 /EX8))
    (pad 15 smd rect (at -1.4 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 58 /EX9))
    (pad 16 smd rect (at -1 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 57 /EX10))
    (pad 17 smd rect (at -0.6 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 56 /EX11))
    (pad 18 smd rect (at -0.2 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 55 /EX12))
    (pad 19 smd rect (at 0.2 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 54 /EX13))
    (pad 20 smd rect (at 0.6 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 53 /EX14))
    (pad 21 smd rect (at 1 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 52 /EX15))
    (pad 22 smd rect (at 1.4 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 48 /BatterySense))
    (pad 23 smd rect (at 1.8 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 33 /Reset))
    (pad 24 smd rect (at 2.2 3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 66 /SWDCLK))
    (pad 25 smd rect (at 3 2.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 40 /Backlight))
    (pad 26 smd rect (at 3 1.8) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U5-Pad26)"))
    (pad 27 smd rect (at 3 1.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U5-Pad27)"))
    (pad 28 smd rect (at 3 1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U5-Pad28)"))
    (pad 29 smd rect (at 3 0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C9-Pad1)"))
    (pad 30 smd rect (at 3 0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U5-Pad30)"))
    (pad 31 smd rect (at 3 -0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 62 /Bal1))
    (pad 32 smd rect (at 3 -0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 63 /Bal2))
    (pad 33 smd rect (at 3 -1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 34 smd rect (at 3 -1.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 35 smd rect (at 3 -1.8) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /VCC))
    (pad 36 smd rect (at 3 -2.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /VCC))
    (pad 37 smd rect (at 2.2 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 43 /XC2))
    (pad 38 smd rect (at 1.8 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 47 /XC1))
    (pad 39 smd rect (at 1.4 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C4-Pad1)"))
    (pad 40 smd rect (at 1 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U5-Pad40)"))
    (pad 41 smd rect (at 0.6 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U5-Pad41)"))
    (pad 42 smd rect (at 0.2 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U5-Pad42)"))
    (pad 43 smd rect (at -0.2 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U5-Pad43)"))
    (pad 44 smd rect (at -0.6 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U5-Pad44)"))
    (pad 45 smd rect (at -1 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U5-Pad45)"))
    (pad 46 smd rect (at -1.4 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U5-Pad46)"))
    (pad 47 smd rect (at -1.8 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 41 /ClockINT))
    (pad 48 smd rect (at -2.2 -3 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask)
      (net 42 /Accel_INT))
    (pad 49 smd rect (at 1.66875 1.66875) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.66875 0.55625) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.66875 -0.55625) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.66875 -1.66875) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.55625 1.66875) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.55625 0.55625) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.55625 -0.55625) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.55625 -1.66875) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.55625 1.66875) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.55625 0.55625) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.55625 -0.55625) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.55625 -1.66875) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.66875 1.66875) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.66875 0.55625) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.66875 -0.55625) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.66875 -1.66875) (size 1.1125 1.1125) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/UQFN-48-1EP_6x6mm_Pitch0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 570D63DF)
    (at 118.25 94.9 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 4.7uf (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 35 /EXTVCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5885A29B)
    (at 131.2 92.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -12.5 -10.5) (layer B.SilkS) hide)
    (fp_text value 4.7k (at -0.04 0.01 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 60 /SCL))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5885A2AA)
    (at 131.25 94.075)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -3.275 -12.125) (layer B.SilkS) hide)
    (fp_text value 4.7k (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 61 /SDA))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58071731)
    (at 139.45 90.475)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.9) (layer B.SilkS) hide)
    (fp_text value .22uf (at 0.1 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5809A7FA)
    (at 142.775 90.475)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 1.9) (layer B.SilkS) hide)
    (fp_text value 4.7uf (at 0.01 -0.03 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 55B03F31)
    (at 120.6 86.15 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 2 270) (layer B.SilkS) hide)
    (fp_text value DIODESCH (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 35 /EXTVCC))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 36 /Regulator_In))
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 55B03F2C)
    (at 124.05 85.675)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L1 (at 0.03 -0.08) (layer F.SilkS))
    (fp_text value 10uH (at 0 2.7) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.45 0) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /Regulator_In))
    (pad 2 smd rect (at 1.45 0) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(L1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23 (layer B.Cu) (tedit 5804639E)
    (at 119.7 91.75 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 2.25 90) (layer B.SilkS) hide)
    (fp_text value MOSFET_P (at -0.05 0.05 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 -1.00076 90) (size 0.8001 0.8001) (layers B.Cu B.Paste B.Mask)
      (net 35 /EXTVCC))
    (pad 2 smd rect (at 0.95 -1.00076 90) (size 0.8001 0.8001) (layers B.Cu B.Paste B.Mask)
      (net 37 /VBAT))
    (pad 3 smd rect (at 0 0.99822 90) (size 0.8001 0.8001) (layers B.Cu B.Paste B.Mask)
      (net 36 /Regulator_In))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer B.Cu) (tedit 55B03DF2)
    (at 133.45 86.3 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at 0 1.27 90) (layer B.SilkS))
    (fp_text value DS3231 (at 0 -1.27 90) (layer B.Fab) hide)
    (pad 8 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 61 /SDA))
    (pad 7 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 60 /SCL))
    (pad 6 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 5 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(U3-Pad4)"))
    (pad 3 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 41 /ClockINT))
    (pad 2 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 1 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(U3-Pad1)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23-5 (layer B.Cu) (tedit 570D642C)
    (at 116 85.75 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -0.05 2.55 360) (layer B.SilkS) hide)
    (fp_text value IC_MCP73831 (at 2.15 0.03 360) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 37 /VBAT))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 35 /EXTVCC))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23-5 (layer B.Cu) (tedit 580464DA)
    (at 124.1 85.45)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at -0.05 2.55) (layer B.SilkS) hide)
    (fp_text value MAX1722 (at 0.05 -0.05 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 36 /Regulator_In))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 36 /Regulator_In))
    (pad 4 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 5 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(L1-Pad2)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module watch-v4:QFN-24-NO-CENTER4x4mm_Pitch0.5mm (layer B.Cu) (tedit 57020D1B)
    (at 140.95 86.375 180)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U4 (at -0.47 0.46 180) (layer B.SilkS))
    (fp_text value LSM9DS0 (at 0 -3.375 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.95 1.25 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(U4-Pad1)"))
    (pad 2 smd rect (at -1.95 0.75 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.95 0.25 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.95 -0.25 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -1.95 -0.75 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -1.95 -1.25 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -1.25 -1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 8 smd rect (at -0.75 -1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C5-Pad2)"))
    (pad 9 smd rect (at -0.25 -1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C5-Pad1)"))
    (pad 10 smd rect (at 0.25 -1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(U4-Pad10)"))
    (pad 11 smd rect (at 0.75 -1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U4-Pad11)"))
    (pad 12 smd rect (at 1.25 -1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U4-Pad12)"))
    (pad 13 smd rect (at 1.95 -1.25 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 42 /Accel_INT))
    (pad 14 smd rect (at 1.95 -0.75 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U4-Pad14)"))
    (pad 15 smd rect (at 1.95 -0.25 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 16 smd rect (at 1.95 0.25 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 17 smd rect (at 1.95 0.75 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 18 smd rect (at 1.95 1.25 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 19 smd rect (at 1.25 1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 20 smd rect (at 0.75 1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 21 smd rect (at 0.25 1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 60 /SCL) (solder_paste_margin_ratio -0.2))
    (pad 22 smd rect (at -0.25 1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(U4-Pad22)"))
    (pad 23 smd rect (at -0.75 1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(U4-Pad23)"))
    (pad 24 smd rect (at -1.25 1.95 90) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 61 /SDA))
    (model Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module watch-v4:USB_Micro-B (layer F.Cu) (tedit 5885A298)
    (at 116.62 91.23 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference XL1 (at 0 -3.75 270) (layer F.SilkS) hide)
    (fp_text value USB_MICRO_B (at -10.005 -2.48 360) (layer F.Fab) hide)
    (pad 5 smd rect (at 1.25 1.17 270) (size 1.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -1.25 1.17 270) (size 1.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 4.11 1.17 270) (size 1.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 3 -1.26 270) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.3009 -1.56254) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 /EXTVCC))
    (pad 2 smd rect (at -0.6509 -1.56254) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 /TX))
    (pad 3 smd rect (at -0.0009 -1.56254) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 /RX))
    (pad 4 smd rect (at 0.6491 -1.56254) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 /Reset))
    (pad 5 smd rect (at 1.2991 -1.56254) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -3 -1.26 270) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -4.11 1.17 270) (size 1.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module watch-v4:SMD-Crystal (layer F.Cu) (tedit 5885A2A6)
    (at 142.75 85.1 180)
    (fp_text reference X1 (at 0.25 2.35 180) (layer F.SilkS) hide)
    (fp_text value 16mhz (at 2.3 2.275 360) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.6 -0.1 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.15 -0.1 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 /XC2))
    (pad 3 smd rect (at 1.6 -1.175 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 /XC1))
    (pad 4 smd rect (at 0.15 -1.175 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58071756)
    (at 128.35 94.025 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -5.03316 3.8947 180) (layer B.SilkS) hide)
    (fp_text value 0.1uf (at -0.09 0.03 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5885A2A2)
    (at 137.11 85.41 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 3.785 -19.16 90) (layer F.SilkS) hide)
    (fp_text value 12pf (at 0.01 0.04 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 /XC1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5885A29F)
    (at 128.45 85.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 3.65 -8.975 90) (layer B.SilkS) hide)
    (fp_text value 0.1uf (at -0.05 -0.05 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5885A248)
    (at 126.85 85.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 3 5.575 360) (layer B.SilkS) hide)
    (fp_text value 1nf (at -0.05 0.05 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5804634E)
    (at 118.55 84.86)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 47Ω (at -0.1 -0.06 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 /EXTVCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58046363)
    (at 118.6 85.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 4.34 2.07 270) (layer B.SilkS) hide)
    (fp_text value 10kΩ (at 0.05 0.05 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5885A290)
    (at 115.75 95.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -0.825 12.55 180) (layer B.SilkS) hide)
    (fp_text value R100kΩ (at 0 -0.01 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 35 /EXTVCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 580461A6)
    (at 115.85 93.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 1uf (at -0.02 -0.03 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 36 /Regulator_In))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58071521)
    (at 115.98 91.18 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.07 -6.52 180) (layer B.SilkS) hide)
    (fp_text value 4.7uf (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 37 /VBAT))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module watch-v4:BALUN-6 (layer F.Cu) (tedit 580717D3)
    (at 145.55 90.8)
    (fp_text reference U6 (at 0 1) (layer F.SilkS))
    (fp_text value BALUN (at -0.025 -1.075) (layer F.Fab) hide)
    (pad 6 smd rect (at 0.6 0.275) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U6-Pad6)"))
    (pad 2 smd rect (at 0.1 -0.275) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.1 0.275) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at 0.6 -0.275) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(ANT1-Pad1)"))
    (pad 3 smd rect (at -0.4 -0.275) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 63 /Bal2))
    (pad 4 smd rect (at -0.4 0.275) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 62 /Bal1))
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 570D629C)
    (at 128.35 89.625 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 10k (at 0.03 -0.01 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 41 /ClockINT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 570D635E)
    (at 115.2 89.05 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 10M (at 0.02 0.01 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 37 /VBAT))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 /BatterySense))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 570D6374)
    (at 116.8 88.95 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 10M (at -0.03 0.01 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 /BatterySense))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58071695)
    (at 135.2 85.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 580866D8)
    (at 145.65 93.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 4 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 47n (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5885A2AD)
    (at 147.45 93.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -11.925 23.2 360) (layer F.SilkS) hide)
    (fp_text value 2n2 (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5885A254)
    (at 118.55 88.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -6.625 3.65 270) (layer B.SilkS) hide)
    (fp_text value 1u (at 0.05 -0.05 360) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 48 /BatterySense))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5885A250)
    (at 115.7 84.96 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference D2 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value LED (at -11.075 3.235 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module watch-v4:antenna (layer F.Cu) (tedit 58425C7B)
    (at 147.3 86.45 90)
    (fp_text reference ANT1 (at 0.127 -1.8415 90) (layer F.SilkS) hide)
    (fp_text value - (at 0.0635 -1.016 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.4605 0 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.5395 0 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(ANT1-Pad1)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5885A595)
    (at 138.95 85.4 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 12pf (at 0 0.025 360) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 43 /XC2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module crennelated:JST_2_pos (layer F.Cu) (tedit 58859526)
    (at 123.55 91.075)
    (fp_text reference LIPOLY1 (at 0 1.3) (layer F.SilkS))
    (fp_text value BATTERY (at 0.0635 -2.2225) (layer F.Fab) hide)
    (pad "" smd rect (at 3.3655 4.572) (size 1.5 1.7) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.3655 4.572) (size 1.5 1.7) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.75 0) (size 0.7 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd oval (at 0.75 0) (size 0.7 2) (layers F.Cu F.Paste F.Mask)
      (net 37 /VBAT))
  )
  (module crennelated:test_points (layer B.Cu) (tedit 5885A9C6)
    (at 123.4222 95.1295)
    (fp_text reference P2 (at 3.683 2.6035) (layer B.SilkS) hide)
    (fp_text value "Test Points" (at -3.937 2.6035) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.0155 1.0795) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 45 /VCC))
    (pad 2 smd rect (at -0.0155 1.0795) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 33 /Reset))
    (pad 3 smd rect (at 1.9845 1.0795) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 66 /SWDCLK))
    (pad 4 smd rect (at -1.9972 -1.0795) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 37 /VBAT))
    (pad 5 smd rect (at 0.0028 -1.0795) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 35 /EXTVCC))
    (pad 6 smd rect (at 2.0028 -1.0795) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 58864129)
    (at 132 86.8)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value F1 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (gr_line (start 114.05 96.5) (end 114.05 97.475) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.075 96.425) (end 149.075 97.475) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "Ourglass\n Rev 6.5\n" (at 123.2 88.75 180) (layer F.SilkS))
  (gr_line (start 147.45 97.5) (end 149.05 97.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.08 83.5) (end 149.08 96.41) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.025 97.5) (end 147.445 97.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114 97.5) (end 140 97.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.05 83.5) (end 114.05 96.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.05 83.5) (end 114.05 83.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.128) (thermal_bridge_width 0.128))
    (polygon
      (pts
        (xy 114.05 96.8) (xy 149.05 96.8) (xy 149.05 89.275) (xy 145.75 89.075) (xy 145.75 83.65)
        (xy 113.95 83.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.128) (thermal_bridge_width 0.128))
    (polygon
      (pts
        (xy 114.05 96.8) (xy 149.05 96.8) (xy 149.1 89.25) (xy 145.675 89.15) (xy 145.725 83.7)
        (xy 113.95 83.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.128) (thermal_bridge_width 0.128))
    (polygon
      (pts
        (xy 114.05 96.8) (xy 149.05 96.8) (xy 149.025 89.3) (xy 145.6 89.1) (xy 145.475 83.775)
        (xy 113.95 83.5)
      )
    )
  )
)
