(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 11)
    (zones 0)
    (modules 3)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.15)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.8 3.8)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
  )
  (module Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical (layer B.Cu) (tedit 5C3B3971)
    (at 3.6 0 180)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (attr smd)
    (fp_text reference J1 (at -2.15 0 270) (layer B.SilkS))
    (fp_text value Conn_Coaxial (at 5 0 90) (layer B.Fab))
    (fp_text user %R (at 0.475 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.475 -1.475 180) (size 2.2 1.05) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.05 0 180) (size 1.05 1) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.475 1.475 180) (size 2.2 1.05) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl
      (offset (xyz 0.4749999928262157 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module s13360-2050ve:S13360-2050VE (layer F.Cu) (tedit 5C711EE2)
    (at 3.6 0 270)
    (fp_text reference D1 (at 0 -2.15 90) (layer F.SilkS))
    (fp_text value S13360-2050VE (at 0 4.445 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd circle (at -0.6 0.6 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 2 smd circle (at 0.6 0.6 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd circle (at 0.6 -0.6 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd circle (at -0.6 -0.6 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KIPRJMOD}/components/s13360-2050ve/s13360-2050ve.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO14580_Pad (layer F.Cu) (tedit 5C710DF7)
    (at -4.25 0)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (attr virtual)
    (fp_text reference H1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 3.23 6.35) (layer F.Fab))
    (fp_text user %R (at 0.055 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_line (start -6.8 -4.1) (end -6.8 -2.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -5.75 -4.1) (end -6.8 -4.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -5.75 -2.25) (end -5.75 -4.1) (layer Edge.Cuts) (width 0.15))
  (gr_text "D1\nH1\nH2" (at -8.255 6.35) (layer F.Fab))
  (gr_line (start 6.8 2.25) (end 6.8 -2.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -6.8 2.25) (end 6.8 2.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -6.8 -2.25) (end -6.8 2.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 6.8 -2.25) (end -5.75 -2.25) (layer Edge.Cuts) (width 0.15))
)
