<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="63.5" y1="53.34" x2="0" y2="53.34" width="0.2032" layer="20"/>
<wire x1="0" y1="53.34" x2="0" y2="0" width="0.2032" layer="20"/>
<wire x1="67.31" y1="0" x2="67.31" y2="17.78" width="0.2032" layer="20"/>
<wire x1="67.31" y1="17.78" x2="63.5" y2="22.86" width="0.2032" layer="20"/>
<wire x1="63.5" y1="22.86" x2="63.5" y2="53.34" width="0.2032" layer="20"/>
<wire x1="0" y1="0" x2="67.31" y2="0" width="0.2032" layer="20"/>
<text>VIN+</text>
<text>RESET</text>
<text>Trackuino THT 2.2+</text>
<text>http://trackuino.org</text>
<text>GND</text>
<text>+ BUZZ -</text>
<text>GND, Vo, Vs</text>
<text>TMP32-ext</text>
<text>5V: bridge J6, J8; buffer on IC4</text>
<text>3.3V: bridge J7; buffers on IC3, IC5</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="trackuino">
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="VENUS638FLPX">
</package>
<package name="HVMDIP">
</package>
<package name="HX1">
</package>
</packages>
</library>
<library name="switch-omron">
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
<package name="W237-103">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="First">
<packages>
<package name="TO220-3">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="BU-SMA-V">
<description>FEMALE &lt;b&gt;SMA CONNECTOR&lt;/b&gt;&lt;p&gt;
Radiall&lt;p&gt;
distributor RS 112-3794</description>
</package>
</packages>
</library>
<library name="tr">
<packages>
<package name="FLAGS_SM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="E2,5-5" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="E2,5-5" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="trackuino" package="TO92" value="LM60 int">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-omron" package="B3F-10XX" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-wago-500" package="W237-102" value="Vin">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
</element>
<element name="X3" library="con-wago-500" package="W237-103" value="LM60 ext">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-103"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="18M7116"/>
</element>
<element name="X4" library="con-wago-500" package="W237-102" value="Buzzer">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
</element>
<element name="R1" library="rcl" package="0207/7" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="0207/7" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="0207/7" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="First" package="TO220-3" value="AP1117">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GPS" library="trackuino" package="VENUS638FLPX" value="VENUS638FLPX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="trackuino" package="HVMDIP" value="IRLD110">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M1" library="trackuino" package="HX1" value="HX1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$1" library="tr" package="FLAGS_SM" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="-"/>
<contactref element="C1" pad="-"/>
<contactref element="U1" pad="3"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="J4" pad="3"/>
<contactref element="J4" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="X2" pad="2"/>
<contactref element="X3" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="GPS" pad="GND"/>
<contactref element="Q1" pad="S"/>
<contactref element="GPS" pad="RX0"/>
<contactref element="M1" pad="0V"/>
<contactref element="M1" pad="BODYGND1"/>
<contactref element="M1" pad="BODYGND2"/>
</signal>
<signal name="+5V">
<contactref element="J4" pad="4"/>
<contactref element="M1" pad="VCC"/>
</signal>
<signal name="+3V3">
<contactref element="IC2" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="GPS" pad="3.3V"/>
</signal>
<signal name="RESET">
<contactref element="J4" pad="6"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="3V3">
<contactref element="J4" pad="5"/>
</signal>
<signal name="VIN">
<contactref element="J4" pad="1"/>
<contactref element="X4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="C2" pad="+"/>
<contactref element="R1" pad="2"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="A0">
<contactref element="J2" pad="6"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="A1">
<contactref element="J2" pad="5"/>
<contactref element="X3" pad="2"/>
</signal>
<signal name="A2">
<contactref element="J2" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="A3">
<contactref element="J2" pad="3"/>
</signal>
<signal name="A4">
<contactref element="J2" pad="2"/>
</signal>
<signal name="A5">
<contactref element="J2" pad="1"/>
</signal>
<signal name="AREF">
<contactref element="J3" pad="1"/>
</signal>
<signal name="RX">
<contactref element="J1" pad="8"/>
<contactref element="GPS" pad="TX0"/>
</signal>
<signal name="TX">
<contactref element="J1" pad="7"/>
</signal>
<signal name="D2">
<contactref element="J1" pad="6"/>
</signal>
<signal name="D3">
<contactref element="J1" pad="5"/>
<contactref element="M1" pad="TXD"/>
</signal>
<signal name="D4">
<contactref element="J1" pad="4"/>
<contactref element="M1" pad="EN"/>
</signal>
<signal name="D5">
<contactref element="J1" pad="3"/>
</signal>
<signal name="D6">
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="D7">
<contactref element="J1" pad="1"/>
<contactref element="X3" pad="1"/>
</signal>
<signal name="D8">
<contactref element="J3" pad="8"/>
</signal>
<signal name="D9">
<contactref element="J3" pad="7"/>
<contactref element="Q1" pad="G"/>
</signal>
<signal name="D10">
<contactref element="J3" pad="6"/>
</signal>
<signal name="D11">
<contactref element="J3" pad="5"/>
</signal>
<signal name="D12">
<contactref element="J3" pad="4"/>
</signal>
<signal name="D13">
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="X4" pad="2"/>
<contactref element="Q1" pad="D@1"/>
<contactref element="Q1" pad="D@2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="RFGND">
<contactref element="M1" pad="RFGND1"/>
<contactref element="M1" pad="RFGND2"/>
<contactref element="X1" pad="5"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="M1" pad="RFOUT"/>
<contactref element="X1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
