(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 404)
    (no_connects 0)
    (area 84.650001 26.3 231.421429 122.700001)
    (thickness 1.6)
    (drawings 24)
    (tracks 1754)
    (zones 0)
    (modules 136)
    (nets 192)
  )
  (page USLetter)
  (title_block
    (title "Minimum Viable Synth - I/O Daughter Board")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 100 100)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 /BKLT_A)
  (net 5 /BKLT_K)
  (net 6 "Net-(C13-Pad1)")
  (net 7 /BTN_~RESET)
  (net 8 /BTN_USER)
  (net 9 /PC13)
  (net 10 "Net-(D1-Pad2)")
  (net 11 /I²C3_SCL)
  (net 12 /I²C3_SDA)
  (net 13 /CTOUCH_WAKE)
  (net 14 /CTOUCH_INT)
  (net 15 /LCD_R0)
  (net 16 /LCD_R1)
  (net 17 /LCD_R2)
  (net 18 /LCD_R3)
  (net 19 /LCD_R4)
  (net 20 /LCD_R5)
  (net 21 /LCD_G0)
  (net 22 /LCD_G1)
  (net 23 /LCD_G2)
  (net 24 /LCD_G3)
  (net 25 /LCD_G4)
  (net 26 /LCD_G5)
  (net 27 /LCD_B0)
  (net 28 /LCD_B1)
  (net 29 /LCD_B2)
  (net 30 /LCD_B3)
  (net 31 /LCD_B4)
  (net 32 /LCD_B5)
  (net 33 /LCD_CLK)
  (net 34 /LCD_DISP)
  (net 35 /LCD_HSYNC)
  (net 36 /LCD_VSYNC)
  (net 37 /LCD_DE)
  (net 38 /RTOUCH_XR)
  (net 39 /RTOUCH_YD)
  (net 40 /RTOUCH_XL)
  (net 41 /RTOUCH_YU)
  (net 42 /PF4)
  (net 43 /PF5)
  (net 44 /PF2)
  (net 45 /PF3)
  (net 46 /PF0)
  (net 47 /PF1)
  (net 48 /PC14)
  (net 49 /PC15)
  (net 50 /PE6)
  (net 51 /PE5)
  (net 52 /PE2)
  (net 53 /PE3)
  (net 54 /PE0)
  (net 55 /PE1)
  (net 56 /BOOT0)
  (net 57 /Vdd)
  (net 58 /PB6)
  (net 59 /PB7)
  (net 60 /PB4)
  (net 61 /PB5)
  (net 62 /PG15)
  (net 63 /PB3)
  (net 64 /PG13)
  (net 65 /PG14)
  (net 66 /PD7)
  (net 67 /PD5)
  (net 68 /PD4)
  (net 69 /PD2)
  (net 70 /PD1)
  (net 71 /PD0)
  (net 72 /PC12)
  (net 73 /PC11)
  (net 74 /PA15)
  (net 75 /PA14)
  (net 76 /PA13)
  (net 77 /MIDI_RX)
  (net 78 /MIDI_TX)
  (net 79 /PC8)
  (net 80 /PG8)
  (net 81 /PG5)
  (net 82 /PG4)
  (net 83 /LCD_PWM)
  (net 84 /N/C)
  (net 85 /PF8)
  (net 86 /PF7)
  (net 87 /PF9)
  (net 88 /PH1)
  (net 89 /PH0)
  (net 90 /PC1)
  (net 91 /PC0)
  (net 92 /PC3)
  (net 93 /PC2)
  (net 94 /PA1)
  (net 95 /PA2)
  (net 96 /PA5)
  (net 97 /PA7)
  (net 98 /PC5)
  (net 99 /PC4)
  (net 100 /PB2)
  (net 101 /PF12)
  (net 102 /PF11)
  (net 103 /PF14)
  (net 104 /PF13)
  (net 105 /PG0)
  (net 106 /PF15)
  (net 107 /PE7)
  (net 108 /PG1)
  (net 109 /PE9)
  (net 110 /PE8)
  (net 111 /PE11)
  (net 112 /PE10)
  (net 113 /PE13)
  (net 114 /PE12)
  (net 115 /PE15)
  (net 116 /PE14)
  (net 117 /PB13)
  (net 118 /PB12)
  (net 119 /PB15)
  (net 120 /PB14)
  (net 121 /PD9)
  (net 122 /PD8)
  (net 123 /PD11)
  (net 124 /PD10)
  (net 125 /PD13)
  (net 126 /PD12)
  (net 127 /PD15)
  (net 128 /PD14)
  (net 129 /PG2)
  (net 130 /SLV1A_MISO)
  (net 131 /SLV1A_SCK)
  (net 132 /SLV1A_MOSI)
  (net 133 /SLV3A_MISO)
  (net 134 /SLV3A_SCK)
  (net 135 /SLV3A_MOSI)
  (net 136 /SLV4A_MISO)
  (net 137 /SLV4A_SCK)
  (net 138 /SLV4A_MOSI)
  (net 139 /SLV5A_MISO)
  (net 140 /SLV5A_SCK)
  (net 141 /SLV5A_MOSI)
  (net 142 /SLV1B_MISO)
  (net 143 /SLV1B_SCK)
  (net 144 /SLV1B_MOSI)
  (net 145 /SLV3B_MISO)
  (net 146 /SLV3B_SCK)
  (net 147 /SLV3B_MOSI)
  (net 148 /SLV4B_MISO)
  (net 149 /SLV4B_SCK)
  (net 150 /SLV4B_MOSI)
  (net 151 /SLV5B_MISO)
  (net 152 /SLV5B_SCK)
  (net 153 /SLV5B_MOSI)
  (net 154 /SLV1C_MISO)
  (net 155 /SLV1C_SCK)
  (net 156 /SLV1C_MOSI)
  (net 157 /SLV3C_MISO)
  (net 158 /SLV3C_SCK)
  (net 159 /SLV3C_MOSI)
  (net 160 /SLV4C_MISO)
  (net 161 /SLV4C_SCK)
  (net 162 /SLV4C_MOSI)
  (net 163 /SLV5C_MISO)
  (net 164 /SLV5C_SCK)
  (net 165 /SLV5C_MOSI)
  (net 166 /SLV1D_MISO)
  (net 167 /SLV1D_SCK)
  (net 168 /SLV1D_MOSI)
  (net 169 /SLV3D_MISO)
  (net 170 /SLV3D_SCK)
  (net 171 /SLV3D_MOSI)
  (net 172 /SLV4D_MISO)
  (net 173 /SLV4D_SCK)
  (net 174 /SLV4D_MOSI)
  (net 175 /SLV5D_MISO)
  (net 176 /SLV5D_SCK)
  (net 177 /SLV5D_MOSI)
  (net 178 /MIDI_TX_5V)
  (net 179 /MIDI_RX_5V)
  (net 180 "Net-(R22-Pad2)")
  (net 181 "Net-(R25-Pad1)")
  (net 182 "Net-(R31-Pad2)")
  (net 183 "Net-(R32-Pad2)")
  (net 184 "Net-(R33-Pad2)")
  (net 185 "Net-(R34-Pad2)")
  (net 186 "Net-(R35-Pad2)")
  (net 187 "Net-(U10-Pad1)")
  (net 188 "Net-(U11-Pad1)")
  (net 189 "Net-(J2-Pad35)")
  (net 190 "Net-(P2-Pad1)")
  (net 191 "Net-(P2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /BKLT_A)
    (add_net /BKLT_K)
    (add_net /BOOT0)
    (add_net /BTN_USER)
    (add_net /BTN_~RESET)
    (add_net /CTOUCH_INT)
    (add_net /CTOUCH_WAKE)
    (add_net /I²C3_SCL)
    (add_net /I²C3_SDA)
    (add_net /LCD_B0)
    (add_net /LCD_B1)
    (add_net /LCD_B2)
    (add_net /LCD_B3)
    (add_net /LCD_B4)
    (add_net /LCD_B5)
    (add_net /LCD_CLK)
    (add_net /LCD_DE)
    (add_net /LCD_DISP)
    (add_net /LCD_G0)
    (add_net /LCD_G1)
    (add_net /LCD_G2)
    (add_net /LCD_G3)
    (add_net /LCD_G4)
    (add_net /LCD_G5)
    (add_net /LCD_HSYNC)
    (add_net /LCD_PWM)
    (add_net /LCD_R0)
    (add_net /LCD_R1)
    (add_net /LCD_R2)
    (add_net /LCD_R3)
    (add_net /LCD_R4)
    (add_net /LCD_R5)
    (add_net /LCD_VSYNC)
    (add_net /MIDI_RX)
    (add_net /MIDI_RX_5V)
    (add_net /MIDI_TX)
    (add_net /MIDI_TX_5V)
    (add_net /N/C)
    (add_net /PA1)
    (add_net /PA13)
    (add_net /PA14)
    (add_net /PA15)
    (add_net /PA2)
    (add_net /PA5)
    (add_net /PA7)
    (add_net /PB12)
    (add_net /PB13)
    (add_net /PB14)
    (add_net /PB15)
    (add_net /PB2)
    (add_net /PB3)
    (add_net /PB4)
    (add_net /PB5)
    (add_net /PB6)
    (add_net /PB7)
    (add_net /PC0)
    (add_net /PC1)
    (add_net /PC11)
    (add_net /PC12)
    (add_net /PC13)
    (add_net /PC14)
    (add_net /PC15)
    (add_net /PC2)
    (add_net /PC3)
    (add_net /PC4)
    (add_net /PC5)
    (add_net /PC8)
    (add_net /PD0)
    (add_net /PD1)
    (add_net /PD10)
    (add_net /PD11)
    (add_net /PD12)
    (add_net /PD13)
    (add_net /PD14)
    (add_net /PD15)
    (add_net /PD2)
    (add_net /PD4)
    (add_net /PD5)
    (add_net /PD7)
    (add_net /PD8)
    (add_net /PD9)
    (add_net /PE0)
    (add_net /PE1)
    (add_net /PE10)
    (add_net /PE11)
    (add_net /PE12)
    (add_net /PE13)
    (add_net /PE14)
    (add_net /PE15)
    (add_net /PE2)
    (add_net /PE3)
    (add_net /PE5)
    (add_net /PE6)
    (add_net /PE7)
    (add_net /PE8)
    (add_net /PE9)
    (add_net /PF0)
    (add_net /PF1)
    (add_net /PF11)
    (add_net /PF12)
    (add_net /PF13)
    (add_net /PF14)
    (add_net /PF15)
    (add_net /PF2)
    (add_net /PF3)
    (add_net /PF4)
    (add_net /PF5)
    (add_net /PF7)
    (add_net /PF8)
    (add_net /PF9)
    (add_net /PG0)
    (add_net /PG1)
    (add_net /PG13)
    (add_net /PG14)
    (add_net /PG15)
    (add_net /PG2)
    (add_net /PG4)
    (add_net /PG5)
    (add_net /PG8)
    (add_net /PH0)
    (add_net /PH1)
    (add_net /RTOUCH_XL)
    (add_net /RTOUCH_XR)
    (add_net /RTOUCH_YD)
    (add_net /RTOUCH_YU)
    (add_net /SLV1A_MISO)
    (add_net /SLV1A_MOSI)
    (add_net /SLV1A_SCK)
    (add_net /SLV1B_MISO)
    (add_net /SLV1B_MOSI)
    (add_net /SLV1B_SCK)
    (add_net /SLV1C_MISO)
    (add_net /SLV1C_MOSI)
    (add_net /SLV1C_SCK)
    (add_net /SLV1D_MISO)
    (add_net /SLV1D_MOSI)
    (add_net /SLV1D_SCK)
    (add_net /SLV3A_MISO)
    (add_net /SLV3A_MOSI)
    (add_net /SLV3A_SCK)
    (add_net /SLV3B_MISO)
    (add_net /SLV3B_MOSI)
    (add_net /SLV3B_SCK)
    (add_net /SLV3C_MISO)
    (add_net /SLV3C_MOSI)
    (add_net /SLV3C_SCK)
    (add_net /SLV3D_MISO)
    (add_net /SLV3D_MOSI)
    (add_net /SLV3D_SCK)
    (add_net /SLV4A_MISO)
    (add_net /SLV4A_MOSI)
    (add_net /SLV4A_SCK)
    (add_net /SLV4B_MISO)
    (add_net /SLV4B_MOSI)
    (add_net /SLV4B_SCK)
    (add_net /SLV4C_MISO)
    (add_net /SLV4C_MOSI)
    (add_net /SLV4C_SCK)
    (add_net /SLV4D_MISO)
    (add_net /SLV4D_MOSI)
    (add_net /SLV4D_SCK)
    (add_net /SLV5A_MISO)
    (add_net /SLV5A_MOSI)
    (add_net /SLV5A_SCK)
    (add_net /SLV5B_MISO)
    (add_net /SLV5B_MOSI)
    (add_net /SLV5B_SCK)
    (add_net /SLV5C_MISO)
    (add_net /SLV5C_MOSI)
    (add_net /SLV5C_SCK)
    (add_net /SLV5D_MISO)
    (add_net /SLV5D_MOSI)
    (add_net /SLV5D_SCK)
    (add_net /Vdd)
    (add_net GND)
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad35)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R31-Pad2)")
    (add_net "Net-(R32-Pad2)")
    (add_net "Net-(R33-Pad2)")
    (add_net "Net-(R34-Pad2)")
    (add_net "Net-(R35-Pad2)")
    (add_net "Net-(U10-Pad1)")
    (add_net "Net-(U11-Pad1)")
  )
  (net_class Double ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
  )
  (net_class Triple ""
    (clearance 0.1524)
    (trace_width 0.4572)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 107 78)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 107 82)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 107 74)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 107 44)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 107 53)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 107 58)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 107 67)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 177.1 88.4)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 161 47)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 160 45)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 159 59)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 184 72)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 195 78)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 198 78)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 170.1 85.5)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 181 85)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 185 47)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 128.1 68.6)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 150.4 66)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 150.4 67.4)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 150.4 68.7)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 151.1 73.9)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 153.3 77.2)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 155.8 72.3)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 153.3 73.6)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 149 73)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 151 54)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 151 48)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 152 50)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 150 56)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 150 58)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 203.7 53)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 194.8 56.8)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 185.7 77.5)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 173.3 51)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 212 55)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 208 55)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 205 53)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 202 53)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 139.5 77.725)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 170 65)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 170 75)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 200 60)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 185 70)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 190 51)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Via (layer F.Cu) (tedit 58351F10)
    (at 185 51)
    (fp_text reference REF** (at 0 1.5) (layer F.Fab) hide)
    (fp_text value Via (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Connectors_Molex:Molex_PicoBlade_53047-0410_04x1.25mm_Straight (layer F.Cu) (tedit 58576788)
    (at 210 65.125 270)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0410")
    (tags "connector molex picoblade")
    (fp_text reference P19 (at 1.875 -3.4 270) (layer F.Fab) hide)
    (fp_text value MIDI (at 1.875 -3.25 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 1.25 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 2.5 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 178 /MIDI_TX_5V))
    (pad 4 thru_hole circle (at 3.75 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 179 /MIDI_RX_5V))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0410.wrl
      (at (xyz 0.07381799999999999 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 203.5 70.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.7 -0.1) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 203.5 60.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.7 -0.1 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 142 48 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 154 48 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 154 62 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 176.547 71.0392 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.1608 0.147 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 154 76 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 1.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 142 76 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 1.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 142 62 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 1.8 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 195.75 70)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 3.65 0.2) (layer F.SilkS))
    (fp_text value 1µF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /BKLT_A))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 195.75 73)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 3.65 0) (layer F.SilkS))
    (fp_text value 1µF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /BKLT_A))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 190.5 67 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 3.3 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 /BKLT_K))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 195.75 49)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 3.65 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 195.75 55.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 3.65 -0.1) (layer F.SilkS))
    (fp_text value 1µF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 164 70.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 /BTN_~RESET))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 164 50.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /BTN_USER))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 195.75 67)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 3.25 0) (layer F.SilkS))
    (fp_text value MBR0540 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 4 /BKLT_A))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 57A876D4)
    (at 195.75 75.75)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 3.25 0.05) (layer F.SilkS))
    (fp_text value 24V (at 0.1 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 /BKLT_A))
    (pad 2 smd rect (at 1.055 0) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 /BKLT_K))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-60xx (layer F.Cu) (tedit 574C3AE3)
    (at 189.15 61)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-60xx, 6.0mmx6.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L1 (at 0 -4) (layer F.SilkS))
    (fp_text value 10µH (at 0 4.5) (layer F.Fab))
    (pad 1 smd rect (at -2.35 0) (size 1.6 5.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2.35 0) (size 1.6 5.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-60xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 195.75 64.25 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -3.25 -0.15 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 /LCD_PWM))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 119.5 40.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -0.05 1.5 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 130 /SLV1A_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 105 40.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -0.05 1.8 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 /SLV1B_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 119.5 47.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -0.05 1.5 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 133 /SLV3A_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 105 47.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.05 1.8 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 145 /SLV3B_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 119.5 54.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -0.05 1.7 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 136 /SLV4A_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 105 54.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -0.05 1.8 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 148 /SLV4B_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 119.5 61.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0.05 1.7 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 139 /SLV5A_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 105 61.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.05 1.8 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 /SLV5B_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 136.75 48 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -0.05 1.8 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 /PB7))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 148.75 48 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -0.05 1.8 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 /PE3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 162.25 83.75)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -0.05 2.05) (layer F.SilkS))
    (fp_text value 1M (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /BTN_~RESET))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 181.797 68.2892 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at -2.603 -0.1108 180) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /I²C3_SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 181.797 65.7892 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at -2.603 -0.0108 180) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /I²C3_SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 119.5 71.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0.05 1.7 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 154 /SLV1C_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 105 71.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0.05 1.8 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 166 /SLV1D_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 181.797 70.7892 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at -2.603 -0.0108 180) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 129 /PG2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 119.5 78.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0.05 1.7 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 157 /SLV3C_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 105 78.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0.05 1.8 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 169 /SLV3D_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 181.797 63.2892 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at -2.603 -0.1108 180) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(R22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 119.5 85.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0.05 1.7 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 160 /SLV4C_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 105 85.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 0.05 1.8 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 172 /SLV4D_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 165.75 83.75)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 0.05 2.05) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R25-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 119.5 92.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 0.05 1.7 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 163 /SLV5C_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 105 92.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 0.05 1.8 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 175 /SLV5D_MISO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 162.25 63.75 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 1M (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /BTN_USER))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 148.75 76 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at -0.05 1.8 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 /PC3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 136.75 76 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at -0.05 1.8 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 /PC8))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 165.75 63.75 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(R31-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 171.797 70.7892)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at -2.797 0.0108) (layer F.SilkS))
    (fp_text value 100K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(R32-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 171.797 68.2892)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at -2.797 -0.0892) (layer F.SilkS))
    (fp_text value 100K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(R33-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 171.797 65.7892)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at -2.797 0.0108) (layer F.SilkS))
    (fp_text value 100K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(R34-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 171.797 63.2892)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at -2.797 0.1108) (layer F.SilkS))
    (fp_text value 100K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(R35-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 55360473)
    (at 195.75 61)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 3.25 0) (layer F.SilkS))
    (fp_text value FAN5333BSX (at -0.05 2.35) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /BKLT_K))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 83 /LCD_PWM))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 55360473)
    (at 195.75 52.25 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at -3.25 0.05 180) (layer F.SilkS))
    (fp_text value SPX3819M5-L-3-3 (at -0.05 2.35 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C13-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 139.5 53)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 -4.3) (layer F.SilkS))
    (fp_text value 74HC244 (at 0 4.3) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 59 /PB7))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 130 /SLV1A_MISO))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 131 /SLV1A_SCK))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 133 /SLV3A_MISO))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 134 /SLV3A_SCK))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 136 /SLV4A_MISO))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 137 /SLV4A_SCK))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 139 /SLV5A_MISO))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 140 /SLV5A_SCK))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 86 /PF7))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 85 /PF8))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 /PE2))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 /PE5))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 /PB3))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 73 /PC11))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 96 /PA5))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 /PB4))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 59 /PB7))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 151.5 53)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U4 (at 0 -4.3) (layer F.SilkS))
    (fp_text value 74HC244 (at 0 4.3) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 /PE3))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 142 /SLV1B_MISO))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 143 /SLV1B_SCK))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 145 /SLV3B_MISO))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 146 /SLV3B_SCK))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 148 /SLV4B_MISO))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 149 /SLV4B_SCK))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 151 /SLV5B_MISO))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 152 /SLV5B_SCK))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 86 /PF7))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 85 /PF8))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 /PE2))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 /PE5))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 /PB3))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 73 /PC11))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 96 /PA5))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 /PB4))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 /PE3))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 151.5 67)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U5 (at 0 -4.3) (layer F.SilkS))
    (fp_text value 74HC244 (at 0 4.3) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 59 /PB7))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 97 /PA7))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 144 /SLV1B_MOSI))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 72 /PC12))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 147 /SLV3B_MOSI))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 /PE6))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 150 /SLV4B_MOSI))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 87 /PF9))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 153 /SLV5B_MOSI))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 87 /PF9))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 141 /SLV5A_MOSI))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 /PE6))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 138 /SLV4A_MOSI))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 72 /PC12))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 135 /SLV3A_MOSI))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 97 /PA7))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 132 /SLV1A_MOSI))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 /PE3))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 176.797 67.0392 180)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U6 (at -0.003 2.8392 180) (layer F.SilkS))
    (fp_text value STMPE811QTR (at 0 2.85 180) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /RTOUCH_YD))
    (pad 2 smd oval (at -1.475 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 129 /PG2))
    (pad 3 smd oval (at -1.475 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd oval (at -1.475 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /I²C3_SCL))
    (pad 5 smd oval (at -0.75 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /I²C3_SDA))
    (pad 6 smd oval (at -0.25 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 7 smd oval (at 0.25 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(R22-Pad2)"))
    (pad 8 smd oval (at 0.75 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(R35-Pad2)"))
    (pad 9 smd oval (at 1.475 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(R34-Pad2)"))
    (pad 10 smd oval (at 1.475 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd oval (at 1.475 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(R33-Pad2)"))
    (pad 12 smd oval (at 1.475 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(R32-Pad2)"))
    (pad 13 smd oval (at 0.75 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 /RTOUCH_XR))
    (pad 14 smd oval (at 0.25 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 15 smd oval (at -0.25 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 /RTOUCH_YU))
    (pad 16 smd oval (at -0.75 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /RTOUCH_XL))
    (pad 17 smd rect (at 0.45 0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 151.5 81)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U7 (at 0 -4.3) (layer F.SilkS))
    (fp_text value 74HC244 (at 0 4.3) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 92 /PC3))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 154 /SLV1C_MISO))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 155 /SLV1C_SCK))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 157 /SLV3C_MISO))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 158 /SLV3C_SCK))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 160 /SLV4C_MISO))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 161 /SLV4C_SCK))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 163 /SLV5C_MISO))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 164 /SLV5C_SCK))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 86 /PF7))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 85 /PF8))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 /PE2))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 /PE5))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 /PB3))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 73 /PC11))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 96 /PA5))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 /PB4))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 92 /PC3))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 139.5 81)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U8 (at 0 -4.3) (layer F.SilkS))
    (fp_text value 74HC244 (at 0 4.3) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 79 /PC8))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 166 /SLV1D_MISO))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 167 /SLV1D_SCK))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 169 /SLV3D_MISO))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 170 /SLV3D_SCK))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 172 /SLV4D_MISO))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 173 /SLV4D_SCK))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 175 /SLV5D_MISO))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 176 /SLV5D_SCK))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 86 /PF7))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 85 /PF8))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 /PE2))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 /PE5))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 /PB3))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 73 /PC11))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 96 /PA5))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 /PB4))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 79 /PC8))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 139.5 67)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U9 (at 0 -4.3) (layer F.SilkS))
    (fp_text value 74HC244 (at 0 4.3) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 92 /PC3))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 97 /PA7))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 168 /SLV1D_MOSI))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 72 /PC12))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 171 /SLV3D_MOSI))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 /PE6))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 174 /SLV4D_MOSI))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 87 /PF9))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 177 /SLV5D_MOSI))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 87 /PF9))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 165 /SLV5C_MOSI))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 /PE6))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 162 /SLV4C_MOSI))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 72 /PC12))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 159 /SLV3C_MOSI))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 97 /PA7))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 156 /SLV1C_MOSI))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 79 /PC8))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 55360473)
    (at 203.5 63.5)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U10 (at 3.3 -0.1) (layer F.SilkS))
    (fp_text value SN74LV1T34DCKR (at -0.05 2.35) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(U10-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 78 /MIDI_TX))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 178 /MIDI_TX_5V))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 55360473)
    (at 203.5 67.5 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U11 (at -3.3 0.1 180) (layer F.SilkS))
    (fp_text value SN74LV1T34DCKR (at -0.05 2.35 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(U11-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 179 /MIDI_RX_5V))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 77 /MIDI_RX))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 123 41)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P3 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 1A" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 130 /SLV1A_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 131 /SLV1A_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 132 /SLV1A_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 59 /PB7))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 123 48)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P4 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 3A" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 133 /SLV3A_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 134 /SLV3A_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 135 /SLV3A_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 59 /PB7))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 123 55)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P5 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 4A" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 136 /SLV4A_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 137 /SLV4A_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 138 /SLV4A_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 59 /PB7))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 123 62.5)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P6 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 5A" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 139 /SLV5A_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 140 /SLV5A_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 141 /SLV5A_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 59 /PB7))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 108.5 41)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P7 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 1B" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 142 /SLV1B_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 143 /SLV1B_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 144 /SLV1B_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 53 /PE3))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 108.5 48)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P8 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 3B" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 145 /SLV3B_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 146 /SLV3B_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 147 /SLV3B_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 53 /PE3))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 108.5 55)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P9 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 4B" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 148 /SLV4B_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 149 /SLV4B_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 150 /SLV4B_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 53 /PE3))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 108.5 62.5)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P10 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 5B" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 151 /SLV5B_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 152 /SLV5B_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 153 /SLV5B_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 53 /PE3))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 123 72.5)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P11 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 1C" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 154 /SLV1C_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 155 /SLV1C_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 156 /SLV1C_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 92 /PC3))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 123 79.5)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P12 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 3C" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 157 /SLV3C_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 158 /SLV3C_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 159 /SLV3C_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 92 /PC3))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 123 86.5)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P13 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 4C" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 160 /SLV4C_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 161 /SLV4C_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 162 /SLV4C_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 92 /PC3))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 123 93.5)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P14 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 5C" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 163 /SLV5C_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 164 /SLV5C_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 165 /SLV5C_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 92 /PC3))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 108.5 72.5)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P15 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 1D" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 166 /SLV1D_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 167 /SLV1D_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 168 /SLV1D_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 79 /PC8))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 108.5 79.5)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P16 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 3D" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 169 /SLV3D_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 170 /SLV3D_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 171 /SLV3D_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 79 /PC8))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 108.5 86.5)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P17 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 4D" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 172 /SLV4D_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 173 /SLV4D_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 174 /SLV4D_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 79 /PC8))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Molex_PicoBlade_53047-0610_06x1.25mm_Straight (layer F.Cu) (tedit 58326060)
    (at 108.5 93.5)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0610")
    (tags "connector molex picoblade")
    (fp_text reference P18 (at 3.125 2.5) (layer F.Fab))
    (fp_text value "Slave 5D" (at 3.125 -3.25) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 175 /SLV5D_MISO))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 176 /SLV5D_SCK))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 177 /SLV5D_MOSI))
    (pad 5 thru_hole circle (at 5 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 79 /PC8))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0610.wrl
      (at (xyz 0.123031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Socket_Strip_Reversed_2x32 locked (layer B.Cu) (tedit 582EB49E)
    (at 134.52 91.13)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at -2.52 -0.73 90) (layer B.SilkS))
    (fp_text value CONN_02X32 (at 0 5) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 190 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 191 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 /LCD_PWM))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 84 /N/C))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 85 /PF8))
    (pad 6 thru_hole oval (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 86 /PF7))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 /LCD_DE))
    (pad 8 thru_hole oval (at 7.62 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 87 /PF9))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 88 /PH1))
    (pad 10 thru_hole oval (at 10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 89 /PH0))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 12.7 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /BTN_~RESET))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 90 /PC1))
    (pad 14 thru_hole oval (at 15.24 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 91 /PC0))
    (pad 15 thru_hole oval (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 92 /PC3))
    (pad 16 thru_hole oval (at 17.78 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 93 /PC2))
    (pad 17 thru_hole oval (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 94 /PA1))
    (pad 18 thru_hole oval (at 20.32 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /BTN_USER))
    (pad 19 thru_hole oval (at 22.86 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /LCD_B5))
    (pad 20 thru_hole oval (at 22.86 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 95 /PA2))
    (pad 21 thru_hole oval (at 25.4 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 96 /PA5))
    (pad 22 thru_hole oval (at 25.4 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /LCD_VSYNC))
    (pad 23 thru_hole oval (at 27.94 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 97 /PA7))
    (pad 24 thru_hole oval (at 27.94 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /LCD_G2))
    (pad 25 thru_hole oval (at 30.48 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 98 /PC5))
    (pad 26 thru_hole oval (at 30.48 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 99 /PC4))
    (pad 27 thru_hole oval (at 33.02 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /LCD_R0))
    (pad 28 thru_hole oval (at 33.02 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /LCD_R3))
    (pad 29 thru_hole oval (at 35.56 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 30 thru_hole oval (at 35.56 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 100 /PB2))
    (pad 31 thru_hole oval (at 38.1 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 101 /PF12))
    (pad 32 thru_hole oval (at 38.1 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 102 /PF11))
    (pad 33 thru_hole oval (at 40.64 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 103 /PF14))
    (pad 34 thru_hole oval (at 40.64 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 104 /PF13))
    (pad 35 thru_hole oval (at 43.18 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 105 /PG0))
    (pad 36 thru_hole oval (at 43.18 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 106 /PF15))
    (pad 37 thru_hole oval (at 45.72 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 107 /PE7))
    (pad 38 thru_hole oval (at 45.72 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 108 /PG1))
    (pad 39 thru_hole oval (at 48.26 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 109 /PE9))
    (pad 40 thru_hole oval (at 48.26 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 110 /PE8))
    (pad 41 thru_hole oval (at 50.8 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 111 /PE11))
    (pad 42 thru_hole oval (at 50.8 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 112 /PE10))
    (pad 43 thru_hole oval (at 53.34 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 113 /PE13))
    (pad 44 thru_hole oval (at 53.34 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 114 /PE12))
    (pad 45 thru_hole oval (at 55.88 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 115 /PE15))
    (pad 46 thru_hole oval (at 55.88 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 116 /PE14))
    (pad 47 thru_hole oval (at 58.42 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /LCD_G5))
    (pad 48 thru_hole oval (at 58.42 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /LCD_G4))
    (pad 49 thru_hole oval (at 60.96 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 117 /PB13))
    (pad 50 thru_hole oval (at 60.96 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 118 /PB12))
    (pad 51 thru_hole oval (at 63.5 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 119 /PB15))
    (pad 52 thru_hole oval (at 63.5 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 120 /PB14))
    (pad 53 thru_hole oval (at 66.04 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 121 /PD9))
    (pad 54 thru_hole oval (at 66.04 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 122 /PD8))
    (pad 55 thru_hole oval (at 68.58 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 123 /PD11))
    (pad 56 thru_hole oval (at 68.58 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 124 /PD10))
    (pad 57 thru_hole oval (at 71.12 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 125 /PD13))
    (pad 58 thru_hole oval (at 71.12 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 126 /PD12))
    (pad 59 thru_hole oval (at 73.66 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 127 /PD15))
    (pad 60 thru_hole oval (at 73.66 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 128 /PD14))
    (pad 61 thru_hole oval (at 76.2 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /CTOUCH_INT))
    (pad 62 thru_hole oval (at 76.2 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 129 /PG2))
    (pad 63 thru_hole oval (at 78.74 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 64 thru_hole oval (at 78.74 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x32.wrl
      (at (xyz 1.55 0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:Socket_Strip_Reversed_2x32 locked (layer B.Cu) (tedit 582EB49E)
    (at 134.52 40.33)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at -2.52 -0.73 90) (layer B.SilkS))
    (fp_text value CONN_02X32 (at 0 5) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 /PF4))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 /PF5))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 /PF2))
    (pad 6 thru_hole oval (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 /PF3))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 /PF0))
    (pad 8 thru_hole oval (at 7.62 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 /PF1))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 /PC14))
    (pad 10 thru_hole oval (at 10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 /PC15))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 /PE6))
    (pad 12 thru_hole oval (at 12.7 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /PC13))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /LCD_DISP))
    (pad 14 thru_hole oval (at 15.24 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 /PE5))
    (pad 15 thru_hole oval (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 /PE2))
    (pad 16 thru_hole oval (at 17.78 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 /PE3))
    (pad 17 thru_hole oval (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 /PE0))
    (pad 18 thru_hole oval (at 20.32 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 /PE1))
    (pad 19 thru_hole oval (at 22.86 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /LCD_B0))
    (pad 20 thru_hole oval (at 22.86 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /LCD_B1))
    (pad 21 thru_hole oval (at 25.4 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 /BOOT0))
    (pad 22 thru_hole oval (at 25.4 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 /Vdd))
    (pad 23 thru_hole oval (at 27.94 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 /PB6))
    (pad 24 thru_hole oval (at 27.94 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 /PB7))
    (pad 25 thru_hole oval (at 30.48 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 /PB4))
    (pad 26 thru_hole oval (at 30.48 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 /PB5))
    (pad 27 thru_hole oval (at 33.02 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 /PG15))
    (pad 28 thru_hole oval (at 33.02 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 /PB3))
    (pad 29 thru_hole oval (at 35.56 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 /PG13))
    (pad 30 thru_hole oval (at 35.56 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 /PG14))
    (pad 31 thru_hole oval (at 38.1 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /LCD_B3))
    (pad 32 thru_hole oval (at 38.1 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /LCD_B4))
    (pad 33 thru_hole oval (at 40.64 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /CTOUCH_WAKE))
    (pad 34 thru_hole oval (at 40.64 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /LCD_G3))
    (pad 35 thru_hole oval (at 43.18 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 /PD7))
    (pad 36 thru_hole oval (at 43.18 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /LCD_B2))
    (pad 37 thru_hole oval (at 45.72 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 /PD5))
    (pad 38 thru_hole oval (at 45.72 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 68 /PD4))
    (pad 39 thru_hole oval (at 48.26 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /LCD_G1))
    (pad 40 thru_hole oval (at 48.26 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 /PD2))
    (pad 41 thru_hole oval (at 50.8 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 /PD1))
    (pad 42 thru_hole oval (at 50.8 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 /PD0))
    (pad 43 thru_hole oval (at 53.34 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 /PC12))
    (pad 44 thru_hole oval (at 53.34 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 /PC11))
    (pad 45 thru_hole oval (at 55.88 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /LCD_R2))
    (pad 46 thru_hole oval (at 55.88 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 /PA15))
    (pad 47 thru_hole oval (at 58.42 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 /PA14))
    (pad 48 thru_hole oval (at 58.42 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 /PA13))
    (pad 49 thru_hole oval (at 60.96 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /LCD_R5))
    (pad 50 thru_hole oval (at 60.96 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /LCD_R4))
    (pad 51 thru_hole oval (at 63.5 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 /MIDI_RX))
    (pad 52 thru_hole oval (at 63.5 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 /MIDI_TX))
    (pad 53 thru_hole oval (at 66.04 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /I²C3_SCL))
    (pad 54 thru_hole oval (at 66.04 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /I²C3_SDA))
    (pad 55 thru_hole oval (at 68.58 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 /PC8))
    (pad 56 thru_hole oval (at 68.58 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /LCD_G0))
    (pad 57 thru_hole oval (at 71.12 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /LCD_HSYNC))
    (pad 58 thru_hole oval (at 71.12 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 /PG8))
    (pad 59 thru_hole oval (at 73.66 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /LCD_CLK))
    (pad 60 thru_hole oval (at 73.66 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /LCD_R1))
    (pad 61 thru_hole oval (at 76.2 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 /PG5))
    (pad 62 thru_hole oval (at 76.2 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 /PG4))
    (pad 63 thru_hole oval (at 78.74 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 64 thru_hole oval (at 78.74 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x32.wrl
      (at (xyz 1.55 0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module daughterfeet:XF2L-0625 locked (layer F.Cu) (tedit 58574360)
    (at 201.61 81.6)
    (fp_text reference J1 (at 4.79 -1.1) (layer F.SilkS))
    (fp_text value XF2L-0625-1A (at 0 6.5) (layer F.Fab) hide)
    (pad 0 smd rect (at 2.79 1.7) (size 2 3) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.25 -0.625 180) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at 1.25 -0.625 180) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /I²C3_SCL))
    (pad 2 smd rect (at 0.75 -0.625 180) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /I²C3_SDA))
    (pad 4 smd rect (at -0.25 -0.625 180) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /CTOUCH_WAKE))
    (pad 5 smd rect (at -0.75 -0.625 180) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /CTOUCH_INT))
    (pad 6 smd rect (at -1.25 -0.625 180) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 0 smd rect (at -2.79 1.7) (size 2 3) (layers F.Cu F.Paste F.Mask))
  )
  (module daughterfeet:FH12A-40S (layer F.Cu) (tedit 5857439B)
    (at 183.78 81)
    (fp_text reference J2 (at -11.88 0) (layer F.SilkS))
    (fp_text value FH12A-40S-0.5SH (at 0 3.15) (layer F.Fab))
    (pad 1 smd rect (at 9.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /BKLT_K))
    (pad 2 smd rect (at 9.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /BKLT_A))
    (pad 3 smd rect (at 8.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 8.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at 7.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /LCD_R0))
    (pad 6 smd rect (at 7.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /LCD_R1))
    (pad 7 smd rect (at 6.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /LCD_R2))
    (pad 8 smd rect (at 6.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /LCD_R3))
    (pad 9 smd rect (at 5.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /LCD_R4))
    (pad 10 smd rect (at 5.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /LCD_R5))
    (pad 11 smd rect (at 4.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /LCD_R0))
    (pad 12 smd rect (at 4.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /LCD_R1))
    (pad 13 smd rect (at 3.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /LCD_G0))
    (pad 14 smd rect (at 3.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /LCD_G1))
    (pad 15 smd rect (at 2.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /LCD_G2))
    (pad 16 smd rect (at 2.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /LCD_G3))
    (pad 17 smd rect (at 1.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /LCD_G4))
    (pad 18 smd rect (at 1.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /LCD_G5))
    (pad 19 smd rect (at 0.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /LCD_G0))
    (pad 20 smd rect (at 0.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /LCD_G1))
    (pad 21 smd rect (at -0.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /LCD_B0))
    (pad 22 smd rect (at -0.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /LCD_B1))
    (pad 23 smd rect (at -1.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /LCD_B2))
    (pad 24 smd rect (at -1.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /LCD_B3))
    (pad 25 smd rect (at -2.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /LCD_B4))
    (pad 26 smd rect (at -2.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /LCD_B5))
    (pad 27 smd rect (at -3.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /LCD_B0))
    (pad 28 smd rect (at -3.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /LCD_B1))
    (pad 29 smd rect (at -4.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 30 smd rect (at -4.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /LCD_CLK))
    (pad 31 smd rect (at -5.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 /LCD_DISP))
    (pad 32 smd rect (at -5.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /LCD_HSYNC))
    (pad 33 smd rect (at -6.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /LCD_VSYNC))
    (pad 34 smd rect (at -6.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /LCD_DE))
    (pad 35 smd rect (at -7.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(J2-Pad35)"))
    (pad 36 smd rect (at -7.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 37 smd rect (at -8.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 /RTOUCH_XR))
    (pad 38 smd rect (at -8.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /RTOUCH_YD))
    (pad 39 smd rect (at -9.25 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /RTOUCH_XL))
    (pad 40 smd rect (at -9.75 0 180) (size 0.25 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 /RTOUCH_YU))
    (pad 0 smd rect (at -11.65 3.25) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at 11.65 3.25) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask))
  )
  (module daughterfeet:MVS-logo (layer B.Cu) (tedit 0)
    (at 173.89 67 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module daughterfeet:BARREL_JACK (layer F.Cu) (tedit 58573BCC)
    (at 216 52 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at -2 6 360) (layer F.SilkS) hide)
    (fp_text value BARREL_JACK (at 0 -5.99948 180) (layer F.Fab))
    (fp_text user "5V DC" (at 13.5 0 270) (layer F.SilkS))
    (fp_text user + (at 10.5 -5.014776 270) (layer F.SilkS))
    (fp_text user - (at 10.5 5 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 6.20014 0 180) (size 3.50012 3.50012) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole rect (at 0.20066 0 180) (size 3.50012 3.50012) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole rect (at 3.2004 4.699 180) (size 3.50012 3.50012) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 /PC13))
    (model Connect.3dshapes/JACK_ALIM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.75 0.75 0.75))
      (rotate (xyz 0 0 0))
    )
  )
  (module daughterfeet:WS-TASV (layer F.Cu) (tedit 5857448A)
    (at 164 77 90)
    (fp_text reference SW1 (at 0 -4 90) (layer F.Fab))
    (fp_text value Reset (at 0 4 90) (layer F.SilkS))
    (pad 1 smd rect (at -3.975 -2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /BTN_~RESET))
    (pad 2 smd rect (at -3.975 2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R25-Pad1)"))
    (pad 3 smd rect (at 3.975 -2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /BTN_~RESET))
    (pad 4 smd rect (at 3.975 2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R25-Pad1)"))
    (model Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module daughterfeet:WS-TASV (layer F.Cu) (tedit 5857448A)
    (at 164 57 90)
    (fp_text reference SW2 (at 0 -4 90) (layer F.Fab))
    (fp_text value User (at 0 4 90) (layer F.SilkS))
    (pad 1 smd rect (at -3.975 -2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /BTN_USER))
    (pad 2 smd rect (at -3.975 2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(R31-Pad2)"))
    (pad 3 smd rect (at 3.975 -2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /BTN_USER))
    (pad 4 smd rect (at 3.975 2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(R31-Pad2)"))
    (model Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module daughterfeet:R_0603_HandSoldering_no_paste (layer F.Cu) (tedit 583CB79E)
    (at 190.5 73 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value N/C (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 5 /BKLT_K))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 190.5 70 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 4.3 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /BKLT_K))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 16.9 (width 0.03) (layer Dwgs.User)
    (gr_text "16.8 mm" (at 213.25 111.35) (layer Dwgs.User))
    (feature1 (pts (xy 203.1 85) (xy 203.1 112.7)))
    (feature2 (pts (xy 220 85) (xy 220 112.7)))
    (crossbar (pts (xy 220 110) (xy 203.1 110)))
    (arrow1a (pts (xy 203.1 110) (xy 204.227 110.586421)))
    (arrow1b (pts (xy 203.1 110) (xy 204.227 109.413579)))
    (arrow2a (pts (xy 220 110) (xy 218.873 110.586421)))
    (arrow2b (pts (xy 220 110) (xy 218.873 109.413579)))
  )
  (dimension 26 (width 0.03) (layer Dwgs.User)
    (gr_text "26.0 mm" (at 209.75 116.35) (layer Dwgs.User))
    (feature1 (pts (xy 194 85) (xy 194 117.7)))
    (feature2 (pts (xy 220 85) (xy 220 117.7)))
    (crossbar (pts (xy 220 115) (xy 194 115)))
    (arrow1a (pts (xy 194 115) (xy 195.227 115.586421)))
    (arrow1b (pts (xy 194 115) (xy 195.227 114.413579)))
    (arrow2a (pts (xy 220 115) (xy 218.873 115.586421)))
    (arrow2b (pts (xy 220 115) (xy 218.873 114.413579)))
  )
  (dimension 6.33 (width 0.03) (layer Dwgs.User)
    (gr_text "6.33 mm" (at 226.35 37.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 213.26 40.33) (xy 227.7 40.33)))
    (feature2 (pts (xy 213.26 34) (xy 227.7 34)))
    (crossbar (pts (xy 225 34) (xy 225 40.33)))
    (arrow1a (pts (xy 225 40.33) (xy 225.586 39.373496)))
    (arrow1b (pts (xy 225 40.33) (xy 224.414 39.373496)))
    (arrow2a (pts (xy 225 34) (xy 225.586 35.126504)))
    (arrow2b (pts (xy 225 34) (xy 224.414 35.126504)))
  )
  (dimension 6.74 (width 0.03) (layer Dwgs.User)
    (gr_text "6.74 mm" (at 216.75 27.65) (layer Dwgs.User))
    (feature1 (pts (xy 213.26 40.33) (xy 213.26 26.3)))
    (feature2 (pts (xy 220 40.33) (xy 220 26.3)))
    (crossbar (pts (xy 220 29) (xy 213.26 29)))
    (arrow1a (pts (xy 213.26 29) (xy 214.627 29.586421)))
    (arrow1b (pts (xy 213.26 29) (xy 214.627 28.413579)))
    (arrow2a (pts (xy 220 29) (xy 218.873 29.586421)))
    (arrow2b (pts (xy 220 29) (xy 218.873 28.413579)))
  )
  (dimension 6.33 (width 0.03) (layer Dwgs.User)
    (gr_text "6.33 mm" (at 226.35 96.75 90) (layer Dwgs.User))
    (feature1 (pts (xy 213.26 93.67) (xy 227.7 93.67)))
    (feature2 (pts (xy 213.26 100) (xy 227.7 100)))
    (crossbar (pts (xy 225 100) (xy 225 93.67)))
    (arrow1a (pts (xy 225 93.67) (xy 224.414 94.626504)))
    (arrow1b (pts (xy 225 93.67) (xy 225.586 94.626504)))
    (arrow2a (pts (xy 225 100) (xy 224.414 98.873496)))
    (arrow2b (pts (xy 225 100) (xy 225.586 98.873496)))
  )
  (dimension 6.74 (width 0.03) (layer Dwgs.User)
    (gr_text "6.74 mm" (at 216.75 106.35) (layer Dwgs.User))
    (feature1 (pts (xy 213.26 93.67) (xy 213.26 107.7)))
    (feature2 (pts (xy 220 93.67) (xy 220 107.7)))
    (crossbar (pts (xy 220 105) (xy 213.26 105)))
    (arrow1a (pts (xy 213.26 105) (xy 214.627 105.586421)))
    (arrow1b (pts (xy 213.26 105) (xy 214.627 104.413579)))
    (arrow2a (pts (xy 220 105) (xy 218.873 105.586421)))
    (arrow2b (pts (xy 220 105) (xy 218.873 104.413579)))
  )
  (dimension 66 (width 0.03) (layer Dwgs.User)
    (gr_text "66 mm" (at 88.65 67 270) (layer Dwgs.User))
    (feature1 (pts (xy 100 34) (xy 87.3 34)))
    (feature2 (pts (xy 100 100) (xy 87.3 100)))
    (crossbar (pts (xy 90 100) (xy 90 34)))
    (arrow1a (pts (xy 90 34) (xy 89.4136 35.126504)))
    (arrow1b (pts (xy 90 34) (xy 90.5864 35.126504)))
    (arrow2a (pts (xy 90 100) (xy 89.4136 98.873496)))
    (arrow2b (pts (xy 90 100) (xy 90.5864 98.873496)))
  )
  (gr_arc (start 102 36) (end 102 34) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_line (start 100 98) (end 100 36) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_arc (start 102 98) (end 100 98) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (dimension 120 (width 0.03) (layer Dwgs.User)
    (gr_text "120 mm" (at 160 121.35) (layer Dwgs.User))
    (feature1 (pts (xy 100 100) (xy 100 122.7)))
    (feature2 (pts (xy 220 100) (xy 220 122.7)))
    (crossbar (pts (xy 220 120) (xy 100 120)))
    (arrow1a (pts (xy 100 120) (xy 101.127 120.586421)))
    (arrow1b (pts (xy 100 120) (xy 101.127 119.413579)))
    (arrow2a (pts (xy 220 120) (xy 218.873 120.586421)))
    (arrow2b (pts (xy 220 120) (xy 218.873 119.413579)))
  )
  (gr_line (start 220 36) (end 220 60) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_line (start 216 64) (end 216 70) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_arc (start 218 74) (end 220 74) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_arc (start 218 70) (end 216 70) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_arc (start 218 60) (end 218 62) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_arc (start 218 64) (end 218 62) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_arc (start 218 98) (end 218 100) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_arc (start 218 36) (end 220 36) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_line (start 220 74) (end 220 98) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_line (start 102 34) (end 218 34) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (gr_line (start 218 100) (end 102 100) (angle -90) (layer Edge.Cuts) (width 0.4572))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 99 33) (xy 221 33) (xy 221 101) (xy 99 101)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 98 32) (xy 222 32) (xy 222 102) (xy 98 102)
      )
    )
  )
)
