(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 24)
    (no_connects 2)
    (area 129.476499 95.186499 174.053501 116.903501)
    (thickness 1.6002)
    (drawings 6)
    (tracks 41)
    (zones 0)
    (modules 7)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 2.7 2.7)
    (pad_drill 2.3)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(J4-Pad2)")
  (net 2 "Net-(J4-Pad3)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(T1-Pad4)")
  (net 5 "Net-(T1-Pad12)")
  (net 6 "Net-(J3-Pad1)")
  (net 7 GND)
  (net 8 +5V)
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(T1-Pad12)")
    (add_net "Net-(T1-Pad4)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.5)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net GND)
  )
  (module Connectors:USB_B (layer F.Cu) (tedit 592CDC59)
    (at 165.48 105.41)
    (descr "USB B connector")
    (tags "USB_B USB_DEV")
    (fp_text reference J4 (at 11.05 1.27 90) (layer F.SilkS))
    (fp_text value USB_B (at 4.7 1.27 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 1 "Net-(J4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 4 thru_hole circle (at 2 0 270) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole circle (at 2 2.54 270) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 2 "Net-(J4-Pad3)"))
    (pad 5 thru_hole circle (at 4.7 7.27 270) (size 2.7 2.7) (drill 2.3) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 5 thru_hole circle (at 4.7 -4.73 270) (size 2.7 2.7) (drill 2.3) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes/USB_B.wrl
      (at (xyz 0.18 -0.05 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module smd-footprints:smd-footprints-TSSOP-16 (layer F.Cu) (tedit 200000)
    (at 149.86 106.68)
    (descr "16-LEAD THIN SHRINK SMALL OUTLINE PACKAGE [TSSOP] (RU-16)")
    (tags "16-LEAD THIN SHRINK SMALL OUTLINE PACKAGE [TSSOP] (RU-16)")
    (attr smd)
    (fp_text reference T1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value INA250 (at 0.635 3.81) (layer F.SilkS))
    (pad 1 smd rect (at -2.87274 -2.2733) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -2.87274 -1.62306) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -2.87274 -0.97282) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -2.87274 -0.32258) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(T1-Pad4)"))
    (pad 5 smd rect (at -2.87274 0.32258) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(T1-Pad4)"))
    (pad 6 smd rect (at -2.87274 0.97282) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 7 smd rect (at -2.87274 1.62306) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 8 smd rect (at -2.87274 2.2733) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 9 smd rect (at 2.87274 2.2733 180) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (pad 10 smd rect (at 2.87274 1.62306 180) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 11 smd rect (at 2.87274 0.97282 180) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 12 smd rect (at 2.87274 0.32258 180) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(T1-Pad12)"))
    (pad 13 smd rect (at 2.87274 -0.32258 180) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(T1-Pad12)"))
    (pad 14 smd rect (at 2.87274 -0.97282 180) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 15 smd rect (at 2.87274 -1.62306 180) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 16 smd rect (at 2.87274 -2.2733 180) (size 0.89916 0.34798) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 592CE4C6)
    (at 142.24 107.95 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value 5V (at 0 4.87 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 592CD60B)
    (at 157.48 111.76)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value GND (at 0 2.33) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 592CD5FE)
    (at 157.48 101.6)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Is (at 0 2.33) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors:USB_A (layer F.Cu) (tedit 5543E289)
    (at 136.02 102.62 270)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference J5 (at 0 -2.35 270) (layer F.SilkS))
    (fp_text value USB_A (at 3.84 7.44 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole circle (at 4.57 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 5 thru_hole circle (at 10.16 2.67 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 5 thru_hole circle (at -3.56 2.67 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module logos:mermaid_m (layer F.Cu) (tedit 0)
    (at 139.7 99.06)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text nixies.us (at 143.51 99.06) (layer F.Mask))
  (gr_text GND (at 142.24 110.49) (layer F.SilkS))
  (gr_line (start 173.99 116.84) (end 173.99 95.25) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 129.54 116.84) (end 173.99 116.84) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 129.54 95.25) (end 129.54 116.84) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 173.99 95.25) (end 129.54 95.25) (layer Edge.Cuts) (width 0.127))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.81 96.52) (xy 172.72 96.52) (xy 172.72 115.57) (xy 130.81 115.57)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.43 96.52) (xy 147.32 96.52) (xy 147.32 101.6) (xy 138.43 101.6)
      )
    )
  )
)
