<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="13.97" y1="19.87" x2="48.4175" y2="19.87" width="0" layer="20"/>
<wire x1="48.4175" y1="19.87" x2="48.4175" y2="57.14" width="0" layer="20"/>
<wire x1="48.4175" y1="57.14" x2="13.97" y2="57.14" width="0" layer="20"/>
<wire x1="13.97" y1="57.14" x2="13.97" y2="19.87" width="0" layer="20"/>
<text>Raspberry PI 
Sensor Manager v 1.0</text>
<text>M.Stubbs</text>
<text>5v</text>
<text>3.3</text>
<text>4</text>
<text>GPIO
 17</text>
<text>27</text>
<text>Gnd</text>
<text>23</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="nrf24l011">
<packages>
<package name="NRF24L01">
</package>
</packages>
</library>
<library name="cr1220">
<packages>
<package name="CR1220_HOLDER">
<description>Keystone 500 CR1220 coin battery holder</description>
</package>
</packages>
</library>
<library name="proto">
<description>For making prototype areas on PC boards</description>
<packages>
<package name="PADSTRIP-3H">
<description>Strip of 3 connected pads, .1 inch pitch</description>
</package>
<package name="PADS-5H">
<description>Unconnected row of 5 pads, for connection to plane&lt;br&gt;
Pad 1 left, pad 5 right, 46mil holes, 70mil dia pads</description>
</package>
<package name="PADSTRIP-5H">
<description>Strip of 5 connected pads, .1 inch pitch&lt;br&gt;
Pad 1 left, pad 5 right</description>
</package>
<package name="PADCONN-2H">
<description>2 pads for connection to a signal, .1 inch pitch&lt;br&gt;
Pad 1 left, pad 2 right</description>
</package>
</packages>
</library>
<library name="ms-raspberry-pi">
<description>Raspberry Pi devices by Jason Tribbeck</description>
<packages>
<package name="GPIO-CONNECTOR">
<description>Basic GPIO connector</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="adafruit" package="DIL08" value="DS1307">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="adafruit" package="TC38H" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="NRF24L01" library="nrf24l011" package="NRF24L01" value="NRF24L01">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="cr1220" package="CR1220_HOLDER" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PR1" library="proto" package="PADSTRIP-3H" value="">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="PR2" library="proto" package="PADSTRIP-3H" value="">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="PR3" library="proto" package="PADSTRIP-3H" value="">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="PR4" library="proto" package="PADSTRIP-3H" value="">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P2" library="proto" package="PADS-5H" value="PAD5-HA">
<attribute name="VALSTAT" value="label"/>
</element>
<element name="SK2" library="ms-raspberry-pi" package="GPIO-CONNECTOR" value="PI-GPIO-PTH"/>
<element name="P1" library="proto" package="PADSTRIP-5H" value="PADSTRIP5-HA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P3" library="proto" package="PADSTRIP-5H" value="PADSTRIP5-HA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P4" library="proto" package="PADCONN-2H" value="">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P5" library="proto" package="PADCONN-2H" value="">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P6" library="proto" package="PADCONN-2H" value="">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P7" library="proto" package="PADCONN-2H" value="">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="NRF24L01" pad="1"/>
<contactref element="U1" pad="-"/>
<contactref element="P2" pad="1"/>
<contactref element="P2" pad="2"/>
<contactref element="P2" pad="3"/>
<contactref element="P2" pad="4"/>
<contactref element="P2" pad="5"/>
<contactref element="SK2" pad="6"/>
<contactref element="SK2" pad="9"/>
<contactref element="SK2" pad="25"/>
<contactref element="SK2" pad="25"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="SK2" pad="2"/>
<contactref element="P1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="NRF24L01" pad="4"/>
<contactref element="SK2" pad="24"/>
</signal>
<signal name="N$1">
<contactref element="NRF24L01" pad="6"/>
<contactref element="SK2" pad="19"/>
</signal>
<signal name="N$8">
<contactref element="NRF24L01" pad="5"/>
<contactref element="SK2" pad="23"/>
</signal>
<signal name="N$11">
<contactref element="NRF24L01" pad="7"/>
<contactref element="SK2" pad="21"/>
</signal>
<signal name="+3V3">
<contactref element="C2" pad="1"/>
<contactref element="NRF24L01" pad="2"/>
<contactref element="SK2" pad="17"/>
</signal>
<signal name="VBAT">
<contactref element="IC1" pad="3"/>
<contactref element="U1" pad="+"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="6"/>
<contactref element="SK2" pad="5"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="5"/>
<contactref element="SK2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="NRF24L01" pad="3"/>
<contactref element="SK2" pad="22"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="1"/>
<contactref element="NRF24L01" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="Q1" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="+3V3@1">
<contactref element="SK2" pad="1"/>
<contactref element="P3" pad="5"/>
</signal>
<signal name="N$13">
<contactref element="SK2" pad="7"/>
<contactref element="P4" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="SK2" pad="15"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="SK2" pad="11"/>
<contactref element="P5" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="SK2" pad="13"/>
<contactref element="P6" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="SK2" pad="16"/>
<contactref element="P7" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
