(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 0)
    (no_connects 0)
    (area -6.425001 -20.395001 80.085001 20.395001)
    (thickness 1.6)
    (drawings 9)
    (tracks 0)
    (zones 0)
    (modules 1)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "" (layer F.Cu) (tedit 5AD156F6)
    (at 0 0)
    (fp_text reference MBread00 (at -2.1 0.7 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad brea thru_hole circle (at 0 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 -3.81) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 -6.35) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 -8.89) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 -11.43) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 -13.97) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 -1.27) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 -16.51) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 0 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 2.54 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 5.08 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 7.62 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 10.16 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 12.7 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 15.24 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 17.78 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 20.32 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 22.86 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 25.4 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 27.94 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 30.48 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 33.02 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 35.56 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 38.1 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 40.64 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 43.18 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 45.72 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 48.26 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 50.8 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 53.34 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 55.88 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 58.42 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 60.96 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 63.5 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 66.04 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 68.58 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 71.12 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
    (pad brea thru_hole circle (at 73.66 -19.05) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.000001))
  )
  (gr_text "PCB Breadboard" (at -3.2 0 90) (layer F.SilkS))
  (gr_arc (start -5.35 19.32) (end -5.35 20.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 79.01 19.32) (end 80.01 19.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 79.01 -19.32) (end 79.01 -20.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start -5.35 -19.32) (end -6.35 -19.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.01 -20.32) (end -5.35 -20.32) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.01 19.32) (end 80.01 -19.32) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -5.35 20.32) (end 79.01 20.32) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -6.35 -19.32) (end -6.35 19.32) (layer Edge.Cuts) (width 0.15))
)
