(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 70)
    (zones 0)
    (modules 17)
    (nets 41)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.000051)
    (solder_mask_min_width 0.000102)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 SW1)
  (net 2 3.3V)
  (net 3 SW2)
  (net 4 SW3)
  (net 5 SW4)
  (net 6 SW5)
  (net 7 SW6)
  (net 8 SW7)
  (net 9 SW8)
  (net 10 SW9)
  (net 11 SW10)
  (net 12 SW11)
  (net 13 SW12)
  (net 14 "Net-(U1-Pad3)")
  (net 15 "Net-(U1-Pad8)")
  (net 16 "Net-(U1-Pad13)")
  (net 17 "Net-(U1-Pad16)")
  (net 18 "Net-(U1-Pad17)")
  (net 19 "Net-(U1-Pad19)")
  (net 20 "Net-(U1-Pad20)")
  (net 21 "Net-(U1-Pad23)")
  (net 22 "Net-(U1-Pad28)")
  (net 23 "Net-(U1-Pad29)")
  (net 24 "Net-(U1-Pad30)")
  (net 25 "Net-(U1-Pad31)")
  (net 26 "Net-(U1-Pad32)")
  (net 27 "Net-(U1-Pad33)")
  (net 28 "Net-(U1-Pad34)")
  (net 29 "Net-(U1-Pad35)")
  (net 30 "Net-(U1-Pad37)")
  (net 31 "Net-(U1-Pad38)")
  (net 32 "Net-(U1-Pad39)")
  (net 33 "Net-(U1-Pad40)")
  (net 34 "Net-(U1-Pad18)")
  (net 35 "Net-(U1-Pad1)")
  (net 36 "Net-(U1-Pad2)")
  (net 37 "Net-(U1-Pad4)")
  (net 38 "Net-(U1-Pad5)")
  (net 39 "Net-(U1-Pad6)")
  (net 40 "Net-(U1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3.3V)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net SW1)
    (add_net SW10)
    (add_net SW11)
    (add_net SW12)
    (add_net SW2)
    (add_net SW3)
    (add_net SW4)
    (add_net SW5)
    (add_net SW6)
    (add_net SW7)
    (add_net SW8)
    (add_net SW9)
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 180.975 107.315)
    (fp_text reference MX4 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 5 SW4))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 160.655 107.315)
    (fp_text reference MX3 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 4 SW3))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model "/Volumes/Macintosh HD/Users/mike/Downloads/Cherry+MX+switch+-+reference/files/switch_mx.stl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MCU_RaspberryPi_and_Boards:RPi_Pico_SMD_TH (layer B.Cu) (tedit 606A72CF)
    (at 133.22 85.09 270)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference U1 (at 0 0 90) (layer B.SilkS))
    (fp_text value Pico (at -0.3175 -2.2225 90) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (fp_text user GP1 (at -12.9 21.6 225) (layer B.SilkS) hide)
    (fp_text user GP2 (at -12.9 16.51 225) (layer B.SilkS) hide)
    (fp_text user GP0 (at -12.8 24.13 225) (layer B.SilkS) hide)
    (fp_text user GP3 (at -12.8 13.97 225) (layer B.SilkS) hide)
    (fp_text user GP4 (at -12.8 11.43 225) (layer B.SilkS) hide)
    (fp_text user GP5 (at -12.8 8.89 225) (layer B.SilkS) hide)
    (fp_text user GP6 (at -12.8 3.81 225) (layer B.SilkS) hide)
    (fp_text user GP8 (at -12.8 -1.27 225) (layer B.SilkS) hide)
    (fp_text user GP9 (at -12.8 -3.81 225) (layer B.SilkS) hide)
    (fp_text user GP10 (at -13.054 -8.89 225) (layer B.SilkS) hide)
    (fp_text user GP11 (at -13.2 -11.43 225) (layer B.SilkS) hide)
    (fp_text user GP12 (at -13.2 -13.97 225) (layer B.SilkS) hide)
    (fp_text user GP13 (at -13.054 -16.51 225) (layer B.SilkS) hide)
    (fp_text user GP14 (at -13.1 -21.59 225) (layer B.SilkS) hide)
    (fp_text user GP15 (at -13.054 -24.13 225) (layer B.SilkS) hide)
    (fp_text user GP16 (at 13.054 -24.13 225) (layer B.SilkS) hide)
    (fp_text user GP17 (at 13.054 -21.59 225) (layer B.SilkS) hide)
    (fp_text user GP18 (at 13.054 -16.51 225) (layer B.SilkS) hide)
    (fp_text user GP19 (at 13.054 -13.97 225) (layer B.SilkS) hide)
    (fp_text user GP20 (at 13.054 -11.43 225) (layer B.SilkS) hide)
    (fp_text user GP21 (at 13.054 -8.9 225) (layer B.SilkS) hide)
    (fp_text user GP22 (at 13.054 -3.81 225) (layer B.SilkS) hide)
    (fp_text user RUN (at 13 -1.27 225) (layer B.SilkS) hide)
    (fp_text user GP26 (at 13.054 1.27 225) (layer B.SilkS) hide)
    (fp_text user GP27 (at 13.054 3.8 225) (layer B.SilkS) hide)
    (fp_text user GP28 (at 13.054 9.144 225) (layer B.SilkS) hide)
    (fp_text user ADC_VREF (at 14 12.5 225) (layer B.SilkS) hide)
    (fp_text user 3V3 (at 12.9 13.9 225) (layer B.SilkS) hide)
    (fp_text user 3V3_EN (at 13.7 17.2 225) (layer B.SilkS) hide)
    (fp_text user VSYS (at 13.2 21.59 225) (layer B.SilkS) hide)
    (fp_text user VBUS (at 13.3 24.2 225) (layer B.SilkS) hide)
    (fp_text user GND (at -12.8 19.05 225) (layer B.SilkS) hide)
    (fp_text user GND (at -12.8 6.35 225) (layer B.SilkS) hide)
    (fp_text user GND (at -12.8 -6.35 225) (layer B.SilkS) hide)
    (fp_text user GND (at -12.8 -19.05 225) (layer B.SilkS) hide)
    (fp_text user GND (at 12.8 -19.05 225) (layer B.SilkS) hide)
    (fp_text user GND (at 12.8 -6.35 225) (layer B.SilkS) hide)
    (fp_text user GND (at 12.8 19.05 225) (layer B.SilkS) hide)
    (fp_text user AGND (at 13.054 6.35 225) (layer B.SilkS) hide)
    (fp_text user SWCLK (at -5.7 -26.2 90) (layer B.SilkS) hide)
    (fp_text user SWDIO (at 5.6 -26.2 90) (layer B.SilkS) hide)
    (fp_text user "Copper Keepouts shown on Dwgs layer" (at 0.1 30.2 90) (layer Cmts.User))
    (pad 1 thru_hole oval (at -8.89 24.13 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at -8.89 21.59 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad2)"))
    (pad 3 thru_hole rect (at -8.89 19.05 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at -8.89 16.51 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at -8.89 13.97 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at -8.89 11.43 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad6)"))
    (pad 7 thru_hole oval (at -8.89 8.89 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad7)"))
    (pad 8 thru_hole rect (at -8.89 6.35 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad8)"))
    (pad 9 thru_hole oval (at -8.89 3.81 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 SW7))
    (pad 10 thru_hole oval (at -8.89 1.27 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 SW8))
    (pad 11 thru_hole oval (at -8.89 -1.27 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 SW9))
    (pad 12 thru_hole oval (at -8.89 -3.81 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 SW10))
    (pad 13 thru_hole rect (at -8.89 -6.35 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad13)"))
    (pad 14 thru_hole oval (at -8.89 -8.89 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 SW11))
    (pad 15 thru_hole oval (at -8.89 -11.43 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 SW12))
    (pad 16 thru_hole oval (at -8.89 -13.97 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad16)"))
    (pad 17 thru_hole oval (at -8.89 -16.51 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad17)"))
    (pad 18 thru_hole rect (at -8.89 -19.05 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at -8.89 -21.59 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad19)"))
    (pad 20 thru_hole oval (at -8.89 -24.13 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad20)"))
    (pad 21 thru_hole oval (at 8.89 -24.13 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 SW6))
    (pad 22 thru_hole oval (at 8.89 -21.59 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 SW5))
    (pad 23 thru_hole rect (at 8.89 -19.05 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad23)"))
    (pad 24 thru_hole oval (at 8.89 -16.51 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 SW4))
    (pad 25 thru_hole oval (at 8.89 -13.97 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 SW3))
    (pad 26 thru_hole oval (at 8.89 -11.43 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 SW2))
    (pad 27 thru_hole oval (at 8.89 -8.89 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 SW1))
    (pad 28 thru_hole rect (at 8.89 -6.35 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad28)"))
    (pad 29 thru_hole oval (at 8.89 -3.81 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad29)"))
    (pad 30 thru_hole oval (at 8.89 -1.27 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad30)"))
    (pad 31 thru_hole oval (at 8.89 1.27 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad31)"))
    (pad 32 thru_hole oval (at 8.89 3.81 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad32)"))
    (pad 33 thru_hole rect (at 8.89 6.35 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad33)"))
    (pad 34 thru_hole oval (at 8.89 8.89 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad34)"))
    (pad 35 thru_hole oval (at 8.89 11.43 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad35)"))
    (pad 36 thru_hole oval (at 8.89 13.97 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 3.3V))
    (pad 37 thru_hole oval (at 8.89 16.51 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad37)"))
    (pad 38 thru_hole rect (at 8.89 19.05 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad38)"))
    (pad 39 thru_hole oval (at 8.89 21.59 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad39)"))
    (pad 40 thru_hole oval (at 8.89 24.13 270) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad40)"))
    (pad 1 smd rect (at -8.89 24.13 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 35 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -8.89 21.59 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 36 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -8.89 19.05 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 14 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -8.89 16.51 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 37 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -8.89 13.97 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 38 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -8.89 11.43 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 39 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -8.89 8.89 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 40 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at -8.89 6.35 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 15 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -8.89 3.81 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 8 SW7))
    (pad 10 smd rect (at -8.89 1.27 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 9 SW8))
    (pad 11 smd rect (at -8.89 -1.27 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 10 SW9))
    (pad 12 smd rect (at -8.89 -3.81 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 11 SW10))
    (pad 13 smd rect (at -8.89 -6.35 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 16 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at -8.89 -8.89 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 12 SW11))
    (pad 15 smd rect (at -8.89 -11.43 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 13 SW12))
    (pad 16 smd rect (at -8.89 -13.97 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 17 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at -8.89 -16.51 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 18 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at -8.89 -19.05 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 34 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at -8.89 -21.59 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 19 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at -8.89 -24.13 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers B.Cu B.Mask)
      (net 20 "Net-(U1-Pad20)"))
    (pad 40 smd rect (at 8.89 24.13 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 33 "Net-(U1-Pad40)"))
    (pad 39 smd rect (at 8.89 21.59 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 32 "Net-(U1-Pad39)"))
    (pad 38 smd rect (at 8.89 19.05 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 31 "Net-(U1-Pad38)"))
    (pad 37 smd rect (at 8.89 16.51 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 30 "Net-(U1-Pad37)"))
    (pad 36 smd rect (at 8.89 13.97 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 2 3.3V))
    (pad 35 smd rect (at 8.89 11.43 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 29 "Net-(U1-Pad35)"))
    (pad 34 smd rect (at 8.89 8.89 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 28 "Net-(U1-Pad34)"))
    (pad 33 smd rect (at 8.89 6.35 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 27 "Net-(U1-Pad33)"))
    (pad 32 smd rect (at 8.89 3.81 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 26 "Net-(U1-Pad32)"))
    (pad 31 smd rect (at 8.89 1.27 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 25 "Net-(U1-Pad31)"))
    (pad 30 smd rect (at 8.89 -1.27 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 24 "Net-(U1-Pad30)"))
    (pad 29 smd rect (at 8.89 -3.81 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 23 "Net-(U1-Pad29)"))
    (pad 28 smd rect (at 8.89 -6.35 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 22 "Net-(U1-Pad28)"))
    (pad 27 smd rect (at 8.89 -8.89 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 1 SW1))
    (pad 26 smd rect (at 8.89 -11.43 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 3 SW2))
    (pad 25 smd rect (at 8.89 -13.97 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 4 SW3))
    (pad 24 smd rect (at 8.89 -16.51 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 5 SW4))
    (pad 23 smd rect (at 8.89 -19.05 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 21 "Net-(U1-Pad23)"))
    (pad 22 smd rect (at 8.89 -21.59 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 6 SW5))
    (pad 21 smd rect (at 8.89 -24.13 270) (size 3.5 1.7) (drill (offset 0.9 0)) (layers B.Cu B.Mask)
      (net 7 SW6))
    (pad "" np_thru_hole oval (at -2.725 24 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 2.725 24 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -2.425 20.97 270) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 2.425 20.97 270) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (model "/Volumes/Macintosh HD/Users/mike/Downloads/KiCad-RP-Pico-main/RP-Pico Libraries/Pico.wrl"
      (offset (xyz -10.5 -25.5 0))
      (scale (xyz 10 10 10))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 120.015 107.315)
    (fp_text reference MX1 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 1 SW1))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 140.335 107.315)
    (fp_text reference MX2 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 3 SW2))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 160.655 85.09)
    (fp_text reference MX5 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 6 SW5))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 180.975 85.09)
    (fp_text reference MX6 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 7 SW6))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 120.015 85.09)
    (fp_text reference MX7 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 8 SW7))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 140.335 85.09)
    (fp_text reference MX8 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 9 SW8))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 120.015 63.5)
    (fp_text reference MX9 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 10 SW9))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 140.335 63.5)
    (fp_text reference MX10 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375 180) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 11 SW10))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 160.655 63.5)
    (fp_text reference MX11 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 12 SW11))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
  )
  (module MX_Only:MXOnly-1U (layer F.Cu) (tedit 5AC9901D)
    (at 180.975 63.5)
    (fp_text reference MX12 (at 0 3.175 180) (layer Dwgs.User))
    (fp_text value MX-NoLED (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 13 SW12))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 2 3.3V))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 190.5 53.975)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 190.5 116.205)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 109.22 53.975)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 109.22 116.205)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0.635) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (dimension 86.362335 (width 0.15) (layer Dwgs.User)
    (gr_text "86.362 mm" (at 149.962765 127.958433 0.4212849042) (layer Dwgs.User))
    (feature1 (pts (xy 193.04 113.665) (xy 193.137517 126.927373)))
    (feature2 (pts (xy 106.68 114.3) (xy 106.777517 127.562373)))
    (crossbar (pts (xy 106.773206 126.975968) (xy 193.133206 126.340968)))
    (arrow1a (pts (xy 193.133206 126.340968) (xy 192.011044 126.935656)))
    (arrow1b (pts (xy 193.133206 126.340968) (xy 192.002421 125.762846)))
    (arrow2a (pts (xy 106.773206 126.975968) (xy 107.903991 127.55409)))
    (arrow2b (pts (xy 106.773206 126.975968) (xy 107.895368 126.38128)))
  )
  (dimension 67.31 (width 0.15) (layer Dwgs.User)
    (gr_text "67.310 mm" (at 199.42 85.09 270) (layer Dwgs.User))
    (feature1 (pts (xy 187.325 118.745) (xy 198.706421 118.745)))
    (feature2 (pts (xy 187.325 51.435) (xy 198.706421 51.435)))
    (crossbar (pts (xy 198.12 51.435) (xy 198.12 118.745)))
    (arrow1a (pts (xy 198.12 118.745) (xy 197.533579 117.618496)))
    (arrow1b (pts (xy 198.12 118.745) (xy 198.706421 117.618496)))
    (arrow2a (pts (xy 198.12 51.435) (xy 197.533579 52.561504)))
    (arrow2b (pts (xy 198.12 51.435) (xy 198.706421 52.561504)))
  )
  (dimension 19.05 (width 0.15) (layer Dwgs.User)
    (gr_text "19.050 mm" (at 120.015 46.325) (layer Dwgs.User))
    (feature1 (pts (xy 129.54 53.975) (xy 129.54 47.038579)))
    (feature2 (pts (xy 110.49 53.975) (xy 110.49 47.038579)))
    (crossbar (pts (xy 110.49 47.625) (xy 129.54 47.625)))
    (arrow1a (pts (xy 129.54 47.625) (xy 128.413496 48.211421)))
    (arrow1b (pts (xy 129.54 47.625) (xy 128.413496 47.038579)))
    (arrow2a (pts (xy 110.49 47.625) (xy 111.616504 48.211421)))
    (arrow2b (pts (xy 110.49 47.625) (xy 111.616504 47.038579)))
  )
  (gr_text "MK Keyboard v1" (at 108.585 104.775 270) (layer F.SilkS))
  (gr_line (start 106.68 118.745) (end 106.68 51.435) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 193.04 118.745) (end 106.68 118.745) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 193.04 51.435) (end 193.04 118.745) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.68 51.435) (end 193.04 51.435) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name 3.3V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.025 126.365) (xy 102.87 125.73) (xy 101.6 44.45) (xy 199.39 44.45)
      )
    )
  )
)
