<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="17.77" x2="0" y2="0.635" width="0" layer="20"/>
<wire x1="0" y1="0.635" x2="0.635" y2="0" width="0" layer="20"/>
<wire x1="0.635" y1="0" x2="13.9575" y2="0" width="0" layer="20"/>
<wire x1="13.9575" y1="0" x2="14.5925" y2="0.635" width="0" layer="20"/>
<wire x1="14.5925" y1="0.635" x2="14.5925" y2="17.77" width="0" layer="20"/>
<wire x1="14.5925" y1="17.77" x2="13.9575" y2="18.405" width="0" layer="20"/>
<wire x1="13.9575" y1="18.405" x2="0.635" y2="18.405" width="0" layer="20"/>
<wire x1="0.635" y1="18.405" x2="0" y2="17.77" width="0" layer="20"/>
<text>general
assembly</text>
<text>power filtering</text>
<text>ABUSE OF POWER 
COMES AS NO 
SURPRISE </text>
</plain>
<libraries>
<library name="supply pins">
<packages>
<package name="PAD3">
<description>&lt;b&gt;Square Pad (w/label) - 80mil Diameter, 47mil Drill&lt;b&gt;</description>
</package>
<package name="PAD1">
<description>&lt;b&gt;Round Pad (w/label) - 80mil Diameter, 47mil Drill&lt;b&gt;</description>
</package>
</packages>
</library>
<library name="caps-elec">
<packages>
<package name="0632">
<description>0.1" (2.54mm) spacing</description>
</package>
</packages>
</library>
<library name="caps-film">
<packages>
<package name="0.2&quot;.SML">
<description>0.2" (5.08mm) spacing
&lt;p&gt;
&lt;b&gt; 
10pf - 180n&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistors">
<packages>
<package name="0.3&quot;.B">
<description>0.3"  (7.62mm) lead spacing, 1/4W (flat)</description>
</package>
</packages>
</library>
<library name="diodes">
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
<package name="3MM_IO">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="jacks">
<packages>
<package name="DC_TS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="+9V" library="supply pins" package="PAD3" value="PADS.SQR_LBL">
<attribute name="NAME"/>
</element>
<element name="C1" library="caps-elec" package="0632" value="47uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="caps-film" package="0.2&quot;.SML" value="100n">
<attribute name="NAME"/>
</element>
<element name="CLR" library="resistors" package="0.3&quot;.B" value="4k7">
<attribute name="NAME"/>
</element>
<element name="D1" library="diodes" package="DO41-3" value="1N5817">
<attribute name="NAME"/>
</element>
<element name="J1" library="jacks" package="DC_TS" value="DC_TS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="L" library="supply pins" package="PAD1" value="PADS.RND_LBL">
<attribute name="NAME"/>
</element>
<element name="LED" library="diodes" package="3MM_IO" value="LED.1">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="GND" library="supply pins" package="PAD1" value="PADS.RND_LBL">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N9V">
<contactref element="D1" pad="C"/>
<contactref element="CLR" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="+9V" pad="1"/>
</signal>
<signal name="L">
<contactref element="LED" pad="K"/>
<contactref element="L" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="PWR"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="CLR" pad="1"/>
<contactref element="LED" pad="A"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="GND"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="GND" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
