(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 1093)
    (no_connects 0)
    (area 17.724999 19.55 259.414286 188.9525)
    (thickness 1.6)
    (drawings 84)
    (tracks 5156)
    (zones 0)
    (modules 421)
    (nets 339)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.14)
    (trace_clearance 0.13)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.14)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.51)
    (via_drill 0.254)
    (via_min_size 0.51)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9 0.9)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 247 186)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000007)
      (usegerberextensions false)
      (gerberprecision 5)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory output/))
  )
  (net 0 "")
  (net 1 5V)
  (net 2 GND)
  (net 3 "Net-(C13-Pad2)")
  (net 4 "Net-(C16-Pad1)")
  (net 5 "Net-(C17-Pad1)")
  (net 6 "Net-(C18-Pad1)")
  (net 7 3V3A)
  (net 8 VDDOUT)
  (net 9 3V3)
  (net 10 "Net-(C24-Pad1)")
  (net 11 "Net-(C25-Pad1)")
  (net 12 Vbatt)
  (net 13 "Net-(C30-Pad1)")
  (net 14 "Net-(C31-Pad1)")
  (net 15 "Net-(C34-Pad1)")
  (net 16 "Net-(C34-Pad2)")
  (net 17 "Net-(C35-Pad1)")
  (net 18 "Net-(C35-Pad2)")
  (net 19 "Net-(C38-Pad1)")
  (net 20 "Net-(C41-Pad1)")
  (net 21 "Net-(C44-Pad1)")
  (net 22 "Net-(C107-Pad1)")
  (net 23 "Net-(C48-Pad1)")
  (net 24 "Net-(C57-Pad1)")
  (net 25 ~EXTRST)
  (net 26 "Net-(C59-Pad1)")
  (net 27 "Net-(C61-Pad1)")
  (net 28 "Net-(C61-Pad2)")
  (net 29 Vsolar)
  (net 30 5Vsec)
  (net 31 "Net-(C65-Pad1)")
  (net 32 "Net-(C67-Pad1)")
  (net 33 "Net-(C72-Pad1)")
  (net 34 "Net-(C78-Pad1)")
  (net 35 "Net-(C82-Pad1)")
  (net 36 "Net-(C86-Pad1)")
  (net 37 "Net-(C96-Pad1)")
  (net 38 "Net-(C96-Pad2)")
  (net 39 NRSTB)
  (net 40 AD1)
  (net 41 AD0)
  (net 42 AD2)
  (net 43 AD3)
  (net 44 AD5)
  (net 45 AD4)
  (net 46 AD6)
  (net 47 AD7)
  (net 48 AD9)
  (net 49 AD8)
  (net 50 AD12)
  (net 51 AD11)
  (net 52 AD13)
  (net 53 AD10)
  (net 54 AD14)
  (net 55 AD15)
  (net 56 AD17)
  (net 57 AD16)
  (net 58 AD18)
  (net 59 AD19)
  (net 60 AD21)
  (net 61 AD20)
  (net 62 AD22)
  (net 63 BTTN)
  (net 64 "Net-(D1-Pad2)")
  (net 65 "Net-(D2-Pad2)")
  (net 66 "Net-(D3-Pad2)")
  (net 67 "Net-(D7-Pad1)")
  (net 68 Vcharge)
  (net 69 "Net-(D12-Pad1)")
  (net 70 "Net-(D13-Pad2)")
  (net 71 "Net-(D16-Pad1)")
  (net 72 ODO-X1)
  (net 73 ODO-X2)
  (net 74 RXD1)
  (net 75 RXD2)
  (net 76 FB-A)
  (net 77 FB-C)
  (net 78 FB-B)
  (net 79 FB-D)
  (net 80 RXD3)
  (net 81 ODO-A1)
  (net 82 ODO-B1)
  (net 83 ODO-C1)
  (net 84 ODO-D1)
  (net 85 ODO-A2)
  (net 86 ODO-B2)
  (net 87 ODO-C2)
  (net 88 ODO-D2)
  (net 89 "Net-(D35-Pad1)")
  (net 90 "Net-(D35-Pad2)")
  (net 91 "Net-(D36-Pad1)")
  (net 92 "Net-(D36-Pad2)")
  (net 93 "Net-(D37-Pad1)")
  (net 94 "Net-(D37-Pad2)")
  (net 95 "Net-(D38-Pad1)")
  (net 96 "Net-(D38-Pad2)")
  (net 97 ADC-RSV)
  (net 98 "Net-(C8-Pad1)")
  (net 99 "Net-(F1-Pad2)")
  (net 100 "Net-(F2-Pad1)")
  (net 101 DIR-D)
  (net 102 "Net-(JP1-Pad2)")
  (net 103 DIR-C)
  (net 104 "Net-(JP2-Pad2)")
  (net 105 "Net-(JP3-Pad2)")
  (net 106 PWM-D)
  (net 107 "Net-(JP4-Pad2)")
  (net 108 PWM-C)
  (net 109 "Net-(JP5-Pad1)")
  (net 110 "Net-(JP7-Pad2)")
  (net 111 LAWN-1R)
  (net 112 "Net-(P2-Pad3)")
  (net 113 "Net-(P2-Pad4)")
  (net 114 "Net-(P3-Pad3)")
  (net 115 "Net-(P3-Pad4)")
  (net 116 "Net-(P4-Pad3)")
  (net 117 "Net-(P4-Pad4)")
  (net 118 "Net-(P5-Pad3)")
  (net 119 "Net-(P5-Pad4)")
  (net 120 "Net-(P6-Pad3)")
  (net 121 "Net-(P6-Pad4)")
  (net 122 "Net-(P7-Pad3)")
  (net 123 "Net-(P7-Pad4)")
  (net 124 SHDN-RLY)
  (net 125 LAWN-2R)
  (net 126 "Net-(P11-Pad3)")
  (net 127 "Net-(P11-Pad4)")
  (net 128 "Net-(P12-Pad3)")
  (net 129 "Net-(P12-Pad4)")
  (net 130 "Net-(P13-Pad3)")
  (net 131 "Net-(P14-Pad3)")
  (net 132 "Net-(P15-Pad3)")
  (net 133 "Net-(P16-Pad3)")
  (net 134 "Net-(P17-Pad3)")
  (net 135 "Net-(P18-Pad3)")
  (net 136 "Net-(P19-Pad3)")
  (net 137 VUSB)
  (net 138 D-)
  (net 139 D+)
  (net 140 UOTGID)
  (net 141 S-END)
  (net 142 "Net-(P26-Pad2)")
  (net 143 "Net-(P27-Pad2)")
  (net 144 "Net-(P28-Pad1)")
  (net 145 "Net-(P28-Pad3)")
  (net 146 "Net-(P30-Pad2)")
  (net 147 CANRX)
  (net 148 CANTX)
  (net 149 "Net-(P34-Pad2)")
  (net 150 "Net-(P35-Pad1)")
  (net 151 "Net-(P35-Pad2)")
  (net 152 "Net-(P35-Pad3)")
  (net 153 "Net-(P35-Pad4)")
  (net 154 "Net-(P36-Pad1)")
  (net 155 "Net-(P36-Pad2)")
  (net 156 "Net-(P36-Pad3)")
  (net 157 "Net-(P36-Pad4)")
  (net 158 "Net-(P39-Pad1)")
  (net 159 "Net-(P39-Pad3)")
  (net 160 "Net-(P39-Pad5)")
  (net 161 "Net-(P39-Pad7)")
  (net 162 "Net-(P39-Pad8)")
  (net 163 "Net-(P39-Pad10)")
  (net 164 TXD0)
  (net 165 EXTERASE)
  (net 166 RXD0)
  (net 167 "Net-(P39-Pad16)")
  (net 168 "Net-(P39-Pad17)")
  (net 169 "Net-(P39-Pad18)")
  (net 170 "Net-(P39-Pad19)")
  (net 171 "Net-(P39-Pad21)")
  (net 172 "Net-(P39-Pad22)")
  (net 173 "Net-(P39-Pad23)")
  (net 174 "Net-(P39-Pad24)")
  (net 175 "Net-(P39-Pad26)")
  (net 176 DAC0)
  (net 177 DAC1)
  (net 178 "Net-(P45-Pad3)")
  (net 179 "Net-(P45-Pad4)")
  (net 180 SDA2)
  (net 181 SCL2)
  (net 182 "Net-(P49-Pad2)")
  (net 183 "Net-(P50-Pad3)")
  (net 184 "Net-(P50-Pad4)")
  (net 185 SPI0_MISO)
  (net 186 SPI0_MOSI)
  (net 187 SPI0_SPCK)
  (net 188 SPI0_CS1)
  (net 189 "Net-(P52-Pad3)")
  (net 190 "Net-(P52-Pad4)")
  (net 191 SPI0_CS2)
  (net 192 TEMP-1)
  (net 193 TEMP-2)
  (net 194 "Net-(P58-Pad3)")
  (net 195 "Net-(P58-Pad4)")
  (net 196 "Net-(P59-Pad3)")
  (net 197 "Net-(P59-Pad4)")
  (net 198 "Net-(P64-Pad3)")
  (net 199 "Net-(P65-Pad3)")
  (net 200 "Net-(P65-Pad4)")
  (net 201 "Net-(P67-Pad5)")
  (net 202 "Net-(P67-Pad6)")
  (net 203 "Net-(P68-Pad5)")
  (net 204 "Net-(P68-Pad6)")
  (net 205 "Net-(P69-Pad5)")
  (net 206 "Net-(P69-Pad6)")
  (net 207 "Net-(P70-Pad5)")
  (net 208 "Net-(P70-Pad6)")
  (net 209 "Net-(P71-Pad1)")
  (net 210 "Net-(P72-Pad1)")
  (net 211 "Net-(P73-Pad1)")
  (net 212 "Net-(P76-Pad1)")
  (net 213 "Net-(P77-Pad1)")
  (net 214 "Net-(P78-Pad1)")
  (net 215 "Net-(Q1-Pad1)")
  (net 216 FWUP)
  (net 217 "Net-(Q2-Pad1)")
  (net 218 "Net-(Q3-Pad1)")
  (net 219 LAWN-1S)
  (net 220 ECHO-1)
  (net 221 TRIG-1)
  (net 222 ECHO-2)
  (net 223 TRIG-2)
  (net 224 ECHO-3)
  (net 225 TRIG-3)
  (net 226 ECHO-4)
  (net 227 TRIG-4)
  (net 228 ECHO-5)
  (net 229 TRIG-5)
  (net 230 ECHO-6)
  (net 231 TRIG-6)
  (net 232 "Net-(C8-Pad2)")
  (net 233 LAWN-2S)
  (net 234 BMP-L1)
  (net 235 BMP-L2)
  (net 236 DROP-1)
  (net 237 DROP-2)
  (net 238 RAIN)
  (net 239 PERI-1)
  (net 240 PERI-2)
  (net 241 PERI-3)
  (net 242 PERI-4)
  (net 243 BMP-R1)
  (net 244 BMP-R2)
  (net 245 "Net-(R45-Pad2)")
  (net 246 "Net-(R46-Pad2)")
  (net 247 "Net-(R47-Pad2)")
  (net 248 "Net-(R50-Pad2)")
  (net 249 SVbatt)
  (net 250 "Net-(R54-Pad1)")
  (net 251 "Net-(R55-Pad1)")
  (net 252 PGOOD)
  (net 253 "Net-(R57-Pad1)")
  (net 254 SV3V3)
  (net 255 SV5V)
  (net 256 PWM-Boost)
  (net 257 PWM-CC)
  (net 258 SVsolar)
  (net 259 "Net-(R70-Pad2)")
  (net 260 SVin)
  (net 261 "Net-(R74-Pad2)")
  (net 262 SVcharge)
  (net 263 TXD1)
  (net 264 "Net-(R84-Pad2)")
  (net 265 SCL)
  (net 266 SDA)
  (net 267 TXD2)
  (net 268 "Net-(R93-Pad2)")
  (net 269 SV5Vsec)
  (net 270 TXD3)
  (net 271 PWM-E)
  (net 272 PWM-A)
  (net 273 PWM-B)
  (net 274 PWM-F)
  (net 275 PWM-G)
  (net 276 PWM-H)
  (net 277 "Net-(RL1-Pad14)")
  (net 278 "Net-(RL1-Pad12)")
  (net 279 SItotal)
  (net 280 SIcharge)
  (net 281 SImow)
  (net 282 LED1)
  (net 283 LED2)
  (net 284 LED3)
  (net 285 BEEPER)
  (net 286 "Net-(U1-Pad5)")
  (net 287 ACTIVITY)
  (net 288 PWM-FAN)
  (net 289 SHUTDOWN)
  (net 290 "Net-(U1-Pad14)")
  (net 291 "Net-(U4-Pad6)")
  (net 292 "Net-(U4-Pad7)")
  (net 293 "Net-(U4-Pad8)")
  (net 294 "Net-(U4-Pad9)")
  (net 295 "Net-(U5-Pad6)")
  (net 296 "Net-(U5-Pad7)")
  (net 297 "Net-(U5-Pad9)")
  (net 298 ~SFLT-1)
  (net 299 ~SFLT-2)
  (net 300 "Net-(U6-Pad28)")
  (net 301 "Net-(U6-Pad29)")
  (net 302 "Net-(U6-Pad30)")
  (net 303 "Net-(U6-Pad31)")
  (net 304 "Net-(U6-Pad46)")
  (net 305 "Net-(U6-Pad50)")
  (net 306 "Net-(U6-Pad51)")
  (net 307 ~SF~-D)
  (net 308 MOT-EN2)
  (net 309 ~SF~-C)
  (net 310 DIR-B)
  (net 311 ~SF~-B)
  (net 312 MOT-EN1)
  (net 313 DIR-A)
  (net 314 ~SF~-A)
  (net 315 "Net-(U6-Pad128)")
  (net 316 STEP)
  (net 317 SDIR)
  (net 318 ~SRST)
  (net 319 "Net-(U7-Pad7)")
  (net 320 "Net-(U7-Pad2)")
  (net 321 "Net-(U8-Pad6)")
  (net 322 "Net-(U8-Pad7)")
  (net 323 "Net-(U8-Pad12)")
  (net 324 "Net-(U8-Pad13)")
  (net 325 "Net-(U15-Pad6)")
  (net 326 "Net-(U15-Pad7)")
  (net 327 "Net-(U15-Pad8)")
  (net 328 "Net-(U15-Pad9)")
  (net 329 "Net-(X4-Pad1)")
  (net 330 "Net-(X4-Pad2)")
  (net 331 "Net-(X4-Pad4)")
  (net 332 "Net-(X5-Pad1)")
  (net 333 "Net-(X5-Pad2)")
  (net 334 "Net-(X5-Pad4)")
  (net 335 "Net-(D7-Pad2)")
  (net 336 "Net-(JP6-Pad1)")
  (net 337 "Net-(JP6-Pad3)")
  (net 338 "Net-(C110-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.13)
    (trace_width 0.14)
    (via_dia 0.51)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ACTIVITY)
    (add_net AD0)
    (add_net AD1)
    (add_net AD10)
    (add_net AD11)
    (add_net AD12)
    (add_net AD13)
    (add_net AD14)
    (add_net AD15)
    (add_net AD16)
    (add_net AD17)
    (add_net AD18)
    (add_net AD19)
    (add_net AD2)
    (add_net AD20)
    (add_net AD21)
    (add_net AD22)
    (add_net AD3)
    (add_net AD4)
    (add_net AD5)
    (add_net AD6)
    (add_net AD7)
    (add_net AD8)
    (add_net AD9)
    (add_net ADC-RSV)
    (add_net BEEPER)
    (add_net BMP-L1)
    (add_net BMP-L2)
    (add_net BMP-R1)
    (add_net BMP-R2)
    (add_net BTTN)
    (add_net CANRX)
    (add_net CANTX)
    (add_net D+)
    (add_net D-)
    (add_net DAC0)
    (add_net DAC1)
    (add_net DIR-A)
    (add_net DIR-B)
    (add_net DIR-C)
    (add_net DIR-D)
    (add_net DROP-1)
    (add_net DROP-2)
    (add_net ECHO-1)
    (add_net ECHO-2)
    (add_net ECHO-3)
    (add_net ECHO-4)
    (add_net ECHO-5)
    (add_net ECHO-6)
    (add_net EXTERASE)
    (add_net FB-A)
    (add_net FB-B)
    (add_net FB-C)
    (add_net FB-D)
    (add_net FWUP)
    (add_net LAWN-1R)
    (add_net LAWN-1S)
    (add_net LAWN-2R)
    (add_net LAWN-2S)
    (add_net LED1)
    (add_net LED2)
    (add_net LED3)
    (add_net MOT-EN1)
    (add_net MOT-EN2)
    (add_net NRSTB)
    (add_net "Net-(C107-Pad1)")
    (add_net "Net-(C110-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C34-Pad2)")
    (add_net "Net-(C35-Pad2)")
    (add_net "Net-(C38-Pad1)")
    (add_net "Net-(C41-Pad1)")
    (add_net "Net-(C44-Pad1)")
    (add_net "Net-(C57-Pad1)")
    (add_net "Net-(C72-Pad1)")
    (add_net "Net-(C78-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C86-Pad1)")
    (add_net "Net-(C96-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(F2-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(JP4-Pad2)")
    (add_net "Net-(JP5-Pad1)")
    (add_net "Net-(JP6-Pad1)")
    (add_net "Net-(JP6-Pad3)")
    (add_net "Net-(JP7-Pad2)")
    (add_net "Net-(P11-Pad3)")
    (add_net "Net-(P11-Pad4)")
    (add_net "Net-(P12-Pad3)")
    (add_net "Net-(P12-Pad4)")
    (add_net "Net-(P13-Pad3)")
    (add_net "Net-(P14-Pad3)")
    (add_net "Net-(P15-Pad3)")
    (add_net "Net-(P16-Pad3)")
    (add_net "Net-(P17-Pad3)")
    (add_net "Net-(P18-Pad3)")
    (add_net "Net-(P19-Pad3)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P26-Pad2)")
    (add_net "Net-(P27-Pad2)")
    (add_net "Net-(P28-Pad1)")
    (add_net "Net-(P28-Pad3)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P30-Pad2)")
    (add_net "Net-(P34-Pad2)")
    (add_net "Net-(P39-Pad1)")
    (add_net "Net-(P39-Pad10)")
    (add_net "Net-(P39-Pad16)")
    (add_net "Net-(P39-Pad17)")
    (add_net "Net-(P39-Pad18)")
    (add_net "Net-(P39-Pad19)")
    (add_net "Net-(P39-Pad21)")
    (add_net "Net-(P39-Pad22)")
    (add_net "Net-(P39-Pad23)")
    (add_net "Net-(P39-Pad24)")
    (add_net "Net-(P39-Pad26)")
    (add_net "Net-(P39-Pad3)")
    (add_net "Net-(P39-Pad5)")
    (add_net "Net-(P39-Pad7)")
    (add_net "Net-(P39-Pad8)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P45-Pad3)")
    (add_net "Net-(P45-Pad4)")
    (add_net "Net-(P49-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P5-Pad4)")
    (add_net "Net-(P50-Pad3)")
    (add_net "Net-(P50-Pad4)")
    (add_net "Net-(P52-Pad3)")
    (add_net "Net-(P52-Pad4)")
    (add_net "Net-(P58-Pad3)")
    (add_net "Net-(P58-Pad4)")
    (add_net "Net-(P59-Pad3)")
    (add_net "Net-(P59-Pad4)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P64-Pad3)")
    (add_net "Net-(P65-Pad3)")
    (add_net "Net-(P65-Pad4)")
    (add_net "Net-(P67-Pad5)")
    (add_net "Net-(P67-Pad6)")
    (add_net "Net-(P68-Pad5)")
    (add_net "Net-(P68-Pad6)")
    (add_net "Net-(P69-Pad5)")
    (add_net "Net-(P69-Pad6)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(P70-Pad5)")
    (add_net "Net-(P70-Pad6)")
    (add_net "Net-(P71-Pad1)")
    (add_net "Net-(P72-Pad1)")
    (add_net "Net-(P73-Pad1)")
    (add_net "Net-(P76-Pad1)")
    (add_net "Net-(P77-Pad1)")
    (add_net "Net-(P78-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(R45-Pad2)")
    (add_net "Net-(R46-Pad2)")
    (add_net "Net-(R47-Pad2)")
    (add_net "Net-(R50-Pad2)")
    (add_net "Net-(R54-Pad1)")
    (add_net "Net-(R55-Pad1)")
    (add_net "Net-(R57-Pad1)")
    (add_net "Net-(R70-Pad2)")
    (add_net "Net-(R74-Pad2)")
    (add_net "Net-(R84-Pad2)")
    (add_net "Net-(R93-Pad2)")
    (add_net "Net-(RL1-Pad12)")
    (add_net "Net-(RL1-Pad14)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U15-Pad6)")
    (add_net "Net-(U15-Pad7)")
    (add_net "Net-(U15-Pad8)")
    (add_net "Net-(U15-Pad9)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U4-Pad9)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad9)")
    (add_net "Net-(U6-Pad128)")
    (add_net "Net-(U6-Pad28)")
    (add_net "Net-(U6-Pad29)")
    (add_net "Net-(U6-Pad30)")
    (add_net "Net-(U6-Pad31)")
    (add_net "Net-(U6-Pad46)")
    (add_net "Net-(U6-Pad50)")
    (add_net "Net-(U6-Pad51)")
    (add_net "Net-(U7-Pad2)")
    (add_net "Net-(U7-Pad7)")
    (add_net "Net-(U8-Pad12)")
    (add_net "Net-(U8-Pad13)")
    (add_net "Net-(U8-Pad6)")
    (add_net "Net-(U8-Pad7)")
    (add_net "Net-(X4-Pad1)")
    (add_net "Net-(X4-Pad2)")
    (add_net "Net-(X4-Pad4)")
    (add_net "Net-(X5-Pad1)")
    (add_net "Net-(X5-Pad2)")
    (add_net "Net-(X5-Pad4)")
    (add_net ODO-A1)
    (add_net ODO-A2)
    (add_net ODO-B1)
    (add_net ODO-B2)
    (add_net ODO-C1)
    (add_net ODO-C2)
    (add_net ODO-D1)
    (add_net ODO-D2)
    (add_net ODO-X1)
    (add_net ODO-X2)
    (add_net PERI-1)
    (add_net PERI-2)
    (add_net PERI-3)
    (add_net PERI-4)
    (add_net PGOOD)
    (add_net PWM-A)
    (add_net PWM-B)
    (add_net PWM-Boost)
    (add_net PWM-C)
    (add_net PWM-CC)
    (add_net PWM-D)
    (add_net PWM-E)
    (add_net PWM-F)
    (add_net PWM-FAN)
    (add_net PWM-G)
    (add_net PWM-H)
    (add_net RAIN)
    (add_net RXD0)
    (add_net RXD1)
    (add_net RXD2)
    (add_net RXD3)
    (add_net S-END)
    (add_net SCL)
    (add_net SCL2)
    (add_net SDA)
    (add_net SDA2)
    (add_net SDIR)
    (add_net SHDN-RLY)
    (add_net SHUTDOWN)
    (add_net SIcharge)
    (add_net SImow)
    (add_net SItotal)
    (add_net SPI0_CS1)
    (add_net SPI0_CS2)
    (add_net SPI0_MISO)
    (add_net SPI0_MOSI)
    (add_net SPI0_SPCK)
    (add_net STEP)
    (add_net SV3V3)
    (add_net SV5V)
    (add_net SV5Vsec)
    (add_net SVbatt)
    (add_net SVcharge)
    (add_net SVin)
    (add_net SVsolar)
    (add_net TEMP-1)
    (add_net TEMP-2)
    (add_net TRIG-1)
    (add_net TRIG-2)
    (add_net TRIG-3)
    (add_net TRIG-4)
    (add_net TRIG-5)
    (add_net TRIG-6)
    (add_net TXD0)
    (add_net TXD1)
    (add_net TXD2)
    (add_net TXD3)
    (add_net UOTGID)
    (add_net VDDOUT)
    (add_net VUSB)
    (add_net ~EXTRST)
    (add_net ~SFLT-1)
    (add_net ~SFLT-2)
    (add_net ~SF~-A)
    (add_net ~SF~-B)
    (add_net ~SF~-C)
    (add_net ~SF~-D)
    (add_net ~SRST)
  )
  (net_class "High power" ""
    (clearance 0.3)
    (trace_width 3)
    (via_dia 0.51)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Mid-power ""
    (clearance 0.13)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D35-Pad1)")
    (add_net "Net-(D35-Pad2)")
    (add_net "Net-(D36-Pad1)")
    (add_net "Net-(D36-Pad2)")
    (add_net "Net-(D37-Pad1)")
    (add_net "Net-(D37-Pad2)")
    (add_net "Net-(D38-Pad1)")
    (add_net "Net-(D38-Pad2)")
    (add_net "Net-(P35-Pad1)")
    (add_net "Net-(P35-Pad2)")
    (add_net "Net-(P35-Pad3)")
    (add_net "Net-(P35-Pad4)")
    (add_net "Net-(P36-Pad1)")
    (add_net "Net-(P36-Pad2)")
    (add_net "Net-(P36-Pad3)")
    (add_net "Net-(P36-Pad4)")
  )
  (net_class Small-power ""
    (clearance 0.13)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3V3)
    (add_net 3V3A)
    (add_net 5V)
    (add_net 5Vsec)
    (add_net GND)
    (add_net "Net-(C34-Pad1)")
    (add_net "Net-(C35-Pad1)")
    (add_net "Net-(C48-Pad1)")
    (add_net "Net-(C59-Pad1)")
    (add_net "Net-(C61-Pad1)")
    (add_net "Net-(C61-Pad2)")
    (add_net "Net-(C65-Pad1)")
    (add_net "Net-(C67-Pad1)")
    (add_net "Net-(C82-Pad1)")
    (add_net "Net-(C96-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net Vbatt)
    (add_net Vcharge)
    (add_net Vsolar)
  )
  (module Connect:USB_Micro-B_10103594-0001LF (layer F.Cu) (tedit 5964F017)
    (at 169 181.6)
    (descr "Micro USB Type B 10103594-0001LF")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P20 (at -1.5 -4.625) (layer F.Fab))
    (fp_text value USB_OTG (at 7 3) (layer F.SilkS))
    (pad 1 smd rect (at -1.3 -1.5 90) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 137 VUSB))
    (pad 2 smd rect (at -0.65 -1.5 90) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 138 D-))
    (pad 3 smd rect (at -0.0009 -1.5 90) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 139 D+))
    (pad 4 smd rect (at 0.65 -1.5 90) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 140 UOTGID))
    (pad 5 smd rect (at 1.3 -1.5 90) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.425 -1.625 90) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.425 -1.625 90) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.725 1.375 90) (size 1.7 1.2) (drill oval 1.2 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.725 1.375 90) (size 1.7 1.2) (drill oval 1.2 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 smd rect (at -0.9625 1.625 90) (size 2.5 1.425) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.9625 1.625 90) (size 2.5 1.425) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module AC-Stuff:Drill-3.5mm (layer F.Cu) (tedit 5964ECDF)
    (at 128 84)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Drill-3.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module AC-Stuff:Drill-3.5mm (layer F.Cu) (tedit 5964ECDF)
    (at 135 166)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Drill-3.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module AC-Stuff:Drill-3.5mm (layer F.Cu) (tedit 5964ECDF)
    (at 242 181)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Drill-3.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module AC-Stuff:Drill-3.5mm (layer F.Cu) (tedit 5964ECDF)
    (at 242 34)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Drill-3.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module AC-Stuff:Drill-3.5mm (layer F.Cu) (tedit 5964ECDF)
    (at 104 34)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Drill-3.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module AC-Stuff:Drill-3.5mm (layer F.Cu) (tedit 5964ECDF)
    (at 24 181)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Drill-3.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module AC-Stuff:Drill-3.5mm (layer F.Cu) (tedit 5964ECDF)
    (at 24 94)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Drill-3.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F36E)
    (at 195.27 142.14 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P16 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value PERI-1 (at -0.02 -2.53 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 133 "Net-(P16-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 54EA0684)
    (at 121 105 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P47 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value I2C2-L3V3 (at 0 -3.1 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 180 SDA2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 181 SCL2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5964DF62)
    (at 43.3 42.24 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D16 (at 0 -2 180) (layer F.Fab))
    (fp_text value PMEG6010 (at 0 1.34 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 68 Vcharge))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FFCA4)
    (at 181.8 113.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C66 (at 0 -1.9) (layer F.Fab))
    (fp_text value 0.1uF (at 0 1.2) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59603C27)
    (at 154 110)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C24 (at 0 -2.1) (layer F.Fab))
    (fp_text value 18pF (at -2 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE77D)
    (at 191.21 92.52)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -2.1) (layer F.Fab))
    (fp_text value 0.1uF (at -2.1 0.025 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE780)
    (at 191.21 86.92)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -2.1) (layer F.Fab))
    (fp_text value 0.1uF (at -2.175 0.05 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE990)
    (at 41.4 148.6 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 -2.1 90) (layer F.Fab))
    (fp_text value 0.1uF (at 3.1 0.05 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE98D)
    (at 41.4 152.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value 0.1uF (at 2.95 -0.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE9C8)
    (at 41.4 138.6 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 -2.1 90) (layer F.Fab))
    (fp_text value 0.1uF (at -2.95 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE8CF)
    (at 72.4 130.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value 100pF (at 0.2 -1.6 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE8FE)
    (at 59.4 141.6 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 -2.1 180) (layer F.Fab))
    (fp_text value 100pF (at 3.25 0.1 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE8D2)
    (at 72.4 126.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value 0.1uF (at -0.05 -1.6 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE900)
    (at 63.4 141.6 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 0 -2.1 180) (layer F.Fab))
    (fp_text value 0.1uF (at 0.15 -1.6 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59611DF3)
    (at 154.4 96.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0 -2 270) (layer F.Fab))
    (fp_text value 0.1uF (at 0.07 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FEF6D)
    (at 154 108.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 0.1uF (at -2 0.4 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59611DF1)
    (at 154.4 97.8)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 0 -1.9) (layer F.Fab))
    (fp_text value 0.1uF (at 0.16 1.17) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59603C1E)
    (at 154.2 116 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C25 (at 0 -2.1 180) (layer F.Fab))
    (fp_text value 18pF (at 2.2 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C25-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeX_EIA-7343 (layer F.Cu) (tedit 595FE896)
    (at 95.2 113.8)
    (descr TantalC_SizeX_EIA-7343)
    (fp_text reference C27 (at 0 -2.7305) (layer F.Fab))
    (fp_text value 47uF (at 0 -0.2 180) (layer F.SilkS))
    (pad 1 smd rect (at 2.99974 0) (size 2.55016 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at -2.99974 0) (size 2.55016 3.79984) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeX_EIA-7343.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE8B3)
    (at 94.8 134 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C28 (at 0 -2.1 180) (layer F.Fab))
    (fp_text value 0.1uF (at 0.15 -1.55 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FE890)
    (at 95.8 117 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C29 (at 0 -2.1 180) (layer F.Fab))
    (fp_text value 0.1uF (at -0.1 -1.6 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5960048A)
    (at 157.05 119.25 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C30 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value 18pF (at -0.05 -1.45 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FF4BC)
    (at 162.9 115.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at 0 -1.9) (layer F.Fab))
    (fp_text value 0.1uF (at -0.1 -1.35) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FF4B9)
    (at 165.9 115.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C33 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 0.1uF (at -0.1 1.15 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FE8AE)
    (at 105.4 130.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at -0.1 -1.15 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C34-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FE88B)
    (at 107.2 112.8 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at 0.1 -1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C35-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C35-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FE8BD)
    (at 97 124.5 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C36 (at 0 -2.3 270) (layer F.Fab))
    (fp_text value 10uF (at 0.05 -0.25 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FE871)
    (at 98.6 107.4 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C37 (at 0 -2.3 270) (layer F.Fab))
    (fp_text value 10uF (at 0.1 -0.2 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FF4D3)
    (at 161.425 120.2 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C38 (at 0 -2.1 90) (layer F.Fab))
    (fp_text value 9pF (at -0.2 -1.425 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C38-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeC_EIA-6032_Reflow (layer F.Cu) (tedit 595FE8C5)
    (at 93.7 124.2 270)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow")
    (tags "Tantal Capacitor Size-C EIA-6032 Reflow")
    (attr smd)
    (fp_text reference C39 (at -0.1 -2.7 270) (layer F.Fab))
    (fp_text value 220uF (at 0 -0.05 360) (layer F.SilkS))
    (pad 2 smd rect (at 2.47 0 270) (size 2.37 2.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.47 0 270) (size 2.37 2.23) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeC_EIA-6032_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_Reflow (layer F.Cu) (tedit 595FE87A)
    (at 94.8 107 270)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow")
    (tags "Tantal Capacitor Size-D EIA-7343 Reflow")
    (attr smd)
    (fp_text reference C40 (at -0.20066 -3.29946 270) (layer F.Fab))
    (fp_text value 100uF (at 0 -0.1 360) (layer F.SilkS))
    (pad 2 smd rect (at 3.12 0 270) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.12 0 270) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5960018F)
    (at 168.025 120.225 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C41 (at 0 -2.1 90) (layer F.Fab))
    (fp_text value 9pF (at -1.475 1.275 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C41-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AC-Stuff:Supercap-Vishay_E3_22_24 (layer F.Cu) (tedit 595FED33)
    (at 150.2 132.2)
    (descr "SuperCapacitor Vishay SMF E3 case 22x24x2.5")
    (tags "supercapacitor 22x24")
    (attr smd)
    (fp_text reference C44 (at 0 -2.3) (layer F.Fab))
    (fp_text value 15F (at 13.644999 11.035) (layer F.SilkS))
    (pad 2 smd rect (at -1 6) (size 6 4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 26 6) (size 6 4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C44-Pad1)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59600181)
    (at 168.2 116.2 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C45 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at -2.4 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C107-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FF9BE)
    (at 168.6 86.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C46 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 0.1uF (at 0.2 -1.4 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FF9BC)
    (at 170.2 86.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C47 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 0.1uF (at 0.2 1.4 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FEA56)
    (at 116.2 111)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C48 (at 0 -2.3) (layer F.Fab))
    (fp_text value 10uF (at 0 -0.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C48-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FEA5A)
    (at 115.8 113.4)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C51 (at 0 -2.1) (layer F.Fab))
    (fp_text value 0.1uF (at -3 0.05) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C48-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5960017C)
    (at 169.77 116.21 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C52 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at -2.41 -0.03 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59600166)
    (at 171.4 116.2 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C53 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at -2.4 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FE85C)
    (at 76.2 93.95)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C54 (at 0 -2.3) (layer F.Fab))
    (fp_text value 10uF (at 0 -0.05 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59600171)
    (at 172.95 116.21 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C55 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at -2.41 -0.05 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FF4AF)
    (at 174.6 116.2 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C56 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at -0.4 -1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 596004B0)
    (at 175.85 122.7 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C57 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at -0.05 -1.05 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C57-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 ~EXTRST))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FE8A5)
    (at 108 121.2 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C58 (at 0 -2.3 270) (layer F.Fab))
    (fp_text value 10uF (at 0 -0.2 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FE844)
    (at 74.3 82.8)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C59 (at 0 -2.3) (layer F.Fab))
    (fp_text value 10uF (at -0.1 -0.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C59-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeC_EIA-6032_Reflow (layer F.Cu) (tedit 595FE8A3)
    (at 111.4 121 270)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow")
    (tags "Tantal Capacitor Size-C EIA-6032 Reflow")
    (attr smd)
    (fp_text reference C60 (at -0.1 -2.7 270) (layer F.Fab))
    (fp_text value 220uF (at 0 -0.1 360) (layer F.SilkS))
    (pad 2 smd rect (at 2.47 0 270) (size 2.37 2.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.47 0 270) (size 2.37 2.23) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeC_EIA-6032_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FE83D)
    (at 79.35 82.8 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C61 (at 0 -2.3 180) (layer F.Fab))
    (fp_text value 10uF (at 0.05 0.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C61-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C61-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeX_EIA-7343 (layer F.Cu) (tedit 595FEA13)
    (at 44.35 65 270)
    (descr TantalC_SizeX_EIA-7343)
    (fp_text reference C62 (at 0 -2.7305 270) (layer F.Fab))
    (fp_text value 47uF (at 0.1 -0.2 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.99974 0 270) (size 2.55016 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 29 Vsolar))
    (pad 2 smd rect (at -2.99974 0 270) (size 2.55016 3.79984) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeX_EIA-7343.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FEA1C)
    (at 47.85 66.6 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C63 (at 0 -2.3 90) (layer F.Fab))
    (fp_text value 10uF (at 0 0.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 29 Vsolar))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FE839)
    (at 82.95 79.3 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C65 (at 0 -2.3 90) (layer F.Fab))
    (fp_text value 10uF (at -0.1 0.15 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C65-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C61-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeX_EIA-7343 (layer F.Cu) (tedit 595FE7FE)
    (at 74.1 65.9 270)
    (descr TantalC_SizeX_EIA-7343)
    (fp_text reference C67 (at 0 -2.7305 270) (layer F.Fab))
    (fp_text value 47uF (at -0.1 0.3 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.99974 0 270) (size 2.55016 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C67-Pad1)"))
    (pad 2 smd rect (at -2.99974 0 270) (size 2.55016 3.79984) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeX_EIA-7343.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FF9A7)
    (at 182.8 92.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C69 (at 0 -1.9) (layer F.Fab))
    (fp_text value 0.1uF (at 2.6 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FF9AB)
    (at 182.8 94.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C70 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at -0.2 -1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FE803)
    (at 77.5 65.8 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C71 (at 0 -2.3 90) (layer F.Fab))
    (fp_text value 10uF (at 0 0.1 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C67-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FFCAB)
    (at 182.8 108.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C72 (at 0 -1.9) (layer F.Fab))
    (fp_text value 0.1uF (at 2.6 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C72-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5964D42A)
    (at 188.2 114.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C76 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10uF (at 0.01 -1.09) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5964D42E)
    (at 194.2 114.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C77 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 10uF (at -0.08 1.06 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeX_EIA-7343 (layer F.Cu) (tedit 595FEA40)
    (at 101.7 70)
    (descr TantalC_SizeX_EIA-7343)
    (fp_text reference C78 (at 0 -2.7305) (layer F.Fab))
    (fp_text value 47uF (at 0.15 0.15 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.99974 0) (size 2.55016 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C78-Pad1)"))
    (pad 2 smd rect (at -2.99974 0) (size 2.55016 3.79984) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeX_EIA-7343.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_Reflow (layer F.Cu) (tedit 5960E881)
    (at 113.9 156 270)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow")
    (tags "Tantal Capacitor Size-D EIA-7343 Reflow")
    (attr smd)
    (fp_text reference C81 (at -0.20066 -3.29946 270) (layer F.Fab))
    (fp_text value 100uF (at 0 -0.05 360) (layer F.SilkS))
    (pad 2 smd rect (at 3.12 0 270) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.12 0 270) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FF216)
    (at 124.925 121.3)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C82 (at 0 -2.3) (layer F.Fab))
    (fp_text value 10uF (at -0.025 -0.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C82-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FF224)
    (at 124.425 123.5)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C83 (at 0 -2.1) (layer F.Fab))
    (fp_text value 0.1uF (at -0.825 1.1) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C82-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5960371F)
    (at 226.6 149.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C85 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 0.1uF (at 2.66 0.35 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FEA38)
    (at 112.4 61.6)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C86 (at 0 -2.1) (layer F.Fab))
    (fp_text value 100pF (at 0.2 1.4) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C86-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FEA36)
    (at 108.4 61.6)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C87 (at 0 -2.1) (layer F.Fab))
    (fp_text value 0.1uF (at -0.05 1.35) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59603724)
    (at 228.2 147.4 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C88 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at 0.04 -1.22 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FED1D)
    (at 177.5 53.1 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C89 (at 0 -2.3 270) (layer F.Fab))
    (fp_text value 10uF (at 0.04 -0.21 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeX_EIA-7343 (layer F.Cu) (tedit 595FEA69)
    (at 101.875 177.025)
    (descr TantalC_SizeX_EIA-7343)
    (fp_text reference C90 (at 0 -2.7305) (layer F.Fab))
    (fp_text value 47uF (at 0.125 -0.225 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.99974 0) (size 2.55016 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at -2.99974 0) (size 2.55016 3.79984) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeX_EIA-7343.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FED22)
    (at 177.5 61.4 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C91 (at 0 -2.3 90) (layer F.Fab))
    (fp_text value 10uF (at 0 0.16 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeC_EIA-6032_Reflow (layer F.Cu) (tedit 5964D40A)
    (at 187.5 75.5 180)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow")
    (tags "Tantal Capacitor Size-C EIA-6032 Reflow")
    (attr smd)
    (fp_text reference C92 (at -0.1 -2.7 180) (layer F.Fab))
    (fp_text value 220uF (at -0.16 0.09 270) (layer F.SilkS))
    (pad 2 smd rect (at 2.47 0 180) (size 2.37 2.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.47 0 180) (size 2.37 2.23) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeC_EIA-6032_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 213.11 151.35 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C93 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value 0.1uF (at 0 2.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FEA6B)
    (at 102.675 180.225 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C94 (at 0 -2.1 180) (layer F.Fab))
    (fp_text value 0.1uF (at 3.025 -0.175 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5960379A)
    (at 190.555 148.91)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C95 (at 0 -1.9) (layer F.Fab))
    (fp_text value 0.1uF (at -1.755 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FEA70)
    (at 114.375 175.825 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C96 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 0.1uF (at 1.075 1.075 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C96-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C96-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FEA78)
    (at 105.875 170.425 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C97 (at 0 -2.3 270) (layer F.Fab))
    (fp_text value 10uF (at 0.125 -0.175 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FED19)
    (at 185.3 53 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C98 (at 0 -2.3 270) (layer F.Fab))
    (fp_text value 10uF (at -0.11 -0.15 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FED13)
    (at 185.3 61.4 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C99 (at 0 -2.3 90) (layer F.Fab))
    (fp_text value 10uF (at -0.04 0.16 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_Reflow (layer F.Cu) (tedit 595FEA7D)
    (at 102.075 170.025 270)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow")
    (tags "Tantal Capacitor Size-D EIA-7343 Reflow")
    (attr smd)
    (fp_text reference C100 (at -0.20066 -3.29946 270) (layer F.Fab))
    (fp_text value 100uF (at -0.025 -0.075 360) (layer F.SilkS))
    (pad 2 smd rect (at 3.12 0 270) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.12 0 270) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 213.14 147.58 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C101 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value 0.1uF (at 0 2.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 222 73 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C103 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value 0.1uF (at 0 2.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 595FF0F0)
    (at 222 121 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C104 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value 0.1uF (at -0.1 1.6 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59603BD6)
    (at 165.6 124.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C107 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value 10nF (at -0.02 -0.31 360) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C107-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 39 NRSTB))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FE979)
    (at 54.125 146 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C108 (at 0 -2.3 270) (layer F.Fab))
    (fp_text value 10uF (at 0.2 -1.825 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FE975)
    (at 54.525 166.7 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C109 (at 0 -2.3 270) (layer F.Fab))
    (fp_text value 10uF (at 0.1 -1.875 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer F.Cu) (tedit 5964D41F)
    (at 186.62 102.74)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference CP1 (at 0 -2.1) (layer F.Fab))
    (fp_text value 10nF (at 0.55 -1.6) (layer F.SilkS))
    (pad 1 smd rect (at -0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 40 AD1))
    (pad 8 smd rect (at 0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 41 AD0))
    (pad 6 smd rect (at 0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 42 AD2))
    (pad 5 smd rect (at 0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 43 AD3))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer F.Cu) (tedit 5964D41A)
    (at 186.62 105.34)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference CP2 (at 0 -2.1) (layer F.Fab))
    (fp_text value 10nF (at 0.83 1.52) (layer F.SilkS))
    (pad 1 smd rect (at -0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 44 AD5))
    (pad 8 smd rect (at 0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 45 AD4))
    (pad 6 smd rect (at 0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 46 AD6))
    (pad 5 smd rect (at 0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 47 AD7))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer F.Cu) (tedit 595FF1E5)
    (at 129.4 111.2)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference CP3 (at 0 -2.1) (layer F.Fab))
    (fp_text value 10nF (at -1.3 -0.4 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 48 AD9))
    (pad 8 smd rect (at 0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 49 AD8))
    (pad 6 smd rect (at 0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 50 AD12))
    (pad 5 smd rect (at 0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 51 AD11))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer F.Cu) (tedit 595FF1E0)
    (at 129.4 113.8)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference CP4 (at 0 -2.1) (layer F.Fab))
    (fp_text value 10nF (at -1.3 -0.5 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 52 AD13))
    (pad 8 smd rect (at 0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 53 AD10))
    (pad 6 smd rect (at 0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 54 AD14))
    (pad 5 smd rect (at 0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 55 AD15))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer F.Cu) (tedit 595FF1ED)
    (at 129.4 116.8)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference CP5 (at 0 -2.1) (layer F.Fab))
    (fp_text value 10nF (at -1.3 0.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 56 AD17))
    (pad 8 smd rect (at 0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 57 AD16))
    (pad 6 smd rect (at 0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 58 AD18))
    (pad 5 smd rect (at 0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 59 AD19))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer F.Cu) (tedit 595FF1F2)
    (at 129.4 119.2)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference CP6 (at 0 -2.1) (layer F.Fab))
    (fp_text value 10nF (at -1.3 0.3 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 60 AD21))
    (pad 8 smd rect (at 0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 61 AD20))
    (pad 6 smd rect (at 0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 62 AD22))
    (pad 5 smd rect (at 0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 63 BTTN))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5964D883)
    (at 77.14 97.45)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 1.91 3.06) (layer F.Fab))
    (fp_text value POWER-5V (at 1.23 2.91) (layer F.SilkS))
    (fp_text user K (at -1.69 1.74) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5964F26A)
    (at 53.6 129.5 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 1.91 3.06 270) (layer F.Fab))
    (fp_text value POWER-BATT (at 2.5 -6.8 360) (layer F.SilkS))
    (fp_text user K (at -1.69 1.74 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5964F256)
    (at 131.3 47.6 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.91 3.06 270) (layer F.Fab))
    (fp_text value POWER-3V3 (at 0.89 7.12 360) (layer F.SilkS))
    (fp_text user K (at -1.69 1.74 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 43.4 138.6 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference D4 (at 0 -1.8 90) (layer F.Fab))
    (fp_text value "TVS 24V" (at 0 1.8 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 595FE988)
    (at 43.4 152.6 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference D5 (at 0 -1.8 270) (layer F.Fab))
    (fp_text value "TVS 24V" (at 0.1 -1.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 595FE97D)
    (at 43.4 148.6 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference D6 (at 0 -1.8 90) (layer F.Fab))
    (fp_text value "TVS 24V" (at 0.05 1.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5964F01D)
    (at 184.83 179.9 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D7 (at 1.91 3.06 180) (layer F.Fab))
    (fp_text value ACTIVITY (at 1.3 -2.9 180) (layer F.SilkS))
    (fp_text user K (at -1.69 1.74 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 335 "Net-(D7-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 595FEA16)
    (at 41.4 63.6 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference D8 (at 0 -1.8 90) (layer F.Fab))
    (fp_text value "TVS 36V" (at -2.65 -0.25 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 Vsolar))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59601A00)
    (at 28.95 46.25)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference D9 (at 0 -1.8) (layer F.Fab))
    (fp_text value "TVS 36V" (at -0.1 -0.85) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 Vcharge))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9)
    (at 179.4 145.4 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D10 (at 0 -2 90) (layer F.Fab))
    (fp_text value PMEG6010 (at 0 2.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C107-Pad1)"))
    (pad 2 smd rect (at 1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C44-Pad1)"))
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 59600964)
    (at 179.4 150 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D11 (at 0 -2 270) (layer F.Fab))
    (fp_text value PMEG6010 (at -5 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C107-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
  )
  (module Diodes_SMD:SMB_Standard (layer F.Cu) (tedit 595FE810)
    (at 71.6 72.9 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D13 (at 0.05 -3.1 180) (layer F.Fab))
    (fp_text value SD2114S040S8R0 (at 1.5 -2.9 180) (layer F.SilkS))
    (fp_text user K (at -3.25 3.3 180) (layer F.Fab))
    (fp_text user A (at 3 3.2 180) (layer F.Fab))
    (pad 1 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C67-Pad1)"))
    (pad 2 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D13-Pad2)"))
    (model Diodes_SMD.3dshapes/SMB_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 595FE81A)
    (at 77.95 73.8 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D14 (at 0 -2 180) (layer F.Fab))
    (fp_text value PMEG6010 (at -0.25 1.3 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C65-Pad1)"))
    (pad 2 smd rect (at 1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C67-Pad1)"))
  )
  (module Diodes_SMD:SMB_Standard (layer F.Cu) (tedit 5964DF5D)
    (at 36.4 37.6 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D15 (at 0.05 -3.1 180) (layer F.Fab))
    (fp_text value SD2114S040S8R0 (at 0.1 2.4 180) (layer F.SilkS))
    (fp_text user K (at -3.25 3.3 180) (layer F.Fab))
    (fp_text user A (at 3 3.2 180) (layer F.Fab))
    (pad 1 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C67-Pad1)"))
    (pad 2 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 68 Vcharge))
    (model Diodes_SMD.3dshapes/SMB_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SMB_Standard (layer F.Cu) (tedit 595FEA46)
    (at 93.5 70)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D17 (at 0.05 -3.1) (layer F.Fab))
    (fp_text value SD2114S040S8R0 (at -6.55 1.8) (layer F.SilkS))
    (fp_text user K (at -3.25 3.3) (layer F.Fab))
    (fp_text user A (at 3 3.2) (layer F.Fab))
    (pad 1 smd rect (at -2.14884 0) (size 2.49936 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C61-Pad1)"))
    (pad 2 smd rect (at 2.14884 0) (size 2.49936 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Diodes_SMD.3dshapes/SMB_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF154)
    (at 213 45 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D18 (at 0 -1.5 90) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -1.8 1.2 90) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 72 ODO-X1))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF157)
    (at 216 45 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D19 (at 0 -1.5 90) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -1.7 1.2 90) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 73 ODO-X2))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FE5D0)
    (at 171.9 55.6 270)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D20 (at 0 -1.5 270) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -0.6 -0.975 270) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 74 RXD1))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 5960F55E)
    (at 179.5 57.2 270)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D21 (at 0 -1.5 270) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -1.29 -0.94 270) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 75 RXD2))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 0)
    (at 211 55 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D22 (at 0 -1.5 90) (layer F.Fab))
    (fp_text value CD0603-Z3 (at 0 1.7 90) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 76 FB-A))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 0)
    (at 211 101 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D23 (at 0 -1.5 90) (layer F.Fab))
    (fp_text value CD0603-Z3 (at 0 1.7 90) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 77 FB-C))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 0)
    (at 211 77 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D24 (at 0 -1.5 90) (layer F.Fab))
    (fp_text value CD0603-Z3 (at 0 1.7 90) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 78 FB-B))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF0F5)
    (at 211 125 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D25 (at 0 -1.5 90) (layer F.Fab))
    (fp_text value CD0603-Z3 (at 0.6 1.1 90) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 79 FB-D))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FE5A8)
    (at 187.3 57.2 270)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D26 (at 0 -1.5 270) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -0.95 0.9 270) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 80 RXD3))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF11E)
    (at 219 55)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D27 (at 0 -1.5) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -1.3 1.2) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 81 ODO-A1))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF10A)
    (at 220 89)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D28 (at 0 -1.5) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -1 1.3) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 82 ODO-B1))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF0FE)
    (at 220 102)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D29 (at 0 -1.5) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -1 1.3) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 83 ODO-C1))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF0E0)
    (at 221 137)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D30 (at 0 -1.5) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -1.2 1.2) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 84 ODO-D1))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF11B)
    (at 219 59)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D31 (at 0 -1.5) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -1 1.3) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 85 ODO-A2))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF10E)
    (at 220 93)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D32 (at 0 -1.5) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -0.8 1.2) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 86 ODO-B2))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF101)
    (at 220 106)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D33 (at 0 -1.5) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -1.1 1.3) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 ODO-C2))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF0EA)
    (at 221 141)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D34 (at 0 -1.5) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -1.1 1.2) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 88 ODO-D2))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 222.8 65.7 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference D35 (at 0 -1.8 270) (layer F.Fab))
    (fp_text value "TVS 24V" (at 0 1.8 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(D35-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(D35-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 222.85 80.3 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference D36 (at 0 -1.8 270) (layer F.Fab))
    (fp_text value "TVS 24V" (at 0 1.8 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(D36-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(D36-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 595FF0F7)
    (at 222.7 114.6 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference D37 (at 0 -1.8 270) (layer F.Fab))
    (fp_text value "TVS 24V" (at 0 1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(D37-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(D37-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 595FF0ED)
    (at 222.75 127.65 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference D38 (at 0 -1.8 270) (layer F.Fab))
    (fp_text value "TVS 24V" (at -0.05 1.25 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(D38-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(D38-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 595FF1FB)
    (at 128.2 121.975 270)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D39 (at 0 -1.5 270) (layer F.Fab))
    (fp_text value CD0603-Z3 (at -0.175 1 270) (layer F.SilkS))
    (pad 2 smd rect (at -0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 97 ADC-RSV))
  )
  (module AC-Stuff:MAXI-Fuse-Clip-29.21 (layer F.Cu) (tedit 595FE9F7)
    (at 72.4 108.6 180)
    (fp_text reference F1 (at 0 0.5 180) (layer F.Fab))
    (fp_text value "50A fuse" (at 14.9 1.1 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 4.42 180) (size 5.2 5.2) (drill 3.86) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(C8-Pad1)"))
    (pad 1 thru_hole circle (at 8.33 4.42 180) (size 5.2 5.2) (drill 3.86) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 21.03 4.42 180) (size 5.2 5.2) (drill 3.86) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at 29.36 4.42 180) (size 5.2 5.2) (drill 3.86) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(F1-Pad2)"))
  )
  (module Varistors:RV_Disc_D21.5_W5.3_P10 (layer F.Cu) (tedit 59601A03)
    (at 34.4 44.6 180)
    (tags "varistor SIOV")
    (fp_text reference F2 (at 5 4.75 180) (layer F.Fab))
    (fp_text value "10A fuse PPTC" (at 4.45 2.1 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(F2-Pad1)"))
    (pad 2 thru_hole circle (at 10 2.2 180) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 68 Vcharge))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596004D6)
    (at 151.4 107.25 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB1 (at 0 -2.1 90) (layer F.Fab))
    (fp_text value MH2029-300Y (at 0.25 -1.4 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C18-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 595FF4CA)
    (at 159.75 116)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB2 (at 0 -2.1) (layer F.Fab))
    (fp_text value MH2029-300Y (at 0.85 1.4) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C31-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 595FFCA7)
    (at 182 111.4)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB3 (at 0 -2.1) (layer F.Fab))
    (fp_text value MH2029-300Y (at 1.6 -1.2) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C72-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 595FF23A)
    (at 121.275 122.15 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB4 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value MH2029-300Y (at -1.45 -1.225 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C82-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F37C)
    (at 203 107)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at 0 -5.1) (layer F.Fab))
    (fp_text value JP_DIR-D (at -2.5 2.41 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 DIR-D))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(JP1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 DIR-C))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F111)
    (at 210 46 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP2 (at 2.4 -2.3 270) (layer F.Fab))
    (fp_text value JP-SLEW (at -2.8 2.2 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(JP2-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F355)
    (at 203 116.575)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP3 (at 0 -5.1) (layer F.Fab))
    (fp_text value JP-SLEW (at -2.44 0.975 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(JP3-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F35F)
    (at 203 129 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP4 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value JP_PWM-D (at 2.36 2.46 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 PWM-D))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(JP4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 108 PWM-C))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F15E)
    (at 170.8 41 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP5 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value JP_RC_5V (at -0.2 8 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(JP5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F24B)
    (at 43.36 162.89)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP7 (at 0 -5.1) (layer F.Fab))
    (fp_text value JP-MSTEP (at -2.41 1.11 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 318 ~SRST))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(JP7-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module AC-Stuff:Choke-PG1096 (layer F.Cu) (tedit 595FEA01)
    (at 40.8 70.1)
    (descr "Choke PG1096 26x26mm")
    (tags "choke 26x26")
    (attr smd)
    (fp_text reference L4 (at 0 -2.3) (layer F.Fab))
    (fp_text value 33uH (at 14.3 13.25) (layer F.SilkS))
    (pad 1 smd rect (at 4.75 2.5) (size 5.5 5.5) (layers F.Cu F.Paste F.Mask)
      (net 29 Vsolar))
    (pad 2 smd rect (at 21.75 2.5) (size 5.5 5.5) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D13-Pad2)"))
    (pad "" smd rect (at 13 23.5) (size 5.5 5.5) (layers F.Cu F.Paste F.Mask))
  )
  (module AC-Stuff:Choke-PG1096 (layer F.Cu) (tedit 595FEA49)
    (at 86.6 73.4)
    (descr "Choke PG1096 26x26mm")
    (tags "choke 26x26")
    (attr smd)
    (fp_text reference L5 (at 0 -2.3) (layer F.Fab))
    (fp_text value 33uH (at 13.3 9.9) (layer F.SilkS))
    (pad 1 smd rect (at 4.75 2.5) (size 5.5 5.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C61-Pad1)"))
    (pad 2 smd rect (at 21.75 2.5) (size 5.5 5.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C78-Pad1)"))
    (pad "" smd rect (at 13 23.5) (size 5.5 5.5) (layers F.Cu F.Paste F.Mask))
  )
  (module Choke_SMD:Choke_SMD_Wuerth-WE-PD2-Typ-MS (layer F.Cu) (tedit 595FEA73)
    (at 110.1 170.35 90)
    (descr "Choke, Drossel, WE-PD2, Typ MS, Wuerth, SMD,")
    (tags "Choke, Drossel, WE-PD2, Typ MS, Wuerth, SMD,")
    (attr smd)
    (fp_text reference L6 (at 0 -5.08 90) (layer F.Fab))
    (fp_text value 4.7uH (at 3.8 -0.9 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.9304 0 90) (size 2.14884 5.4991) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C96-Pad1)"))
    (pad 2 smd rect (at 1.9304 0 90) (size 2.14884 5.4991) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F1D6)
    (at 147.8 76.8)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.Fab))
    (fp_text value LAWN-1 (at -4.8 -0.2) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 111 LAWN-1R))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FE65A)
    (at 158.17 55.67 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value SONAR-1 (at -0.05 -1.25 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(P2-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FE655)
    (at 154.47 55.67 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value SONAR-2 (at -0.1 9.2 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(P3-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FE650)
    (at 150.67 55.67 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value SONAR-3 (at -0.125 -1.175 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(P4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(P4-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FE66F)
    (at 146.87 55.67 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value SONAR-4 (at -0.1 9.175 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(P5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(P5-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FE676)
    (at 143.07 55.67 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value SONAR-5 (at -0.05 -1.25 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(P6-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(P6-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FE67A)
    (at 139.27 55.67 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value SONAR-6 (at -0.075 9.1 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(P7-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(P7-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F2A1)
    (at 56.2 126.25 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 0 -5.1 270) (layer F.Fab))
    (fp_text value "E-OFF button" (at 0.55 -3.2 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 336 "Net-(JP6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F1CF)
    (at 151.8 76.8)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 -5.1) (layer F.Fab))
    (fp_text value LAWN-2 (at 4.8 -0.4) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 125 LAWN-2R))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F291)
    (at 47 126.4 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P10 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value "E-ON button" (at -2.8 1 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 337 "Net-(JP6-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5964F386)
    (at 190.21 95.32 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P11 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value BUMPER-1 (at -2.94 3.83 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(P11-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 127 "Net-(P11-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FE728)
    (at 190.21 89.72 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P12 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value BUMPER-2 (at 0.075 -2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 128 "Net-(P12-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 129 "Net-(P12-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F2F3)
    (at 127.86 89.71)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P13 (at 0 -5.1) (layer F.Fab))
    (fp_text value RAIN (at 0.14 8.69) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 130 "Net-(P13-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5964F2FC)
    (at 133.06 89.71)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P14 (at 0 -5.1) (layer F.Fab))
    (fp_text value DROP-1 (at -0.31 -2.51) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 131 "Net-(P14-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5964F305)
    (at 138.26 89.71)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P15 (at 0 -5.1) (layer F.Fab))
    (fp_text value DROP-2 (at 1.34 -2.46) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(P15-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F36C)
    (at 195.27 136.94 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P17 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value PERI-2 (at 1.16 -2.49 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(P17-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F2DF)
    (at 117.46 89.71)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P18 (at 0 -5.1) (layer F.Fab))
    (fp_text value PERI-3 (at -0.26 -2.71) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 135 "Net-(P18-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F2E9)
    (at 122.66 89.71)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P19 (at 0 -5.1) (layer F.Fab))
    (fp_text value PERI-4 (at 0.54 -2.71) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 136 "Net-(P19-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 5964F217)
    (at 32.4 106.6 90)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference P21 (at 2.1 8.5 90) (layer F.Fab))
    (fp_text value "LiFePo4 Bat" (at -4 -3.8 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 99 "Net-(F1-Pad2)"))
    (pad 4 thru_hole circle (at 4.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 99 "Net-(F1-Pad2)"))
    (pad "" np_thru_hole circle (at 2.1 -7.3 90) (size 3 3) (drill 3) (layers *.Cu))
    (model Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 5964F22E)
    (at 32.4 136.6 90)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference P22 (at 2.1 8.5 90) (layer F.Fab))
    (fp_text value "Power Mow1" (at -3.2 3.8 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (pad 4 thru_hole circle (at 4.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (pad "" np_thru_hole circle (at 2.1 -7.3 90) (size 3 3) (drill 3) (layers *.Cu))
    (model Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 5964F23B)
    (at 32.4 147.6 90)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference P23 (at 2.1 8.5 90) (layer F.Fab))
    (fp_text value "Power Mow2" (at -3.2 3.6 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (pad 4 thru_hole circle (at 4.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (pad "" np_thru_hole circle (at 2.1 -7.3 90) (size 3 3) (drill 3) (layers *.Cu))
    (model Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 5964F247)
    (at 32.4 158.6 90)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference P24 (at 2.1 8.5 90) (layer F.Fab))
    (fp_text value "Power Mow3" (at -3.8 0.4 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (pad 4 thru_hole circle (at 4.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (pad "" np_thru_hole circle (at 2.1 -7.3 90) (size 3 3) (drill 3) (layers *.Cu))
    (model Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F332)
    (at 177.3 126.54)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P25 (at 0 -5.1) (layer F.Fab))
    (fp_text value S-END (at 3.3 5.16 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 141 S-END))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F03D)
    (at 196.4 183.05 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P26 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value LED1 (at -0.8 -2.15 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 335 "Net-(D7-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 142 "Net-(P26-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F033)
    (at 192.8 183.05 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P27 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value LED2 (at 0 -2.15 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 335 "Net-(D7-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 143 "Net-(P27-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F050)
    (at 181.6 170.1)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P28 (at 0 -5.1) (layer F.Fab))
    (fp_text value FAN (at -1.84 2.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 144 "Net-(P28-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 335 "Net-(D7-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 145 "Net-(P28-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F223)
    (at 27.4 119.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P29 (at 0 -5.1) (layer F.Fab))
    (fp_text value Batt-Extconn (at -1.4 -2.8) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(C8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F02C)
    (at 189.18 183.07 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P30 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value LED3-HC (at 2.18 -2.13 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 335 "Net-(D7-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 146 "Net-(P30-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 5964F207)
    (at 32.4 65.6 90)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference P31 (at 2.1 8.5 90) (layer F.Fab))
    (fp_text value "Solar panel" (at -3 4.4 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 29 Vsolar))
    (pad 4 thru_hole circle (at 4.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 29 Vsolar))
    (pad "" np_thru_hole circle (at 2.1 -7.3 90) (size 3 3) (drill 3) (layers *.Cu))
    (model Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 5964F1FC)
    (at 32.4 54.6 90)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference P32 (at 2.1 8.5 90) (layer F.Fab))
    (fp_text value "Charge in" (at -2.8 4.6 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 100 "Net-(F2-Pad1)"))
    (pad 4 thru_hole circle (at 4.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 100 "Net-(F2-Pad1)"))
    (pad "" np_thru_hole circle (at 2.1 -7.3 90) (size 3 3) (drill 3) (layers *.Cu))
    (model Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5964F1E5)
    (at 120.56 66.64 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P33 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value CAN (at 0 -3.1 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 147 CANRX))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 148 CANTX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F049)
    (at 178.1 166.34 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P34 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value Beeper (at 2.74 1.3 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 335 "Net-(D7-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 149 "Net-(P34-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5964F2B2)
    (at 63.125 170.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P35 (at 0 -5.1) (layer F.Fab))
    (fp_text value STEPPER-1 (at 2.475 3.2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 150 "Net-(P35-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 151 "Net-(P35-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 152 "Net-(P35-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(P35-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5964F2B8)
    (at 63.125 149.8)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P36 (at 0 -5.1) (layer F.Fab))
    (fp_text value STEPPER-2 (at 2.475 3.6 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 154 "Net-(P36-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 155 "Net-(P36-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 156 "Net-(P36-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 157 "Net-(P36-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FEAAE)
    (at 68.4 165.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P37 (at 0 -5.1) (layer F.Fab))
    (fp_text value 5Vsec-1 (at 1.68 4.49 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FEAAA)
    (at 72.4 165.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P38 (at 0 -5.1) (layer F.Fab))
    (fp_text value 5Vsec-2 (at 1.68 4.34 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x13 (layer F.Cu) (tedit 5964F2C6)
    (at 118.4 141)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P39 (at 0 -5.1) (layer F.Fab))
    (fp_text value Orange_PI_Zero (at 5.2 13.55 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 158 "Net-(P39-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 159 "Net-(P39-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 160 "Net-(P39-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 161 "Net-(P39-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 162 "Net-(P39-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 163 "Net-(P39-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 164 TXD0))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 165 EXTERASE))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 166 RXD0))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 ~EXTRST))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 167 "Net-(P39-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 168 "Net-(P39-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 169 "Net-(P39-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 170 "Net-(P39-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 171 "Net-(P39-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 172 "Net-(P39-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 173 "Net-(P39-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 174 "Net-(P39-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 175 "Net-(P39-Pad26)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x13.wrl
      (at (xyz 0.05 -0.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FEAA5)
    (at 76.4 165.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P40 (at 0 -5.1) (layer F.Fab))
    (fp_text value 5Vsec-3 (at 1.68 4.53 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FEA9D)
    (at 80.4 165.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P41 (at 0 -5.1) (layer F.Fab))
    (fp_text value 5Vsec-4 (at 1.725 4.6 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5964F347)
    (at 187.4 120.8 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P42 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value DAC-1 (at -0.85 -2.25 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 176 DAC0))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5964F345)
    (at 187.4 116.8 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P43 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value DAC-2 (at 1.2 -2.3 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 177 DAC1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5964F2CD)
    (at 108.7 153.4)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P44 (at 0 -5.1) (layer F.Fab))
    (fp_text value GPS (at -3.05 3.15 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 162 "Net-(P39-Pad8)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 163 "Net-(P39-Pad10)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5964F0F5)
    (at 208 38 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P45 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value ODO-X (at 3.6 4.4 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 178 "Net-(P45-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 179 "Net-(P45-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FEA92)
    (at 84.4 165.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P46 (at 0 -5.1) (layer F.Fab))
    (fp_text value 5Vsec-5 (at 1.7 4.55 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 595FEA89)
    (at 88.4 165.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P48 (at 0 -5.1) (layer F.Fab))
    (fp_text value 5Vsec-6 (at 1.7 4.5 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 5Vsec))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 595FF25D)
    (at 136.6 125.4 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P49 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value BUTTON (at 0 -2 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 182 "Net-(P49-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5964F16A)
    (at 174.5 51.8)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P50 (at 0 -5.1) (layer F.Fab))
    (fp_text value SERIAL-1 (at 0.1 -3) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 183 "Net-(P50-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 184 "Net-(P50-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5964F1A0)
    (at 189.735 79.724523 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P51 (at 0 -5.1 270) (layer F.Fab))
    (fp_text value SPI-1 (at -2.524523 12.735 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 185 SPI0_MISO))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 186 SPI0_MOSI))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 187 SPI0_SPCK))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 188 SPI0_CS1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5964F07B)
    (at 216 147.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P52 (at 0 -5.1) (layer F.Fab))
    (fp_text value I2C-L5V-1 (at 0 16.6 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 189 "Net-(P52-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 190 "Net-(P52-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5964F083)
    (at 224 147.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P53 (at 0 -5.1) (layer F.Fab))
    (fp_text value I2C-L5V-2 (at -4 16.8 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 189 "Net-(P52-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 190 "Net-(P52-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5964F08D)
    (at 220 147.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P54 (at 0 -5.1) (layer F.Fab))
    (fp_text value I2C-L5V-3 (at 4 16.8 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 189 "Net-(P52-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 190 "Net-(P52-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5964F1A5)
    (at 190 71.5 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P55 (at 0 -5.1 270) (layer F.Fab))
    (fp_text value SPI-2 (at -2.7 12.8 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 185 SPI0_MISO))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 186 SPI0_MOSI))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 187 SPI0_SPCK))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 191 SPI0_CS2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 59601589)
    (at 140.375 123.175)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P56 (at 0 -5.1) (layer F.Fab))
    (fp_text value TEMP-1 (at 0 4.4) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 192 TEMP-1))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 59601590)
    (at 144.175 123.175)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P57 (at 0 -5.1) (layer F.Fab))
    (fp_text value TEMP-2 (at 0 4.4) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 193 TEMP-2))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5964F179)
    (at 182.3 51.8)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P58 (at 0 -5.1) (layer F.Fab))
    (fp_text value SERIAL-2 (at 0.3 -3) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 194 "Net-(P58-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 195 "Net-(P58-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5964F0A9)
    (at 210.2 147.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P59 (at 0 -5.1) (layer F.Fab))
    (fp_text value I2C-L3V3-1 (at 0 17.2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 196 "Net-(P59-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 197 "Net-(P59-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5964F0A7)
    (at 206.2 147.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P60 (at 0 -5.1) (layer F.Fab))
    (fp_text value I2C-L3V3-2 (at -0.2 17.2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 196 "Net-(P59-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 197 "Net-(P59-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5964F09A)
    (at 202.2 147.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P61 (at 0 -5.1) (layer F.Fab))
    (fp_text value I2C-L3V3-3 (at -0.2 17.2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 196 "Net-(P59-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 197 "Net-(P59-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5960E93F)
    (at 198.2 147.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P62 (at 0 -5.1) (layer F.Fab))
    (fp_text value I2C-L3V3-4 (at -0.05 -2.2) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 196 "Net-(P59-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 197 "Net-(P59-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5960E8AE)
    (at 194.2 147.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P63 (at 0 -5.1) (layer F.Fab))
    (fp_text value I2C-L3V3-5 (at 0.35 12.65) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 196 "Net-(P59-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 197 "Net-(P59-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 595FF228)
    (at 121.85 126.325 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P64 (at 0 -5.1 90) (layer F.Fab))
    (fp_text value ADC-RSV (at -1.875 3.15 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 198 "Net-(P64-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5964F185)
    (at 189.9 51.8)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P65 (at 0 -5.1) (layer F.Fab))
    (fp_text value SERIAL-3 (at 0.5 -3) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 199 "Net-(P65-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 200 "Net-(P65-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 595FF25B)
    (at 132.875 125.3 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P66 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value RES-ADC (at 1.075 -2.1 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 198 "Net-(P64-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 ADC-RSV))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5964F0E4)
    (at 239 61)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P67 (at 0 -5.1) (layer F.Fab))
    (fp_text value MOTOR-A (at 4 6.8 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(D35-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(D35-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 201 "Net-(P67-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 202 "Net-(P67-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5964F0D8)
    (at 239 79)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P68 (at 0 -5.1) (layer F.Fab))
    (fp_text value MOTOR-B (at 3.8 6.2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(D36-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(D36-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 203 "Net-(P68-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 204 "Net-(P68-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5964F0CA)
    (at 239 109)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P69 (at 0 -5.1) (layer F.Fab))
    (fp_text value MOTOR-C (at 4 7.6 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(D37-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(D37-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 205 "Net-(P69-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 206 "Net-(P69-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5964F0C3)
    (at 239 127)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P70 (at 0 -5.1) (layer F.Fab))
    (fp_text value MOTOR-D (at 4 8 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(D38-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(D38-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 5V))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 207 "Net-(P70-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 208 "Net-(P70-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F101)
    (at 202.4 43.4 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P71 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value PWM-A (at -0.4 9.8 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 209 "Net-(P71-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(JP5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F107)
    (at 198.4 43.4 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P72 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value PWM-B (at -0.2 9.8 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 210 "Net-(P72-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(JP5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F11F)
    (at 194.4 43.4 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P73 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value PWM-E1 (at -0.2 10.2 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 211 "Net-(P73-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(JP5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F129)
    (at 190.4 43.4 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P74 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value PWM-E2 (at -0.2 10.2 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 211 "Net-(P73-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(JP5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F133)
    (at 186.4 43.4 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P75 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value PWM-E3 (at -0.2 10.2 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 211 "Net-(P73-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(JP5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F14B)
    (at 182.4 43.4 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P76 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value PWM-F (at -0.2 9.8 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 212 "Net-(P76-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(JP5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F149)
    (at 178.4 43.4 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P77 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value PWM-G (at -0.2 9.8 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 213 "Net-(P77-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(JP5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F156)
    (at 174.4 43.4 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P78 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value PWM-H (at -0.2 9.8 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 214 "Net-(P78-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(JP5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5960DD1D)
    (at 164.4 129)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.25) (layer F.Fab))
    (fp_text value FDV301N (at -3.8 0.2) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 216 FWUP))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Horizontal_LargePads (layer F.Cu) (tedit 5964EB94)
    (at 55.4 64.6)
    (descr "TO-220, Neutral, Horizontal, Large Pads,")
    (tags "TO-220, Neutral, Horizontal, Large Pads,")
    (fp_text reference Q2 (at 0.24892 -22.84984) (layer F.Fab))
    (fp_text value IRLB8748 (at 0.1 -21.6) (layer F.SilkS))
    (pad 2 thru_hole oval (at 0 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(D13-Pad2)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 217 "Net-(Q2-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 -16.764 90) (size 3.79984 3.79984) (drill 3.79984) (layers *.Cu *.Mask F.SilkS))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Horizontal_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Horizontal_LargePads (layer F.Cu) (tedit 5964EB8F)
    (at 90.4 64.6)
    (descr "TO-220, Neutral, Horizontal, Large Pads,")
    (tags "TO-220, Neutral, Horizontal, Large Pads,")
    (fp_text reference Q3 (at 0.24892 -22.84984) (layer F.Fab))
    (fp_text value IRLB8748 (at -0.4 -21.6) (layer F.SilkS))
    (pad 2 thru_hole oval (at 0 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(C67-Pad1)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 218 "Net-(Q3-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(C61-Pad1)"))
    (pad "" np_thru_hole circle (at 0 -16.764 90) (size 3.79984 3.79984) (drill 3.79984) (layers *.Cu *.Mask F.SilkS))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Horizontal_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE861)
    (at 84 99.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 1K5 (at -0.1 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE8E6)
    (at 57.2 129.1 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 5K1 (at 0 -1.3 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 147.4 82)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.9) (layer F.Fab))
    (fp_text value 2M (at 0 1.9) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 219 LAWN-1S))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 111 LAWN-1R))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5964D865)
    (at 131.3 53.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 620 (at -0.12 -1.18 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE613)
    (at 160.87 51.47 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 2K2 (at -1.225 0.925 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 220 ECHO-1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE602)
    (at 160.87 48.67 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 1K5 (at 2.25 0.05 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 220 ECHO-1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(P2-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE5FF)
    (at 160.77 54.42 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 620 (at -2.25 0.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 221 TRIG-1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(P2-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE6B1)
    (at 153.67 39.37 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 2K2 (at 2.175 -0.05 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 222 ECHO-2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE6B4)
    (at 153.67 42.07 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 1K5 (at -0.775 2.075 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 222 ECHO-2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(P3-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE6B7)
    (at 153.67 44.77 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 620 (at 0.525 1.375 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 223 TRIG-2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(P3-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE665)
    (at 153.67 64.37 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 2K2 (at 2.3 0.05 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 224 ECHO-3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE639)
    (at 153.67 61.67 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 1K5 (at -0.4 -2.125 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 224 ECHO-3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(P4-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE661)
    (at 153.67 58.97 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 620 (at 0.5 -1.325 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 225 TRIG-3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(P4-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE6AC)
    (at 144.57 39.37 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 2K2 (at 2.05 -0.025 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 226 ECHO-4))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE6A8)
    (at 144.57 42.07 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 1K5 (at -0.725 2.15 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 226 ECHO-4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(P5-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE6A3)
    (at 144.57 44.77 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 620 (at 0.5 1.325 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 227 TRIG-4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(P5-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 144.67 64.37 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 2K2 (at 0 1.9 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 228 ECHO-5))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 144.67 61.67 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 1K5 (at 0 1.9 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 228 ECHO-5))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(P6-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 144.67 58.97 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 620 (at 0 1.9 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 229 TRIG-5))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(P6-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE681)
    (at 136.67 51.17 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 2K2 (at -0.9 -0.95 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 230 ECHO-6))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE689)
    (at 136.67 48.47 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 1K5 (at 2.275 0.025 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 230 ECHO-6))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(P7-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE68E)
    (at 136.67 54.12 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 620 (at -2.275 0.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 231 TRIG-6))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(P7-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59640F23)
    (at 42.5 129.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10K (at 0 1.2) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(C8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 151.4 82)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 0 -1.9) (layer F.Fab))
    (fp_text value 2M (at 0 1.9) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 LAWN-2S))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 125 LAWN-2R))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE754)
    (at 200.61 93.02 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 1K5 (at 0.3 -1.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 234 BMP-L1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(P11-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE757)
    (at 200.61 87.52 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 1K5 (at 0.175 -1.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 235 BMP-L2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(P12-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7E6)
    (at 135.66 95.11 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 1K5 (at 2 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 236 DROP-1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(P14-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7D6)
    (at 140.86 95.11 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 1K5 (at 2 0.4 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 237 DROP-2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(P15-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7CB)
    (at 130.46 95.11 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 1K5 (at 2 -0.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 238 RAIN))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(P13-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE791)
    (at 200.67 139.54)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at 0 -1.9) (layer F.Fab))
    (fp_text value 1K5 (at 1.6 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 239 PERI-1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(P16-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7A1)
    (at 200.67 134.34)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at 0 -1.9) (layer F.Fab))
    (fp_text value 1K5 (at 1.55 0.025 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 240 PERI-2))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(P17-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7AD)
    (at 120.06 95.11 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 1K5 (at 1.525 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 241 PERI-3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(P18-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7C4)
    (at 125.26 95.11 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 1K5 (at 1.6 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 242 PERI-4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(P19-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7CE)
    (at 130.46 92.31 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 2K2 (at 2 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 238 RAIN))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE74D)
    (at 197.11 92.62)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at 0 -1.9) (layer F.Fab))
    (fp_text value 1K5 (at -0.025 -1.175) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 243 BMP-R1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(P11-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE767)
    (at 197.11 87.02)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R36 (at 0 -1.9) (layer F.Fab))
    (fp_text value 1K5 (at 0.225 -1.2) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 244 BMP-R2))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(P12-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7EB)
    (at 135.66 92.31 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R37 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 2K2 (at -2 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 236 DROP-1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7DB)
    (at 140.86 92.31 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R38 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 2K2 (at -2 0.4 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 237 DROP-2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE797)
    (at 197.87 139.54)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R39 (at 0 -1.9) (layer F.Fab))
    (fp_text value 2K2 (at -2.075 0.025) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 239 PERI-1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7A6)
    (at 197.87 134.34)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R40 (at 0 -1.9) (layer F.Fab))
    (fp_text value 2K2 (at -2.025 -0.1) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 240 PERI-2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7A9)
    (at 120.06 92.31 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R41 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 2K2 (at -2.05 -0.075 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 241 PERI-3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE7C7)
    (at 125.26 92.36 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R42 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 2K2 (at -2.05 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 242 PERI-4))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE750)
    (at 200.61 95.72 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R43 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 2K2 (at -0.1 1.075 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 234 BMP-L1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE75B)
    (at 200.61 90.22 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R44 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 2K2 (at -0.1 1.05 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 235 BMP-L2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 595FECA7)
    (at 195.4 177 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R45 (at 0 -2.1 90) (layer F.Fab))
    (fp_text value 470R (at 0.29 1.55 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(P26-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(R45-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 595FECC4)
    (at 191.2 177 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R46 (at 0 -2.1 90) (layer F.Fab))
    (fp_text value 133R (at -0.49 -1.41 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(P30-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(R46-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FECC7)
    (at 188.5 176.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R47 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 5K1 (at -0.02 -1.19 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(R47-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE76B)
    (at 194.41 92.62 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R48 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 2K2 (at 0.05 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 243 BMP-R1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE788)
    (at 194.41 87.02 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R49 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 2K2 (at 0.25 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 244 BMP-R2))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 595FECBD)
    (at 193.3 177 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R50 (at 0 -2.1 90) (layer F.Fab))
    (fp_text value 470R (at -1.76 -0.42 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(P27-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(R50-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5963C301)
    (at 204.2 94.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R51 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 43K (at -0.1 1.15 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 249 SVbatt))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5963C2FD)
    (at 204.17 97.31 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R52 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 4K75 (at 0.06 1.14 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 249 SVbatt))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59600487)
    (at 155.2 119.1 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R53 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 6K8 (at 0.1 1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960C219)
    (at 155.5 123.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R54 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 39R (at -2.08 -1.63 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(R54-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 139 D+))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960C1C5)
    (at 157.2 123.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R55 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 39R (at -1.96 1.65 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(R55-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 138 D-))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 103.6 118.7 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R56 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 5K1 (at 0 1.9 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 252 PGOOD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59600491)
    (at 161.75 80 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R57 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 2K2 (at 0.05 1.3 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(R57-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 165 EXTERASE))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 596014B4)
    (at 136.7 117.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R58 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 4K75 (at -2.6 1.6 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 254 SV3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960E868)
    (at 136.7 119.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R59 (at 0 -1.9) (layer F.Fab))
    (fp_text value 43K (at -0.55 1.1) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 254 SV3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960E872)
    (at 125.27 129.03 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R60 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 4K75 (at 0.05 1.25 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 255 SV5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960E870)
    (at 122.61 129.03 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R61 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 43K (at 0.05 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 255 SV5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 160.6 129.8 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R62 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 620 (at 0 1.9 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 252 PGOOD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59600496)
    (at 166.75 84.1 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R63 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 10K (at 2 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(R57-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960099E)
    (at 177.2 144.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R64 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 25R (at 2.2 0.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C44-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960C248)
    (at 167.4 128.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R65 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 10K (at -2.13 -0.3 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 216 FWUP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE850)
    (at 70.75 89.85 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R66 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 5K1 (at 0.15 -1.25 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 256 PWM-Boost))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE857)
    (at 70.775 87.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R67 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 5K1 (at 0.025 1.175 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 257 PWM-CC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 596004AB)
    (at 173.6 122.05)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R68 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10K (at 0 -1.15) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C57-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 71.92 57.74 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R69 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 43K (at 0 1.9 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 258 SVsolar))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 Vsolar))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 595FE815)
    (at 69.4 78.6 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R70 (at 0 -2.1 270) (layer F.Fab))
    (fp_text value 6R (at 0 1.4 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(R70-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 75.02 57.74 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R71 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 4K75 (at 0 1.9 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 258 SVsolar))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FEA33)
    (at 99.4 65.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R72 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 4K75 (at 0.05 1.3 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 260 SVin))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FEA32)
    (at 96.4 65.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R73 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 43K (at 0 1.25 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 260 SVin))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C67-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 83.4 66.05 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R74 (at 0 -2.1 180) (layer F.Fab))
    (fp_text value 6R (at 0 2.1 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 261 "Net-(R74-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960199C)
    (at 46.9 42.19 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R75 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 43K (at -0.1 1.3 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 262 SVcharge))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(D16-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59601A08)
    (at 49.65 42.19)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R76 (at 0 -1.9) (layer F.Fab))
    (fp_text value 4K75 (at 0 -1.15) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 262 SVcharge))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF14D)
    (at 213 42 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R77 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 5K1 (at -0.1 1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(P45-Pad3)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 ODO-X1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF14F)
    (at 216 42 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R78 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 5K1 (at -0.1 1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(P45-Pad4)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 ODO-X2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5964F54E)
    (at 130 102.4 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R79 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 10K (at 1 1.4 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 181 SCL2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 596037A2)
    (at 127.4 107.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R80 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 10K (at -2.15 0.34 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 180 SDA2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960E863)
    (at 142.6 118.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R81 (at 0 -1.9) (layer F.Fab))
    (fp_text value 5K1 (at 0.05 -1.2) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(P49-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE5CD)
    (at 171.9 58.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R82 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 1K5 (at -1.95 0.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(P50-Pad4)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 RXD1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE5D9)
    (at 171.8 52.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R83 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 620R (at 1.75 0.175 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(P50-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 263 TXD1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 230.6 152.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R84 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 10K (at 0 1.9 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(R84-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960372A)
    (at 228.8 150.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R85 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 10K (at -1.9 -0.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(P52-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 596037D1)
    (at 227.2 158.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R86 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10K (at 2.01 -0.07) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(P52-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 596037C9)
    (at 190.09 158.67)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R87 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10K (at 2.03 -0.14) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 265 SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59603791)
    (at 190.52 147.26)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R88 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10K (at -2.02 0.02) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 266 SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960F55B)
    (at 179.5 60 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R89 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 1K5 (at 1.92 -0.07 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(P58-Pad4)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 RXD2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960F550)
    (at 179.51 54.07 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R90 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 620R (at 2.58 -0.29 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(P58-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 267 TXD2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960E86A)
    (at 140.375 120.575 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R91 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 10K (at 0.375 1.075 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 192 TEMP-1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59601581)
    (at 144.175 120.575)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R92 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10K (at 2.2 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 193 TEMP-2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 596037AA)
    (at 190.655 150.56)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R93 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10K (at 1.665 -0.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "Net-(R93-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 596037BD)
    (at 187.6 152.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R94 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 10K (at -0.18 0.93 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(P59-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 596037B7)
    (at 187.6 155.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R95 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 10K (at 0.42 -0.93 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(P59-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 136.69 114.24 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R96 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 43K (at 0 1.9 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 269 SV5Vsec))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 596014AF)
    (at 136.7 115.9)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R97 (at 0 -1.9) (layer F.Fab))
    (fp_text value 4K75 (at 2.6 1.6) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 269 SV5Vsec))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE5A4)
    (at 187.3 60.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R98 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 1K5 (at 2.175 -0.225 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(P65-Pad4)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 RXD3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE5AD)
    (at 187.3 54 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R99 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 620R (at 2.525 -0.075 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(P65-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 270 TXD3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE70C)
    (at 194.4 46 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R100 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 620R (at 2.65 -0.05 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(P73-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 271 PWM-E))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE717)
    (at 202.4 46 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R101 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 620R (at 2.05 0.425 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(P71-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 272 PWM-A))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE713)
    (at 198.4 46 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R102 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 620R (at 2 0.575 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(P72-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 273 PWM-B))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE707)
    (at 182.4 46 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R103 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 620R (at 2.05 0.675 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(P76-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 274 PWM-F))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE700)
    (at 178.4 46 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R104 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 620R (at 2.05 0.85 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(P77-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 275 PWM-G))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FE702)
    (at 174.4 46 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R105 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 620R (at 1.975 0.775 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(P78-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 276 PWM-H))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF123)
    (at 222 55 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R106 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 5K1 (at -0.2 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(P67-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 ODO-A1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF121)
    (at 222 59 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R107 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 5K1 (at -0.1 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(P67-Pad6)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 ODO-A2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF116)
    (at 223 89 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R108 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 5K1 (at 0 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(P68-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 ODO-B1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF113)
    (at 223 93 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R109 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 5K1 (at -0.2 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(P68-Pad6)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 ODO-B2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF106)
    (at 223 102 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R110 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 5K1 (at -0.1 1.4 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(P69-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 ODO-C1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF104)
    (at 223 106 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R111 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 5K1 (at -0.1 1.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(P69-Pad6)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 ODO-C2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF0E2)
    (at 224 137 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R112 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 5K1 (at -0.1 1.3 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(P70-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 ODO-D1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF0E5)
    (at 224 141 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R113 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 5K1 (at -0.1 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(P70-Pad6)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 ODO-D2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF1FE)
    (at 129.875 124.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R114 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 43K (at 0.05 1.075 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 ADC-RSV))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(P64-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 595FF1F8)
    (at 129.875 122.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R115 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 4K75 (at 0.05 -1.125 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 ADC-RSV))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5960C92E)
    (at 178.34 123.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R116 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 5K1 (at 0.13 1.14 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 141 S-END))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 53.9 68.22 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R117 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 10K (at 0 1.9 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59601439)
    (at 87.2 69.2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R118 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10K (at 0 -1.2) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C61-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AC-Stuff:Relay_RT314F12 (layer F.Cu) (tedit 595FE8EA)
    (at 47.45 121.55)
    (descr "Relay, SPST, bistable, RT314, 20A, 250V, AC,")
    (tags "Relay, SPST, bistable, 20A, 250V, AC, Relay, 1 x ein,")
    (fp_text reference RL1 (at 12.446 -11.176) (layer F.Fab))
    (fp_text value RT314F12 (at 10.1 -0.35) (layer F.SilkS))
    (pad A2 thru_hole circle (at 0 -7.5) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 232 "Net-(C8-Pad2)"))
    (pad A1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 337 "Net-(JP6-Pad3)"))
    (pad 11 thru_hole circle (at 20.3 -7.5) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(C8-Pad1)"))
    (pad 11 thru_hole circle (at 20.3 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(C8-Pad1)"))
    (pad 14 thru_hole circle (at 25.34 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 277 "Net-(RL1-Pad14)"))
    (pad 14 thru_hole circle (at 25.34 -7.5) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 277 "Net-(RL1-Pad14)"))
    (pad 12 thru_hole circle (at 15.26 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 278 "Net-(RL1-Pad12)"))
    (pad 12 thru_hole circle (at 15.26 -7.5) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 278 "Net-(RL1-Pad12)"))
    (pad A3 thru_hole circle (at 0 -3.75) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 336 "Net-(JP6-Pad1)"))
    (model Relays_ThroughHole.3dshapes/Relay_SPST_Schrack-RP-3SL_bistable.wrl
      (at (xyz 0.496 0.1417 0))
      (scale (xyz 0.42 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Convex_8x0602 (layer F.Cu) (tedit 54539007)
    (at 190.22 104.04)
    (descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RP1 (at 0 -3) (layer F.Fab))
    (fp_text value 150R (at 0 3) (layer F.SilkS))
    (pad 1 smd rect (at -0.9 -1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 AD0))
    (pad 16 smd rect (at 0.9 -1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 258 SVsolar))
    (pad 8 smd rect (at -0.9 1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 AD7))
    (pad 9 smd rect (at 0.9 1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 262 SVcharge))
    (pad 2 smd rect (at -0.9 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 AD1))
    (pad 3 smd rect (at -0.9 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 AD2))
    (pad 4 smd rect (at -0.9 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 AD3))
    (pad 5 smd rect (at -0.9 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 AD4))
    (pad 6 smd rect (at -0.9 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 AD5))
    (pad 7 smd rect (at -0.9 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 AD6))
    (pad 15 smd rect (at 0.9 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 279 SItotal))
    (pad 14 smd rect (at 0.9 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 240 PERI-2))
    (pad 13 smd rect (at 0.9 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 239 PERI-1))
    (pad 11 smd rect (at 0.9 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 249 SVbatt))
    (pad 12 smd rect (at 0.9 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 280 SIcharge))
    (pad 10 smd rect (at 0.9 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 260 SVin))
    (model Resistors_SMD.3dshapes/R_Array_Convex_8x0602.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Convex_8x0602 (layer F.Cu) (tedit 595FF1D7)
    (at 132.5 112.5)
    (descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RP2 (at 0 -3) (layer F.Fab))
    (fp_text value 150R (at 0.1 0.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.9 -1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 AD8))
    (pad 16 smd rect (at 0.9 -1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 76 FB-A))
    (pad 8 smd rect (at -0.9 1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 AD15))
    (pad 9 smd rect (at 0.9 1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 236 DROP-1))
    (pad 2 smd rect (at -0.9 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 AD9))
    (pad 3 smd rect (at -0.9 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 AD12))
    (pad 4 smd rect (at -0.9 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 AD11))
    (pad 5 smd rect (at -0.9 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 AD10))
    (pad 6 smd rect (at -0.9 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 AD13))
    (pad 7 smd rect (at -0.9 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 AD14))
    (pad 15 smd rect (at 0.9 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 78 FB-B))
    (pad 14 smd rect (at 0.9 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 281 SImow))
    (pad 13 smd rect (at 0.9 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 241 PERI-3))
    (pad 11 smd rect (at 0.9 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 77 FB-C))
    (pad 12 smd rect (at 0.9 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 242 PERI-4))
    (pad 10 smd rect (at 0.9 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 79 FB-D))
    (model Resistors_SMD.3dshapes/R_Array_Convex_8x0602.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Convex_8x0602 (layer F.Cu) (tedit 595FF1DA)
    (at 132.5 118)
    (descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RP3 (at 0 -3) (layer F.Fab))
    (fp_text value 150R (at 0.1 -0.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.9 -1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 AD16))
    (pad 16 smd rect (at 0.9 -1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 237 DROP-2))
    (pad 8 smd rect (at -0.9 1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 63 BTTN))
    (pad 9 smd rect (at 0.9 1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(P49-Pad2)"))
    (pad 2 smd rect (at -0.9 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 AD17))
    (pad 3 smd rect (at -0.9 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 AD18))
    (pad 4 smd rect (at -0.9 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 AD19))
    (pad 5 smd rect (at -0.9 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 AD20))
    (pad 6 smd rect (at -0.9 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 60 AD21))
    (pad 7 smd rect (at -0.9 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 62 AD22))
    (pad 15 smd rect (at 0.9 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 269 SV5Vsec))
    (pad 14 smd rect (at 0.9 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 255 SV5V))
    (pad 13 smd rect (at 0.9 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 254 SV3V3))
    (pad 11 smd rect (at 0.9 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 193 TEMP-2))
    (pad 12 smd rect (at 0.9 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 192 TEMP-1))
    (pad 10 smd rect (at 0.9 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 97 ADC-RSV))
    (model Resistors_SMD.3dshapes/R_Array_Convex_8x0602.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 5964F1BA)
    (at 167.1 81.2)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at -0.9 -2.7) (layer F.Fab))
    (fp_text value ERASE (at 4.3 -2.6) (layer F.SilkS))
    (pad 2 smd rect (at 2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 1 smd rect (at -2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(R57-Pad1)"))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 5964F31C)
    (at 171 125)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW2 (at -0.9 -2.7) (layer F.Fab))
    (fp_text value RESET (at -0.15 2.35) (layer F.SilkS))
    (pad 2 smd rect (at 2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C57-Pad1)"))
    (pad 1 smd rect (at -2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Housings_SOIC:SOIC-18_7.5x11.6mm_Pitch1.27mm (layer F.Cu) (tedit 595FECE7)
    (at 189.85 169 270)
    (descr "18-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -6.875 270) (layer F.Fab))
    (fp_text value ULN2803A (at -2.82 -3.43 360) (layer F.SilkS))
    (pad 1 smd rect (at -4.7 -5.08 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 282 LED1))
    (pad 2 smd rect (at -4.7 -3.81 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 283 LED2))
    (pad 3 smd rect (at -4.7 -2.54 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 284 LED3))
    (pad 4 smd rect (at -4.7 -1.27 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 285 BEEPER))
    (pad 5 smd rect (at -4.7 0 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 286 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -4.7 1.27 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 287 ACTIVITY))
    (pad 7 smd rect (at -4.7 2.54 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 288 PWM-FAN))
    (pad 8 smd rect (at -4.7 3.81 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 289 SHUTDOWN))
    (pad 9 smd rect (at -4.7 5.08 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 4.7 5.08 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 335 "Net-(D7-Pad2)"))
    (pad 11 smd rect (at 4.7 3.81 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 124 SHDN-RLY))
    (pad 12 smd rect (at 4.7 2.54 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(P28-Pad1)"))
    (pad 13 smd rect (at 4.7 1.27 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(R47-Pad2)"))
    (pad 14 smd rect (at 4.7 0 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 290 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 4.7 -1.27 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(P34-Pad2)"))
    (pad 16 smd rect (at 4.7 -2.54 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(R46-Pad2)"))
    (pad 17 smd rect (at 4.7 -3.81 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(R50-Pad2)"))
    (pad 18 smd rect (at 4.7 -5.08 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(R45-Pad2)"))
    (model Housings_SOIC.3dshapes/SOIC-18_7.5x11.6mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 595FE8D6)
    (at 66.4 127.6 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U2 (at 0 -1.27 270) (layer F.Fab))
    (fp_text value ACS725LLCTR-30AB-T (at 0.55 -0.1 270) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 279 SItotal))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C16-Pad1)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 278 "Net-(RL1-Pad12)"))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 278 "Net-(RL1-Pad12)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 61.4 136.6 180)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at 0 -1.27 180) (layer F.Fab))
    (fp_text value ACS725LLCTR-30AB-T (at 0 1.27 180) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 7 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 281 SImow))
    (pad 6 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C17-Pad1)"))
    (pad 5 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (pad 3 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C13-Pad2)"))
    (pad 2 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 1 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 101.4 130.6)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U4 (at 0 -2.85) (layer F.Fab))
    (fp_text value TS30042-M033QFNR (at 0 2.85) (layer F.SilkS))
    (pad 1 smd oval (at -1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C34-Pad1)"))
    (pad 2 smd oval (at -1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 3 smd oval (at -1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 4 smd oval (at -1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd oval (at -0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 6 smd oval (at -0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 291 "Net-(U4-Pad6)"))
    (pad 7 smd oval (at 0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 292 "Net-(U4-Pad7)"))
    (pad 8 smd oval (at 0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 293 "Net-(U4-Pad8)"))
    (pad 9 smd oval (at 1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 294 "Net-(U4-Pad9)"))
    (pad 10 smd oval (at 1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C34-Pad2)"))
    (pad 11 smd oval (at 1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 12 smd oval (at 1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C34-Pad1)"))
    (pad 13 smd oval (at 0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C34-Pad1)"))
    (pad 14 smd oval (at 0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd oval (at -0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd oval (at -0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C34-Pad1)"))
    (pad 17 smd rect (at 0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 102.8 113.7)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U5 (at 0 -2.85) (layer F.Fab))
    (fp_text value TS30042-M050QFNR (at 0 2.85) (layer F.SilkS))
    (pad 1 smd oval (at -1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C35-Pad1)"))
    (pad 2 smd oval (at -1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 3 smd oval (at -1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 4 smd oval (at -1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd oval (at -0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 6 smd oval (at -0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 295 "Net-(U5-Pad6)"))
    (pad 7 smd oval (at 0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 296 "Net-(U5-Pad7)"))
    (pad 8 smd oval (at 0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 252 PGOOD))
    (pad 9 smd oval (at 1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 297 "Net-(U5-Pad9)"))
    (pad 10 smd oval (at 1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C35-Pad2)"))
    (pad 11 smd oval (at 1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 12 smd oval (at 1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C35-Pad1)"))
    (pad 13 smd oval (at 0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C35-Pad1)"))
    (pad 14 smd oval (at 0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd oval (at -0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd oval (at -0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C35-Pad1)"))
    (pad 17 smd rect (at 0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-144_20x20mm_Pitch0.5mm (layer F.Cu) (tedit 595FEF9F)
    (at 168.55 100.975)
    (descr "144-Lead Plastic Low Profile Quad Flatpack (PL) - 20x20x1.40 mm Body [LQFP], 2.00 mm Footprint (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U6 (at 0 -12.475) (layer F.Fab))
    (fp_text value ATSAM3X8EA-AU (at -5.25 -7.875) (layer F.SilkS))
    (pad 1 smd rect (at -10.7 -8.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 298 ~SFLT-1))
    (pad 2 smd rect (at -10.7 -8.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 164 TXD0))
    (pad 3 smd rect (at -10.7 -7.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 RXD1))
    (pad 4 smd rect (at -10.7 -7.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 263 TXD1))
    (pad 5 smd rect (at -10.7 -6.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 RXD2))
    (pad 6 smd rect (at -10.7 -6.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 267 TXD2))
    (pad 7 smd rect (at -10.7 -5.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 221 TRIG-1))
    (pad 8 smd rect (at -10.7 -5.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 223 TRIG-2))
    (pad 9 smd rect (at -10.7 -4.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 180 SDA2))
    (pad 10 smd rect (at -10.7 -4.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 11 smd rect (at -10.7 -3.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 12 smd rect (at -10.7 -3.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at -10.7 -2.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 225 TRIG-3))
    (pad 14 smd rect (at -10.7 -2.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 227 TRIG-4))
    (pad 15 smd rect (at -10.7 -1.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 229 TRIG-5))
    (pad 16 smd rect (at -10.7 -1.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 231 TRIG-6))
    (pad 17 smd rect (at -10.7 -0.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 270 TXD3))
    (pad 18 smd rect (at -10.7 -0.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 80 RXD3))
    (pad 19 smd rect (at -10.7 0.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 299 ~SFLT-2))
    (pad 20 smd rect (at -10.7 0.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 125 LAWN-2R))
    (pad 21 smd rect (at -10.7 1.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 275 PWM-G))
    (pad 22 smd rect (at -10.7 1.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 233 LAWN-2S))
    (pad 23 smd rect (at -10.7 2.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 148 CANTX))
    (pad 24 smd rect (at -10.7 2.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 147 CANRX))
    (pad 25 smd rect (at -10.7 3.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 219 LAWN-1S))
    (pad 26 smd rect (at -10.7 3.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 LAWN-1R))
    (pad 27 smd rect (at -10.7 4.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 166 RXD0))
    (pad 28 smd rect (at -10.7 4.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 300 "Net-(U6-Pad28)"))
    (pad 29 smd rect (at -10.7 5.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 301 "Net-(U6-Pad29)"))
    (pad 30 smd rect (at -10.7 5.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 302 "Net-(U6-Pad30)"))
    (pad 31 smd rect (at -10.7 6.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 303 "Net-(U6-Pad31)"))
    (pad 32 smd rect (at -10.7 6.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 289 SHUTDOWN))
    (pad 33 smd rect (at -10.7 7.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 34 smd rect (at -10.7 7.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C18-Pad1)"))
    (pad 35 smd rect (at -10.7 8.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C24-Pad1)"))
    (pad 36 smd rect (at -10.7 8.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C25-Pad1)"))
    (pad 37 smd rect (at -8.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 139 D+))
    (pad 38 smd rect (at -8.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 138 D-))
    (pad 39 smd rect (at -7.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 137 VUSB))
    (pad 40 smd rect (at -7.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C30-Pad1)"))
    (pad 41 smd rect (at -6.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C31-Pad1)"))
    (pad 42 smd rect (at -6.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(R54-Pad1)"))
    (pad 43 smd rect (at -5.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(R55-Pad1)"))
    (pad 44 smd rect (at -5.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 45 smd rect (at -4.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 46 smd rect (at -4.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 304 "Net-(U6-Pad46)"))
    (pad 47 smd rect (at -3.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 NRSTB))
    (pad 48 smd rect (at -3.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C38-Pad1)"))
    (pad 49 smd rect (at -2.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C41-Pad1)"))
    (pad 50 smd rect (at -2.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 305 "Net-(U6-Pad50)"))
    (pad 51 smd rect (at -1.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 306 "Net-(U6-Pad51)"))
    (pad 52 smd rect (at -1.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C107-Pad1)"))
    (pad 53 smd rect (at -0.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 216 FWUP))
    (pad 54 smd rect (at -0.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 55 smd rect (at 0.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 238 RAIN))
    (pad 56 smd rect (at 0.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 57 smd rect (at 1.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 58 smd rect (at 1.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 59 smd rect (at 2.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 272 PWM-A))
    (pad 60 smd rect (at 2.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 282 LED1))
    (pad 61 smd rect (at 3.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 62 smd rect (at 3.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 63 smd rect (at 4.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 283 LED2))
    (pad 64 smd rect (at 4.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 284 LED3))
    (pad 65 smd rect (at 5.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 285 BEEPER))
    (pad 66 smd rect (at 5.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 106 PWM-D))
    (pad 67 smd rect (at 6.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 141 S-END))
    (pad 68 smd rect (at 6.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 274 PWM-F))
    (pad 69 smd rect (at 7.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C57-Pad1)"))
    (pad 70 smd rect (at 7.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 181 SCL2))
    (pad 71 smd rect (at 8.25 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 287 ACTIVITY))
    (pad 72 smd rect (at 8.75 10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 108 PWM-C))
    (pad 73 smd rect (at 10.7 8.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 74 smd rect (at 10.7 8.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 75 smd rect (at 10.7 7.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C72-Pad1)"))
    (pad 76 smd rect (at 10.7 7.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 176 DAC0))
    (pad 77 smd rect (at 10.7 6.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 177 DAC1))
    (pad 78 smd rect (at 10.7 6.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 AD7))
    (pad 79 smd rect (at 10.7 5.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 AD6))
    (pad 80 smd rect (at 10.7 5.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 AD5))
    (pad 81 smd rect (at 10.7 4.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 AD4))
    (pad 82 smd rect (at 10.7 4.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 AD3))
    (pad 83 smd rect (at 10.7 3.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 AD2))
    (pad 84 smd rect (at 10.7 3.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 AD1))
    (pad 85 smd rect (at 10.7 2.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 AD0))
    (pad 86 smd rect (at 10.7 2.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 266 SDA))
    (pad 87 smd rect (at 10.7 1.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 265 SCL))
    (pad 88 smd rect (at 10.7 1.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 AD10))
    (pad 89 smd rect (at 10.7 0.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 AD11))
    (pad 90 smd rect (at 10.7 0.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 AD12))
    (pad 91 smd rect (at 10.7 -0.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 101 DIR-D))
    (pad 92 smd rect (at 10.7 -0.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 307 ~SF~-D))
    (pad 93 smd rect (at 10.7 -1.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 308 MOT-EN2))
    (pad 94 smd rect (at 10.7 -1.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 234 BMP-L1))
    (pad 95 smd rect (at 10.7 -2.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 243 BMP-R1))
    (pad 96 smd rect (at 10.7 -2.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 235 BMP-L2))
    (pad 97 smd rect (at 10.7 -3.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 244 BMP-R2))
    (pad 98 smd rect (at 10.7 -3.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 103 DIR-C))
    (pad 99 smd rect (at 10.7 -4.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 309 ~SF~-C))
    (pad 100 smd rect (at 10.7 -4.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 310 DIR-B))
    (pad 101 smd rect (at 10.7 -5.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 311 ~SF~-B))
    (pad 102 smd rect (at 10.7 -5.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 312 MOT-EN1))
    (pad 103 smd rect (at 10.7 -6.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 313 DIR-A))
    (pad 104 smd rect (at 10.7 -6.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 105 smd rect (at 10.7 -7.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 106 smd rect (at 10.7 -7.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 107 smd rect (at 10.7 -8.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 314 ~SF~-A))
    (pad 108 smd rect (at 10.7 -8.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 185 SPI0_MISO))
    (pad 109 smd rect (at 8.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 186 SPI0_MOSI))
    (pad 110 smd rect (at 8.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 187 SPI0_SPCK))
    (pad 111 smd rect (at 7.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 188 SPI0_CS1))
    (pad 112 smd rect (at 7.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 191 SPI0_CS2))
    (pad 113 smd rect (at 6.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 81 ODO-A1))
    (pad 114 smd rect (at 6.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 85 ODO-A2))
    (pad 115 smd rect (at 5.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 82 ODO-B1))
    (pad 116 smd rect (at 5.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 273 PWM-B))
    (pad 117 smd rect (at 4.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 ODO-B2))
    (pad 118 smd rect (at 4.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 83 ODO-C1))
    (pad 119 smd rect (at 3.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 87 ODO-C2))
    (pad 120 smd rect (at 3.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 84 ODO-D1))
    (pad 121 smd rect (at 2.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 88 ODO-D2))
    (pad 122 smd rect (at 2.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 ODO-X1))
    (pad 123 smd rect (at 1.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 ODO-X2))
    (pad 124 smd rect (at 1.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 125 smd rect (at 0.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 126 smd rect (at 0.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 127 smd rect (at -0.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 63 BTTN))
    (pad 128 smd rect (at -0.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 315 "Net-(U6-Pad128)"))
    (pad 129 smd rect (at -1.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 140 UOTGID))
    (pad 130 smd rect (at -1.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(R57-Pad1)"))
    (pad 131 smd rect (at -2.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 316 STEP))
    (pad 132 smd rect (at -2.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 271 PWM-E))
    (pad 133 smd rect (at -3.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 288 PWM-FAN))
    (pad 134 smd rect (at -3.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 256 PWM-Boost))
    (pad 135 smd rect (at -4.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 257 PWM-CC))
    (pad 136 smd rect (at -4.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 276 PWM-H))
    (pad 137 smd rect (at -5.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 317 SDIR))
    (pad 138 smd rect (at -5.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 318 ~SRST))
    (pad 139 smd rect (at -6.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 220 ECHO-1))
    (pad 140 smd rect (at -6.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 222 ECHO-2))
    (pad 141 smd rect (at -7.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 224 ECHO-3))
    (pad 142 smd rect (at -7.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 226 ECHO-4))
    (pad 143 smd rect (at -8.25 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 228 ECHO-5))
    (pad 144 smd rect (at -8.75 -10.7 90) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 230 ECHO-6))
    (model Housings_QFP.3dshapes/LQFP-144_20x20mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 595FE89E)
    (at 116.4 118.6)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U7 (at 0 -1.27) (layer F.Fab))
    (fp_text value LP2986IM-3.3 (at 0.3 -0.1) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C48-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 319 "Net-(U7-Pad7)"))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C48-Pad1)"))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 320 "Net-(U7-Pad2)"))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 320 "Net-(U7-Pad2)"))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 76.9 88.4 90)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U8 (at 0 -6 90) (layer F.Fab))
    (fp_text value SI8238AB-D-IS1 (at 0 6 90) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 256 PWM-Boost))
    (pad 2 smd rect (at -2.7 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 257 PWM-CC))
    (pad 3 smd rect (at -2.7 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 4 smd rect (at -2.7 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -2.7 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.7 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 321 "Net-(U8-Pad6)"))
    (pad 7 smd rect (at -2.7 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 322 "Net-(U8-Pad7)"))
    (pad 8 smd rect (at -2.7 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 9 smd rect (at 2.7 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C61-Pad1)"))
    (pad 10 smd rect (at 2.7 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 261 "Net-(R74-Pad2)"))
    (pad 11 smd rect (at 2.7 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C61-Pad2)"))
    (pad 12 smd rect (at 2.7 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 323 "Net-(U8-Pad12)"))
    (pad 13 smd rect (at 2.7 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 324 "Net-(U8-Pad13)"))
    (pad 14 smd rect (at 2.7 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 2.7 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(R70-Pad2)"))
    (pad 16 smd rect (at 2.7 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C59-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 595FE82A)
    (at 74.4 78.85)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U9 (at -0.09906 -4.24942) (layer F.Fab))
    (fp_text value L78L12A (at -3 -2.25) (layer F.SilkS))
    (pad 1 smd rect (at -1.50114 1.85166) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C59-Pad1)"))
    (pad 2 smd rect (at 0 1.85166) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.50114 1.85166) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 0 -1.09982) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd trapezoid (at 0 0.7493 180) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 595FE825)
    (at 79.4 78.85)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U10 (at -0.09906 -4.24942) (layer F.Fab))
    (fp_text value L78L12A (at 2.7 -3.25) (layer F.SilkS))
    (pad 1 smd rect (at -1.50114 1.85166) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C61-Pad2)"))
    (pad 2 smd rect (at 0 1.85166) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C61-Pad1)"))
    (pad 3 smd rect (at 1.50114 1.85166) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C65-Pad1)"))
    (pad 2 smd rect (at 0 -1.09982) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C61-Pad1)"))
    (pad 2 smd trapezoid (at 0 0.7493 180) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C61-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:QSOP-16_3.9x4.9mm_Pitch0.635mm (layer F.Cu) (tedit 595FF245)
    (at 123.6 117.35 180)
    (descr "16-Lead Plastic Shrink Small Outline Narrow Body (QR)-.150\" Body [QSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U11 (at 0 -3.5 180) (layer F.Fab))
    (fp_text value MAX11617EEE (at -1.3 0.85 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.6543 -2.2225 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 62 AD22))
    (pad 2 smd rect (at -2.6543 -1.5875 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 60 AD21))
    (pad 3 smd rect (at -2.6543 -0.9525 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 61 AD20))
    (pad 4 smd rect (at -2.6543 -0.3175 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 59 AD19))
    (pad 5 smd rect (at -2.6543 0.3175 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 49 AD8))
    (pad 6 smd rect (at -2.6543 0.9525 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 48 AD9))
    (pad 7 smd rect (at -2.6543 1.5875 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 52 AD13))
    (pad 8 smd rect (at -2.6543 2.2225 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 54 AD14))
    (pad 9 smd rect (at 2.6543 2.2225 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 55 AD15))
    (pad 10 smd rect (at 2.6543 1.5875 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 57 AD16))
    (pad 11 smd rect (at 2.6543 0.9525 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 56 AD17))
    (pad 12 smd rect (at 2.6543 0.3175 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 58 AD18))
    (pad 13 smd rect (at 2.6543 -0.3175 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 181 SCL2))
    (pad 14 smd rect (at 2.6543 -0.9525 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 180 SDA2))
    (pad 15 smd rect (at 2.6543 -1.5875 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 2.6543 -2.2225 180) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C82-Pad1)"))
    (model Housings_SSOP.3dshapes/QSOP-16_3.9x4.9mm_Pitch0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 595FEA3C)
    (at 110.4 67.6)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U12 (at 0 -1.27) (layer F.Fab))
    (fp_text value ACS725LLCTR-30AB-T (at 0.9 1.1) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3A))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 280 SIcharge))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C86-Pad1)"))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C78-Pad1)"))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C78-Pad1)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 227.8 154.4 90)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U13 (at 0 -2.6 90) (layer F.Fab))
    (fp_text value PCA9512ADP (at 0 2.6 90) (layer F.SilkS))
    (pad 1 smd rect (at -2.2 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at -2.2 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(P52-Pad4)"))
    (pad 3 smd rect (at -2.2 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 265 SCL))
    (pad 4 smd rect (at -2.2 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.2 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(R84-Pad2)"))
    (pad 6 smd rect (at 2.2 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 266 SDA))
    (pad 7 smd rect (at 2.2 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(P52-Pad3)"))
    (pad 8 smd rect (at 2.2 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (model Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 596037B1)
    (at 190.43 154.61 90)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U14 (at 0 -2.6 90) (layer F.Fab))
    (fp_text value PCA9512ADP (at 0.58 1.14 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.2 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at -2.2 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(P59-Pad4)"))
    (pad 3 smd rect (at -2.2 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 265 SCL))
    (pad 4 smd rect (at -2.2 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.2 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 268 "Net-(R93-Pad2)"))
    (pad 6 smd rect (at 2.2 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 266 SDA))
    (pad 7 smd rect (at 2.2 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(P59-Pad3)"))
    (pad 8 smd rect (at 2.2 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (model Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 596419D8)
    (at 110.075 176.625)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U15 (at 0 -2.85) (layer F.Fab))
    (fp_text value TS30042-M050QFNR (at 0 2.85) (layer F.SilkS))
    (pad 1 smd oval (at -1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C96-Pad1)"))
    (pad 2 smd oval (at -1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 3 smd oval (at -1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 4 smd oval (at -1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd oval (at -0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 6 smd oval (at -0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 325 "Net-(U15-Pad6)"))
    (pad 7 smd oval (at 0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 326 "Net-(U15-Pad7)"))
    (pad 8 smd oval (at 0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 327 "Net-(U15-Pad8)"))
    (pad 9 smd oval (at 1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 328 "Net-(U15-Pad9)"))
    (pad 10 smd oval (at 1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C96-Pad2)"))
    (pad 11 smd oval (at 1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 12 smd oval (at 1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C96-Pad1)"))
    (pad 13 smd oval (at 0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C96-Pad1)"))
    (pad 14 smd oval (at 0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd oval (at -0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd oval (at -0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C96-Pad1)"))
    (pad 17 smd rect (at 0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 17 smd rect (at -0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 595FE853)
    (at 69.8 93.05)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference W12 (at 0 -5.1) (layer F.Fab))
    (fp_text value TST-Boost (at 0.8 1.95) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 256 PWM-Boost))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 69.8 84)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference W13 (at 0 -5.1) (layer F.Fab))
    (fp_text value TST-CC (at 0 -3.1) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 257 PWM-CC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 595FE808)
    (at 78.15 70)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference W14 (at 0 -5.1) (layer F.Fab))
    (fp_text value TST-CHG (at 3.85 -0.2) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(C67-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 59601880)
    (at 162.65 124.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference W15 (at 0 -5.1) (layer F.Fab))
    (fp_text value ~MASTER-RESET (at -1.65 2.1) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 NRSTB))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Crystals:crystal_FA238-TSX3225 (layer F.Cu) (tedit 595FEF75)
    (at 153.8 113 270)
    (descr "crystal Epson Toyocom FA-238 and TSX-3225 series")
    (fp_text reference X1 (at -0.1 -2.3 270) (layer F.Fab))
    (fp_text value 12MHz (at 0 2.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0.8 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C24-Pad1)"))
    (pad 3 smd rect (at 1.1 0.8 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 -0.8 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 -0.8 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C25-Pad1)"))
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 0))
    )
  )
  (module AC-Stuff:POLULU-DUAL_MC33926 (layer F.Cu) (tedit 595FF161)
    (at 207.25 51.825)
    (descr "Polulu Dual MC33926 driver")
    (tags "mc33926 polulu motor driver")
    (fp_text reference X2 (at 0 -5.1) (layer F.Fab))
    (fp_text value Dual_MC33926_1 (at 7.05 43.675) (layer F.SilkS))
    (pad 18 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 FB-A))
    (pad 17 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 314 ~SF~-A))
    (pad 16 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (pad 14 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 272 PWM-A))
    (pad 13 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 313 DIR-A))
    (pad 12 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(JP2-Pad2)"))
    (pad 10 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 312 MOT-EN1))
    (pad 9 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 FB-B))
    (pad 8 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 311 ~SF~-B))
    (pad 7 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (pad 5 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 273 PWM-B))
    (pad 4 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 310 DIR-B))
    (pad 3 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (pad 2 thru_hole oval (at 0 40.64) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole oval (at 0 43.18) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 Vbatt))
    (pad 19 thru_hole oval (at 22.8 30.28) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(D36-Pad2)"))
    (pad 20 thru_hole oval (at 22.8 26.78) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(D36-Pad1)"))
    (pad 21 thru_hole oval (at 22.8 23.28) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 22 thru_hole oval (at 22.8 19.78) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 12 Vbatt))
    (pad 23 thru_hole oval (at 22.8 16.28) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(D35-Pad2)"))
    (pad 24 thru_hole oval (at 22.8 12.78) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(D35-Pad1)"))
  )
  (module AC-Stuff:POLULU-DUAL_MC33926 (layer F.Cu) (tedit 595FF167)
    (at 207.325 99.575)
    (descr "Polulu Dual MC33926 driver")
    (tags "mc33926 polulu motor driver")
    (fp_text reference X3 (at 0 -5.1) (layer F.Fab))
    (fp_text value Dual_MC33926_2 (at 6.375 43.525) (layer F.SilkS))
    (pad 18 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 77 FB-C))
    (pad 17 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 309 ~SF~-C))
    (pad 16 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (pad 14 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 108 PWM-C))
    (pad 13 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 DIR-C))
    (pad 12 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(JP3-Pad2)"))
    (pad 10 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 308 MOT-EN2))
    (pad 9 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 FB-D))
    (pad 8 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 307 ~SF~-D))
    (pad 7 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (pad 5 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(JP4-Pad2)"))
    (pad 4 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(JP1-Pad2)"))
    (pad 3 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 3V3))
    (pad 2 thru_hole oval (at 0 40.64) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole oval (at 0 43.18) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 Vbatt))
    (pad 19 thru_hole oval (at 22.8 30.28) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(D38-Pad2)"))
    (pad 20 thru_hole oval (at 22.8 26.78) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(D38-Pad1)"))
    (pad 21 thru_hole oval (at 22.8 23.28) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 22 thru_hole oval (at 22.8 19.78) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 12 Vbatt))
    (pad 23 thru_hole oval (at 22.8 16.28) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(D37-Pad2)"))
    (pad 24 thru_hole oval (at 22.8 12.78) (size 3 2.8) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(D37-Pad1)"))
  )
  (module AC-Stuff:POLOLU-DRV8825 (layer F.Cu) (tedit 595FE9E6)
    (at 54.12 175.67)
    (fp_text reference X4 (at -0.525 0.2) (layer F.Fab))
    (fp_text value DRV8825_1 (at 0.075 -2.4) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 329 "Net-(X4-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 330 "Net-(X4-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(JP7-Pad2)"))
    (pad 4 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 331 "Net-(X4-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 338 "Net-(C110-Pad1)"))
    (pad 6 thru_hole circle (at -7.62 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 318 ~SRST))
    (pad 7 thru_hole circle (at -7.62 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 316 STEP))
    (pad 8 thru_hole circle (at -7.62 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 317 SDIR))
    (pad 9 thru_hole circle (at 5.08 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole circle (at 5.08 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 298 ~SFLT-1))
    (pad 11 thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(P35-Pad4)"))
    (pad 12 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 152 "Net-(P35-Pad3)"))
    (pad 13 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 151 "Net-(P35-Pad2)"))
    (pad 14 thru_hole circle (at 5.08 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 150 "Net-(P35-Pad1)"))
    (pad 15 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 16 thru_hole circle (at 5.08 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 12 Vbatt))
  )
  (module AC-Stuff:POLOLU-DRV8825 (layer F.Cu) (tedit 595FE9DC)
    (at 54.125 154.8)
    (fp_text reference X5 (at -0.925 1.2) (layer F.Fab))
    (fp_text value DRV8825_2 (at -0.325 -1) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 332 "Net-(X5-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 333 "Net-(X5-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(JP7-Pad2)"))
    (pad 4 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 334 "Net-(X5-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 338 "Net-(C110-Pad1)"))
    (pad 6 thru_hole circle (at -7.62 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 318 ~SRST))
    (pad 7 thru_hole circle (at -7.62 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 316 STEP))
    (pad 8 thru_hole circle (at -7.62 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 317 SDIR))
    (pad 9 thru_hole circle (at 5.08 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole circle (at 5.08 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 299 ~SFLT-2))
    (pad 11 thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 157 "Net-(P36-Pad4)"))
    (pad 12 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 156 "Net-(P36-Pad3)"))
    (pad 13 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 155 "Net-(P36-Pad2)"))
    (pad 14 thru_hole circle (at 5.08 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 154 "Net-(P36-Pad1)"))
    (pad 15 thru_hole circle (at 5.08 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 16 thru_hole circle (at 5.08 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 12 Vbatt))
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59601893)
    (at 164.75 120.8)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference Y1 (at 0 -2.3) (layer F.Fab))
    (fp_text value 32.768KHz (at 0.05 1.6) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C38-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C41-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE966)
    (at 70.4 180.6 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C79 (at 0 -3.937 270) (layer F.Fab))
    (fp_text value 100uF (at 0.1 0 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE957)
    (at 70.4 158.6 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C68 (at 0 -3.937 270) (layer F.Fab))
    (fp_text value 100uF (at -0.05 -0.2 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE96C)
    (at 86.4 180.6 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C84 (at 0 -3.937 270) (layer F.Fab))
    (fp_text value 100uF (at -0.05 -0.25 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE95F)
    (at 86.4 158.6 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C64 (at 0 -3.937 270) (layer F.Fab))
    (fp_text value 100uF (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE95B)
    (at 78.4 158.6 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C73 (at 0 -3.937 270) (layer F.Fab))
    (fp_text value 100uF (at -0.05 0.05 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE968)
    (at 78.4 180.6 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C75 (at 0 -3.937 270) (layer F.Fab))
    (fp_text value 100uF (at 0 -0.25 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_SMD:Choke_SMD_7.3x7.3_H3.5 (layer F.Cu) (tedit 595FE885)
    (at 111.4 105.6)
    (descr "Choke, SMD, 7.3x7.3mm 3.5mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L3 (at 0 -4.445) (layer F.Fab))
    (fp_text value 47uH (at 0.2 0.3) (layer F.SilkS))
    (pad 1 smd rect (at -3.2 0) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 3.2 0) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C48-Pad1)"))
  )
  (module Capacitors_SMD:c_elec_8x10.5 (layer F.Cu) (tedit 595FE8C2)
    (at 87.1 122.9 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (attr smd)
    (fp_text reference C43 (at 0 -5.08 90) (layer F.Fab))
    (fp_text value 470uF (at 0.1 0.1 180) (layer F.SilkS))
    (pad 1 smd rect (at 3.2512 0 90) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at -3.2512 0 90) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeX_EIA-7343 (layer F.Cu) (tedit 595FE8B5)
    (at 94 130.7)
    (descr TantalC_SizeX_EIA-7343)
    (fp_text reference C26 (at 0 -2.7305) (layer F.Fab))
    (fp_text value 47uF (at 0 -0.1 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.99974 0) (size 2.55016 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at -2.99974 0) (size 2.55016 3.79984) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeX_EIA-7343.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_SMD:Choke_SMD_Wuerth-WE-PD2-Typ-MS (layer F.Cu) (tedit 595FE8AB)
    (at 101.3 124.8 90)
    (descr "Choke, Drossel, WE-PD2, Typ MS, Wuerth, SMD,")
    (tags "Choke, Drossel, WE-PD2, Typ MS, Wuerth, SMD,")
    (attr smd)
    (fp_text reference L1 (at 0 -5.08 90) (layer F.Fab))
    (fp_text value 4.7uH (at 3.95 -0.1 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.9304 0 90) (size 2.14884 5.4991) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 1.9304 0 90) (size 2.14884 5.4991) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
  )
  (module Capacitors_SMD:c_elec_8x10.5 (layer F.Cu) (tedit 595FEA7B)
    (at 94.875 169.425 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (attr smd)
    (fp_text reference C102 (at 0 -5.08 90) (layer F.Fab))
    (fp_text value 470uF (at 0.125 0.275 180) (layer F.SilkS))
    (pad 1 smd rect (at 3.2512 0 90) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 2 smd rect (at -3.2512 0 90) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10.5 (layer F.Cu) (tedit 595FE877)
    (at 87.6 106.2 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (attr smd)
    (fp_text reference C42 (at 0 -5.08 90) (layer F.Fab))
    (fp_text value 470uF (at 0.1 0 180) (layer F.SilkS))
    (pad 1 smd rect (at 3.2512 0 90) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at -3.2512 0 90) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_SMD:Choke_SMD_Wuerth-WE-PD2-Typ-MS (layer F.Cu) (tedit 595FE883)
    (at 103 107.6 90)
    (descr "Choke, Drossel, WE-PD2, Typ MS, Wuerth, SMD,")
    (tags "Choke, Drossel, WE-PD2, Typ MS, Wuerth, SMD,")
    (attr smd)
    (fp_text reference L2 (at 0 -5.08 90) (layer F.Fab))
    (fp_text value 4.7uH (at 4.1 -0.8 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.9304 0 90) (size 2.14884 5.4991) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C35-Pad1)"))
    (pad 2 smd rect (at 1.9304 0 90) (size 2.14884 5.4991) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
  )
  (module AC-Stuff:CPCASE-12.5 (layer F.Cu) (tedit 0)
    (at 38.05 119.875 90)
    (descr "Aluminum capacitor 12.5mm diameter, 12.8mm base (NIC)")
    (attr smd)
    (fp_text reference C8 (at 0 0 90) (layer F.Fab))
    (fp_text value 680uF (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -5.05 0 270) (size 5.8 2.5) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 5.05 0 270) (size 5.8 2.5) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(C8-Pad2)"))
  )
  (module Capacitors_SMD:c_elec_8x10.5 (layer F.Cu) (tedit 595FEE03)
    (at 111.8 145.9 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (attr smd)
    (fp_text reference C80 (at 0 -5.08 90) (layer F.Fab))
    (fp_text value 470uF (at 0.04 -0.04 180) (layer F.SilkS))
    (pad 1 smd rect (at 3.2512 0 90) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 30 5Vsec))
    (pad 2 smd rect (at -3.2512 0 90) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AC-Stuff:CPCASE-12.5 (layer F.Cu) (tedit 0)
    (at 73.4 144.5 270)
    (descr "Aluminum capacitor 12.5mm diameter, 12.8mm base (NIC)")
    (attr smd)
    (fp_text reference C10 (at 0 0 270) (layer F.Fab))
    (fp_text value 680uF (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -5.05 0 90) (size 5.8 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 5.05 0 90) (size 5.8 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module AC-Stuff:CPCASE-12.5 (layer F.Cu) (tedit 0)
    (at 227.8 42.8 180)
    (descr "Aluminum capacitor 12.5mm diameter, 12.8mm base (NIC)")
    (attr smd)
    (fp_text reference C9 (at 0 0 180) (layer F.Fab))
    (fp_text value 680uF (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -5.05 0) (size 5.8 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 5.05 0) (size 5.8 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module AC-Stuff:CPCASE-12.5 (layer F.Cu) (tedit 0)
    (at 87.3 144.5 270)
    (descr "Aluminum capacitor 12.5mm diameter, 12.8mm base (NIC)")
    (attr smd)
    (fp_text reference C7 (at 0 0 270) (layer F.Fab))
    (fp_text value 680uF (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -5.05 0 90) (size 5.8 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 Vbatt))
    (pad 2 smd rect (at 5.05 0 90) (size 5.8 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE630)
    (at 149.17 62.47 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C6 (at 0 -3.937 90) (layer F.Fab))
    (fp_text value 100uF (at 0.05 0.025 180) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 90) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at -2.75082 0 90) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE623)
    (at 140.12 62.47 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C5 (at 0 -3.937 90) (layer F.Fab))
    (fp_text value 100uF (at 0.05 0.475 180) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 90) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at -2.75082 0 90) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE697)
    (at 149.07 41.27 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C3 (at 0 -3.937 270) (layer F.Fab))
    (fp_text value 100uF (at -0.025 0.05 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE693)
    (at 139.97 41.27 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C2 (at 0 -3.937 270) (layer F.Fab))
    (fp_text value 100uF (at 0 0.05 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE633)
    (at 158.17 62.47 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C1 (at 0 -3.937 90) (layer F.Fab))
    (fp_text value 100uF (at -0.05 -0.125 180) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 90) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at -2.75082 0 90) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.7 (layer F.Cu) (tedit 595FE69B)
    (at 158.17 41.27 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C4 (at 0 -3.937 270) (layer F.Fab))
    (fp_text value 100uF (at -0.075 -0.05 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FED0E)
    (at 192.9 52.8 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C105 (at 0 -2.3 270) (layer F.Fab))
    (fp_text value 10uF (at -0.11 -0.18 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 595FED0B)
    (at 192.9 61.4 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C106 (at 0 -2.3 90) (layer F.Fab))
    (fp_text value 10uF (at -0.09 0.15 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5964F05A)
    (at 177.6 170.1)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP8 (at 0 -5) (layer F.Fab))
    (fp_text value JP_12V (at -2.4 1.5 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0.06) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 Vbatt))
    (pad 2 thru_hole oval (at 0 2.6) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 335 "Net-(D7-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FEF6C)
    (at 154 106.6 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 0 -1.9 180) (layer F.Fab))
    (fp_text value 10uF (at 0.2 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FF4C2)
    (at 162.95 117.35)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10uF (at 1.45 0.85) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59600161)
    (at 172.2 118.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C50 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10uF (at 0.7 1.3 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5960018C)
    (at 170 119.2 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C49 (at 0 -1.9 270) (layer F.Fab))
    (fp_text value 10uF (at 1.3 -1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 VDDOUT))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 595FFC9C)
    (at 182.8 107)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C74 (at 0 -1.9) (layer F.Fab))
    (fp_text value 10uF (at 2.4 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C72-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 59600979)
    (at 177.2 148.2 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D12 (at 0 -2 270) (layer F.Fab))
    (fp_text value PMEG6010 (at 5 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 9 3V3))
  )
  (module StmSmoke:WirePad_SMD_1x1mm (layer F.Cu) (tedit 5960C261)
    (at 149.8 101.2)
    (fp_text reference W3 (at 0 0.5) (layer F.Fab))
    (fp_text value TST-PB29 (at -0.09412 -2.201001) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 301 "Net-(U6-Pad29)"))
  )
  (module StmSmoke:WirePad_SMD_1x1mm (layer F.Cu) (tedit 5960C257)
    (at 148.05 100.05)
    (fp_text reference W2 (at 0 0.5) (layer F.Fab))
    (fp_text value TST-PB28 (at -0.09412 -2.201001) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 300 "Net-(U6-Pad28)"))
  )
  (module StmSmoke:WirePad_SMD_1x1mm (layer F.Cu) (tedit 5960C26B)
    (at 148.15 102.3)
    (fp_text reference W4 (at 0 0.5) (layer F.Fab))
    (fp_text value TST-PB30 (at -0.09412 -2.201001) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 302 "Net-(U6-Pad30)"))
  )
  (module StmSmoke:WirePad_SMD_1x1mm (layer F.Cu) (tedit 5960C273)
    (at 149.8 103.6)
    (fp_text reference W5 (at 0 0.5) (layer F.Fab))
    (fp_text value TST-PB31 (at -0.09412 -2.201001) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 303 "Net-(U6-Pad31)"))
  )
  (module StmSmoke:WirePad_SMD_1x1mm (layer F.Cu) (tedit 5960C1CF)
    (at 159.7 123.45)
    (fp_text reference W11 (at 0 0.5) (layer F.Fab))
    (fp_text value JTAGSEL (at -0.09412 -2.201001) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 304 "Net-(U6-Pad46)"))
  )
  (module StmSmoke:WirePad_SMD_1x1mm (layer F.Cu) (tedit 5960C1D5)
    (at 159.65 125.62)
    (fp_text reference W16 (at 0 0.5) (layer F.Fab))
    (fp_text value TST (at -0.09412 -2.201001) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 306 "Net-(U6-Pad51)"))
  )
  (module StmSmoke:WirePad_SMD_1x1mm (layer F.Cu) (tedit 5960C304)
    (at 166.85 77.4)
    (fp_text reference W10 (at 0 0.5) (layer F.Fab))
    (fp_text value TST-PB10 (at -0.09412 -2.201001) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 315 "Net-(U6-Pad128)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5964F274)
    (at 49.3 132.7 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP6 (at 3.9 -1 270) (layer F.Fab))
    (fp_text value JP_RL (at 2.9 2.5 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 336 "Net-(JP6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 124 SHDN-RLY))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 337 "Net-(JP6-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module AC-Stuff:Drill-3.5mm (layer F.Cu) (tedit 5964ECDF)
    (at 24 34)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Drill-3.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5965048D)
    (at 43.8 171.9 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C110 (at 0 -2.1 90) (layer F.Fab))
    (fp_text value 0.1uF (at 0.1 -1.5 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 338 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59650478)
    (at 43.9 176.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R119 (at 0 -1.9 90) (layer F.Fab))
    (fp_text value 1K5 (at 0 -1.3 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 318 ~SRST))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 338 "Net-(C110-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 157 (width 0.3) (layer F.Fab)
    (gr_text "6,1811 in" (at 250.15 107.5 270) (layer F.Fab))
    (feature1 (pts (xy 247 186) (xy 251.5 186)))
    (feature2 (pts (xy 247 29) (xy 251.5 29)))
    (crossbar (pts (xy 248.8 29) (xy 248.8 186)))
    (arrow1a (pts (xy 248.8 186) (xy 248.213579 184.873496)))
    (arrow1b (pts (xy 248.8 186) (xy 249.386421 184.873496)))
    (arrow2a (pts (xy 248.8 29) (xy 248.213579 30.126504)))
    (arrow2b (pts (xy 248.8 29) (xy 249.386421 30.126504)))
  )
  (dimension 229 (width 0.3) (layer F.Fab)
    (gr_text "9,0157 in" (at 132.5 25.55) (layer F.Fab))
    (feature1 (pts (xy 247 29) (xy 247 24.2)))
    (feature2 (pts (xy 18 29) (xy 18 24.2)))
    (crossbar (pts (xy 18 26.9) (xy 247 26.9)))
    (arrow1a (pts (xy 247 26.9) (xy 245.873496 27.486421)))
    (arrow1b (pts (xy 247 26.9) (xy 245.873496 26.313579)))
    (arrow2a (pts (xy 18 26.9) (xy 19.126504 27.486421)))
    (arrow2b (pts (xy 18 26.9) (xy 19.126504 26.313579)))
  )
  (dimension 229 (width 0.3) (layer F.Fab)
    (gr_text "229,000 mm" (at 132.5 21.05) (layer F.Fab))
    (feature1 (pts (xy 18 29) (xy 18 19.7)))
    (feature2 (pts (xy 247 29) (xy 247 19.7)))
    (crossbar (pts (xy 247 22.4) (xy 18 22.4)))
    (arrow1a (pts (xy 18 22.4) (xy 19.126504 21.813579)))
    (arrow1b (pts (xy 18 22.4) (xy 19.126504 22.986421)))
    (arrow2a (pts (xy 247 22.4) (xy 245.873496 21.813579)))
    (arrow2b (pts (xy 247 22.4) (xy 245.873496 22.986421)))
  )
  (dimension 157 (width 0.3) (layer F.Fab)
    (gr_text "157,000 mm" (at 252.05 107.5 270) (layer F.Fab))
    (feature1 (pts (xy 247 186) (xy 253.4 186)))
    (feature2 (pts (xy 247 29) (xy 253.4 29)))
    (crossbar (pts (xy 250.7 29) (xy 250.7 186)))
    (arrow1a (pts (xy 250.7 186) (xy 250.113579 184.873496)))
    (arrow1b (pts (xy 250.7 186) (xy 251.286421 184.873496)))
    (arrow2a (pts (xy 250.7 29) (xy 250.113579 30.126504)))
    (arrow2b (pts (xy 250.7 29) (xy 251.286421 30.126504)))
  )
  (gr_text ~CS (at 177.1 66.2 90) (layer F.SilkS))
  (gr_text SPCK (at 179.9 67 90) (layer F.SilkS))
  (gr_text MOSI (at 182.5 67 90) (layer F.SilkS))
  (gr_text MISO (at 185.1 67 90) (layer F.SilkS))
  (gr_text GND (at 187.6 67.1 90) (layer F.SilkS))
  (gr_text +3.3V (at 190 67.1 90) (layer F.SilkS))
  (gr_text RXD (at 196.7 59.6) (layer F.SilkS))
  (gr_text TXD (at 196.7 56.8) (layer F.SilkS))
  (gr_text +3.3V (at 196.4 62.1) (layer F.SilkS))
  (gr_text +5V (at 196.5 51.8) (layer F.SilkS))
  (gr_text GND (at 196.6 54.5) (layer F.SilkS))
  (gr_text M1 (at 245.4 60.9) (layer F.SilkS))
  (gr_text M2 (at 245.4 63.5) (layer F.SilkS))
  (gr_text M2 (at 245.4 81.5) (layer F.SilkS))
  (gr_text M1 (at 245.5 127) (layer F.SilkS))
  (gr_text M1 (at 245.4 78.7) (layer F.SilkS))
  (gr_text M2 (at 245.5 129.7) (layer F.SilkS))
  (gr_text M2 (at 245.1 111.6) (layer F.SilkS))
  (gr_text M1 (at 245.1 108.9) (layer F.SilkS))
  (gr_text GND (at 245.5 132.2) (layer F.SilkS))
  (gr_text GND (at 245.4 114.2) (layer F.SilkS))
  (gr_text GND (at 245.4 84.4) (layer F.SilkS))
  (gr_text GND (at 245.5 66.5) (layer F.SilkS))
  (gr_text +5V (at 245.3 134.8) (layer F.SilkS))
  (gr_text +5V (at 245.2 116.7) (layer F.SilkS))
  (gr_text +5V (at 245.4 86.5) (layer F.SilkS))
  (gr_text +5V (at 245.4 68.6) (layer F.SilkS))
  (gr_text GND (at 210.8 32 90) (layer F.SilkS))
  (gr_text +5V (at 208 32.1 90) (layer F.SilkS))
  (gr_text GND (at 205.5 38.3) (layer F.SilkS))
  (gr_text ECHO (at 164.2 47.8) (layer F.SilkS))
  (gr_text TRIG (at 164.2 50.5) (layer F.SilkS))
  (gr_text GND (at 164.3 53.1) (layer F.SilkS))
  (gr_text +5V (at 164.1 55.7) (layer F.SilkS))
  (gr_text Tx (at 128 63 90) (layer F.SilkS))
  (gr_text Rx (at 126 63 90) (layer F.SilkS))
  (gr_text +5V (at 121 63 90) (layer F.SilkS))
  (gr_text +3.3V (at 131 63 90) (layer F.SilkS))
  (gr_text GND (at 123 63 90) (layer F.SilkS))
  (gr_text GND (at 150 74) (layer F.SilkS))
  (gr_text GND (at 144 92) (layer F.SilkS))
  (gr_text +5V (at 143 90) (layer F.SilkS))
  (gr_text +3.3V (at 143 98) (layer F.SilkS))
  (gr_text +3.3V (at 131 101 90) (layer F.SilkS))
  (gr_text GND (at 124 109 90) (layer F.SilkS))
  (gr_text +5V (at 121 109 90) (layer F.SilkS))
  (gr_text GND (at 148 126) (layer F.SilkS))
  (gr_text GND (at 125 132 90) (layer F.SilkS))
  (gr_text +5V (at 122 132 90) (layer F.SilkS))
  (gr_text GND (at 92 176) (layer F.SilkS))
  (gr_text +5V (at 91 163) (layer F.SilkS))
  (gr_text + (at 199 183) (layer F.SilkS))
  (gr_text + (at 183 173) (layer F.SilkS))
  (gr_text + (at 178 162) (layer F.SilkS))
  (gr_text +3.3V (at 195 125 90) (layer F.SilkS))
  (gr_text GND (at 190 125 90) (layer F.SilkS))
  (gr_text +5V (at 187 125 90) (layer F.SilkS))
  (gr_text GND (at 198 131 90) (layer F.SilkS))
  (gr_text +5V (at 195 131 90) (layer F.SilkS))
  (gr_text "SDA\n" (at 235 152) (layer F.SilkS))
  (gr_text "SCL\n" (at 235 155) (layer F.SilkS))
  (gr_text "GND\n" (at 233 150) (layer F.SilkS))
  (gr_text +3.3V (at 233 158) (layer F.SilkS))
  (gr_text +5V (at 233 147) (layer F.SilkS))
  (gr_line (start 18 186) (end 18 29) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 247 186) (end 18 186) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 247 185) (end 247 186) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 247 29) (end 247 185) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 18 29) (end 247 29) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "PB10\n" (at 167 76) (layer F.SilkS))
  (gr_text "PB31\n" (at 151.73 103.53) (layer F.SilkS))
  (gr_text "PB30\n" (at 150.17 102.3) (layer F.SilkS))
  (gr_text PB29 (at 151.76 101.22) (layer F.SilkS))
  (gr_text "PB28\n\n" (at 149.96 100.51) (layer F.SilkS))
  (gr_text "TST\n\n" (at 159.64 125.06) (layer F.SilkS))
  (gr_text "JTAGSEL\n" (at 159.76 122.31) (layer F.SilkS))
  (gr_text "680uF\n" (at 227.8 42.5 90) (layer F.SilkS))
  (gr_text "680uF\n" (at 37.82 120.16) (layer F.SilkS))
  (gr_text "680uF\n" (at 87.5 144.55) (layer F.SilkS))
  (gr_text "680uF\n" (at 73.55 144.75) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 240 140) (xy 209.8 140) (xy 209.8 141.3) (xy 205 141.3) (xy 205 127.5)
        (xy 202.5 127.5) (xy 202.5 102.5) (xy 205 102.5) (xy 205 45) (xy 167.5 45)
        (xy 167.5 35) (xy 102.5 35) (xy 102.5 70) (xy 110 70) (xy 110 105)
        (xy 105 105) (xy 105 110) (xy 115 110) (xy 115 100) (xy 112.5 100)
        (xy 112.5 75) (xy 115 75) (xy 115 67.5) (xy 110 67.5) (xy 107.5 65)
        (xy 107.5 37.5) (xy 162.5 37.5) (xy 162.5 50) (xy 200 50) (xy 202.5 52.5)
        (xy 202.5 97.5) (xy 200 101.25) (xy 200 132.5) (xy 202.5 132.5) (xy 202.5 145)
        (xy 237.5 145) (xy 237.5 182.5) (xy 117.5 182.5) (xy 117.5 162.5) (xy 102.5 162.5)
        (xy 102.5 147.5) (xy 100 147.5) (xy 100 137.5) (xy 102.5 137.5) (xy 110 130)
        (xy 110 120) (xy 105 120) (xy 105 132.5) (xy 97.5 132.5) (xy 97.5 167.5)
        (xy 112.5 167.5) (xy 112.5 185) (xy 20 185) (xy 20 30) (xy 240 30)
        (xy 240 140)
      )
    )
  )
  (zone (net 278) (net_name "Net-(RL1-Pad12)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.48 123.81) (xy 64.470427 123.865202) (xy 65 125) (xy 65 127.4) (xy 61.4 127.4)
        (xy 61.4 125.588296) (xy 60.78 124.16) (xy 60.78 112.14) (xy 64.48 112.13) (xy 64.48 123.81)
      )
    )
  )
  (zone (net 98) (net_name "Net-(C8-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.02 99.8) (xy 76.3 99.8) (xy 76.3 108.3) (xy 75.02 108.3) (xy 75.02 109.08)
        (xy 70.14 111.4) (xy 70.14 123.22) (xy 65.85 123.24) (xy 65.86 112.15) (xy 64.94 108.31)
        (xy 61.02 108.31) (xy 61.02 108.3) (xy 59.4 108.3) (xy 59.4 99.8) (xy 61.02 99.8)
        (xy 61.02 99.79) (xy 75.02 99.8)
      )
    )
  )
  (zone (net 277) (net_name "Net-(RL1-Pad14)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.14 112.26) (xy 71.14 123.41) (xy 74.43 123.41) (xy 74.42 112.26)
      )
    )
  )
  (zone (net 99) (net_name "Net-(F1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.8 99.4) (xy 35.8 109.2) (xy 55.6 109.2) (xy 55.6 99.4)
      )
    )
  )
  (zone (net 12) (net_name Vbatt) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.999399 128.042066) (xy 72.16 133.87) (xy 86.75 133.88) (xy 88.25 135.83) (xy 96.13 135.83)
        (xy 96.13 136.37) (xy 92.33 142.42) (xy 72.03 142.44) (xy 69.75 138.92) (xy 62.803165 135)
        (xy 61.8 135) (xy 61.8 128) (xy 65 128) (xy 64.999399 128.042066)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C13-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41.4 130.9) (xy 41.4 133.3) (xy 42.377778 134.4) (xy 54.480645 134.4) (xy 56.9 131.9)
        (xy 61.1 131.9) (xy 61.1 135) (xy 57.1 139) (xy 45.3 139) (xy 44.009302 138.354651)
        (xy 40.3 138.39881) (xy 40.3 146.3) (xy 42.6 146.3) (xy 44.2 147.3) (xy 44.2 148.4)
        (xy 43 148.4) (xy 42.7 148.1) (xy 40.3 148.1) (xy 40.3 153.1) (xy 42.5 153.1)
        (xy 42.9 152.9) (xy 44.3 152.9) (xy 44.3 153.9) (xy 43.1168 154.3872) (xy 42.8 155.1)
        (xy 40.3 155.1) (xy 40.3 161.8) (xy 35.2 161.8) (xy 35.2 128.9) (xy 39.5 128.9)
        (xy 41.4 130.9)
      )
    )
  )
  (zone (net 30) (net_name 5Vsec) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.4 159.5) (xy 94.62449 162.5) (xy 98.9 162.5) (xy 101.161905 164.4) (xy 113.6 164.4)
        (xy 113.6 169.5) (xy 104.9 169.5) (xy 102.9 168.1) (xy 96.172727 168.1) (xy 90.2 169)
        (xy 66.3 168.9) (xy 66.3 164.2) (xy 66.7 163.5) (xy 68.2 159.4) (xy 90.4 159.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.7 171.4) (xy 106.7 172.8) (xy 105.6 174.3) (xy 101.7 174.3) (xy 101.7 178.3)
        (xy 102.3 179.3) (xy 102.3 181.1) (xy 98.1 181.1) (xy 93 174.4) (xy 93 170.7)
        (xy 96.8 170.7) (xy 98.5 171.8) (xy 104.4 171.8) (xy 104.9 171.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.3 125.4) (xy 97.9 125.4) (xy 97.9 126.8) (xy 97.867324 126.812394) (xy 97.7 127.9)
        (xy 95 127.9) (xy 92.5 129.1) (xy 92.5 132.2) (xy 94.3 133.3) (xy 94.3 134.6)
        (xy 91.1 134.6) (xy 85.4 128.2) (xy 85.4 124.2) (xy 89.2 124.2) (xy 92.3 125.4)
      )
    )
  )
  (zone (net 9) (net_name 3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104 123.9) (xy 104 121.7) (xy 95 120.4) (xy 92.2 120.4) (xy 89.2 117.7)
        (xy 85.2 117.7) (xy 85.2 121.6) (xy 89.5 121.6) (xy 91.8 123) (xy 94.7 123)
        (xy 96 123.9)
      )
    )
  )
  (zone (net 1) (net_name 5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.9 106.8) (xy 109.1 106.8) (xy 109.1 102.7) (xy 99.8 102.7) (xy 92.9 102.7)
        (xy 89.1 101.1) (xy 86.1 101.1) (xy 86.1 104.9) (xy 92.8 104.9) (xy 93.4 105.2)
        (xy 96.4 105.2) (xy 97.7 106.8)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.3 117.6) (xy 95.3 116.3) (xy 93.7 115.3) (xy 93.7 112.5) (xy 96 111.4)
        (xy 99.3 111.4) (xy 99.5 109.5) (xy 99.5 108.4) (xy 97.3 108.4) (xy 96.2 108.9)
        (xy 93.4 108.9) (xy 89.1 107.7) (xy 86.1 107.7) (xy 86.1 111.4) (xy 92.8 117.6)
      )
    )
  )
  (zone (net 12) (net_name Vbatt) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 240 49) (xy 230 49) (xy 230 35) (xy 124 35) (xy 124 57)
        (xy 117 69) (xy 117 74.3) (xy 91.3 108) (xy 91.2 136.8) (xy 77.4 136.8)
        (xy 77.4 106.6) (xy 83.5 100.1) (xy 83.5 86.4) (xy 110.6 71.7) (xy 110.6 68.7)
        (xy 111 68.7) (xy 111 68) (xy 114 64) (xy 117 56) (xy 117 35)
        (xy 107 35) (xy 107 30) (xy 240 30) (xy 240 49)
      )
    )
  )
  (zone (net 34) (net_name "Net-(C78-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.5 73) (xy 103.3 71.3) (xy 103.3 68.5) (xy 110 68.5) (xy 110 72.1)
        (xy 111.2 73) (xy 111.2 78.7) (xy 105.5 78.7)
      )
    )
  )
  (zone (net 27) (net_name "Net-(C61-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.2 65.6) (xy 89.9 68.8) (xy 88.5 73.1) (xy 88.5 78.7) (xy 94.4 78.7)
        (xy 94.4 73.2) (xy 92.8 71.3) (xy 93.9 65.6)
      )
    )
  )
  (zone (net 32) (net_name "Net-(C67-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.4 74) (xy 72.4 67.5) (xy 76.6 66.5) (xy 78.5 66.5) (xy 79.4 69)
        (xy 79.4 71.3) (xy 76.7 74)
      )
    )
  )
  (zone (net 70) (net_name "Net-(D13-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.7 65.9) (xy 59.1 71.4) (xy 59.7 75.3) (xy 70.7 75.3) (xy 70.7 71)
        (xy 67.6 71) (xy 65.7 69.7) (xy 57.8 67.2) (xy 56.2 65.9)
      )
    )
  )
  (zone (net 29) (net_name Vsolar) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.7 75.3) (xy 36.1 67.7) (xy 36.1 59.7) (xy 40.2 59.7) (xy 40.2 64.9)
        (xy 45.7 66.7) (xy 48.7 67.6) (xy 48.7 75.3)
      )
    )
  )
  (zone (net 100) (net_name "Net-(F2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33.4 46) (xy 35.8 48.8) (xy 35.8 56.8) (xy 40.5 56.8) (xy 40.6 47.9)
        (xy 36 43) (xy 33.4 43)
      )
    )
  )
  (zone (net 68) (net_name Vcharge) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 44.3) (xy 27.9 44.3) (xy 35.8 39.6) (xy 35.8 35.8) (xy 32.4 35.8)
        (xy 22.5 40.4)
      )
    )
  )
  (zone (net 32) (net_name "Net-(C67-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.4 36.1) (xy 41.1 36.1) (xy 50 44.4) (xy 50 51.2) (xy 64.3 56.2)
        (xy 73.7 67.3) (xy 73.8 70.6) (xy 71.9 70.6) (xy 62.5 60.4) (xy 45.9 54.9)
        (xy 44.9 47.3) (xy 38.5 39.1) (xy 38.5 36.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 44) (xy 43 60) (xy 67 60) (xy 67 44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79 44) (xy 79 58) (xy 103 58) (xy 103 44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 44) (xy 67 60) (xy 43 60) (xy 43 44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79 44) (xy 103 44) (xy 103 58) (xy 79 58)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79 44) (xy 79 58) (xy 103 58) (xy 103 44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79 44) (xy 103 44) (xy 103 58) (xy 79 58)
      )
    )
  )
)
