<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="15.24" width="0.2032" layer="20"/>
<wire x1="0" y1="15.24" x2="15.24" y2="15.24" width="0.2032" layer="20"/>
<wire x1="15.24" y1="15.24" x2="15.24" y2="0" width="0.2032" layer="20"/>
<wire x1="15.24" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<text>X</text>
<text>Y</text>
<text>Z</text>
<text>William</text>
<text>FXAS21002</text>
<text>Breakout</text>
<text>GND</text>
<text>INT</text>
<text>SCL</text>
<text>SDA</text>
<text>VCC</text>
<text>W&amp;M Physics</text>
<text>VIMS</text>
<text>William</text>
<text>Laney</text>
<text>FXAS21002</text>
<text>Breakout</text>
<text>2016</text>
<text>VCC</text>
<text>10k</text>
<text>10k</text>
<text>1.0uF</text>
<text>0.1uF</text>
<text>0.1uF</text>
<text>47k</text>
<text>FXAS21002</text>
<text>Laney</text>
<text>0.1uF</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="1X06">
</package>
</packages>
</library>
<library name="sharkdunio">
<packages>
<package name="24QFN">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0805" value="0.1uF"/>
<element name="C2" library="SparkFun-Passives" package="0805" value="0.1uF"/>
<element name="C3" library="SparkFun-Passives" package="0805" value="0.1uF"/>
<element name="C4" library="SparkFun-Passives" package="0805" value="1.0uF"/>
<element name="JP5" library="SparkFun" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="47k"/>
<element name="U$1" library="sharkdunio" package="24QFN" value="FXAS21002"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="21"/>
<contactref element="U$1" pad="22"/>
<contactref element="U$1" pad="23"/>
<contactref element="U$1" pad="24"/>
<contactref element="U$1" pad="20"/>
<contactref element="U$1" pad="19"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="10"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="13"/>
<contactref element="U$1" pad="1"/>
<contactref element="JP5" pad="6"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="11"/>
<contactref element="R1" pad="1"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="12"/>
<contactref element="R2" pad="2"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="18"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="17"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U$1" pad="15"/>
<contactref element="R3" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="16"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="4"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="INT2">
<contactref element="U$1" pad="2"/>
<contactref element="JP5" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
