(kicad_pcb (version 4) (host pcbnew 4.0.4-1.fc25-product)
  (general
    (links 0)
    (no_connects 3)
    (area 32.924999 158.674999 92.775001 207.715001)
    (thickness 1.6)
    (drawings 49)
    (tracks 380)
    (zones 0)
    (modules 31)
    (nets 41)
  )
  (page USLedger)
  (title_block
    (title "Flicker Light Node Hardware")
    (rev 0.1.0)
    (company "Christopher Woodall")
    (comment 1 2016)
    (comment 2 OSHW)
    (comment 3 "CC BY 4.0")
    (comment 4 github.com/cwoodall/flighter-lights-node-hardware)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 33 158.75)
    (grid_origin 33 158.75)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory output/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 +9V)
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(F1-Pad1)")
  (net 8 /LED_BLUE)
  (net 9 "Net-(IC1-Pad2)")
  (net 10 /LED_RED)
  (net 11 /LED_GREEN)
  (net 12 /NRF24_CE)
  (net 13 /NRF24_CSN)
  (net 14 /NRF24_MO)
  (net 15 /NRF24_MI)
  (net 16 /NRF24_SCK)
  (net 17 "Net-(IC1-Pad22)")
  (net 18 "Net-(IC1-Pad25)")
  (net 19 /FTDI_RX)
  (net 20 /FTDI_TX)
  (net 21 "Net-(IC1-Pad28)")
  (net 22 "Net-(P1-Pad3)")
  (net 23 "Net-(P1-Pad6)")
  (net 24 /NRF24_IRQ)
  (net 25 "Net-(P5-Pad2)")
  (net 26 "Net-(P5-Pad3)")
  (net 27 "Net-(P5-Pad4)")
  (net 28 "Net-(P6-Pad2)")
  (net 29 "Net-(P6-Pad3)")
  (net 30 "Net-(P6-Pad4)")
  (net 31 "Net-(IC1-Pad7)")
  (net 32 "Net-(IC1-Pad8)")
  (net 33 "Net-(IC1-Pad12)")
  (net 34 "Net-(IC1-Pad19)")
  (net 35 /VADC)
  (net 36 "Net-(IC1-Pad26)")
  (net 37 "Net-(IC1-Pad27)")
  (net 38 "Net-(IC1-Pad29)")
  (net 39 "Net-(IC1-Pad32)")
  (net 40 "Net-(IC1-Pad24)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +9V)
    (add_net /FTDI_RX)
    (add_net /FTDI_TX)
    (add_net /LED_BLUE)
    (add_net /LED_GREEN)
    (add_net /LED_RED)
    (add_net /NRF24_CE)
    (add_net /NRF24_CSN)
    (add_net /NRF24_IRQ)
    (add_net /NRF24_MI)
    (add_net /NRF24_MO)
    (add_net /NRF24_SCK)
    (add_net /VADC)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad29)")
    (add_net "Net-(IC1-Pad32)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P5-Pad4)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad4)")
  )
  (module Radio_Modules:NRF24L01 (layer F.Cu) (tedit 5587F36C)
    (at 72.5 203.74 270)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference P3 (at -0.59 -1.2 360) (layer F.SilkS))
    (fp_text value CONN_02X04 (at -8.382 7.112 270) (layer F.Fab) hide)
    (pad 7 thru_hole oval (at -9.144 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /NRF24_MI))
    (pad 8 thru_hole oval (at -9.144 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /NRF24_IRQ))
    (pad 5 thru_hole oval (at -6.604 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /NRF24_SCK))
    (pad 6 thru_hole oval (at -6.604 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /NRF24_MO))
    (pad 3 thru_hole oval (at -4.064 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /NRF24_CE))
    (pad 4 thru_hole oval (at -4.064 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /NRF24_CSN))
    (pad 1 thru_hole rect (at -1.524 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 69.5 205.74)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.9 0.01) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 63.75 176.24)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.65 0.01) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 70.9 186.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.41 90) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 48 180.74)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.9 -1.99) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +9V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 47 184.24 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -2 540) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 61.25 168.24)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.45 0.01) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +9V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 72 167.74)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.6 -0.09) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +9V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 45 159.74)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -2.5 0.01) (layer F.SilkS))
    (fp_text value GREEN (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1812 (layer F.Cu) (tedit 5572A4A8)
    (at 37 174.24 270)
    (descr "Resistor SMD 1812, flow soldering, Panasonic (see ERJ12)")
    (tags "resistor 1812")
    (attr smd)
    (fp_text reference F1 (at -0.09 -3.1 360) (layer F.SilkS))
    (fp_text value "PTC RESTTBLE 2.6A 16V CHIP 1812" (at 0 3.175 270) (layer F.Fab))
    (pad 1 smd rect (at -2.4384 0 270) (size 1.6 3.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 2.4384 0 270) (size 1.6 3.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +9V))
  )
  (module xess:HDR_1x6 (layer F.Cu) (tedit 58629A28)
    (at 88.5 178.24 90)
    (descr "PIN HEADER")
    (tags "PIN HEADER")
    (attr virtual)
    (fp_text reference P1 (at -6.41 -2.8 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at -3.81 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -6.35 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(P1-Pad3)"))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /FTDI_RX))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /FTDI_TX))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(P1-Pad6)"))
  )
  (module xess:HDR_1x2 (layer F.Cu) (tedit 58629A4E)
    (at 38.77 168.24)
    (descr "PIN HEADER")
    (tags "PIN HEADER")
    (attr virtual)
    (fp_text reference P2 (at 3.93 0.21) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module xess:HDR_2x3 (layer F.Cu) (tedit 58629A2C)
    (at 87 193.74 270)
    (descr "PIN HEADER")
    (tags "PIN HEADER")
    (attr virtual)
    (fp_text reference P4 (at 2.61 4 360) (layer F.SilkS))
    (fp_text value CONN_02X03 (at -0.381 3.81 270) (layer F.SilkS) hide)
    (pad 5 thru_hole circle (at 2.54 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(IC1-Pad29)"))
    (pad 3 thru_hole circle (at 0 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /NRF24_SCK))
    (pad 1 thru_hole rect (at -2.54 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /NRF24_MI))
    (pad 2 thru_hole circle (at -2.54 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 4 thru_hole circle (at 0 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /NRF24_MO))
    (pad 6 thru_hole circle (at 2.54 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors_Molex:Molex_Microfit3_Header_02x02_Straight_43045-0428 (layer F.Cu) (tedit 55B72257)
    (at 58 163.74)
    (descr "Microfit3 Header Straight 02x02 43045-0428")
    (tags "connector Microfit 02x02 header straight 3mm")
    (fp_text reference P5 (at -8.7 1.01) (layer F.SilkS))
    (fp_text value CONN_01X04 (at -2 -8) (layer F.Fab))
    (pad "" np_thru_hole circle (at -6 -4) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 +9V))
    (pad 2 thru_hole circle (at -3 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P5-Pad2)"))
    (pad 3 thru_hole circle (at 0 -3) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P5-Pad3)"))
    (pad 4 thru_hole circle (at -3 -3) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P5-Pad4)"))
    (pad "" np_thru_hole circle (at 3 -3.94) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connectors_Molex:Molex_Microfit3_Header_02x02_Straight_43045-0428 (layer F.Cu) (tedit 55B72257)
    (at 71 163.74)
    (descr "Microfit3 Header Straight 02x02 43045-0428")
    (tags "connector Microfit 02x02 header straight 3mm")
    (fp_text reference P6 (at -6.4 3.61) (layer F.SilkS))
    (fp_text value CONN_01X04 (at -2 -8) (layer F.Fab))
    (pad "" np_thru_hole circle (at -6 -4) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 +9V))
    (pad 2 thru_hole circle (at -3 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P6-Pad2)"))
    (pad 3 thru_hole circle (at 0 -3) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P6-Pad3)"))
    (pad 4 thru_hole circle (at -3 -3) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P6-Pad4)"))
    (pad "" np_thru_hole circle (at 3 -3.94) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 57.5 171.24)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.8 -0.19) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 11 /LED_GREEN))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P5-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 62 171.24)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -0.8 2.61) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_BLUE))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(P5-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 55 175.74)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -2.8 0.21) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 10 /LED_RED))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P5-Pad4)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 70.5 171.24)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -0.7 2.51) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 11 /LED_GREEN))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P6-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 74 175.24)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at -2.9 0.31) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_BLUE))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P6-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 66.5 171.24)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 2.51) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 10 /LED_RED))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P6-Pad4)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 51.5 180.99 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 360) (layer F.SilkS))
    (fp_text value 200K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +9V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 /VADC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 51.5 184.49 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -0.04 -2.1 360) (layer F.SilkS))
    (fp_text value 100K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 /VADC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 73.75 182.74 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.59 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(IC1-Pad29)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 45 162.74)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 3.3 0.11) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 0)
    (at 40 183.042 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 4.392 3.4 360) (layer F.SilkS))
    (fp_text value LD1117S33CTR (at 0 0.762 90) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302 90) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302 90) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 2.286 3.302 90) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 4 +9V))
    (pad 1 smd rect (at -2.286 3.302 90) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 58629A20)
    (at 76.99 197.31)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580_Pad (at 0 3.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 58629A1D)
    (at 76.99 169.31)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580_Pad (at 0 3.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 58629A1A)
    (at 48.99 169.31)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580_Pad (at 0 3.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Housings_QFP:LQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 64.25 182.74 270)
    (descr "LQFP32: plastic low profile quad flat package; 32 leads; body 7 x 7 x 1.4 mm (see NXP sot358-1_po.pdf and sot358-1_fr.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at -4.49 -5.05 360) (layer F.SilkS))
    (fp_text value ATMEGA168PA-A (at 0 5.85 270) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_BLUE))
    (pad 2 smd rect (at -4.25 -2 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 -0.4 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -4.25 0.4 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 1.2 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -4.25 2 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /LED_RED))
    (pad 10 smd rect (at -2 4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /LED_GREEN))
    (pad 11 smd rect (at -1.2 4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 12 smd rect (at -0.4 4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /NRF24_CE))
    (pad 14 smd rect (at 1.2 4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /NRF24_CSN))
    (pad 15 smd rect (at 2 4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /NRF24_MO))
    (pad 16 smd rect (at 2.8 4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /NRF24_MI))
    (pad 17 smd rect (at 4.25 2.8 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /NRF24_SCK))
    (pad 18 smd rect (at 4.25 2 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 19 smd rect (at 4.25 1.2 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 21 smd rect (at 4.25 -0.4 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 -1.2 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /VADC))
    (pad 24 smd rect (at 4.25 -2.8 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(IC1-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 2 -4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(IC1-Pad29)"))
    (pad 30 smd rect (at -1.2 -4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /FTDI_RX))
    (pad 31 smd rect (at -2 -4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /FTDI_TX))
    (pad 32 smd rect (at -2.8 -4.25) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(IC1-Pad32)"))
    (model Housings_QFP.3dshapes/LQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module xess:oshw-logo2 (layer F.Cu) (tedit 532BC9FC)
    (at 38.5 193.45)
    (fp_text reference "" (at 0.69 -1.09) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
  )
  (gr_text + (at 35.1 168.15) (layer F.SilkS))
  (gr_text FTDI (at 88.5 169.35 360) (layer F.SilkS))
  (gr_text "ICSP\n" (at 87 188.75) (layer F.SilkS))
  (gr_text STATUS (at 48.5 159.75) (layer F.SilkS))
  (gr_text "Flicker Light Node [v 0.1.0]\nC. Woodall - Dec. 2016" (at 82.3 159.35 270) (layer F.SilkS))
  (gr_line (start 84.9 207.64) (end 41.1 207.64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.9 207.64) (end 84.9 199.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 33 199.85) (end 33 165.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.1 199.85) (end 33 199.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.1 207.64) (end 41.1 199.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.7 199.54) (end 84.9 199.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.7 165.75) (end 92.7 199.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.7 165.75) (end 92.7 165.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.7 158.75) (end 84.7 165.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41 158.75) (end 84.7 158.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41 165.74) (end 41 158.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 33 165.74) (end 41 165.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 7 (width 0.3) (layer Dwgs.User)
    (gr_text "7.000 mm" (at 81.35 162.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 87.5 165.75) (xy 80 165.75)))
    (feature2 (pts (xy 87.5 158.75) (xy 80 158.75)))
    (crossbar (pts (xy 82.7 158.75) (xy 82.7 165.75)))
    (arrow1a (pts (xy 82.7 165.75) (xy 82.113579 164.623496)))
    (arrow1b (pts (xy 82.7 165.75) (xy 83.286421 164.623496)))
    (arrow2a (pts (xy 82.7 158.75) (xy 82.113579 159.876504)))
    (arrow2b (pts (xy 82.7 158.75) (xy 83.286421 159.876504)))
  )
  (dimension 8 (width 0.3) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 88.7 155.9) (layer Dwgs.User))
    (feature1 (pts (xy 92.7 159.45) (xy 92.7 154.55)))
    (feature2 (pts (xy 84.7 159.45) (xy 84.7 154.55)))
    (crossbar (pts (xy 84.7 157.25) (xy 92.7 157.25)))
    (arrow1a (pts (xy 92.7 157.25) (xy 91.573496 157.836421)))
    (arrow1b (pts (xy 92.7 157.25) (xy 91.573496 156.663579)))
    (arrow2a (pts (xy 84.7 157.25) (xy 85.826504 157.836421)))
    (arrow2b (pts (xy 84.7 157.25) (xy 85.826504 156.663579)))
  )
  (dimension 7.8 (width 0.3) (layer Dwgs.User)
    (gr_text "7.800 mm" (at 88.85 217.45) (layer Dwgs.User))
    (feature1 (pts (xy 92.75 205) (xy 92.75 218.8)))
    (feature2 (pts (xy 84.95 205) (xy 84.95 218.8)))
    (crossbar (pts (xy 84.95 216.1) (xy 92.75 216.1)))
    (arrow1a (pts (xy 92.75 216.1) (xy 91.623496 215.513579)))
    (arrow1b (pts (xy 92.75 216.1) (xy 91.623496 216.686421)))
    (arrow2a (pts (xy 84.95 216.1) (xy 86.076504 215.513579)))
    (arrow2b (pts (xy 84.95 216.1) (xy 86.076504 216.686421)))
  )
  (dimension 8.1 (width 0.3) (layer Dwgs.User)
    (gr_text "8.100 mm" (at 81.3 203.65 90) (layer Dwgs.User))
    (feature1 (pts (xy 87.55 199.6) (xy 79.95 199.6)))
    (feature2 (pts (xy 87.55 207.7) (xy 79.95 207.7)))
    (crossbar (pts (xy 82.65 207.7) (xy 82.65 199.6)))
    (arrow1a (pts (xy 82.65 199.6) (xy 82.063579 200.726504)))
    (arrow1b (pts (xy 82.65 199.6) (xy 83.236421 200.726504)))
    (arrow2a (pts (xy 82.65 207.7) (xy 82.063579 206.573496)))
    (arrow2b (pts (xy 82.65 207.7) (xy 83.236421 206.573496)))
  )
  (dimension 8.1 (width 0.3) (layer Dwgs.User)
    (gr_text "8.100 mm" (at 37.05 211.3) (layer Dwgs.User))
    (feature1 (pts (xy 41.1 205.05) (xy 41.1 212.65)))
    (feature2 (pts (xy 33 205.05) (xy 33 212.65)))
    (crossbar (pts (xy 33 209.95) (xy 41.1 209.95)))
    (arrow1a (pts (xy 41.1 209.95) (xy 39.973496 210.536421)))
    (arrow1b (pts (xy 41.1 209.95) (xy 39.973496 209.363579)))
    (arrow2a (pts (xy 33 209.95) (xy 34.126504 210.536421)))
    (arrow2b (pts (xy 33 209.95) (xy 34.126504 209.363579)))
  )
  (dimension 7.8 (width 0.3) (layer Dwgs.User)
    (gr_text "7.800 mm" (at 23.25 203.75 90) (layer Dwgs.User))
    (feature1 (pts (xy 35.7 199.85) (xy 21.9 199.85)))
    (feature2 (pts (xy 35.7 207.65) (xy 21.9 207.65)))
    (crossbar (pts (xy 24.6 207.65) (xy 24.6 199.85)))
    (arrow1a (pts (xy 24.6 199.85) (xy 25.186421 200.976504)))
    (arrow1b (pts (xy 24.6 199.85) (xy 24.013579 200.976504)))
    (arrow2a (pts (xy 24.6 207.65) (xy 25.186421 206.523496)))
    (arrow2b (pts (xy 24.6 207.65) (xy 24.013579 206.523496)))
  )
  (dimension 8 (width 0.3) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 37 155.9) (layer Dwgs.User))
    (feature1 (pts (xy 41 159.45) (xy 41 154.55)))
    (feature2 (pts (xy 33 159.45) (xy 33 154.55)))
    (crossbar (pts (xy 33 157.25) (xy 41 157.25)))
    (arrow1a (pts (xy 41 157.25) (xy 39.873496 157.836421)))
    (arrow1b (pts (xy 41 157.25) (xy 39.873496 156.663579)))
    (arrow2a (pts (xy 33 157.25) (xy 34.126504 157.836421)))
    (arrow2b (pts (xy 33 157.25) (xy 34.126504 156.663579)))
  )
  (dimension 7 (width 0.3) (layer Dwgs.User)
    (gr_text "7.000 mm" (at 29.65 162.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 35.8 165.75) (xy 28.3 165.75)))
    (feature2 (pts (xy 35.8 158.75) (xy 28.3 158.75)))
    (crossbar (pts (xy 31 158.75) (xy 31 165.75)))
    (arrow1a (pts (xy 31 165.75) (xy 30.413579 164.623496)))
    (arrow1b (pts (xy 31 165.75) (xy 31.586421 164.623496)))
    (arrow2a (pts (xy 31 158.75) (xy 30.413579 159.876504)))
    (arrow2b (pts (xy 31 158.75) (xy 31.586421 159.876504)))
  )
  (dimension 48.9 (width 0.3) (layer Dwgs.User)
    (gr_text "48.900 mm" (at 27.15 183.2 90) (layer Dwgs.User))
    (feature1 (pts (xy 33 158.75) (xy 25.8 158.75)))
    (feature2 (pts (xy 33 207.65) (xy 25.8 207.65)))
    (crossbar (pts (xy 28.5 207.65) (xy 28.5 158.75)))
    (arrow1a (pts (xy 28.5 158.75) (xy 29.086421 159.876504)))
    (arrow1b (pts (xy 28.5 158.75) (xy 27.913579 159.876504)))
    (arrow2a (pts (xy 28.5 207.65) (xy 29.086421 206.523496)))
    (arrow2b (pts (xy 28.5 207.65) (xy 27.913579 206.523496)))
  )
  (dimension 59.75 (width 0.3) (layer Dwgs.User)
    (gr_text "59.750 mm" (at 62.875 154.4) (layer Dwgs.User))
    (feature1 (pts (xy 92.75 158.75) (xy 92.75 153.05)))
    (feature2 (pts (xy 33 158.75) (xy 33 153.05)))
    (crossbar (pts (xy 33 155.75) (xy 92.75 155.75)))
    (arrow1a (pts (xy 92.75 155.75) (xy 91.623496 156.336421)))
    (arrow1b (pts (xy 92.75 155.75) (xy 91.623496 155.163579)))
    (arrow2a (pts (xy 33 155.75) (xy 34.126504 156.336421)))
    (arrow2b (pts (xy 33 155.75) (xy 34.126504 155.163579)))
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93 158.24) (xy 93 208.24) (xy 31.5 208.24) (xy 31.5 158.24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34 179.24) (xy 39.5 179.24) (xy 39.5 188.24) (xy 33.5 188.24) (xy 33.5 179.24)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31.5 208.24) (xy 93 208.24) (xy 93 158.24) (xy 31.5 158.24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.494 188.468) (xy 55.013933 188.468) (xy 55.013933 211.836) (xy 32.972106 211.836) (xy 32.718106 188.468)
        (xy 42.652 188.468) (xy 43.668 187.452) (xy 47.478 187.452)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.494 188.468) (xy 54.816106 188.468) (xy 54.816106 211.836) (xy 32.972106 211.836) (xy 32.718106 188.468)
        (xy 42.652 188.468) (xy 43.668 187.452) (xy 47.478 187.452)
      )
    )
  )
)
