(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-rc2-dev-329-gd1ab62f)")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 73)
    (zones 0)
    (modules 23)
    (nets 12)
  )
  (page A)
  (title_block
    (title Power5)
    (date 2018-02-16)
    (rev n/c)
    (company dmfe)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2.54)
    (user_trace_width 0.635)
    (user_trace_width 0.889)
    (user_trace_width 1.27)
    (user_trace_width 2.032)
    (user_trace_width 2.54)
    (user_trace_width 3.175)
    (user_trace_width 3.81)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.524)
    (via_drill 0.7112)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 10.16 10.16)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +24V)
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 +5V)
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D3-Pad1)")
  (net 8 "Net-(D5-Pad3)")
  (net 9 "Net-(R1-Pad2)")
  (net 10 "Net-(D7-Pad2)")
  (net 11 "Net-(D8-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 1.524)
    (via_drill 0.7112)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D5-Pad3)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(R1-Pad2)")
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5ABD855F)
    (at 130.81 105.41 180)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D7 (at 5.08 2.54 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (fp_text user %R (at 1.47 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5ABD83F6)
    (at 118.11 105.41)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at -2.660001 -0.3575) (layer F.SilkS))
    (fp_text value 6K8 (at 3.81 1.86) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(D7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5ABD8413)
    (at 118.11 100.33)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at -2.660001 -0.3575) (layer F.SilkS))
    (fp_text value 6K8 (at 3.81 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 5A87BB44)
    (at 81.28 133.985)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 5A87BB29)
    (at 81.28 95.25)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module TO_SOT_Packages_SMD:TO-252-2_Rectifier (layer F.Cu) (tedit 5A8745EE)
    (at 89.535 129.54 90)
    (descr TO-252-2)
    (tags "TO-252-2 Rectifier")
    (attr smd)
    (fp_text reference D6 (at -0.575 -4.55 90) (layer F.SilkS))
    (fp_text value SBR545 (at -0.625 4.8 90) (layer F.Fab))
    (fp_text user %R (at -0.05 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.575 -2.3) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.575 2.28) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.825 0) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2_Rectifier (layer F.Cu) (tedit 5A8745E9)
    (at 161.29 133.985)
    (descr TO-252-2)
    (tags "TO-252-2 Rectifier")
    (attr smd)
    (fp_text reference D5 (at -0.575 -4.55) (layer F.SilkS))
    (fp_text value SBR545 (at -0.625 4.8) (layer F.Fab))
    (fp_text user %R (at -0.05 0) (layer F.Fab))
    (pad 3 smd rect (at 2.825 0 270) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D5-Pad3)"))
    (pad 2 smd rect (at -4.575 2.28 270) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.575 -2.3 270) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2_Rectifier (layer F.Cu) (tedit 5A8745DB)
    (at 99.61 129.54 90)
    (descr TO-252-2)
    (tags "TO-252-2 Rectifier")
    (attr smd)
    (fp_text reference D4 (at -0.575 -4.55 90) (layer F.SilkS))
    (fp_text value SBR545 (at -0.625 4.8 90) (layer F.Fab))
    (fp_text user %R (at -0.05 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.575 -2.3) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.575 2.28) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.825 0) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2_Rectifier (layer F.Cu) (tedit 5A8745D3)
    (at 99.695 113.665 90)
    (descr TO-252-2)
    (tags "TO-252-2 Rectifier")
    (attr smd)
    (fp_text reference D3 (at -0.575 -4.55 90) (layer F.SilkS))
    (fp_text value SBR545 (at -0.625 4.8 90) (layer F.Fab))
    (fp_text user %R (at -0.05 0 90) (layer F.Fab))
    (pad 3 smd rect (at 2.825 0) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (pad 2 smd rect (at -4.575 2.28) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 1 smd rect (at -4.575 -2.3) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2_Rectifier (layer F.Cu) (tedit 5A8745CB)
    (at 109.855 129.54 90)
    (descr TO-252-2)
    (tags "TO-252-2 Rectifier")
    (attr smd)
    (fp_text reference D2 (at -0.575 -4.55 90) (layer F.SilkS))
    (fp_text value SBR545 (at -0.625 4.8 90) (layer F.Fab))
    (fp_text user %R (at -0.05 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.575 -2.3) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.575 2.28) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.825 0) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D14.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 125.095 125.095 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=14mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 14mm Electrolytic Capacitor")
    (fp_text reference C1 (at 0.635 4.445) (layer F.SilkS))
    (fp_text value 330uf (at 2.5 8.31 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D14.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 135.89 116.84 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C2 (at 2.5 -2.26 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 2.5 2.26 90) (layer F.Fab))
    (fp_text user %R (at 2.634999 -0.0725 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 159.385 104.775 90)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C3 (at 1.27 -5.08 180) (layer F.SilkS))
    (fp_text value 4700uf (at 3.75 10.31 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2_Rectifier (layer F.Cu) (tedit 5A87458A)
    (at 109.855 113.665 90)
    (descr TO-252-2)
    (tags "TO-252-2 Rectifier")
    (attr smd)
    (fp_text reference D1 (at -0.575 -4.55 90) (layer F.SilkS))
    (fp_text value SBR545 (at -0.625 4.8 90) (layer F.Fab))
    (fp_text user %R (at -0.05 0 90) (layer F.Fab))
    (pad 3 smd rect (at 2.825 0) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (pad 2 smd rect (at -4.575 2.28) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -4.575 -2.3) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MC-G_04x5.08mm_Angled (layer F.Cu) (tedit 59566E60)
    (at 89.535 103.505 270)
    (descr "Generic Phoenix Contact connector footprint for series: MC-G; number of pins: 04; pin pitch: 5.08mm; Angled || order number: 1836202 8A 320V")
    (tags "phoenix_contact connector MC_01x04_G_5.08mm")
    (fp_text reference J1 (at 7.62 -2.8 270) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 7.62 9 270) (layer F.Fab))
    (fp_text user %R (at -4.445 0.635) (layer F.Fab))
    (pad 4 thru_hole oval (at 15.24 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 10.16 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MC-G_04x5.08mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_Radial_ThroughHole:Choke_Radial_27mm_2,8mm-Drills_CD_Bobin_Type_No1410311 (layer F.Cu) (tedit 0)
    (at 174.625 118.11 270)
    (descr "Choke, Radial, Bobin Type, Diameter, 27mm, 2.8mm Drill, C&D, No.1410311, 22uH, 11A,")
    (tags "Choke, Radial, Bobin Type, Diameter, 27mm, 2.8mm Drill, C&D, No.1410311, 22uH, 11A,")
    (fp_text reference L1 (at 0.635 0) (layer F.SilkS))
    (fp_text value 180uH (at 1.905 14.986 270) (layer F.Fab))
    (pad 2 thru_hole circle (at -12.065 0 270) (size 5.00126 5.00126) (drill 2.79908) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at 12.065 0 270) (size 5.00126 5.00126) (drill 2.79908) (layers *.Cu *.Mask)
      (net 8 "Net-(D5-Pad3)"))
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 139.7 109.22)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at -2.54 0) (layer F.SilkS))
    (fp_text value 68K (at 3.81 1.86) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 147.32 106.045 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 10.16 0 180) (layer F.SilkS))
    (fp_text value Rx1 (at 3.81 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 139.7 102.87)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at -2.660001 -0.3575) (layer F.SilkS))
    (fp_text value 6K8 (at 3.81 1.86) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-5_Horizontal_StaggeredType2 (layer F.Cu) (tedit 5A87B6F9)
    (at 147.32 116.84 180)
    (descr "TO-220-5, Horizontal, RM 1.7mm, Pentawatt, Multiwatt-5, staggered type-2")
    (tags "TO-220-5 Horizontal RM 1.7mm Pentawatt Multiwatt-5 staggered type-2")
    (fp_text reference U1 (at 3.4 -20.1 180) (layer F.SilkS))
    (fp_text value MC34167 (at 3.4 5.7 180) (layer F.Fab))
    (fp_text user %R (at 3.4 -20.1 180) (layer F.Fab))
    (pad 5 thru_hole oval (at 6.8 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 4 thru_hole oval (at 5.1 3.8 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (pad 3 thru_hole oval (at 3.4 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 1.7 3.8 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D5-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (pad 3 thru_hole circle (at 3.4 -16.18 180) (size 10.16 10.16) (drill 3.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-5_Horizontal_StaggeredType2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 5A87BB34)
    (at 184.15 95.25)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 5A87BB3B)
    (at 184.15 133.985)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5ABD8572)
    (at 130.81 100.33 180)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D8 (at 5.08 2.54 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (fp_text user %R (at 1.47 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D8-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text SBR545 (at 159.385 127) (layer F.SilkS))
  (gr_text "2200uF to\n 4700uF" (at 172.085 94.615) (layer F.SilkS))
  (gr_text "330uF 35V" (at 125.095 118.745) (layer F.SilkS))
  (gr_text MC34167 (at 135.89 127.635 90) (layer F.SilkS))
  (gr_text "180uH 5.5A" (at 174.625 114.935) (layer F.SilkS))
  (gr_text In (at 133.985 105.41) (layer F.SilkS))
  (gr_text Out (at 134.62 100.33) (layer F.SilkS))
  (gr_text "5Amp Switching Regulator" (at 122.555 95.25) (layer F.SilkS))
  (gr_text "POWER 5 Rev A" (at 102.235 104.775) (layer F.SilkS))
  (gr_text +OUT (at 80.01 118.745) (layer F.SilkS))
  (gr_text GND (at 79.375 113.665) (layer F.SilkS))
  (gr_text AC (at 78.74 108.585) (layer F.SilkS))
  (gr_text AC (at 78.74 103.505) (layer F.SilkS))
  (gr_text "DMFE 2018" (at 99.695 101.6) (layer F.SilkS))
  (gr_line (start 76.2 139.7) (end 76.2 90.17) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.23 139.7) (end 76.2 139.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.23 90.17) (end 189.23 139.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.2 90.17) (end 189.23 90.17) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.63 90.805) (xy 177.8 90.805) (xy 187.96 101.6) (xy 187.96 127) (xy 177.8 139.065)
        (xy 87.63 139.065) (xy 77.47 128.27) (xy 77.47 101.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.34 91.44) (xy 180.34 99.695) (xy 187.96 99.695) (xy 187.96 91.44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.34 139.065) (xy 180.34 130.175) (xy 187.96 130.175) (xy 187.96 139.065)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.47 130.175) (xy 85.09 130.175) (xy 85.09 137.795) (xy 77.47 137.795)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.47 91.44) (xy 85.725 91.44) (xy 85.725 99.695) (xy 78.105 99.695) (xy 77.47 99.695)
      )
    )
  )
)
