(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 126)
    (no_connects 0)
    (area 99.949999 99.949999 130.050001 165.050001)
    (thickness 1.6)
    (drawings 25)
    (tracks 550)
    (zones 0)
    (modules 60)
    (nets 71)
  )
  (page USLetter portrait)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3556)
    (user_trace_width 0.635)
    (trace_clearance 0.2286)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.254)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.65 1.06)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /AVDD)
  (net 3 /SCL)
  (net 4 /SDA)
  (net 5 "Net-(C1-Pad1)")
  (net 6 GND)
  (net 7 "Net-(C2-Pad1)")
  (net 8 "Net-(C13-Pad2)")
  (net 9 "Net-(C14-Pad2)")
  (net 10 "Net-(C15-Pad2)")
  (net 11 "Net-(C6-Pad1)")
  (net 12 +3V3)
  (net 13 "Net-(C12-Pad1)")
  (net 14 "Net-(C13-Pad1)")
  (net 15 "Net-(C14-Pad1)")
  (net 16 "Net-(C15-Pad1)")
  (net 17 "Net-(C16-Pad1)")
  (net 18 "Net-(C16-Pad2)")
  (net 19 "Net-(C17-Pad1)")
  (net 20 "Net-(C17-Pad2)")
  (net 21 "Net-(C22-Pad1)")
  (net 22 "Net-(C22-Pad2)")
  (net 23 "Net-(C23-Pad1)")
  (net 24 "Net-(C23-Pad2)")
  (net 25 "Net-(JP1-Pad1)")
  (net 26 "Net-(P1-Pad2)")
  (net 27 "Net-(P1-Pad3)")
  (net 28 "Net-(P1-Pad4)")
  (net 29 "Net-(P1-Pad5)")
  (net 30 "Net-(P2-Pad2)")
  (net 31 "Net-(P2-Pad3)")
  (net 32 "Net-(P2-Pad4)")
  (net 33 "Net-(P2-Pad5)")
  (net 34 "Net-(P3-Pad3)")
  (net 35 "Net-(P3-Pad4)")
  (net 36 /PCM_CLK)
  (net 37 /ID_SC)
  (net 38 /ID_SD)
  (net 39 /PCM_FS)
  (net 40 /PCM_DIN)
  (net 41 /PCM_DOUT)
  (net 42 "Net-(R1-Pad1)")
  (net 43 "Net-(R2-Pad1)")
  (net 44 "Net-(R3-Pad2)")
  (net 45 "Net-(R4-Pad2)")
  (net 46 "Net-(R5-Pad2)")
  (net 47 "Net-(R6-Pad2)")
  (net 48 "Net-(R9-Pad1)")
  (net 49 "Net-(R10-Pad1)")
  (net 50 "Net-(U1-Pad2)")
  (net 51 "Net-(P4-Pad7)")
  (net 52 "Net-(P4-Pad8)")
  (net 53 "Net-(P4-Pad10)")
  (net 54 "Net-(P4-Pad11)")
  (net 55 "Net-(P4-Pad13)")
  (net 56 "Net-(P4-Pad15)")
  (net 57 "Net-(P4-Pad16)")
  (net 58 "Net-(P4-Pad18)")
  (net 59 "Net-(P4-Pad19)")
  (net 60 "Net-(P4-Pad21)")
  (net 61 "Net-(P4-Pad22)")
  (net 62 "Net-(P4-Pad23)")
  (net 63 "Net-(P4-Pad24)")
  (net 64 "Net-(P4-Pad26)")
  (net 65 "Net-(P4-Pad29)")
  (net 66 "Net-(P4-Pad31)")
  (net 67 "Net-(P4-Pad32)")
  (net 68 "Net-(P4-Pad33)")
  (net 69 "Net-(P4-Pad36)")
  (net 70 "Net-(P4-Pad37)")
  (net_class Default "This is the default net class."
    (clearance 0.2286)
    (trace_width 0.3556)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net +5V)
    (add_net /AVDD)
    (add_net /ID_SC)
    (add_net /ID_SD)
    (add_net /PCM_CLK)
    (add_net /PCM_DIN)
    (add_net /PCM_DOUT)
    (add_net /PCM_FS)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P4-Pad10)")
    (add_net "Net-(P4-Pad11)")
    (add_net "Net-(P4-Pad13)")
    (add_net "Net-(P4-Pad15)")
    (add_net "Net-(P4-Pad16)")
    (add_net "Net-(P4-Pad18)")
    (add_net "Net-(P4-Pad19)")
    (add_net "Net-(P4-Pad21)")
    (add_net "Net-(P4-Pad22)")
    (add_net "Net-(P4-Pad23)")
    (add_net "Net-(P4-Pad24)")
    (add_net "Net-(P4-Pad26)")
    (add_net "Net-(P4-Pad29)")
    (add_net "Net-(P4-Pad31)")
    (add_net "Net-(P4-Pad32)")
    (add_net "Net-(P4-Pad33)")
    (add_net "Net-(P4-Pad36)")
    (add_net "Net-(P4-Pad37)")
    (add_net "Net-(P4-Pad7)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U1-Pad2)")
  )
  (module OSHW-logo:OSHW-logo_silkscreen-front_4mm (layer F.Cu) (tedit 0)
    (at 117.5 119.25 90)
    (fp_text reference G*** (at 0 2.1209 90) (layer F.SilkS) hide)
    (fp_text value OSHW-logo_silkscreen-front_4mm (at 0 -2.1209 90) (layer F.SilkS) hide)
  )
  (module my_components:Cap_Elec_Radial_5mm (layer F.Cu) (tedit 599E48D5)
    (at 125 108.5 270)
    (descr "Electrolythic Capacitor, Radial, 5 mm diameter,  2 mm lead spacing")
    (tags "CAPACITOR CP")
    (fp_text reference C15 (at -3 2.5 360) (layer F.SilkS))
    (fp_text value 1uF (at 3 2.5 360) (layer F.SilkS))
    (fp_text user + (at -2.25 -2.5 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.00076 0 270) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 1.00076 0 270) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C15-Pad2)"))
    (model discret/c_vert_c2v10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 599DCADE)
    (at 108.5 102 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -1.5 -1.5 180) (layer F.SilkS))
    (fp_text value 22pF (at 0.25 -3 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 599E01C3)
    (at 121.5 102)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2 1.5) (layer F.SilkS))
    (fp_text value 22pF (at 1.25 1.5) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DF10C)
    (at 113 129 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.75 0 180) (layer B.SilkS))
    (fp_text value 220pF (at 4 0 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C13-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DF102)
    (at 113 123 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -2.75 0 180) (layer B.SilkS))
    (fp_text value 220pF (at 0 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DF039)
    (at 121.5 114 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 3 0 180) (layer B.SilkS))
    (fp_text value 220pF (at 0.25 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C15-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DF083)
    (at 115 120 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.25 -1.5 180) (layer B.SilkS))
    (fp_text value 0.01uF (at 1.25 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DEFC9)
    (at 115 114)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 2.25 1.5) (layer B.SilkS))
    (fp_text value 0.1uF (at -1.5 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DEFC2)
    (at 115 105)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 2.25 1.5) (layer B.SilkS))
    (fp_text value 0.1uF (at -1.5 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DF2A8)
    (at 110 158.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -2.25 -1.5 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 1.5 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DF35C)
    (at 115 117 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -3.25 0 180) (layer B.SilkS))
    (fp_text value 0.1uF (at -2.75 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DF33B)
    (at 121.5 117)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 6 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 1.25 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DEF8A)
    (at 121.5 102)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -3.25 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Elec_Radial_5mm (layer F.Cu) (tedit 599E467D)
    (at 114.5 131.75)
    (descr "Electrolythic Capacitor, Radial, 5 mm diameter,  2 mm lead spacing")
    (tags "CAPACITOR CP")
    (fp_text reference C13 (at -3.5 -2) (layer F.SilkS))
    (fp_text value 1uF (at -3.75 -0.5) (layer F.SilkS))
    (fp_text user + (at -3.25 1) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.00076 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 1.00076 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C13-Pad2)"))
    (model discret/c_vert_c2v10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Elec_Radial_5mm (layer F.Cu) (tedit 599E4673)
    (at 114.5 126.25)
    (descr "Electrolythic Capacitor, Radial, 5 mm diameter,  2 mm lead spacing")
    (tags "CAPACITOR CP")
    (fp_text reference C14 (at -3.5 -2) (layer F.SilkS))
    (fp_text value 1uF (at -3.75 -0.5) (layer F.SilkS))
    (fp_text user + (at -3.25 1) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.00076 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at 1.00076 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C14-Pad2)"))
    (model discret/c_vert_c2v10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Elec_Radial_5mm (layer F.Cu) (tedit 599DF464)
    (at 114.5 142.75)
    (descr "Electrolythic Capacitor, Radial, 5 mm diameter,  2 mm lead spacing")
    (tags "CAPACITOR CP")
    (fp_text reference C16 (at -3.5 -3.5) (layer F.SilkS))
    (fp_text value 10uF (at -3.5 -2) (layer F.SilkS))
    (fp_text user + (at -3.25 0.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.00076 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C16-Pad1)"))
    (pad 2 thru_hole circle (at 1.00076 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C16-Pad2)"))
    (model discret/c_vert_c2v10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Elec_Radial_5mm (layer F.Cu) (tedit 599E4625)
    (at 114.5 137.25)
    (descr "Electrolythic Capacitor, Radial, 5 mm diameter,  2 mm lead spacing")
    (tags "CAPACITOR CP")
    (fp_text reference C17 (at -3.75 -3) (layer F.SilkS))
    (fp_text value 10uF (at -3.75 -1.5) (layer F.SilkS))
    (fp_text user + (at -3.25 0.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.00076 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 1.00076 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C17-Pad2)"))
    (model discret/c_vert_c2v10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DF303)
    (at 115 108)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 3.25 0) (layer B.SilkS))
    (fp_text value 10uF (at 2 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DF35F)
    (at 108.5 120)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 1 1.5) (layer B.SilkS))
    (fp_text value 10uF (at 0.75 3) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DF344)
    (at 121.5 120)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 3.5 0) (layer B.SilkS))
    (fp_text value 10uF (at 3 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 599DEFC5)
    (at 115 102 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at -1.75 -1.5 180) (layer B.SilkS))
    (fp_text value 10uF (at 1.75 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Elec_Radial_6.3mm (layer F.Cu) (tedit 599E4698)
    (at 115 156)
    (descr "Electrolythic Capacitor, Radial, 6.3 mm diameter,  2.5 mm lead spacing")
    (tags "CAPACITOR CP")
    (fp_text reference C22 (at -4.5 -3.75) (layer F.SilkS))
    (fp_text value 220uF (at -4.5 -2.25) (layer F.SilkS))
    (fp_text user + (at -3.81 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.25 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(C22-Pad1)"))
    (pad 2 thru_hole circle (at 1.25 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C22-Pad2)"))
    (model discret/c_vert_c2v10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Elec_Radial_6.3mm (layer F.Cu) (tedit 599E468E)
    (at 115 149)
    (descr "Electrolythic Capacitor, Radial, 6.3 mm diameter,  2.5 mm lead spacing")
    (tags "CAPACITOR CP")
    (fp_text reference C23 (at -4.5 -3.75) (layer F.SilkS))
    (fp_text value 220uF (at -4.5 -2.25) (layer F.SilkS))
    (fp_text user + (at -3.81 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.25 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C23-Pad1)"))
    (pad 2 thru_hole circle (at 1.25 0) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C23-Pad2)"))
    (model discret/c_vert_c2v10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Pin_Header_2x1_2.54mm_NoKey (layer F.Cu) (tedit 599DC46F)
    (at 120.5 162)
    (descr "Pin Header, 2x1, 2.54mm pitch, no key")
    (tags "CONN 2x1 NOKEY")
    (fp_text reference JP1 (at -2 2.25) (layer F.SilkS))
    (fp_text value ID_WP (at 2 2.25) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Audio_3.5mm_Stereo (layer F.Cu) (tedit 599E45A8)
    (at 130 127.5 270)
    (descr "Connector, Audio Stereo 3.5mm")
    (tags "3.5MM STEREO AUDIO CONN")
    (fp_text reference P1 (at 5 12.25 270) (layer F.SilkS))
    (fp_text value "Line Input" (at -2.25 12.25 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 2.99974 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole circle (at -5.00126 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at -2.49936 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P1-Pad3)"))
    (pad 4 thru_hole circle (at 2.49936 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at 5.00126 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P1-Pad5)"))
    (pad "" thru_hole circle (at 0 8.001 270) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -5.00126 2.99974 270) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 5.00126 2.99974 270) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
  )
  (module my_components:Conn_Audio_3.5mm_Stereo (layer F.Cu) (tedit 599E45AD)
    (at 130 140 270)
    (descr "Connector, Audio Stereo 3.5mm")
    (tags "3.5MM STEREO AUDIO CONN")
    (fp_text reference P2 (at 5 12.5 270) (layer F.SilkS))
    (fp_text value "Line Output" (at -1.75 12.25 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 2.99974 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole circle (at -5.00126 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P2-Pad2)"))
    (pad 3 thru_hole circle (at -2.49936 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(P2-Pad3)"))
    (pad 4 thru_hole circle (at 2.49936 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P2-Pad4)"))
    (pad 5 thru_hole circle (at 5.00126 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(P2-Pad5)"))
    (pad "" thru_hole circle (at 0 8.001 270) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -5.00126 2.99974 270) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 5.00126 2.99974 270) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
  )
  (module my_components:Conn_Audio_3.5mm_Stereo (layer F.Cu) (tedit 599E4778)
    (at 130 152.5 270)
    (descr "Connector, Audio Stereo 3.5mm")
    (tags "3.5MM STEREO AUDIO CONN")
    (fp_text reference P3 (at 0 12.25 270) (layer F.SilkS))
    (fp_text value Headphones (at 7 9.25 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 2.99974 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole circle (at -5.00126 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C23-Pad2)"))
    (pad 3 thru_hole circle (at -2.49936 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P3-Pad3)"))
    (pad 4 thru_hole circle (at 2.49936 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P3-Pad4)"))
    (pad 5 thru_hole circle (at 5.00126 8.001 270) (size 1.80086 1.80086) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C22-Pad2)"))
    (pad "" thru_hole circle (at 0 8.001 270) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -5.00126 2.99974 270) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 5.00126 2.99974 270) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask F.SilkS))
  )
  (module my_components:Microphone (layer F.Cu) (tedit 599E45EA)
    (at 127 116 270)
    (descr Microphone)
    (tags MICROPHONE)
    (fp_text reference MK1 (at 3 5.75 360) (layer F.SilkS))
    (fp_text value Mic (at 4.5 5.75 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 1.99898 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C15-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 1.99898 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module my_components:Conn_Pin_Header_20x2_2.54mm (layer F.Cu) (tedit 599E55D7)
    (at 103.5 132.5 90)
    (descr "Pin Header, 20x2, 2.54mm pitch")
    (tags "CONN PIN HEADER 20x2")
    (fp_text reference P4 (at -24.25 3.75 90) (layer F.SilkS))
    (fp_text value RPi_Header (at -18.5 3.75 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -24.13 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 +3V3))
    (pad 2 thru_hole circle (at -24.13 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole circle (at -21.59 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SDA))
    (pad 4 thru_hole circle (at -21.59 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 5 thru_hole circle (at -19.05 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SCL))
    (pad 6 thru_hole circle (at -19.05 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 7 thru_hole circle (at -16.51 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(P4-Pad7)"))
    (pad 8 thru_hole circle (at -16.51 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(P4-Pad8)"))
    (pad 9 thru_hole circle (at -13.97 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 10 thru_hole circle (at -13.97 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(P4-Pad10)"))
    (pad 11 thru_hole circle (at -11.43 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(P4-Pad11)"))
    (pad 12 thru_hole circle (at -11.43 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /PCM_CLK))
    (pad 13 thru_hole circle (at -8.89 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(P4-Pad13)"))
    (pad 14 thru_hole circle (at -8.89 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 15 thru_hole circle (at -6.35 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(P4-Pad15)"))
    (pad 16 thru_hole circle (at -6.35 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(P4-Pad16)"))
    (pad 17 thru_hole circle (at -3.81 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 +3V3))
    (pad 18 thru_hole circle (at -3.81 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(P4-Pad18)"))
    (pad 19 thru_hole circle (at -1.27 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(P4-Pad19)"))
    (pad 20 thru_hole circle (at -1.27 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 21 thru_hole circle (at 1.27 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(P4-Pad21)"))
    (pad 22 thru_hole circle (at 1.27 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(P4-Pad22)"))
    (pad 23 thru_hole circle (at 3.81 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(P4-Pad23)"))
    (pad 24 thru_hole circle (at 3.81 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(P4-Pad24)"))
    (pad 25 thru_hole circle (at 6.35 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 26 thru_hole circle (at 6.35 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(P4-Pad26)"))
    (pad 28 thru_hole circle (at 8.89 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /ID_SC))
    (pad 27 thru_hole circle (at 8.89 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /ID_SD))
    (pad 30 thru_hole circle (at 11.43 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 29 thru_hole circle (at 11.43 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(P4-Pad29)"))
    (pad 31 thru_hole circle (at 13.97 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(P4-Pad31)"))
    (pad 32 thru_hole circle (at 13.97 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P4-Pad32)"))
    (pad 33 thru_hole circle (at 16.51 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(P4-Pad33)"))
    (pad 34 thru_hole circle (at 16.51 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 35 thru_hole circle (at 19.05 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /PCM_FS))
    (pad 36 thru_hole circle (at 19.05 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(P4-Pad36)"))
    (pad 37 thru_hole circle (at 21.59 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(P4-Pad37)"))
    (pad 38 thru_hole circle (at 21.59 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /PCM_DIN))
    (pad 39 thru_hole circle (at 24.13 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 40 thru_hole circle (at 24.13 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /PCM_DOUT))
    (model pin_array/pins_array_13x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF2D7)
    (at 108.5 105 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.25 -1.5 180) (layer B.SilkS))
    (fp_text value 33 (at 2.5 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 /SDA))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF2CD)
    (at 108.5 102 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -3 0 180) (layer B.SilkS))
    (fp_text value 33 (at -1.25 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 /SCL))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF332)
    (at 108.5 117)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1 1.5) (layer B.SilkS))
    (fp_text value 33 (at -1.5 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 36 /PCM_CLK))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DEBC5)
    (at 108.5 108)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.5 1.5) (layer B.SilkS))
    (fp_text value 33 (at -1.5 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 41 /PCM_DOUT))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF331)
    (at 108.5 114)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 1 1.5) (layer B.SilkS))
    (fp_text value 33 (at -1.5 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 39 /PCM_FS))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DEBE7)
    (at 108.5 111)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.5 1.5) (layer B.SilkS))
    (fp_text value 33 (at -1.5 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 40 /PCM_DIN))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF19F)
    (at 118.75 145 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -5.75 0 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(P2-Pad5)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C16-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF372)
    (at 118.75 135 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -5.75 0 180) (layer B.SilkS))
    (fp_text value 100 (at 1 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(P2-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C17-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF2E2)
    (at 121.5 105)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 1.5 1.5) (layer B.SilkS))
    (fp_text value 330 (at -1.5 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C15-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF2FC)
    (at 121.5 108)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 6 0) (layer B.SilkS))
    (fp_text value 680 (at 0.75 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C15-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF261)
    (at 116 158.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -3.5 0 360) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF292)
    (at 116 161.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 3.5 -1.25 180) (layer B.SilkS))
    (fp_text value 3.9k (at 0 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 37 /ID_SC))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF38C)
    (at 110 161.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -0.25 -1.5 360) (layer B.SilkS))
    (fp_text value 3.9k (at 3 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 38 /ID_SD))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF36B)
    (at 118.75 129 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -5.75 0 180) (layer B.SilkS))
    (fp_text value 5.6k (at 1 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF370)
    (at 118.75 132)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 5.75 0) (layer B.SilkS))
    (fp_text value 5.6k (at -1 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C13-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(P1-Pad5)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF367)
    (at 118.75 126 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at -5.75 0 180) (layer B.SilkS))
    (fp_text value 5.6k (at 1 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C14-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF0CA)
    (at 118.75 123)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 5.75 0) (layer B.SilkS))
    (fp_text value 5.6k (at -0.25 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(P1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF30D)
    (at 121.5 111)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 1.25 1.5) (layer B.SilkS))
    (fp_text value 47k (at -1.75 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C15-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF1AD)
    (at 118.75 142 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at -5.75 0 180) (layer B.SilkS))
    (fp_text value 47k (at 0 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C16-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF375)
    (at 118.75 138 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at -5.75 0 180) (layer B.SilkS))
    (fp_text value 47k (at 1 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C17-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF23D)
    (at 118.75 154 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at -5.75 0 180) (layer B.SilkS))
    (fp_text value 47k (at 0 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(C22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 599DF37A)
    (at 118.75 151 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at -5.75 0 180) (layer B.SilkS))
    (fp_text value 47k (at 1 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(C23-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_SSOP28 (layer F.Cu) (tedit 599DC5D3)
    (at 116 111)
    (descr SSOP-28)
    (tags SSOP-28)
    (attr smd)
    (fp_text reference U1 (at -3.5 5.5) (layer F.SilkS))
    (fp_text value WM8731 (at 1.75 5.5) (layer F.SilkS))
    (pad 1 smd rect (at -4.225 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at -3.575 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.925 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R3-Pad2)"))
    (pad 4 smd rect (at -2.275 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R4-Pad2)"))
    (pad 5 smd rect (at -1.625 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R5-Pad2)"))
    (pad 6 smd rect (at -0.975 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R6-Pad2)"))
    (pad 7 smd rect (at -0.325 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R5-Pad2)"))
    (pad 8 smd rect (at 0.325 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /AVDD))
    (pad 9 smd rect (at 0.975 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C22-Pad1)"))
    (pad 10 smd rect (at 1.625 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C23-Pad1)"))
    (pad 11 smd rect (at 2.275 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 12 smd rect (at 2.925 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C16-Pad1)"))
    (pad 13 smd rect (at 3.575 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C17-Pad1)"))
    (pad 14 smd rect (at 4.225 3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /AVDD))
    (pad 15 smd rect (at 4.225 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 16 smd rect (at 3.575 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C12-Pad1)"))
    (pad 17 smd rect (at 2.925 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R10-Pad1)"))
    (pad 18 smd rect (at 2.275 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R9-Pad1)"))
    (pad 19 smd rect (at 1.625 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C14-Pad1)"))
    (pad 20 smd rect (at 0.975 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C13-Pad1)"))
    (pad 21 smd rect (at 0.325 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 22 smd rect (at -0.325 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 23 smd rect (at -0.975 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R1-Pad1)"))
    (pad 24 smd rect (at -1.625 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R2-Pad1)"))
    (pad 25 smd rect (at -2.275 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 26 smd rect (at -2.925 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C1-Pad1)"))
    (pad 27 smd rect (at -3.575 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 28 smd rect (at -4.225 -3.6) (size 0.395 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model smd/cms_soj28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.256 0.5 0.25))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_SOT23-5_Hand_Soldering (layer F.Cu) (tedit 599E59D4)
    (at 111 119)
    (descr "5-pin SOT23 package - Hand Soldering")
    (tags IC_SOT23-5_Hand_Soldering)
    (attr smd)
    (fp_text reference U2 (at 0 2.25) (layer F.SilkS))
    (fp_text value TPS79333DBVR (at 0.5 3.75) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.5 0) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at -1.5 0.95) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 1.5 0.95) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (pad 5 smd rect (at 1.5 -0.95) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /AVDD))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_SOIC8_Narrow (layer F.Cu) (tedit 599E5938)
    (at 113 162 270)
    (descr "Module  SOIC 8 Pin Narrow")
    (tags SOIC-8N)
    (attr smd)
    (fp_text reference U3 (at -4.75 2.75 360) (layer F.SilkS))
    (fp_text value CAT24C32W (at -3.25 4.75 360) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 7 smd rect (at -0.635 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(JP1-Pad1)"))
    (pad 6 smd rect (at 0.635 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 37 /ID_SC))
    (pad 5 smd rect (at 1.905 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 38 /ID_SD))
    (pad 4 smd rect (at 1.905 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 0.635 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at -0.635 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -1.905 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model smd/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Crystal_5.0x3.2mm (layer F.Cu) (tedit 599DCAF8)
    (at 115 103 180)
    (descr "Quartz Crystal, 5.0mm x 3.2mm, SMT")
    (tags "CRYSTAL SMT")
    (fp_text reference X1 (at 4 -2.5 180) (layer F.SilkS))
    (fp_text value 12.288MHz (at -1.25 -2.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.9 0 180) (size 1.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.9 0 180) (size 1.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C1-Pad1)"))
  )
  (module my_components:Hole_2.75mm (layer F.Cu) (tedit 599A541D)
    (at 103.5 161.5 90)
    (descr "Mounting Hole, 2.75mm")
    (tags "HOLE 2.75MM")
    (fp_text reference HOLE1 (at 0 -3.048 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.175 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 3.75 3.75) (drill 2.75) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module my_components:Hole_2.75mm (layer F.Cu) (tedit 599A541D)
    (at 103.5 103.5 90)
    (descr "Mounting Hole, 2.75mm")
    (tags "HOLE 2.75MM")
    (fp_text reference HOLE2 (at 0 -3.048 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.175 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 3.75 3.75) (drill 2.75) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module my_components:Hole_2.75mm (layer F.Cu) (tedit 599A541D)
    (at 126.5 161.5 90)
    (descr "Mounting Hole, 2.75mm")
    (tags "HOLE 2.75MM")
    (fp_text reference HOLE3 (at 0 -3.048 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.175 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 3.75 3.75) (drill 2.75) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module my_components:Hole_2.75mm (layer F.Cu) (tedit 599A541D)
    (at 126.5 103.5 90)
    (descr "Mounting Hole, 2.75mm")
    (tags "HOLE 2.75MM")
    (fp_text reference HOLE4 (at 0 -3.048 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.175 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 3.75 3.75) (drill 2.75) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (gr_line (start 100 161.5) (end 100 103.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.5 165) (end 103.5 165) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130 103.5) (end 130 161.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.5 100) (end 126.5 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 103.5 103.5) (end 100 103.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 126.5 103.5) (end 126.5 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 126.5 161.5) (end 130 161.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 103.5 161.5) (end 103.5 165) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text www.malinov.com (at 109.75 111.75 90) (layer F.SilkS))
  (gr_text "I2S Audio pHAT - Version 3.0\n(C) 2014,2017 Sergey Kiselev" (at 107.75 134.25 90) (layer F.SilkS))
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130 165) (xy 100 165) (xy 100 100) (xy 130 100) (xy 130 165)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130 165) (xy 100 165) (xy 100 100) (xy 130 100) (xy 130 165)
      )
    )
  )
)
