<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="108" x2="0" y2="50.25" width="0.254" layer="20"/>
<wire x1="20.32" y1="49.25" x2="20.32" y2="31.47" width="0.254" layer="20"/>
<wire x1="0" y1="30.47" x2="0" y2="1" width="0.254" layer="20"/>
<text>MAIN CONTROL BOARD</text>
<text>LH</text>
<text>1</text>
<text>1</text>
<text>HST</text>
<text>BEAGLEBONE</text>
<text>FPC</text>
<text>ACTUATOR</text>
<wire x1="1" y1="0" x2="220" y2="0" width="0.254" layer="20"/>
<wire x1="1" y1="109" x2="180.340109375" y2="109" width="0.254" layer="20"/>
<wire x1="180.340109375" y1="109" x2="220" y2="86.1" width="0.254" layer="20"/>
<wire x1="220" y1="86.1" x2="220" y2="0" width="0.254" layer="20"/>
<wire x1="1" y1="109" x2="0" y2="108" width="0.254" layer="20" curve="90"/>
<wire x1="20.32" y1="49.25" x2="1" y2="49.25" width="0.254" layer="20"/>
<wire x1="0" y1="50.25" x2="1" y2="49.25" width="0.254" layer="20" curve="90"/>
<wire x1="20.32" y1="31.47" x2="1" y2="31.47" width="0.254" layer="20"/>
<wire x1="1" y1="31.47" x2="0" y2="30.47" width="0.254" layer="20" curve="90"/>
<wire x1="0" y1="1" x2="1" y2="0" width="0.254" layer="20" curve="90"/>
<text>+</text>
<text>+</text>
<text>_</text>
<text>_</text>
<text>LIA_REF</text>
<text>CHAIBIO.COM</text>
<text>001450</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>REV D</text>
<text>FAN_RPM</text>
<text>GND</text>
<text>GND</text>
<text>LHOUT</text>
<text>1</text>
<text>1</text>
<text>NOTES: (UNLESS OTHERWISE SPECIFIED)
1. FABRICATE AND INSPECT PER IPC-6012 CLASS 3 IN CONJUCTION
   WITH SUPPLIED GERBER FILES
2. MATERIAL POLYCLAD TU-768 OR APPROVED EQUIVALENT.
   1 OZ COPPER ALL LAYERS
3. FINISH
  A. SURFACE AND HOLE PLATING FOR HOLES AND VIAS PER 
     IPC-6012, CLASS 3
  B. COPPER SURFACE PLATING TYPE: LEAD-FREE HASL.
  C. APPLY SOLDERMASK TO BOTH SIDES: GREEN.
4. SPECIFIED HOLE DIAMTERS ARE APPLICABLE AFTER PLATING.
5. WARP AND TWIST SHALL NOT EXCEED 0.0075 INCHES PER INCH 
   IN ANY DIRECTION.
6. BOARD MATERIAL SHOULD HAVE A MINIMUM FLAMMABILITY RATING 
   94V-0. FABRICATOR'S UL LOGO OR DESIGNATOR SHALL BE PLACED
   IN A OPEN AREA ON THE BOOTOM SIDE OF THE PCB
7. SOLDERMASK AND SILKSCREEN LEGENDS SHALL NOT INFRINGE ON
   ANY EXPOSED COPPER.
8. FABRICATOR SHALL PRINT AT THE BOTTOM THE DATE OF MANUFACTURE
   AND/OR THE LOT CODE.
9. GERBER LAYERS ARE SHOWN AS VIEWED FROM THE TOP SIDE OF THE
   BOARD.
10. ANY CHANGES MADE BY THE PCB FABRICATOR TO THE PCB FILES
    AND/OR GERBER MUST BE APPROVED BY CHAI BIOTECHNOLOGIES
11. RoHS C OF C REQUIRED WITH EACH DELIVERY</text>
<text>DRILL CHART: TOP TO BOTTOM</text>
<text>SILKSCREEN TOP
SOLDERMASK TOP
TOP (0.333oz + plating)
PP TU-768P (7.485 mil)
L2 (GND)
CORE TU-768 (40.551 mil)
L3 (12V/5V) (1oz)
PP TU-768P (7.320 mil)
BOTTOM (0.333oz + plating)
SOLDERMASK BOTTOM
SILKSCREEN BOTTOM</text>
<text>LAMINATION CROSS-SECTION DETAIL</text>
<text>FINISHED BOARD THICKNESS : 1.6MM +/-0.16 MM</text>
<text>CHAI BIOTECHNOLOGIES</text>
<text>MAINBOARD DUAL CHANNEL PCB</text>
<text>001450</text>
<text>REV D</text>
<text>DWG NO.</text>
<text>REVISION</text>
<text>SIGNATURES</text>
<text>DATE</text>
<text>DRAWN</text>
<text>CHECKED</text>
<text>ENGRG</text>
<text>ISSUED</text>
<text>ECO#</text>
<text>REVISIONS</text>
<text>REV.</text>
<text>DATE</text>
<text>DESCRIPTION</text>
<text>DRWN</text>
<text>CHK'D</text>
<text>APPV'D</text>
<text>D</text>
<text>7-17-16</text>
<text>FIX GROUND OF LID HEATER IC.</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>Fix the +/- 10 V supply.</text>
<text>ADDED BBB MOUNTING HOLES. EMI CONSIDERATIONS. CHANGE 3.3V 
REGULATOR, LCD CONNECTOR POWERED FROM 12V INSTEAD OF
 3.3V. MOVE BBB TO THE LEFT.</text>
<text>2</text>
<text>INITIAL RELEASE</text>
<text>ECO-000117</text>
<text>ECO-000120</text>
<text>ECO-000138</text>
<text>7-17-16</text>
<text>KISTER GENESIS JIMENEZ</text>
<text>KGMJ</text>
<text>FABRICATION FILES: 001450.ZIP
   DRILL FILE: 001450.drd
   OUTLINE: 001450.oln
   TOP COPPER: 001450.L1
   INTERNAL LAYER 2: 001450.L2
   INTERNAL LAYER 3: 001450.L3
   BOTTOM LAYER:  001450.L4
   TOP SILKSCREEN: 001450.slk
   BOTTOM SILKSCREEN: 001450.bsk
   TOP SOLDERMASK: 001450.smt
   BOTTOM SOLDERMASK: 001450.smb
   TOP STENCIL: 001450.tps
   BOTTOM STENCIL: 001450.bps
   IPC FILE: 001450.ipc
</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X4">
</package>
</packages>
</library>
<library name="QPCR-IC">
<packages>
<package name="POWERSSO-12">
</package>
<package name="SO8">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
<package name="QFN38-5X7">
<description>&lt;b&gt;UHF Package 38-Lead Plastic QFN (5mm × 7mm)&lt;/b&gt;&lt;p&gt;
(Reference LTC DWG # 05-08-1701)&lt;br&gt;
Source: &lt;a href="http://cds.linear.com/docs/Datasheet/2444589fb.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="SO23-6L">
</package>
<package name="MULTIPOWERSO-30">
</package>
<package name="SO28W">
<description>&lt;B&gt;28-Lead Plastic Small Outline (SO) &lt;/B&gt; Wide, 300 mil Body (SOIC)&lt;/B&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
</package>
<package name="SOIC20R">
<description>&lt;b&gt;20-LeadStandard Small Outline Package SOIC Wide Body (R-20)&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD811.pdf</description>
</package>
<package name="VQFN-14">
</package>
<package name="DFN14">
</package>
<package name="PG-DSO-8-EP">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="QPCR-switches">
<packages>
<package name="MJTP1236">
</package>
<package name="D2F-FL-A">
</package>
</packages>
</library>
<library name="QPCR-inductor">
<packages>
<package name="MURATA-39H722C">
</package>
<package name="0805">
</package>
<package name="1210">
</package>
</packages>
</library>
<library name="QPCR-connectors">
<packages>
<package name="52893-3096">
<description>&lt;b&gt;52893-3096 ZIF Type (0.5 mm-pitch)&lt;/b&gt; Bottom-contact Type&lt;p&gt;
Easy-On™ Type FFC/FPC Connector, Right Angle, Surface Mount, ZIF, Bottom
Contact Style, Gold Contact Plating, 30 Circuits &lt;p&gt;
Source : http://www.molex.com/webdocs/datasheets/pdf/en-us/0528933096_FFC_FPC_CONNECTORS.pdf</description>
</package>
<package name="MOLEX-1X2_LOCK">
</package>
<package name="PHOENIX1935776">
</package>
<package name="501951-3010">
</package>
<package name="70545-0038">
<description>MOLEX &lt;br/&gt;
Headers &amp; Wire Housings VERT HDR TRI-PEG 4P single row</description>
</package>
<package name="1X02">
</package>
<package name="172065-0002">
</package>
<package name="23X2PTH">
</package>
<package name="78119-X18X">
</package>
</packages>
</library>
<library name="QPCR-capacitors">
<packages>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_FM_A_35V_HORIZONTAL">
</package>
<package name="0603">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="QCPR_specials">
<packages>
<package name=".4064MM">
</package>
<package name="BEAGLEBONE">
</package>
<package name="KF2-M2-ET">
</package>
<package name="S1711-46R">
</package>
<package name="SMTSOB-256-2ET">
</package>
</packages>
</library>
<library name="QCPR-resistors">
<packages>
<package name="0805">
</package>
<package name="0603">
</package>
</packages>
</library>
<library name="QCPR-diodes">
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
</packages>
</library>
<library name="drilegend">
<packages>
<package name="DRILEGEND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC10" library="QPCR-IC" package="SOIC20R" value="001024">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="QPCR-capacitors" package="0805" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="QCPR-resistors" package="0805" value="1.1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="QPCR-capacitors" package="0805" value="0.22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="QPCR-capacitors" package="0805" value="0.22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="QCPR-resistors" package="0805" value="1800">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="QCPR-resistors" package="0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="QCPR-resistors" package="0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U10" library="QCPR_specials" package="BEAGLEBONE" value="BEAGLEBONE">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="QPCR-IC" package="MULTIPOWERSO-30" value="VNH5019A-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="QCPR-resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="QCPR-resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="QCPR-resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="QCPR-resistors" package="0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="QCPR-resistors" package="0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="QPCR-IC" package="MULTIPOWERSO-30" value="VNH5019A-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="QCPR-resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="QCPR-resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="QCPR-resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="QCPR-resistors" package="0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="QCPR-resistors" package="0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="QPCR-IC" package="QFN38-5X7" value="LTC2445CUHF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="QCPR-resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="QCPR-resistors" package="0805" value="6.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HST" library="QPCR-connectors" package="MOLEX-1X2_LOCK" value="22-11-2022"/>
<element name="R14" library="QCPR-resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HBT1" library="QPCR-connectors" package="MOLEX-1X2_LOCK" value="22-11-2022">
<attribute name="NAME"/>
</element>
<element name="HBT2" library="QPCR-connectors" package="MOLEX-1X2_LOCK" value="22-11-2022">
<attribute name="NAME"/>
</element>
<element name="R30" library="QCPR-resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="QCPR-resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="QCPR-resistors" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC15" library="QPCR-IC" package="SOT23-5" value="LVL SHIFTER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC16" library="QPCR-IC" package="SOT23-5" value="LVL SHIFTER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LH" library="SparkFun-Connectors" package="MOLEX-1X4" value="22-11-2042"/>
<element name="LCD_CTP" library="QPCR-connectors" package="52893-3096" value="52893-3096">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="QPCR-capacitors" package="0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="QCPR-resistors" package="0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="QCPR-resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="QCPR-resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="QCPR-resistors" package="0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="QCPR-resistors" package="0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="QCPR-resistors" package="0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R55" library="QCPR-resistors" package="0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R56" library="QCPR-resistors" package="0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R57" library="QCPR-resistors" package="0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R58" library="QCPR-resistors" package="0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="QCPR-resistors" package="0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="QPCR-capacitors" package="PANASONIC_E" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="QPCR-capacitors" package="PANASONIC_FM_A_35V_HORIZONTAL" value="1200uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="QPCR-capacitors" package="PANASONIC_FM_A_35V_HORIZONTAL" value="1200uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC14" library="QPCR-IC" package="POWERSSO-12" value="VN5050J-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="QCPR-resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="QCPR-diodes" package="SMA-DIODE" value="1n4001">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="QPCR-capacitors" package="PANASONIC_E" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="QCPR-resistors" package="0805" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC22" library="QPCR-IC" package="SO23-6L" value="001298">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="QCPR-resistors" package="0805" value="43K 0.1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="QCPR-resistors" package="0805" value="43K 0.1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="QPCR-capacitors" package="0805" value="0.47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="QPCR-capacitors" package="0805" value="0.47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="QCPR-resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="QCPR-resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="QPCR-IC" package="SO8" value="LT1368">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="QCPR-resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="QCPR-resistors" package="0805" value="6.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="QPCR-capacitors" package="PANASONIC_E" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="QPCR-IC" package="SOT23-5" value="74LVC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="QCPR-resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="QPCR-capacitors" package="0805" value="33pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C53" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="QPCR-capacitors" package="0805" value="820pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="QCPR-resistors" package="0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="QPCR-capacitors" package="0805" value="8pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BOOT_SW" library="QPCR-switches" package="MJTP1236" value="MJTP1236">
<attribute name="NAME"/>
</element>
<element name="R48" library="QCPR-resistors" package="0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="QPCR-IC" package="SO8" value="NCP3170">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="QPCR-capacitors" package="PANASONIC_E" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="QCPR-resistors" package="0805" value="24.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R60" library="QCPR-resistors" package="0805" value="4.75k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R61" library="QCPR-resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="QPCR-capacitors" package="0805" value="150pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R62" library="QCPR-resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C57" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="QPCR-inductor" package="MURATA-39H722C" value="7.2uH">
<attribute name="NAME"/>
</element>
<element name="R63" library="QCPR-resistors" package="0603" value="20">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC11" library="QPCR-IC" package="SO8" value="OPA2134">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C58" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C59" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C60" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C61" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C62" library="QPCR-capacitors" package="0805" value="820pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LID_SWITCH" library="QPCR-switches" package="D2F-FL-A" value="001395">
<attribute name="NAME"/>
</element>
<element name="ZONE1" library="QPCR-connectors" package="PHOENIX1935776" value="PELTIER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ZONE2" library="QPCR-connectors" package="PHOENIX1935776" value="PELTIER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED+HEATER" library="QPCR-connectors" package="501951-3010" value="001143">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN" library="QPCR-connectors" package="70545-0038" value="001149">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SHORT2" library="QCPR_specials" package=".4064MM" value="SHORT.4064MM"/>
<element name="C64" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C65" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C66" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C71" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C80" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC13" library="QPCR-IC" package="SOT23-5" value="LVL SHIFTER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HBT3" library="QPCR-connectors" package="1X02" value="M02PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HBT4" library="QPCR-connectors" package="1X02" value="M02PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="QCPR-resistors" package="0805" value="43K 0.1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="QCPR-resistors" package="0805" value="43K 0.1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C84" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C85" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C86" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C87" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C88" library="QPCR-capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C89" library="QPCR-capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INPUT_POWER" library="QPCR-connectors" package="172065-0002" value="001251">
<attribute name="NAME"/>
</element>
<element name="IC12" library="QPCR-IC" package="SO28W" value="001025">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C90" library="QPCR-capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L7" library="QPCR-inductor" package="1210" value="100uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L5" library="QPCR-inductor" package="0805" value="1uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC19" library="QPCR-IC" package="SOT23-5" value="LVL SHIFTER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="QCPR-resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="N1" library="QCPR_specials" package="KF2-M2-ET" value="001399">
<attribute name="NAME"/>
</element>
<element name="N2" library="QCPR_specials" package="KF2-M2-ET" value="001399">
<attribute name="NAME"/>
</element>
<element name="IC8" library="QPCR-IC" package="SOIC20R" value="001024">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="QPCR-capacitors" package="0805" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="QCPR-resistors" package="0805" value="1.1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="QPCR-capacitors" package="0805" value="0.22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C63" library="QPCR-capacitors" package="0805" value="0.22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R64" library="QCPR-resistors" package="0805" value="1800">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R65" library="QCPR-resistors" package="0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R66" library="QCPR-resistors" package="0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C75" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C76" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C77" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C78" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C79" library="QPCR-capacitors" package="0805" value="0.47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C81" library="QPCR-capacitors" package="0805" value="0.47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R67" library="QCPR-resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R68" library="QCPR-resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R69" library="QCPR-resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R70" library="QCPR-resistors" package="0805" value="6.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C82" library="QPCR-capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC17" library="QPCR-IC" package="SO8" value="OPA2134">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC18" library="QPCR-IC" package="SO28W" value="001025">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD_REAR" library="QPCR-connectors" package="78119-X18X" value="001442">
<attribute name="NAME"/>
</element>
<element name="PD_FRONT" library="QPCR-connectors" package="78119-X18X" value="001442">
<attribute name="NAME"/>
</element>
<element name="R71" library="QCPR-resistors" package="0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC23" library="QPCR-IC" package="VQFN-14" value="001552">
<attribute name="NAME"/>
</element>
<element name="P8" library="QPCR-connectors" package="23X2PTH" value="001364">
<attribute name="NAME"/>
</element>
<element name="P9" library="QPCR-connectors" package="23X2PTH" value="001364">
<attribute name="NAME"/>
</element>
<element name="C83" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C91" library="QPCR-capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC20" library="QPCR-IC" package="DFN14" value="001653">
<attribute name="NAME"/>
</element>
<element name="C92" library="QPCR-capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C93" library="QPCR-capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C94" library="QPCR-capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C95" library="QPCR-capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="QPCR-capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C97" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C98" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R72" library="QCPR-resistors" package="0603" value="750K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R73" library="QCPR-resistors" package="0805" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R74" library="QCPR-resistors" package="0603" value="750K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R75" library="QCPR-resistors" package="0805" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="QPCR-inductor" package="0805" value="1uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C96" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="QCPR-resistors" package="0805" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C73" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="QCPR-resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="QCPR-resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C99" library="QPCR-capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C67" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C68" library="QPCR-capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC9" library="QPCR-IC" package="PG-DSO-8-EP" value="001654">
<attribute name="NAME"/>
</element>
<element name="C69" library="QPCR-capacitors" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="QPCR-capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="QCPR-resistors" package="0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="QCPR-resistors" package="0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="QCPR-resistors" package="0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="QCPR-resistors" package="0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SH1" library="QCPR_specials" package="S1711-46R" value="001659">
<attribute name="NAME"/>
</element>
<element name="SH2" library="QCPR_specials" package="S1711-46R" value="001659">
<attribute name="NAME"/>
</element>
<element name="IC2" library="QPCR-IC" package="SOT223" value="001660">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="QPCR-inductor" package="0805" value="1uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="QPCR-capacitors" package="PANASONIC_E" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="QPCR-capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="N3" library="QCPR_specials" package="SMTSOB-256-2ET" value="001669">
<attribute name="NAME"/>
</element>
<element name="N4" library="QCPR_specials" package="SMTSOB-256-2ET" value="001669">
<attribute name="NAME"/>
</element>
<element name="N5" library="QCPR_specials" package="SMTSOB-256-2ET" value="001669">
<attribute name="NAME"/>
</element>
<element name="N6" library="QCPR_specials" package="SMTSOB-256-2ET" value="001669">
<attribute name="NAME"/>
</element>
<element name="C36" library="QPCR-capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DRILEGEND" library="drilegend" package="DRILEGEND" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U10" pad="1"/>
<contactref element="U10" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="IC10" pad="14"/>
<contactref element="C11" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC4" pad="6"/>
<contactref element="IC4" pad="31"/>
<contactref element="IC4" pad="32"/>
<contactref element="IC4" pad="33"/>
<contactref element="IC4" pad="30"/>
<contactref element="IC16" pad="3"/>
<contactref element="IC15" pad="3"/>
<contactref element="R14" pad="1"/>
<contactref element="C27" pad="2"/>
<contactref element="U10" pad="90"/>
<contactref element="U10" pad="89"/>
<contactref element="U10" pad="91"/>
<contactref element="U10" pad="92"/>
<contactref element="IC4" pad="EXP"/>
<contactref element="IC4" pad="1"/>
<contactref element="IC4" pad="4"/>
<contactref element="C33" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="R39" pad="1"/>
<contactref element="R38" pad="1"/>
<contactref element="R51" pad="1"/>
<contactref element="R52" pad="1"/>
<contactref element="R53" pad="1"/>
<contactref element="R54" pad="1"/>
<contactref element="R55" pad="1"/>
<contactref element="R56" pad="1"/>
<contactref element="R57" pad="1"/>
<contactref element="R58" pad="1"/>
<contactref element="IC4" pad="7"/>
<contactref element="IC1" pad="28"/>
<contactref element="IC1" pad="26"/>
<contactref element="IC1" pad="27"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC5" pad="18"/>
<contactref element="IC5" pad="20"/>
<contactref element="IC5" pad="19"/>
<contactref element="IC5" pad="28"/>
<contactref element="IC5" pad="26"/>
<contactref element="IC5" pad="27"/>
<contactref element="C15" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="R33" pad="1"/>
<contactref element="IC22" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="C48" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="C49" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="IC10" pad="17"/>
<contactref element="C12" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="C24" pad="2"/>
<contactref element="LCD_CTP" pad="1"/>
<contactref element="LCD_CTP" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="C53" pad="2"/>
<contactref element="BOOT_SW" pad="1"/>
<contactref element="C17" pad="-"/>
<contactref element="C23" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="IC11" pad="3"/>
<contactref element="IC11" pad="5"/>
<contactref element="HBT1" pad="1"/>
<contactref element="HBT2" pad="1"/>
<contactref element="C58" pad="2"/>
<contactref element="LED+HEATER" pad="P$27"/>
<contactref element="LED+HEATER" pad="P$28"/>
<contactref element="LED+HEATER" pad="P$29"/>
<contactref element="LED+HEATER" pad="P$30"/>
<contactref element="FAN" pad="4"/>
<contactref element="SHORT2" pad="P$1"/>
<contactref element="C80" pad="2"/>
<contactref element="IC13" pad="3"/>
<contactref element="HBT4" pad="2"/>
<contactref element="HBT3" pad="2"/>
<contactref element="C86" pad="2"/>
<contactref element="C87" pad="2"/>
<contactref element="C84" pad="2"/>
<contactref element="C85" pad="2"/>
<contactref element="C88" pad="2"/>
<contactref element="C89" pad="2"/>
<contactref element="INPUT_POWER" pad="P$2"/>
<contactref element="IC12" pad="12"/>
<contactref element="C90" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="IC19" pad="3"/>
<contactref element="IC17" pad="5"/>
<contactref element="R66" pad="1"/>
<contactref element="C75" pad="2"/>
<contactref element="C76" pad="2"/>
<contactref element="C77" pad="2"/>
<contactref element="C78" pad="2"/>
<contactref element="IC18" pad="12"/>
<contactref element="IC8" pad="14"/>
<contactref element="C81" pad="2"/>
<contactref element="C79" pad="2"/>
<contactref element="R69" pad="2"/>
<contactref element="IC8" pad="17"/>
<contactref element="C82" pad="1"/>
<contactref element="IC17" pad="3"/>
<contactref element="C51" pad="2"/>
<contactref element="PD_REAR" pad="P$18"/>
<contactref element="PD_REAR" pad="P$1"/>
<contactref element="PD_FRONT" pad="P$18"/>
<contactref element="PD_FRONT" pad="P$1"/>
<contactref element="IC23" pad="P$1"/>
<contactref element="IC23" pad="P$7"/>
<contactref element="IC23" pad="P$4"/>
<contactref element="IC23" pad="P$13"/>
<contactref element="IC23" pad="P$10"/>
<contactref element="C91" pad="2"/>
<contactref element="C83" pad="2"/>
<contactref element="IC20" pad="P$12"/>
<contactref element="C93" pad="2"/>
<contactref element="C92" pad="2"/>
<contactref element="C95" pad="2"/>
<contactref element="C94" pad="2"/>
<contactref element="IC20" pad="P$15"/>
<contactref element="C98" pad="1"/>
<contactref element="C97" pad="2"/>
<contactref element="R73" pad="1"/>
<contactref element="R75" pad="2"/>
<contactref element="C19" pad="-"/>
<contactref element="C96" pad="2"/>
<contactref element="C71" pad="2"/>
<contactref element="R35" pad="1"/>
<contactref element="C73" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="R37" pad="2"/>
<contactref element="C99" pad="2"/>
<contactref element="C67" pad="2"/>
<contactref element="C68" pad="1"/>
<contactref element="IC9" pad="P$6"/>
<contactref element="IC9" pad="P$9"/>
<contactref element="C65" pad="2"/>
<contactref element="C60" pad="2"/>
<contactref element="C59" pad="2"/>
<contactref element="C66" pad="2"/>
<contactref element="C64" pad="2"/>
<contactref element="C61" pad="2"/>
<contactref element="C62" pad="2"/>
<contactref element="C14" pad="-"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="LED+HEATER" pad="P$8"/>
<contactref element="LED+HEATER" pad="P$9"/>
<contactref element="LED+HEATER" pad="P$13"/>
<contactref element="LED+HEATER" pad="P$12"/>
<contactref element="LED+HEATER" pad="P$11"/>
<contactref element="LED+HEATER" pad="P$10"/>
<contactref element="LED+HEATER" pad="P$14"/>
<contactref element="U10" pad="M4"/>
<contactref element="U10" pad="M3"/>
<contactref element="U10" pad="M2"/>
<contactref element="U10" pad="M1"/>
<contactref element="R23" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="SH2" pad="P1"/>
<contactref element="SH1" pad="P1"/>
<contactref element="IC2" pad="1"/>
<contactref element="C35" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C28" pad="-"/>
<contactref element="C25" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="C40" pad="-"/>
<contactref element="C22" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="LH" pad="4"/>
<contactref element="LH" pad="3"/>
<contactref element="LCD_CTP" pad="3"/>
<contactref element="U10" pad="47"/>
<contactref element="U10" pad="48"/>
<contactref element="IC14" pad="P$2"/>
<contactref element="IC14" pad="P$1"/>
<contactref element="C36" pad="2"/>
</signal>
<signal name="VDD_3V3EXP">
<contactref element="U10" pad="49"/>
<contactref element="U10" pad="50"/>
</signal>
<signal name="SYS_5V">
<contactref element="U10" pad="53"/>
</signal>
<signal name="DIM">
<contactref element="U10" pad="88"/>
<contactref element="LCD_CTP" pad="28"/>
</signal>
<signal name="B11">
<contactref element="U10" pad="45"/>
<contactref element="LCD_CTP" pad="11"/>
</signal>
<signal name="B12">
<contactref element="U10" pad="46"/>
<contactref element="LCD_CTP" pad="10"/>
</signal>
<signal name="B13">
<contactref element="U10" pad="43"/>
<contactref element="LCD_CTP" pad="9"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="B14">
<contactref element="U10" pad="44"/>
<contactref element="LCD_CTP" pad="8"/>
</signal>
<signal name="B15">
<contactref element="U10" pad="41"/>
<contactref element="LCD_CTP" pad="7"/>
</signal>
<signal name="G13">
<contactref element="U10" pad="42"/>
<contactref element="LCD_CTP" pad="17"/>
</signal>
<signal name="G14">
<contactref element="U10" pad="39"/>
<contactref element="LCD_CTP" pad="16"/>
</signal>
<signal name="G15">
<contactref element="U10" pad="40"/>
<contactref element="LCD_CTP" pad="15"/>
</signal>
<signal name="G16">
<contactref element="U10" pad="37"/>
<contactref element="LCD_CTP" pad="14"/>
</signal>
<signal name="G17">
<contactref element="U10" pad="36"/>
<contactref element="LCD_CTP" pad="13"/>
</signal>
<signal name="R11">
<contactref element="U10" pad="34"/>
<contactref element="LCD_CTP" pad="22"/>
</signal>
<signal name="R12">
<contactref element="U10" pad="35"/>
<contactref element="LCD_CTP" pad="21"/>
</signal>
<signal name="R13">
<contactref element="U10" pad="31"/>
<contactref element="LCD_CTP" pad="20"/>
</signal>
<signal name="R14">
<contactref element="U10" pad="32"/>
<contactref element="LCD_CTP" pad="19"/>
</signal>
<signal name="LCD_EN">
<contactref element="U10" pad="30"/>
<contactref element="LCD_CTP" pad="23"/>
</signal>
<signal name="LCD_HSYNC">
<contactref element="U10" pad="29"/>
<contactref element="LCD_CTP" pad="25"/>
</signal>
<signal name="LCD_PCLK">
<contactref element="U10" pad="28"/>
<contactref element="LCD_CTP" pad="27"/>
</signal>
<signal name="LCD_VSYNC">
<contactref element="U10" pad="27"/>
<contactref element="LCD_CTP" pad="24"/>
</signal>
<signal name="LCD_ON/OFF">
<contactref element="U10" pad="73"/>
<contactref element="LCD_CTP" pad="26"/>
</signal>
<signal name="R15">
<contactref element="U10" pad="33"/>
<contactref element="LCD_CTP" pad="18"/>
</signal>
<signal name="G18">
<contactref element="U10" pad="38"/>
<contactref element="LCD_CTP" pad="12"/>
</signal>
<signal name="I2C_SDA">
<contactref element="U10" pad="66"/>
<contactref element="LCD_CTP" pad="6"/>
</signal>
<signal name="RST">
<contactref element="U10" pad="56"/>
</signal>
<signal name="I2C_IRQ">
<contactref element="U10" pad="69"/>
<contactref element="LCD_CTP" pad="4"/>
</signal>
<signal name="I2C_SCL">
<contactref element="U10" pad="65"/>
<contactref element="LCD_CTP" pad="5"/>
</signal>
<signal name="PELTIER1_PWM">
<contactref element="U10" pad="13"/>
<contactref element="R57" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="PELTIER2_PWM">
<contactref element="U10" pad="19"/>
<contactref element="R58" pad="2"/>
<contactref element="R43" pad="1"/>
</signal>
<signal name="MOSI1">
<contactref element="U10" pad="76"/>
<contactref element="LED+HEATER" pad="P$23"/>
</signal>
<signal name="SCK1">
<contactref element="U10" pad="77"/>
<contactref element="LED+HEATER" pad="P$21"/>
</signal>
<signal name="MUX_CONTROL_PIN0">
<contactref element="IC12" pad="17"/>
<contactref element="IC18" pad="17"/>
<contactref element="IC23" pad="P$3"/>
</signal>
<signal name="MUX_CONTROL_PIN1">
<contactref element="IC12" pad="16"/>
<contactref element="IC18" pad="16"/>
<contactref element="IC23" pad="P$6"/>
</signal>
<signal name="MUX_CONTROL_PIN2">
<contactref element="IC12" pad="15"/>
<contactref element="IC18" pad="15"/>
<contactref element="IC23" pad="P$11"/>
</signal>
<signal name="MUX_CONTROL_PIN3">
<contactref element="IC12" pad="14"/>
<contactref element="IC18" pad="14"/>
<contactref element="IC23" pad="P$8"/>
</signal>
<signal name="SPI_CS">
<contactref element="IC4" pad="36"/>
<contactref element="U10" pad="63"/>
</signal>
<signal name="SCK0">
<contactref element="U10" pad="68"/>
<contactref element="IC4" pad="38"/>
</signal>
<signal name="MOSI0">
<contactref element="U10" pad="64"/>
<contactref element="IC15" pad="2"/>
</signal>
<signal name="MISO0">
<contactref element="U10" pad="67"/>
<contactref element="IC16" pad="4"/>
</signal>
<signal name="PELTIER2_INB">
<contactref element="U10" pad="17"/>
<contactref element="R42" pad="1"/>
<contactref element="R53" pad="2"/>
</signal>
<signal name="PELTIER2_INA">
<contactref element="U10" pad="15"/>
<contactref element="R41" pad="1"/>
<contactref element="R54" pad="2"/>
</signal>
<signal name="PELTIER1_INB">
<contactref element="U10" pad="11"/>
<contactref element="R8" pad="1"/>
<contactref element="R55" pad="2"/>
</signal>
<signal name="PELTIER1_INA">
<contactref element="U10" pad="9"/>
<contactref element="R7" pad="1"/>
<contactref element="R56" pad="2"/>
</signal>
<signal name="MISO1">
<contactref element="U10" pad="75"/>
<contactref element="LED+HEATER" pad="P$26"/>
</signal>
<signal name="LED_DIGIPOT_CS">
<contactref element="U10" pad="18"/>
<contactref element="LED+HEATER" pad="P$20"/>
<contactref element="R71" pad="1"/>
</signal>
<signal name="LED_CONTROL_CS">
<contactref element="U10" pad="12"/>
<contactref element="LED+HEATER" pad="P$24"/>
</signal>
<signal name="XERR">
<contactref element="U10" pad="8"/>
<contactref element="LED+HEATER" pad="P$18"/>
</signal>
<signal name="VPRG">
<contactref element="U10" pad="14"/>
<contactref element="LED+HEATER" pad="P$19"/>
</signal>
<signal name="LID_OPEN/CLOSE">
<contactref element="U10" pad="26"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="FAN_PWM">
<contactref element="R52" pad="2"/>
<contactref element="U10" pad="60"/>
<contactref element="IC19" pad="2"/>
</signal>
<signal name="LID_HEATER_PWM">
<contactref element="R51" pad="2"/>
<contactref element="IC14" pad="P$3"/>
<contactref element="U10" pad="62"/>
</signal>
<signal name="FAN_RPM">
<contactref element="R30" pad="1"/>
<contactref element="R32" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="IC11" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="C27" pad="1"/>
<contactref element="U10" pad="52"/>
<contactref element="U10" pad="51"/>
<contactref element="C53" pad="1"/>
<contactref element="C54" pad="1"/>
<contactref element="R63" pad="2"/>
<contactref element="LED+HEATER" pad="P$15"/>
<contactref element="LED+HEATER" pad="P$16"/>
<contactref element="IC19" pad="5"/>
<contactref element="L4" pad="P$1"/>
<contactref element="IC23" pad="P$14"/>
<contactref element="IC15" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="IC5" pad="23"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC5" pad="13"/>
<contactref element="IC1" pad="23"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="13"/>
<contactref element="R31" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="C38" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C37" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="IC14" pad="P$13"/>
<contactref element="C40" pad="+"/>
<contactref element="C42" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="FAN" pad="3"/>
<contactref element="C66" pad="1"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC5" pad="12"/>
<contactref element="INPUT_POWER" pad="P$1"/>
<contactref element="L2" pad="1"/>
<contactref element="L7" pad="1"/>
<contactref element="C99" pad="1"/>
<contactref element="C14" pad="+"/>
<contactref element="L5" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="LCD_CTP" pad="29"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="C4" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="IC11" pad="6"/>
</signal>
<signal name="N$42">
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="IC10" pad="1"/>
<contactref element="IC10" pad="16"/>
<contactref element="IC11" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="IC10" pad="19"/>
<contactref element="IC10" pad="15"/>
<contactref element="IC10" pad="20"/>
</signal>
<signal name="N$33">
<contactref element="IC10" pad="12"/>
<contactref element="IC10" pad="13"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="IC16" pad="5"/>
<contactref element="R5" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R40" pad="2"/>
<contactref element="R44" pad="1"/>
<contactref element="R45" pad="2"/>
<contactref element="IC3" pad="5"/>
<contactref element="LID_SWITCH" pad="COM"/>
<contactref element="LED+HEATER" pad="P$17"/>
<contactref element="IC13" pad="5"/>
<contactref element="R71" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="2"/>
<contactref element="C35" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="LCD_CTP" pad="30"/>
<contactref element="IC6" pad="6"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="OUTA2">
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="25"/>
<contactref element="IC1" pad="30"/>
<contactref element="ZONE1" pad="2"/>
</signal>
<signal name="OUTB2">
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC1" pad="21"/>
<contactref element="ZONE1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R7" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="C86" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="C87" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="IC1" pad="5"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="IC1" pad="9"/>
<contactref element="R40" pad="1"/>
</signal>
<signal name="OUTA3">
<contactref element="IC5" pad="1"/>
<contactref element="IC5" pad="25"/>
<contactref element="IC5" pad="30"/>
<contactref element="ZONE2" pad="2"/>
</signal>
<signal name="OUTB3">
<contactref element="IC5" pad="15"/>
<contactref element="IC5" pad="16"/>
<contactref element="IC5" pad="21"/>
<contactref element="ZONE2" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="R41" pad="2"/>
<contactref element="IC5" pad="4"/>
<contactref element="C84" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="R42" pad="2"/>
<contactref element="IC5" pad="10"/>
<contactref element="C85" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="R43" pad="2"/>
<contactref element="IC5" pad="7"/>
<contactref element="C88" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="IC5" pad="5"/>
<contactref element="R44" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="IC5" pad="9"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="7"/>
<contactref element="R9" pad="2"/>
<contactref element="C89" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="IC15" pad="4"/>
<contactref element="IC4" pad="34"/>
</signal>
<signal name="N$29">
<contactref element="IC4" pad="37"/>
<contactref element="IC16" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="R11" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="LID_SWITCH" pad="NO"/>
</signal>
<signal name="LHOUT1">
<contactref element="LH" pad="1"/>
<contactref element="IC14" pad="P$11"/>
<contactref element="IC14" pad="P$10"/>
<contactref element="IC14" pad="P$9"/>
<contactref element="IC14" pad="P$8"/>
<contactref element="D2" pad="C"/>
<contactref element="LED+HEATER" pad="P$1"/>
<contactref element="LED+HEATER" pad="P$2"/>
<contactref element="LED+HEATER" pad="P$3"/>
<contactref element="LED+HEATER" pad="P$4"/>
<contactref element="LED+HEATER" pad="P$5"/>
<contactref element="LED+HEATER" pad="P$6"/>
</signal>
<signal name="LT_SENSOR">
<contactref element="LH" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="IC4" pad="22"/>
<contactref element="LED+HEATER" pad="P$7"/>
<contactref element="C90" pad="2"/>
</signal>
<signal name="N$53">
<contactref element="R30" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="FAN" pad="2"/>
</signal>
<signal name="N$51">
</signal>
<signal name="N$69">
</signal>
<signal name="OUTA1">
</signal>
<signal name="N$72">
<contactref element="IC13" pad="2"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$73">
</signal>
<signal name="N$74">
</signal>
<signal name="N$76">
</signal>
<signal name="N$77">
</signal>
<signal name="N$78">
</signal>
<signal name="N$80">
</signal>
<signal name="N$81">
</signal>
<signal name="N$82">
</signal>
<signal name="N$83">
</signal>
<signal name="N$84">
</signal>
<signal name="N$85">
</signal>
<signal name="N$86">
</signal>
<signal name="N$87">
</signal>
<signal name="N$88">
</signal>
<signal name="N$89">
</signal>
<signal name="N$90">
</signal>
<signal name="N$91">
</signal>
<signal name="N$92">
</signal>
<signal name="N$93">
</signal>
<signal name="N$94">
</signal>
<signal name="N$95">
</signal>
<signal name="N$96">
</signal>
<signal name="N$97">
</signal>
<signal name="N$98">
</signal>
<signal name="N$99">
</signal>
<signal name="N$100">
</signal>
<signal name="N$101">
</signal>
<signal name="N$102">
</signal>
<signal name="!MCU_RESET">
<contactref element="U10" pad="16"/>
</signal>
<signal name="!MCU_SS">
<contactref element="U10" pad="10"/>
</signal>
<signal name="HEATSINK_ADC_IN">
<contactref element="HST" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="U10" pad="82"/>
</signal>
<signal name="N$50">
</signal>
<signal name="N$9">
</signal>
<signal name="N$49">
<contactref element="IC4" pad="3"/>
<contactref element="R38" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="IC4" pad="35"/>
<contactref element="R39" pad="2"/>
</signal>
<signal name="LIA_REFERENCE_PWM">
<contactref element="IC10" pad="10"/>
<contactref element="R5" pad="1"/>
<contactref element="U10" pad="74"/>
<contactref element="IC3" pad="2"/>
<contactref element="LED+HEATER" pad="P$22"/>
<contactref element="IC8" pad="10"/>
</signal>
<signal name="N$14">
<contactref element="IC14" pad="P$4"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="LIA_IN">
<contactref element="R27" pad="2"/>
<contactref element="C48" pad="1"/>
<contactref element="IC4" pad="21"/>
</signal>
<signal name="V+">
<contactref element="R12" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="IC22" pad="5"/>
<contactref element="IC4" pad="29"/>
<contactref element="C32" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="IC22" pad="6"/>
<contactref element="C67" pad="1"/>
<contactref element="C68" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC22" pad="1"/>
<contactref element="C44" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="R26" pad="2"/>
<contactref element="C47" pad="1"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="IC4" pad="24"/>
<contactref element="IC7" pad="3"/>
</signal>
<signal name="N$31">
<contactref element="IC4" pad="27"/>
<contactref element="IC7" pad="5"/>
</signal>
<signal name="ADCINP">
<contactref element="IC4" pad="25"/>
<contactref element="IC7" pad="2"/>
<contactref element="IC7" pad="1"/>
<contactref element="C49" pad="1"/>
</signal>
<signal name="ADCINN">
<contactref element="IC4" pad="26"/>
<contactref element="IC7" pad="6"/>
<contactref element="IC7" pad="7"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R22" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="IC10" pad="9"/>
</signal>
<signal name="-10V">
<contactref element="IC12" pad="27"/>
<contactref element="C9" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="IC11" pad="4"/>
<contactref element="IC10" pad="8"/>
<contactref element="C8" pad="1"/>
<contactref element="IC7" pad="4"/>
<contactref element="C80" pad="1"/>
<contactref element="C77" pad="1"/>
<contactref element="IC18" pad="27"/>
<contactref element="C82" pad="2"/>
<contactref element="IC17" pad="4"/>
<contactref element="IC8" pad="8"/>
<contactref element="C76" pad="1"/>
<contactref element="IC20" pad="P$5"/>
<contactref element="C95" pad="1"/>
<contactref element="R74" pad="1"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="+10V">
<contactref element="IC12" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="IC11" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R34" pad="1"/>
<contactref element="IC10" pad="11"/>
<contactref element="C78" pad="1"/>
<contactref element="IC18" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="IC17" pad="8"/>
<contactref element="C75" pad="1"/>
<contactref element="IC8" pad="11"/>
<contactref element="R70" pad="1"/>
<contactref element="IC20" pad="P$10"/>
<contactref element="C94" pad="1"/>
<contactref element="R72" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="LED_PWM_CONTROL">
<contactref element="R6" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="LED+HEATER" pad="P$25"/>
</signal>
<signal name="N$22">
<contactref element="R6" pad="2"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="BBB_ADC_GND">
<contactref element="U10" pad="80"/>
<contactref element="HST" pad="2"/>
</signal>
<signal name="BBB_ADC_REF">
<contactref element="U10" pad="78"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="AIN0">
<contactref element="U10" pad="85"/>
</signal>
<signal name="N$35">
<contactref element="BOOT_SW" pad="2"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="+5V/2">
<contactref element="C62" pad="1"/>
<contactref element="C61" pad="1"/>
<contactref element="IC12" pad="18"/>
<contactref element="IC22" pad="4"/>
<contactref element="IC22" pad="3"/>
<contactref element="C43" pad="1"/>
<contactref element="IC4" pad="28"/>
<contactref element="C11" pad="1"/>
<contactref element="IC7" pad="8"/>
<contactref element="C18" pad="1"/>
<contactref element="IC18" pad="18"/>
<contactref element="IC9" pad="P$1"/>
<contactref element="C69" pad="1"/>
<contactref element="IC9" pad="P$2"/>
</signal>
<signal name="N$52">
<contactref element="IC6" pad="5"/>
<contactref element="C55" pad="1"/>
<contactref element="R62" pad="2"/>
</signal>
<signal name="N$55">
<contactref element="C57" pad="1"/>
<contactref element="R62" pad="1"/>
</signal>
<signal name="N$57">
<contactref element="C56" pad="2"/>
<contactref element="R61" pad="2"/>
</signal>
<signal name="N$58">
<contactref element="R61" pad="1"/>
<contactref element="IC6" pad="4"/>
<contactref element="R60" pad="2"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R47" pad="2"/>
<contactref element="R63" pad="1"/>
<contactref element="C56" pad="1"/>
</signal>
<signal name="N$56">
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC11" pad="2"/>
<contactref element="IC12" pad="28"/>
</signal>
<signal name="N$1">
<contactref element="IC6" pad="7"/>
<contactref element="R17" pad="2"/>
<contactref element="C58" pad="1"/>
</signal>
<signal name="SPI_BUSY">
<contactref element="IC13" pad="4"/>
<contactref element="U10" pad="87"/>
</signal>
<signal name="HBT1">
<contactref element="HBT1" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="IC4" pad="9"/>
</signal>
<signal name="HBT2">
<contactref element="HBT2" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="IC4" pad="10"/>
</signal>
<signal name="HBT3">
<contactref element="IC4" pad="13"/>
<contactref element="R21" pad="1"/>
<contactref element="HBT3" pad="1"/>
</signal>
<signal name="HBT4">
<contactref element="IC4" pad="14"/>
<contactref element="HBT4" pad="1"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="HBT5">
<contactref element="IC4" pad="17"/>
</signal>
<signal name="N$16">
<contactref element="R29" pad="2"/>
<contactref element="FAN" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="IC19" pad="4"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="GNDA">
<contactref element="SHORT2" pad="P$2"/>
<contactref element="IC6" pad="3"/>
<contactref element="C55" pad="2"/>
<contactref element="C57" pad="2"/>
<contactref element="R60" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="C45" pad="2"/>
<contactref element="R50" pad="2"/>
<contactref element="R65" pad="2"/>
<contactref element="IC17" pad="1"/>
</signal>
<signal name="N$60">
<contactref element="R66" pad="2"/>
<contactref element="C63" pad="2"/>
<contactref element="C52" pad="2"/>
<contactref element="R65" pad="1"/>
</signal>
<signal name="N$61">
<contactref element="C63" pad="1"/>
<contactref element="R64" pad="1"/>
<contactref element="IC17" pad="6"/>
</signal>
<signal name="N$62">
<contactref element="R64" pad="2"/>
<contactref element="C52" pad="1"/>
<contactref element="IC8" pad="1"/>
<contactref element="IC8" pad="16"/>
<contactref element="IC17" pad="7"/>
</signal>
<signal name="N$63">
<contactref element="IC8" pad="19"/>
<contactref element="IC8" pad="15"/>
<contactref element="IC8" pad="20"/>
</signal>
<signal name="N$64">
<contactref element="IC8" pad="12"/>
<contactref element="IC8" pad="13"/>
<contactref element="R67" pad="1"/>
</signal>
<signal name="N$65">
<contactref element="R67" pad="2"/>
<contactref element="C79" pad="1"/>
<contactref element="R68" pad="1"/>
</signal>
<signal name="N$66">
<contactref element="R69" pad="1"/>
<contactref element="R70" pad="2"/>
<contactref element="IC8" pad="9"/>
</signal>
<signal name="N$67">
<contactref element="C45" pad="1"/>
<contactref element="R50" pad="1"/>
<contactref element="IC17" pad="2"/>
<contactref element="IC18" pad="28"/>
</signal>
<signal name="LIA_IN2">
<contactref element="IC4" pad="18"/>
<contactref element="R68" pad="2"/>
<contactref element="C81" pad="1"/>
</signal>
<signal name="INA1">
<contactref element="IC12" pad="19"/>
<contactref element="PD_REAR" pad="P$2"/>
</signal>
<signal name="INA2">
<contactref element="IC12" pad="20"/>
<contactref element="PD_REAR" pad="P$4"/>
</signal>
<signal name="INA3">
<contactref element="IC12" pad="21"/>
<contactref element="PD_REAR" pad="P$6"/>
</signal>
<signal name="INA4">
<contactref element="IC12" pad="22"/>
<contactref element="PD_REAR" pad="P$8"/>
</signal>
<signal name="INA5">
<contactref element="IC12" pad="23"/>
<contactref element="PD_REAR" pad="P$10"/>
</signal>
<signal name="INA6">
<contactref element="IC12" pad="24"/>
<contactref element="PD_REAR" pad="P$12"/>
</signal>
<signal name="INA7">
<contactref element="IC12" pad="25"/>
<contactref element="PD_REAR" pad="P$14"/>
</signal>
<signal name="INA8">
<contactref element="IC12" pad="26"/>
<contactref element="PD_REAR" pad="P$16"/>
</signal>
<signal name="INA9">
<contactref element="IC12" pad="11"/>
<contactref element="PD_FRONT" pad="P$16"/>
</signal>
<signal name="INA10">
<contactref element="IC12" pad="10"/>
<contactref element="PD_FRONT" pad="P$14"/>
</signal>
<signal name="INA11">
<contactref element="IC12" pad="9"/>
<contactref element="PD_FRONT" pad="P$12"/>
</signal>
<signal name="INA12">
<contactref element="IC12" pad="8"/>
<contactref element="PD_FRONT" pad="P$10"/>
</signal>
<signal name="INA13">
<contactref element="IC12" pad="7"/>
<contactref element="PD_FRONT" pad="P$8"/>
</signal>
<signal name="INA14">
<contactref element="IC12" pad="6"/>
<contactref element="PD_FRONT" pad="P$6"/>
</signal>
<signal name="INA15">
<contactref element="IC12" pad="5"/>
<contactref element="PD_FRONT" pad="P$4"/>
</signal>
<signal name="INA16">
<contactref element="IC12" pad="4"/>
<contactref element="PD_FRONT" pad="P$2"/>
</signal>
<signal name="INB1">
<contactref element="IC18" pad="19"/>
<contactref element="PD_REAR" pad="P$3"/>
</signal>
<signal name="INB2">
<contactref element="IC18" pad="20"/>
<contactref element="PD_REAR" pad="P$5"/>
</signal>
<signal name="INB3">
<contactref element="IC18" pad="21"/>
<contactref element="PD_REAR" pad="P$7"/>
</signal>
<signal name="INB4">
<contactref element="IC18" pad="22"/>
<contactref element="PD_REAR" pad="P$9"/>
</signal>
<signal name="INB5">
<contactref element="IC18" pad="23"/>
<contactref element="PD_REAR" pad="P$11"/>
</signal>
<signal name="INB6">
<contactref element="IC18" pad="24"/>
<contactref element="PD_REAR" pad="P$13"/>
</signal>
<signal name="INB7">
<contactref element="IC18" pad="25"/>
<contactref element="PD_REAR" pad="P$15"/>
</signal>
<signal name="INB8">
<contactref element="IC18" pad="26"/>
<contactref element="PD_REAR" pad="P$17"/>
</signal>
<signal name="INB9">
<contactref element="IC18" pad="11"/>
<contactref element="PD_FRONT" pad="P$17"/>
</signal>
<signal name="INB10">
<contactref element="IC18" pad="10"/>
<contactref element="PD_FRONT" pad="P$15"/>
</signal>
<signal name="INB11">
<contactref element="IC18" pad="9"/>
<contactref element="PD_FRONT" pad="P$13"/>
</signal>
<signal name="INB12">
<contactref element="IC18" pad="8"/>
<contactref element="PD_FRONT" pad="P$11"/>
</signal>
<signal name="INB13">
<contactref element="IC18" pad="7"/>
<contactref element="PD_FRONT" pad="P$9"/>
</signal>
<signal name="INB14">
<contactref element="IC18" pad="6"/>
<contactref element="PD_FRONT" pad="P$7"/>
</signal>
<signal name="INB15">
<contactref element="IC18" pad="5"/>
<contactref element="PD_FRONT" pad="P$5"/>
</signal>
<signal name="INB16">
<contactref element="IC18" pad="4"/>
<contactref element="PD_FRONT" pad="P$3"/>
</signal>
<signal name="MUX0">
<contactref element="IC23" pad="P$2"/>
<contactref element="U10" pad="57"/>
</signal>
<signal name="MUX1">
<contactref element="IC23" pad="P$5"/>
<contactref element="U10" pad="59"/>
</signal>
<signal name="MUX2">
<contactref element="IC23" pad="P$12"/>
<contactref element="U10" pad="61"/>
</signal>
<signal name="MUX3">
<contactref element="IC23" pad="P$9"/>
<contactref element="U10" pad="58"/>
</signal>
<signal name="N$68">
<contactref element="IC20" pad="P$6"/>
<contactref element="C92" pad="1"/>
</signal>
<signal name="C+">
<contactref element="IC20" pad="P$8"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="C-">
<contactref element="IC20" pad="P$7"/>
<contactref element="C21" pad="2"/>
</signal>
<signal name="ADJ+">
<contactref element="IC20" pad="P$13"/>
<contactref element="R73" pad="2"/>
<contactref element="R72" pad="1"/>
</signal>
<signal name="BYP+">
<contactref element="IC20" pad="P$14"/>
<contactref element="C97" pad="1"/>
</signal>
<signal name="BYP-">
<contactref element="IC20" pad="P$3"/>
<contactref element="C98" pad="2"/>
</signal>
<signal name="ADJ-">
<contactref element="IC20" pad="P$4"/>
<contactref element="R74" pad="2"/>
<contactref element="R75" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC20" pad="P$2"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="IC20" pad="P$1"/>
<contactref element="IC20" pad="P$11"/>
<contactref element="C96" pad="1"/>
<contactref element="C71" pad="1"/>
<contactref element="C19" pad="+"/>
<contactref element="IC20" pad="P$9"/>
<contactref element="L2" pad="2"/>
<contactref element="C73" pad="1"/>
<contactref element="C93" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC6" pad="8"/>
<contactref element="L4" pad="P$2"/>
</signal>
<signal name="N$21">
<contactref element="L7" pad="2"/>
<contactref element="C59" pad="1"/>
<contactref element="C65" pad="1"/>
<contactref element="C60" pad="1"/>
<contactref element="C64" pad="1"/>
<contactref element="IC9" pad="P$8"/>
<contactref element="IC9" pad="P$5"/>
</signal>
<signal name="N$25">
<contactref element="IC1" pad="8"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="R37" pad="1"/>
<contactref element="IC5" pad="8"/>
</signal>
<signal name="N$39">
</signal>
<signal name="N$59">
<contactref element="IC9" pad="P$4"/>
<contactref element="C69" pad="2"/>
</signal>
<signal name="F12V">
<contactref element="C17" pad="+"/>
<contactref element="C91" pad="1"/>
<contactref element="IC6" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C83" pad="1"/>
<contactref element="L5" pad="2"/>
</signal>
<signal name="GND4">
<contactref element="R19" pad="1"/>
</signal>
<signal name="GND3">
<contactref element="R20" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="R23" pad="1"/>
</signal>
<signal name="GND1">
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="L1" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="C28" pad="+"/>
<contactref element="C29" pad="1"/>
<contactref element="C30" pad="1"/>
</signal>
<signal name="N$15">
</signal>
</signals>
</board>
</drawing>
</eagle>
