(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 66)
    (zones 0)
    (modules 7)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad10)")
  (net 2 "Net-(J1-Pad9)")
  (net 3 "Net-(J1-Pad8)")
  (net 4 "Net-(J1-Pad7)")
  (net 5 "Net-(J1-Pad6)")
  (net 6 "Net-(J1-Pad5)")
  (net 7 "Net-(J1-Pad4)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x10_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 121.6 94.3)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference J3 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Conn_01x10 (at 0 13.125) (layer F.Fab))
    (fp_text user %R (at 0 5.715 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 11.43) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 8.89) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 6.35) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 127 109.75)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 107.75 109.75)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 127 90.25)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 -3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 107.75 90.25)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 -3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 125 94.925)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J2 (at -2.75 5.064) (layer F.SilkS) hide)
    (fp_text value Conn_01x10 (at 4.2 5.064 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module wgmt-conn:TE_1-1734592-0 (layer F.Cu) (tedit 5E55F008)
    (at 113.75 100 270)
    (fp_text reference J1 (at -0.011 2.5 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10 (at 0.239 5.75 90) (layer F.Fab))
    (pad S2 smd rect (at 3.92 1.7 270) (size 2.3 3.1) (layers F.Cu F.Paste F.Mask))
    (pad S1 smd rect (at -3.92 1.7 270) (size 2.3 3.1) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.25 0 270) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad10)"))
    (pad 9 smd rect (at 1.75 0 270) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad9)"))
    (pad 8 smd rect (at 1.25 0 270) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad8)"))
    (pad 7 smd rect (at 0.75 0 270) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad7)"))
    (pad 6 smd rect (at 0.25 0 270) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at -0.25 0 270) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 4 smd rect (at -0.75 0 270) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at -1.25 0 270) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -1.75 0 270) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -2.25 0 270) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad1)"))
  )
  (gr_text 1 (at 123.1 92.5) (layer F.SilkS))
  (gr_text 1 (at 115.2 96.6) (layer F.SilkS))
  (gr_text "FPC Breakout\n10pos 0.5mm" (at 117.6 100 90) (layer B.SilkS))
  (gr_arc (start 128 110.7) (end 128 112.7) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.6 110.7) (end 104.6 110.7) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 128 89.3) (end 130 89.3) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.6 89.3) (end 106.6 87.3) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104.6 89.3) (end 104.6 110.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 130 89.3) (end 130 110.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.6 112.7) (end 128 112.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.6 87.3) (end 128 87.3) (layer Edge.Cuts) (width 0.05))
  (dimension 25.5 (width 0.15) (layer Dwgs.User)
    (gr_text "25.500 mm" (at 139.3 87.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 131 100) (xy 138.586421 100)))
    (feature2 (pts (xy 131 74.5) (xy 138.586421 74.5)))
    (crossbar (pts (xy 138 74.5) (xy 138 100)))
    (arrow1a (pts (xy 138 100) (xy 137.413579 98.873496)))
    (arrow1b (pts (xy 138 100) (xy 138.586421 98.873496)))
    (arrow2a (pts (xy 138 74.5) (xy 137.413579 75.626504)))
    (arrow2b (pts (xy 138 74.5) (xy 138.586421 75.626504)))
  )
  (dimension 25.5 (width 0.15) (layer Dwgs.User)
    (gr_text "25.500 mm" (at 117 66.200001) (layer Dwgs.User))
    (feature1 (pts (xy 129.75 70) (xy 129.75 66.91358)))
    (feature2 (pts (xy 104.25 70) (xy 104.25 66.91358)))
    (crossbar (pts (xy 104.25 67.500001) (xy 129.75 67.500001)))
    (arrow1a (pts (xy 129.75 67.500001) (xy 128.623496 68.086422)))
    (arrow1b (pts (xy 129.75 67.500001) (xy 128.623496 66.91358)))
    (arrow2a (pts (xy 104.25 67.500001) (xy 105.376504 68.086422)))
    (arrow2b (pts (xy 104.25 67.500001) (xy 105.376504 66.91358)))
  )
)
